**3GPP TSG-SA3 Meeting #84-LI-e-a *s3i220020***

**Online, , 24th Jan 2022 - 28th Jan 2022**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **33.128** | **CR** | **0301** | **rev** | **-** | **Current version:** | **17.3.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Fixing parameter names |
|  |  |
| ***Source to WG:*** | SA3LI (National Technical Assistance, Nokia, Nokia Shanghai Bell) |
| ***Source to TSG:*** | SA3 |
|  |  |
| ***Work item code:*** | LI17 |  | ***Date:*** | 2022-01-26 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | Type names related to IP addresses in Table 6.2.3-7 don't match the actual names in ETSI TS 103 221-1. |
|  |  |
| ***Summary of change:*** | The type names are corrected. |
|  |  |
| ***Consequences if not approved:*** | Developers are unecessarily baffled. |
|  |  |
| ***Clauses affected:*** | 6.2.3.3.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

 FIRST CHANGE

#### 6.2.3.3 Triggering of the CC-POI from CC-TF over LI\_T3

##### 6.2.3.3.1 LI\_T3 interface specifics

When interception of communication contents is authorised or the delivery of packet header information is authorised and approach 2 described in clause 6.2.3.5 is used, the CC-TF present in the SMF sends a trigger to the CC-POI present in the UPF over the LI\_T3 interface.

When the CC-TF in the SMF detects that a PDU session is being established for a target UE (i.e. when the SMF sends the N4: Session Establishment Request), it shall send an activation message to the CC-POI in the UPF over the LI\_T3 interface. The activation message shall contain the correlation identifiers that the CC-POI in the UPF shall use with the xCC. This can be achieved by sending an ActivateTask message as defined in ETSI TS 103 221-1 [7] clause 6.2.1 with the following details.

Table 6.2.3-6: ActivateTask message for triggering the CC-POI in the UPF

|  |  |  |
| --- | --- | --- |
| ETSI TS 103 221-1 [7] field name | Description | M/C/O |
| XID | Allocated by the CC-TF as per ETSI TS 103 221-1 [7]. | M |
| TargetIdentifiers | Packet detection criteria as determined by the CC-TF in the SMF, which enables the UPF to isolate target traffic. The CC-POI in the UPF shall support at least the identifier types given in Table 6.2.3-7.NOTE: This value is the target identifier for the CC-POI in the UPF and may be different from the target identifier specified in the warrant. | M |
| DeliveryType | Set to “X3Only”. | M |
| ListOfDIDs | Delivery endpoints for LI\_X3. These delivery endpoints shall be configured by the CC-TF in the SMF using the CreateDestination message as described in ETSI TS 103 221-1 [7] clause 6.3.1 prior to first use. | M |
| CorrelationID | Correlation ID to assign to X3 PDUs generated by the CC-POI in the UPF. This field is populated with the same CorrelationID the IRI-POI in the SMF uses for the associated xIRI. | M |
| ProductID | Shall be set to the XID of the Task Object associated with the interception at the CC-TF. This value shall be used by the CC-POI in the UPF to fill the XID of X3 PDUs. | M |

Table 6.2.3-7: Target Identifier Types for LI\_T3

|  |  |  |  |
| --- | --- | --- | --- |
| Identifier type | Owner | ETSI TS 103 221-1 [7] TargetIdentifier type | Definition |
| GTP Tunnel ID | 3GPP | gtpuTunnelId | F-TEID (see XSD schema) |
| UE IP Address | ETSI | IPv4Address or IPv6Address | See ETSI TS 103 221-1 [7] |
| UE port | ETSI | TCPPort or UDPPort | See ETSI TS 103 221-1 [7] |
| PFCP Session ID | 3GPP | TargetIdentifierExtension / FSEID | F-SEID (see XSD schema) |
| PDR ID | 3GPP | TargetIdentifierExtension / PDRID | 32 bit unsigned integer (see XSD schema) |
| QER ID | 3GPP | TargetIdentifierExtension / QERID | 32 bit unsigned integer (see XSD schema) |
| Network Instance | 3GPP | TargetIdentifierExtension / NetworkInstance | Octet string (see XSD schema) |
| GTP Tunnel Direction | 3GPP | TargetIdentifierExtension / GTPTunnelDirection | Enumeration (see XSD schema) |

When the CC-TF in the SMF detects that a targeted PDU session is changing (i.e. when the SMF sends the N4 Session Modification Request to the UPF) in a way that requires changes to the interception already activated by the CC-POI in the UPF, the CC-TF shall modify the interception at the CC-POI in the UPF over the LI\_T3 interface. This is achieved by sending a ModifyTask message as defined in ETSI TS 103 221-1 [7] clause 6.2.2. The ModifyTask message contains the same details as the ActivateTask message with the following fields updated as appropriate.

Table 6.2.3-8: Parameters that may be changed in a ModifyTask message when updating interception at the CC-POI in the UPF

|  |  |  |
| --- | --- | --- |
| ETSI TS 103 221-1 [7] field name | Description | M/C/O |
| TargetIdentifiers | Updated packet detection criteria as determined by the CC-TF in the SMF.NOTE: See notes on TargetIdentifiers in Table 6.2.3-6. | M |

When the CC-TF in the SMF detects that a targeted PDU session is changing (i.e. when the SMF sends the N4 Session Modification Request to the UPF) for which the interception had not been previously activated in the CC-POI in the UPF (e.g. in case of previous unsuccessful LI activation at the CC-POI in the UPF by the CC-TF in the SMF), the CC-TF shall send an activation message to the CC-POI in the UPF over the LI\_T3 interface. The activation message shall contain the correlation identifiers that the CC-POI in the UPF shall use with the xCC. This can be achieved by sending an ActivateTask message as defined in ETSI TS 103 221-1 [7] clause 6.2.1 with the details provided by Table 6.2.3-6.

When the CC-TF in the SMF detects that the PDU session has been released (i.e. when the SMF sends the N4: Session Release Request to the UPF) for a target UE, it shall send a deactivation message to the CC-POI in the UPF over the LI\_T3 interface. When using ETSI TS 103 221-1 [7] this is achieved by sending a DeactivateTask message with the XID field set to the XID associated with the interception, as described in ETSI TS 103 221-1 [7] clause 6.2.3.

By default, interception shall occur at the anchor UPF as described in 6.2.3.3.3.

When a warrant that includes the service scoping of CC is activated for a target UE with an established PDU session and when the IRI-POI present in the SMF generates the xIRI containing an SMFStartOfInterceptionWithEstablishedPDUSession record (see clause 6.2.3.2.5), the CC-TF present in the SMF shall send an activation message to the CC-POI present in the UPF to generate the xCC.