**3GPP TSG-SA3 Meeting #84-LI-e-a *s3i220022***

**Online, , 24th Jan 2022 - 28th Jan 2022**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **33.128** | **CR** | **0302** | **rev** | **1** | **Current version:** | **17.3.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Clarification of LI at the UDM | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | SA3-LI (OTD) | | | | | | | | | |
| ***Source to TSG:*** | SA3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | LI17 | | | | |  | ***Date:*** | | | 2022-01-24 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | In review of the current 33.128 support for LI at the UDM, it was discovered that an empty clause, 7.2.2.3.5, existed. To accompany this, there was also no method to report information requests to the UDM nor UE authentication requests. These clauses are also added. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Build out of 7.2.2.3.5 Location Information result, add two new clauses for reporting of information available at the UDM. Modify and add to existing ASN.1 to support the newly defined capability. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | CSPs will not be able to fully meet their LI obligations. Information available at the UDM will not be fully reported to LEAs. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 7.2.2.3.X (new), 7.2.2.3.Y (new), 7.2.2.3.Z (new), Annex A (ASN.1) | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | Related to CR 0157 (s3i220023).  The ASN.1 for this change can be found on the Forge  Merge Request: <https://forge.3gpp.org/rep/sa3/li/-/merge_requests/9>  Commit hash: <https://forge.3gpp.org/rep/sa3/li/-/merge_requests/9/diffs?commit_id=7ed26f72521119653f42a1aa2a95d24b32941b56> | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

\*\*\*START OF CHANGES \*\*\*

\*\*\*START OF FIRST CHANGE \*\*\*

##### 7.2.2.3.X Location information result

The IRI-POI in the UDM shall generate an xIRI containing the UDMLocationInformationResult record when it detects the following events:

- When UDM receives the LocationInfoRequest from an NF service consumer (i.e. HSS) as part of Nudm\_MT\_ProvideLocationInfo service operation (see TS 29.503 [25], clause 6.7.6.2.3) and the UDM sends the LocationInfoResult as part of Nudm\_MT\_ProvideLocationInfo service operation (see TS 29.503 [25], clause 6.7.6.2.4).

When a target UE is registered to both 3GPP and non-3GPP access, two separate xIRIs each containing the LocationInfoResult report record may be generated by the IRI-POI in the UDM.

Table 7.2.2.3.X-1: Payload for UDMLocationInfoResult record

|  |  |  |
| --- | --- | --- |
| Field name | Description | M/C/O |
| sUPI | SUPI currently associated with the target, see TS 29.571 [17]. | M |
| pEI | PEI currently associated with the target UE, when known, see TS 29.571 [17]. | C |
| gPSI | GPSI currently associated with the target UE, when known, see TS 29.571 [17]. | C |
| locationInfoRequest | Indicates the information requested in the LocationInfoRequest sent to the UDM from the HSS. At least one of the parameters in Table 7.2.2.3.X-2 shall be included. See NOTE below table 7.2.2.3.X-2. | M |
| vPLMNId | PLMNID of the visited PLMN, if UE is currently registered to visited network. | C |
| currentLocationIndicator | Shall indicate if the UE location is current or last known. Include if provided in the LocationInfoResult. | C |
| aMFinstanceID | Provides the NF instance ID of the serving AMF for 3GPP access. Shall be included if provided in the LocationInfoResult. | C |
| sMSFinstanceID | Provides the NF instance ID of the serving SMSF. Shall be included if provided in the LocationInfoResult. | C |
| location | Location information available at the UDM at the time of the LocationInfoRequest, include if in LocationInfoResult. Location information may be suppressed if location is not provided in the Service Scoping options, see clause 5.2.4. | C |
| rATType | Shall provide the current RAT type of the UE, if present in the LocationInfoResult. | C |
| problemDetails | Indicates the reason for LocationInfoResult failure. See TS 29.571 [17], clause 5.2.4.1. Shall be included if provided in the LocationInfoResult. | C |

Table 7.2.2.3.X-2: Payload for LocationInfoRequest parameter

|  |  |
| --- | --- |
| Field name | Description |
| req5GSLocation | Boolean that indicates If 5GS location is requested. |
| reqCurrentLocation | Boolean that indicates if current location is requested. |
| reqRatType | Boolean indicates if Rat Type is requested. |
| reqTimeZone | Boolean indicates if time zone is requested. |
| reqServingNode | Boolean indicates if serving node instance ID is requested. |

NOTE: The absence of one or more of the parameters in table 7.2.2.3.X-2 assumes that it was not included in the LocationInfoRequest.

##### 7.2.2.3.Y UE Information request

The IRI-POI in the UDM shall generate an xIRI containing the UDMUEInfromationRequest record when it detects the following events:

- When the UDM receives the ProvideUeInfo GET request from the NF service consumer as part of Nudm\_MT\_ProvideUeInfo service operation (see TS 29.503 [25], clause 6.7.6.2.2) and the UDM returns a UeInfo response.

Table 7.2.2.3.Y-1: Payload for UDMUEInformationResponse record

|  |  |  |
| --- | --- | --- |
| Field name | Description | M/C/O |
| sUPI | SUPI currently associated with the target UE, see TS 29.571 [17]. | M |
| tADSInfo | Contains the UE Context Information as known at the UDM. See TS 29.518 [22], clause 6.3.6.2.4. Shall be included if UE Context is returned in the UeInfo response. | C |
| fiveGSUserStateInfo | Describes the 5GS user state of the UE as known at the UDM. See TS 29.518 [22], clause 6.2.6.3.11. Shall be included if 5GS user state is returned in the UeInfo response. | C |
| fiveGSRVCCInfo | Indicates whether the UE supports 5G SRVCC. See TS 29.503 [25], clause 6.7.6.2.5. Shall be included if returned in the UeInfo response. | C |
| problemDetails | Indicates the reason for UeInfo response failure. See TS 29.571 [17], clause 5.2.4.1. Shall be included if provided in the UeInfo response. | C |

##### 7.2.2.3.Z UE Authentication report

The IRI-POI in the UDM shall generate an xIRI containing the UDMUEAuthenticationReport record when it detects the following events:

- When the UDM receives the AuthenticationInfoRequest from the AUSF as part of Nudm\_UEAuthentication service operation (see TS 29.503 [25], clause 6.3.6.2.2) and the UDM sends the AuthenticationInfoResult to the AUSF as part of the Nudm\_UEAuthentication service operation (see TS 29.503 [25], clause 6.3.6.2.3).

- When the UDM receives the HSSAuthenticationInfoRequest from the HSS as part of the Nudm\_UEAuthentication service operation (see TS 29.503 [25], clause 6.3.6.2.10) and the UDM sends the HSSAuthenticationInfoResult to the AUSF as part of the Nudm\_UEAuthentication service operation (see TS 29.503 [25], clause 6.3.6.2.11).

When a target UE registers from both 3GPP and non-3GPP access, two separate xIRIs each containing the UDMUEAuthentication report record may be generated by the IRI-POI in the UDM.

Table 7.2.2.3.Z-1: Payload for UDMUEAuthenticationInfoResponse record

|  |  |  |
| --- | --- | --- |
| Field name | Description | M/C/O |
| sUPI | SUPI currently associated with the target UE, see TS 29.571 [17]. | M |
| authenticationInfoRequest | Indicateds information provided in the UEAuthenticationInfoRequest. See Table 7.2.2.3.Z-2 for details of payload. | M |
| aKMAIndicator | Indicates whether AKMA keys are needed for the UE, Shall be included if AKMA keys are requested in the AuthenticationInfoRequest. | C |
| problemDetails | Shall Indicate reason for AuthenticationInfoResultfailure. Shall be included if failure occurs. See TS 29.571 [17], clause 5.2.4.1. | C |

Table 7.2.2.3.Z-2: Payload for AuthenticationInfoRequest parameter

|  |  |  |
| --- | --- | --- |
| Field name | Description | M/C/O |
| infoRequestType | Indicates whether the AuthenticationInfoRequest was sent by the HSS, AUSF or other. | M |
| rGAuthCtx | Contains the UE ID (i.e. SUPI, SUCI) provided in the authentication indication, at least one shall be present. | M |
| authType | Indicates the authentication method provided by the HSS or AUSF in the AuthenticationInfoRequest. | M |
| servingNetworkName | Serving network name. See TS 33.501 [11] clause 6.1.1.4. | M |
| aUSFInstanceID | Identifies the AUSF instance which generated the AuthenticationInformatoinRequest. Shall be included if known. | C |
| cellCagInfo | Provides CAG cell information (e.g. CAGId) if UE is attempting registration from a CAG. | C |
| n5GCIndicator | Boolean value that indicates whether the device is a N5GC device. Include if provided in the AuthenticationInfoRequest. | C |

\*\*\*END OF FIRST CHANGE \*\*\*

\*\*\*START OF SECOND CHANGE \*\*\*

Annex A (normative):  
ASN.1 Schema for the Internal and External Interfaces

TS33128Payloads

{itu-t(0) identified-organization(4) etsi(0) securityDomain(2) lawfulIntercept(2) threeGPP(4) ts33128(19) r17(17) version2(2)}

DEFINITIONS IMPLICIT TAGS EXTENSIBILITY IMPLIED ::=

BEGIN

-- =============

-- Relative OIDs

-- =============

tS33128PayloadsOID RELATIVE-OID ::= {threeGPP(4) ts33128(19) r17(17) version2(2)}

xIRIPayloadOID RELATIVE-OID ::= {tS33128PayloadsOID xIRI(1)}

xCCPayloadOID RELATIVE-OID ::= {tS33128PayloadsOID xCC(2)}

iRIPayloadOID RELATIVE-OID ::= {tS33128PayloadsOID iRI(3)}

cCPayloadOID RELATIVE-OID ::= {tS33128PayloadsOID cC(4)}

lINotificationPayloadOID RELATIVE-OID ::= {tS33128PayloadsOID lINotification(5)}

-- ===============

-- X2 xIRI payload

-- ===============

XIRIPayload ::= SEQUENCE

{

xIRIPayloadOID [1] RELATIVE-OID,

event [2] XIRIEvent

}

XIRIEvent ::= CHOICE

{

-- Access and mobility related events, see clause 6.2.2

registration [1] AMFRegistration,

deregistration [2] AMFDeregistration,

locationUpdate [3] AMFLocationUpdate,

startOfInterceptionWithRegisteredUE [4] AMFStartOfInterceptionWithRegisteredUE,

unsuccessfulAMProcedure [5] AMFUnsuccessfulProcedure,

-- PDU session-related events, see clause 6.2.3

pDUSessionEstablishment [6] SMFPDUSessionEstablishment,

pDUSessionModification [7] SMFPDUSessionModification,

pDUSessionRelease [8] SMFPDUSessionRelease,

startOfInterceptionWithEstablishedPDUSession [9] SMFStartOfInterceptionWithEstablishedPDUSession,

unsuccessfulSMProcedure [10] SMFUnsuccessfulProcedure,

-- Subscriber-management related events, see clause 7.2.2

servingSystemMessage [11] UDMServingSystemMessage,

-- SMS-related events, see clause 6.2.5, see also sMSReport ([56] below)

sMSMessage [12] SMSMessage,

-- LALS-related events, see clause 7.3.3

lALSReport [13] LALSReport,

-- PDHR/PDSR-related events, see clause 6.2.3.4.1

pDHeaderReport [14] PDHeaderReport,

pDSummaryReport [15] PDSummaryReport,

-- tag 16 is reserved because there is no equivalent mDFCellSiteReport in XIRIEvent

-- MMS-related events, see clause 7.4.2

mMSSend [17] MMSSend,

mMSSendByNonLocalTarget [18] MMSSendByNonLocalTarget,

mMSNotification [19] MMSNotification,

mMSSendToNonLocalTarget [20] MMSSendToNonLocalTarget,

mMSNotificationResponse [21] MMSNotificationResponse,

mMSRetrieval [22] MMSRetrieval,

mMSDeliveryAck [23] MMSDeliveryAck,

mMSForward [24] MMSForward,

mMSDeleteFromRelay [25] MMSDeleteFromRelay,

mMSDeliveryReport [26] MMSDeliveryReport,

mMSDeliveryReportNonLocalTarget [27] MMSDeliveryReportNonLocalTarget,

mMSReadReport [28] MMSReadReport,

mMSReadReportNonLocalTarget [29] MMSReadReportNonLocalTarget,

mMSCancel [30] MMSCancel,

mMSMBoxStore [31] MMSMBoxStore,

mMSMBoxUpload [32] MMSMBoxUpload,

mMSMBoxDelete [33] MMSMBoxDelete,

mMSMBoxViewRequest [34] MMSMBoxViewRequest,

mMSMBoxViewResponse [35] MMSMBoxViewResponse,

-- PTC-related events, see clause 7.5.2

pTCRegistration [36] PTCRegistration,

pTCSessionInitiation [37] PTCSessionInitiation,

pTCSessionAbandon [38] PTCSessionAbandon,

pTCSessionStart [39] PTCSessionStart,

pTCSessionEnd [40] PTCSessionEnd,

pTCStartOfInterception [41] PTCStartOfInterception,

pTCPreEstablishedSession [42] PTCPreEstablishedSession,

pTCInstantPersonalAlert [43] PTCInstantPersonalAlert,

pTCPartyJoin [44] PTCPartyJoin,

pTCPartyDrop [45] PTCPartyDrop,

pTCPartyHold [46] PTCPartyHold,

pTCMediaModification [47] PTCMediaModification,

pTCGroupAdvertisement [48] PTCGroupAdvertisement,

pTCFloorControl [49] PTCFloorControl,

pTCTargetPresence [50] PTCTargetPresence,

pTCParticipantPresence [51] PTCParticipantPresence,

pTCListManagement [52] PTCListManagement,

pTCAccessPolicy [53] PTCAccessPolicy,

-- More Subscriber-management related events, see clause 7.2.2

subscriberRecordChangeMessage [54] UDMSubscriberRecordChangeMessage,

cancelLocationMessage [55] UDMCancelLocationMessage,

-- SMS-related events continued from choice 12

sMSReport [56] SMSReport,

-- MA PDU session-related events, see clause 6.2.3.2.7

sMFMAPDUSessionEstablishment [57] SMFMAPDUSessionEstablishment,

sMFMAPDUSessionModification [58] SMFMAPDUSessionModification,

sMFMAPDUSessionRelease [59] SMFMAPDUSessionRelease,

startOfInterceptionWithEstablishedMAPDUSession [60] SMFStartOfInterceptionWithEstablishedMAPDUSession,

unsuccessfulMASMProcedure [61] SMFMAUnsuccessfulProcedure,

-- Identifier Association events, see clauses 6.2.2.2.7 and 6.3.2.2.2

aMFIdentifierAssociation [62] AMFIdentifierAssociation,

mMEIdentifierAssociation [63] MMEIdentifierAssociation,

-- PDU to MA PDU session-related events, see clause 6.2.3.2.8

sMFPDUtoMAPDUSessionModification [64] SMFPDUtoMAPDUSessionModification,

-- NEF services related events, see clause 7.7.2

nEFPDUSessionEstablishment [65] NEFPDUSessionEstablishment,

nEFPDUSessionModification [66] NEFPDUSessionModification,

nEFPDUSessionRelease [67] NEFPDUSessionRelease,

nEFUnsuccessfulProcedure [68] NEFUnsuccessfulProcedure,

nEFStartOfInterceptionWithEstablishedPDUSession [69] NEFStartOfInterceptionWithEstablishedPDUSession,

nEFdeviceTrigger [70] NEFDeviceTrigger,

nEFdeviceTriggerReplace [71] NEFDeviceTriggerReplace,

nEFdeviceTriggerCancellation [72] NEFDeviceTriggerCancellation,

nEFdeviceTriggerReportNotify [73] NEFDeviceTriggerReportNotify,

nEFMSISDNLessMOSMS [74] NEFMSISDNLessMOSMS,

nEFExpectedUEBehaviourUpdate [75] NEFExpectedUEBehaviourUpdate,

-- SCEF services related events, see clause 7.8.2

sCEFPDNConnectionEstablishment [76] SCEFPDNConnectionEstablishment,

sCEFPDNConnectionUpdate [77] SCEFPDNConnectionUpdate,

sCEFPDNConnectionRelease [78] SCEFPDNConnectionRelease,

sCEFUnsuccessfulProcedure [79] SCEFUnsuccessfulProcedure,

sCEFStartOfInterceptionWithEstablishedPDNConnection [80] SCEFStartOfInterceptionWithEstablishedPDNConnection,

sCEFdeviceTrigger [81] SCEFDeviceTrigger,

sCEFdeviceTriggerReplace [82] SCEFDeviceTriggerReplace,

sCEFdeviceTriggerCancellation [83] SCEFDeviceTriggerCancellation,

sCEFdeviceTriggerReportNotify [84] SCEFDeviceTriggerReportNotify,

sCEFMSISDNLessMOSMS [85] SCEFMSISDNLessMOSMS,

sCEFCommunicationPatternUpdate [86] SCEFCommunicationPatternUpdate,

-- EPS Events, see clause 6.3

-- MME Events, see clause 6.3.2.2

mMEAttach [87] MMEAttach,

mMEDetach [88] MMEDetach,

mMELocationUpdate [89] MMELocationUpdate,

mMEStartOfInterceptionWithEPSAttachedUE [90] MMEStartOfInterceptionWithEPSAttachedUE,

mMEUnsuccessfulProcedure [91] MMEUnsuccessfulProcedure,

-- AKMA key management events, see clause 7.9.1

aAnFAnchorKeyRegister [92] AAnFAnchorKeyRegister,

aAnFKAKMAApplicationKeyGet [93] AAnFKAKMAApplicationKeyGet,

aAnFStartOfInterceptWithEstablishedAKMAKeyMaterial [94] AAnFStartOfInterceptWithEstablishedAKMAKeyMaterial,

aAnFAKMAContextRemovalRecord [95] AAnFAKMAContextRemovalRecord,

aFAKMAApplicationKeyRefresh [96] AFAKMAApplicationKeyRefresh,

aFStartOfInterceptWithEstablishedAKMAApplicationKey [97] AFStartOfInterceptWithEstablishedAKMAApplicationKey,

aFAuxiliarySecurityParameterEstablishment [98] AFAuxiliarySecurityParameterEstablishment,

aFApplicationKeyRemoval [99] AFApplicationKeyRemoval,

-- HR LI Events, see clause 7.10.3.3

n9HRPDUSessionInfo [100] N9HRPDUSessionInfo,

s8HRBearerInfo [101] S8HRBearerInfo,

-- Separated Location Reporting, see clause 7.3.4

separatedLocationReporting [102] SeparatedLocationReporting,

-- STIR SHAKEN and RCD/eCNAM Events, see clause 7.11.2

sTIRSHAKENSignatureGeneration [103] STIRSHAKENSignatureGeneration,

sTIRSHAKENSignatureValidation [104] STIRSHAKENSignatureValidation,

-- IMS events, see clause 7.11.4.2

iMSMessage [105] IMSMessage,

startOfInterceptionForActiveIMSSession [106] StartOfInterceptionForActiveIMSSession,

-- UDM events, see clause 7.2.2

uDMLocationInformationResult [904] UDMLocationInformationResult,

uDMUEInformationResponse [905] UDMUEInformationResponse,

uDMUEAuthenticationResponse [906] UDMUEAuthenticationResponse

}

-- ==============

-- X3 xCC payload

-- ==============

-- No additional xCC payload definitions required in the present document.

-- ===============

-- HI2 IRI payload

-- ===============

IRIPayload ::= SEQUENCE

{

iRIPayloadOID [1] RELATIVE-OID,

event [2] IRIEvent,

targetIdentifiers [3] SEQUENCE OF IRITargetIdentifier OPTIONAL

}

IRIEvent ::= CHOICE

{

-- Registration-related events, see clause 6.2.2

registration [1] AMFRegistration,

deregistration [2] AMFDeregistration,

locationUpdate [3] AMFLocationUpdate,

startOfInterceptionWithRegisteredUE [4] AMFStartOfInterceptionWithRegisteredUE,

unsuccessfulRegistrationProcedure [5] AMFUnsuccessfulProcedure,

-- PDU session-related events, see clause 6.2.3

pDUSessionEstablishment [6] SMFPDUSessionEstablishment,

pDUSessionModification [7] SMFPDUSessionModification,

pDUSessionRelease [8] SMFPDUSessionRelease,

startOfInterceptionWithEstablishedPDUSession [9] SMFStartOfInterceptionWithEstablishedPDUSession,

unsuccessfulSessionProcedure [10] SMFUnsuccessfulProcedure,

-- Subscriber-management related events, see clause 7.2.2

servingSystemMessage [11] UDMServingSystemMessage,

-- SMS-related events, see clause 6.2.5, see also sMSReport ([56] below)

sMSMessage [12] SMSMessage,

-- LALS-related events, see clause 7.3.3

lALSReport [13] LALSReport,

-- PDHR/PDSR-related events, see clause 6.2.3.4.1

pDHeaderReport [14] PDHeaderReport,

pDSummaryReport [15] PDSummaryReport,

-- MDF-related events, see clause 7.3.2

mDFCellSiteReport [16] MDFCellSiteReport,

-- MMS-related events, see clause 7.4.2

mMSSend [17] MMSSend,

mMSSendByNonLocalTarget [18] MMSSendByNonLocalTarget,

mMSNotification [19] MMSNotification,

mMSSendToNonLocalTarget [20] MMSSendToNonLocalTarget,

mMSNotificationResponse [21] MMSNotificationResponse,

mMSRetrieval [22] MMSRetrieval,

mMSDeliveryAck [23] MMSDeliveryAck,

mMSForward [24] MMSForward,

mMSDeleteFromRelay [25] MMSDeleteFromRelay,

mMSDeliveryReport [26] MMSDeliveryReport,

mMSDeliveryReportNonLocalTarget [27] MMSDeliveryReportNonLocalTarget,

mMSReadReport [28] MMSReadReport,

mMSReadReportNonLocalTarget [29] MMSReadReportNonLocalTarget,

mMSCancel [30] MMSCancel,

mMSMBoxStore [31] MMSMBoxStore,

mMSMBoxUpload [32] MMSMBoxUpload,

mMSMBoxDelete [33] MMSMBoxDelete,

mMSMBoxViewRequest [34] MMSMBoxViewRequest,

mMSMBoxViewResponse [35] MMSMBoxViewResponse,

-- PTC-related events, see clause 7.5.2

pTCRegistration [36] PTCRegistration,

pTCSessionInitiation [37] PTCSessionInitiation,

pTCSessionAbandon [38] PTCSessionAbandon,

pTCSessionStart [39] PTCSessionStart,

pTCSessionEnd [40] PTCSessionEnd,

pTCStartOfInterception [41] PTCStartOfInterception,

pTCPreEstablishedSession [42] PTCPreEstablishedSession,

pTCInstantPersonalAlert [43] PTCInstantPersonalAlert,

pTCPartyJoin [44] PTCPartyJoin,

pTCPartyDrop [45] PTCPartyDrop,

pTCPartyHold [46] PTCPartyHold,

pTCMediaModification [47] PTCMediaModification,

pTCGroupAdvertisement [48] PTCGroupAdvertisement,

pTCFloorControl [49] PTCFloorControl,

pTCTargetPresence [50] PTCTargetPresence,

pTCParticipantPresence [51] PTCParticipantPresence,

pTCListManagement [52] PTCListManagement,

pTCAccessPolicy [53] PTCAccessPolicy,

-- More Subscriber-management related events, see clause 7.2.2

subscriberRecordChangeMessage [54] UDMSubscriberRecordChangeMessage,

cancelLocationMessage [55] UDMCancelLocationMessage,

-- SMS-related events, continued from choice 12

sMSReport [56] SMSReport,

-- MA PDU session-related events, see clause 6.2.3.2.7

sMFMAPDUSessionEstablishment [57] SMFMAPDUSessionEstablishment,

sMFMAPDUSessionModification [58] SMFMAPDUSessionModification,

sMFMAPDUSessionRelease [59] SMFMAPDUSessionRelease,

startOfInterceptionWithEstablishedMAPDUSession [60] SMFStartOfInterceptionWithEstablishedMAPDUSession,

unsuccessfulMASMProcedure [61] SMFMAUnsuccessfulProcedure,

-- Identifier Association events, see clauses 6.2.2.2.7 and 6.3.2.2.2

aMFIdentifierAssociation [62] AMFIdentifierAssociation,

mMEIdentifierAssociation [63] MMEIdentifierAssociation,

-- PDU to MA PDU session-related events, see clause 6.2.3.2.8

sMFPDUtoMAPDUSessionModification [64] SMFPDUtoMAPDUSessionModification,

-- NEF services related events, see clause 7.7.2,

nEFPDUSessionEstablishment [65] NEFPDUSessionEstablishment,

nEFPDUSessionModification [66] NEFPDUSessionModification,

nEFPDUSessionRelease [67] NEFPDUSessionRelease,

nEFUnsuccessfulProcedure [68] NEFUnsuccessfulProcedure,

nEFStartOfInterceptionWithEstablishedPDUSession [69] NEFStartOfInterceptionWithEstablishedPDUSession,

nEFdeviceTrigger [70] NEFDeviceTrigger,

nEFdeviceTriggerReplace [71] NEFDeviceTriggerReplace,

nEFdeviceTriggerCancellation [72] NEFDeviceTriggerCancellation,

nEFdeviceTriggerReportNotify [73] NEFDeviceTriggerReportNotify,

nEFMSISDNLessMOSMS [74] NEFMSISDNLessMOSMS,

nEFExpectedUEBehaviourUpdate [75] NEFExpectedUEBehaviourUpdate,

-- SCEF services related events, see clause 7.8.2

sCEFPDNConnectionEstablishment [76] SCEFPDNConnectionEstablishment,

sCEFPDNConnectionUpdate [77] SCEFPDNConnectionUpdate,

sCEFPDNConnectionRelease [78] SCEFPDNConnectionRelease,

sCEFUnsuccessfulProcedure [79] SCEFUnsuccessfulProcedure,

sCEFStartOfInterceptionWithEstablishedPDNConnection [80] SCEFStartOfInterceptionWithEstablishedPDNConnection,

sCEFdeviceTrigger [81] SCEFDeviceTrigger,

sCEFdeviceTriggerReplace [82] SCEFDeviceTriggerReplace,

sCEFdeviceTriggerCancellation [83] SCEFDeviceTriggerCancellation,

sCEFdeviceTriggerReportNotify [84] SCEFDeviceTriggerReportNotify,

sCEFMSISDNLessMOSMS [85] SCEFMSISDNLessMOSMS,

sCEFCommunicationPatternUpdate [86] SCEFCommunicationPatternUpdate,

-- EPS Events, see clause 6.3

-- MME Events, see clause 6.3.2.2

mMEAttach [87] MMEAttach,

mMEDetach [88] MMEDetach,

mMELocationUpdate [89] MMELocationUpdate,

mMEStartOfInterceptionWithEPSAttachedUE [90] MMEStartOfInterceptionWithEPSAttachedUE,

mMEUnsuccessfulProcedure [91] MMEUnsuccessfulProcedure,

-- AKMA key management events, see clause 7.9.1

aAnFAnchorKeyRegister [92] AAnFAnchorKeyRegister,

aAnFKAKMAApplicationKeyGet [93] AAnFKAKMAApplicationKeyGet,

aAnFStartOfInterceptWithEstablishedAKMAKeyMaterial [94] AAnFStartOfInterceptWithEstablishedAKMAKeyMaterial,

aAnFAKMAContextRemovalRecord [95] AAnFAKMAContextRemovalRecord,

aFAKMAApplicationKeyRefresh [96] AFAKMAApplicationKeyRefresh,

aFStartOfInterceptWithEstablishedAKMAApplicationKey [97] AFStartOfInterceptWithEstablishedAKMAApplicationKey,

aFAuxiliarySecurityParameterEstablishment [98] AFAuxiliarySecurityParameterEstablishment,

aFApplicationKeyRemoval [99] AFApplicationKeyRemoval,

-- tag 100 is reserved because there is no equivalent n9HRPDUSessionInfo in IRIEvent.

-- tag 101 is reserved because there is no equivalent S8HRBearerInfo in IRIEvent.

-- Separated Location Reporting, see clause 7.3.4

separatedLocationReporting [102] SeparatedLocationReporting,

-- STIR SHAKEN and RCD/eCNAM Events, see clause 7.11.3

sTIRSHAKENSignatureGeneration [103] STIRSHAKENSignatureGeneration,

sTIRSHAKENSignatureValidation [104] STIRSHAKENSignatureValidation,

-- IMS events, see clause 7.11.4.2

iMSMessage [105] IMSMessage,

startOfInterceptionForActiveIMSSession [106]StartOfInterceptionForActiveIMSSession,

-- UDM events, see clause 7.2.2

uDMLocationInformationResult [904] UDMLocationInformationResult,

uDMUEInformationResponse [905] UDMUEInformationResponse,

uDMUEAuthenticationResponse [906] UDMUEAuthenticationResponse

}

IRITargetIdentifier ::= SEQUENCE

{

identifier [1] TargetIdentifier,

provenance [2] TargetIdentifierProvenance OPTIONAL

}

-- ==============

-- HI3 CC payload

-- ==============

CCPayload ::= SEQUENCE

{

cCPayloadOID [1] RELATIVE-OID,

pDU [2] CCPDU

}

CCPDU ::= CHOICE

{

uPFCCPDU [1] UPFCCPDU,

extendedUPFCCPDU [2] ExtendedUPFCCPDU,

mMSCCPDU [3] MMSCCPDU,

nIDDCCPDU [4] NIDDCCPDU,

pTCCCPDU [5] PTCCCPDU

}

-- ===========================

-- HI4 LI notification payload

-- ===========================

LINotificationPayload ::= SEQUENCE

{

lINotificationPayloadOID [1] RELATIVE-OID,

notification [2] LINotificationMessage

}

LINotificationMessage ::= CHOICE

{

lINotification [1] LINotification

}

-- =================

-- HR LI definitions

-- =================

N9HRPDUSessionInfo ::= SEQUENCE

{

sUPI [1] SUPI,

pEI [2] PEI OPTIONAL,

pDUSessionID [3] PDUSessionID,

location [4] Location OPTIONAL,

sNSSAI [5] SNSSAI OPTIONAL,

dNN [6] DNN OPTIONAL,

messageCause [7] N9HRMessageCause

}

S8HRBearerInfo ::= SEQUENCE

{

iMSI [1] IMSI,

iMEI [2] IMEI OPTIONAL,

bearerID [3] EPSBearerID,

linkedBearerID [4] EPSBearerID OPTIONAL,

location [5] Location OPTIONAL,

aPN [6] APN OPTIONAL,

sGWIPAddress [7] IPAddress OPTIONAL,

messageCause [8] S8HRMessageCause

}

-- ================

-- HR LI parameters

-- ================

N9HRMessageCause ::= ENUMERATED

{

pDUSessionEstablished(1),

pDUSessionModified(2),

pDUSessionReleased(3),

updatedLocationAvailable(4),

sMFChanged(5),

other(6),

hRLIEnabled(7)

}

S8HRMessageCause ::= ENUMERATED

{

bearerActivated(1),

bearerModified(2),

bearerDeleted(3),

pDNDisconnected(4),

updatedLocationAvailable(5),

sGWChanged(6),

other(7),

hRLIEnabled(8)

}

-- ==================

-- 5G NEF definitions

-- ==================

-- See clause 7.7.2.1.2 for details of this structure

NEFPDUSessionEstablishment ::= SEQUENCE

{

sUPI [1] SUPI,

gPSI [2] GPSI,

pDUSessionID [3] PDUSessionID,

sNSSAI [4] SNSSAI,

nEFID [5] NEFID,

dNN [6] DNN,

rDSSupport [7] RDSSupport,

sMFID [8] SMFID,

aFID [9] AFID

}

-- See clause 7.7.2.1.3 for details of this structure

NEFPDUSessionModification ::= SEQUENCE

{

sUPI [1] SUPI,

gPSI [2] GPSI,

sNSSAI [3] SNSSAI,

initiator [4] Initiator,

rDSSourcePortNumber [5] RDSPortNumber OPTIONAL,

rDSDestinationPortNumber [6] RDSPortNumber OPTIONAL,

applicationID [7] ApplicationID OPTIONAL,

aFID [8] AFID OPTIONAL,

rDSAction [9] RDSAction OPTIONAL,

serializationFormat [10] SerializationFormat OPTIONAL

}

-- See clause 7.7.2.1.4 for details of this structure

NEFPDUSessionRelease ::= SEQUENCE

{

sUPI [1] SUPI,

gPSI [2] GPSI,

pDUSessionID [3] PDUSessionID,

timeOfFirstPacket [4] Timestamp OPTIONAL,

timeOfLastPacket [5] Timestamp OPTIONAL,

uplinkVolume [6] INTEGER OPTIONAL,

downlinkVolume [7] INTEGER OPTIONAL,

releaseCause [8] NEFReleaseCause

}

-- See clause 7.7.2.1.5 for details of this structure

NEFUnsuccessfulProcedure ::= SEQUENCE

{

failureCause [1] NEFFailureCause,

sUPI [2] SUPI,

gPSI [3] GPSI OPTIONAL,

pDUSessionID [4] PDUSessionID,

dNN [5] DNN OPTIONAL,

sNSSAI [6] SNSSAI OPTIONAL,

rDSDestinationPortNumber [7] RDSPortNumber,

applicationID [8] ApplicationID,

aFID [9] AFID

}

-- See clause 7.7.2.1.6 for details of this structure

NEFStartOfInterceptionWithEstablishedPDUSession ::= SEQUENCE

{

sUPI [1] SUPI,

gPSI [2] GPSI,

pDUSessionID [3] PDUSessionID,

dNN [4] DNN,

sNSSAI [5] SNSSAI,

nEFID [6] NEFID,

rDSSupport [7] RDSSupport,

sMFID [8] SMFID,

aFID [9] AFID

}

-- See clause 7.7.3.1.1 for details of this structure

NEFDeviceTrigger ::= SEQUENCE

{

sUPI [1] SUPI,

gPSI [2] GPSI,

triggerId [3] TriggerID,

aFID [4] AFID,

triggerPayload [5] TriggerPayload OPTIONAL,

validityPeriod [6] INTEGER OPTIONAL,

priorityDT [7] PriorityDT OPTIONAL,

sourcePortId [8] PortNumber OPTIONAL,

destinationPortId [9] PortNumber OPTIONAL

}

-- See clause 7.7.3.1.2 for details of this structure

NEFDeviceTriggerReplace ::= SEQUENCE

{

sUPI [1] SUPI,

gPSI [2] GPSI,

triggerId [3] TriggerID,

aFID [4] AFID,

triggerPayload [5] TriggerPayload OPTIONAL,

validityPeriod [6] INTEGER OPTIONAL,

priorityDT [7] PriorityDT OPTIONAL,

sourcePortId [8] PortNumber OPTIONAL,

destinationPortId [9] PortNumber OPTIONAL

}

-- See clause 7.7.3.1.3 for details of this structure

NEFDeviceTriggerCancellation ::= SEQUENCE

{

sUPI [1] SUPI,

gPSI [2] GPSI,

triggerId [3] TriggerID

}

-- See clause 7.7.3.1.4 for details of this structure

NEFDeviceTriggerReportNotify ::= SEQUENCE

{

sUPI [1] SUPI,

gPSI [2] GPSI,

triggerId [3] TriggerID,

deviceTriggerDeliveryResult [4] DeviceTriggerDeliveryResult

}

-- See clause 7.7.4.1.1 for details of this structure

NEFMSISDNLessMOSMS ::= SEQUENCE

{

sUPI [1] SUPI,

gPSI [2] GPSI,

terminatingSMSParty [3] AFID,

sMS [4] SMSTPDUData OPTIONAL,

sourcePort [5] PortNumber OPTIONAL,

destinationPort [6] PortNumber OPTIONAL

}

-- See clause 7.7.5.1.1 for details of this structure

NEFExpectedUEBehaviourUpdate ::= SEQUENCE

{

gPSI [1] GPSI,

expectedUEMovingTrajectory [2] SEQUENCE OF UMTLocationArea5G OPTIONAL,

stationaryIndication [3] StationaryIndication OPTIONAL,

communicationDurationTime [4] INTEGER OPTIONAL,

periodicTime [5] INTEGER OPTIONAL,

scheduledCommunicationTime [6] ScheduledCommunicationTime OPTIONAL,

scheduledCommunicationType [7] ScheduledCommunicationType OPTIONAL,

batteryIndication [8] BatteryIndication OPTIONAL,

trafficProfile [9] TrafficProfile OPTIONAL,

expectedTimeAndDayOfWeekInTrajectory [10] SEQUENCE OF UMTLocationArea5G OPTIONAL,

aFID [11] AFID,

validityTime [12] Timestamp OPTIONAL

}

-- ==========================

-- Common SCEF/NEF parameters

-- ==========================

RDSSupport ::= BOOLEAN

RDSPortNumber ::= INTEGER (0..15)

RDSAction ::= ENUMERATED

{

reservePort(1),

releasePort(2)

}

SerializationFormat ::= ENUMERATED

{

xml(1),

json(2),

cbor(3)

}

ApplicationID ::= OCTET STRING

NIDDCCPDU ::= OCTET STRING

TriggerID ::= UTF8String

PriorityDT ::= ENUMERATED

{

noPriority(1),

priority(2)

}

TriggerPayload ::= OCTET STRING

DeviceTriggerDeliveryResult ::= ENUMERATED

{

success(1),

unknown(2),

failure(3),

triggered(4),

expired(5),

unconfirmed(6),

replaced(7),

terminate(8)

}

StationaryIndication ::= ENUMERATED

{

stationary(1),

mobile(2)

}

BatteryIndication ::= ENUMERATED

{

batteryRecharge(1),

batteryReplace(2),

batteryNoRecharge(3),

batteryNoReplace(4),

noBattery(5)

}

ScheduledCommunicationTime ::= SEQUENCE

{

days [1] SEQUENCE OF Daytime

}

UMTLocationArea5G ::= SEQUENCE

{

timeOfDay [1] Daytime,

durationSec [2] INTEGER,

location [3] NRLocation

}

Daytime ::= SEQUENCE

{

daysOfWeek [1] Day OPTIONAL,

timeOfDayStart [2] Timestamp OPTIONAL,

timeOfDayEnd [3] Timestamp OPTIONAL

}

Day ::= ENUMERATED

{

monday(1),

tuesday(2),

wednesday(3),

thursday(4),

friday(5),

saturday(6),

sunday(7)

}

TrafficProfile ::= ENUMERATED

{

singleTransUL(1),

singleTransDL(2),

dualTransULFirst(3),

dualTransDLFirst(4),

multiTrans(5)

}

ScheduledCommunicationType ::= ENUMERATED

{

downlinkOnly(1),

uplinkOnly(2),

bidirectional(3)

}

-- =================

-- 5G NEF parameters

-- =================

NEFFailureCause ::= ENUMERATED

{

userUnknown(1),

niddConfigurationNotAvailable(2),

contextNotFound(3),

portNotFree(4),

portNotAssociatedWithSpecifiedApplication(5)

}

NEFReleaseCause ::= ENUMERATED

{

sMFRelease(1),

dNRelease(2),

uDMRelease(3),

cHFRelease(4),

localConfigurationPolicy(5),

unknownCause(6)

}

AFID ::= UTF8String

NEFID ::= UTF8String

-- ==================

-- SCEF definitions

-- ==================

-- See clause 7.8.2.1.2 for details of this structure

SCEFPDNConnectionEstablishment ::= SEQUENCE

{

iMSI [1] IMSI OPTIONAL,

mSISDN [2] MSISDN OPTIONAL,

externalIdentifier [3] NAI OPTIONAL,

iMEI [4] IMEI OPTIONAL,

ePSBearerID [5] EPSBearerID,

sCEFID [6] SCEFID,

aPN [7] APN,

rDSSupport [8] RDSSupport,

sCSASID [9] SCSASID

}

-- See clause 7.8.2.1.3 for details of this structure

SCEFPDNConnectionUpdate ::= SEQUENCE

{

iMSI [1] IMSI OPTIONAL,

mSISDN [2] MSISDN OPTIONAL,

externalIdentifier [3] NAI OPTIONAL,

initiator [4] Initiator,

rDSSourcePortNumber [5] RDSPortNumber OPTIONAL,

rDSDestinationPortNumber [6] RDSPortNumber OPTIONAL,

applicationID [7] ApplicationID OPTIONAL,

sCSASID [8] SCSASID OPTIONAL,

rDSAction [9] RDSAction OPTIONAL,

serializationFormat [10] SerializationFormat OPTIONAL

}

-- See clause 7.8.2.1.4 for details of this structure

SCEFPDNConnectionRelease ::= SEQUENCE

{

iMSI [1] IMSI OPTIONAL,

mSISDN [2] MSISDN OPTIONAL,

externalIdentifier [3] NAI OPTIONAL,

ePSBearerID [4] EPSBearerID,

timeOfFirstPacket [5] Timestamp OPTIONAL,

timeOfLastPacket [6] Timestamp OPTIONAL,

uplinkVolume [7] INTEGER OPTIONAL,

downlinkVolume [8] INTEGER OPTIONAL,

releaseCause [9] SCEFReleaseCause

}

-- See clause 7.8.2.1.5 for details of this structure

SCEFUnsuccessfulProcedure ::= SEQUENCE

{

failureCause [1] SCEFFailureCause,

iMSI [2] IMSI OPTIONAL,

mSISDN [3] MSISDN OPTIONAL,

externalIdentifier [4] NAI OPTIONAL,

ePSBearerID [5] EPSBearerID,

aPN [6] APN,

rDSDestinationPortNumber [7] RDSPortNumber OPTIONAL,

applicationID [8] ApplicationID OPTIONAL,

sCSASID [9] SCSASID

}

-- See clause 7.8.2.1.6 for details of this structure

SCEFStartOfInterceptionWithEstablishedPDNConnection ::= SEQUENCE

{

iMSI [1] IMSI OPTIONAL,

mSISDN [2] MSISDN OPTIONAL,

externalIdentifier [3] NAI OPTIONAL,

iMEI [4] IMEI OPTIONAL,

ePSBearerID [5] EPSBearerID,

sCEFID [6] SCEFID,

aPN [7] APN,

rDSSupport [8] RDSSupport,

sCSASID [9] SCSASID

}

-- See clause 7.8.3.1.1 for details of this structure

SCEFDeviceTrigger ::= SEQUENCE

{

iMSI [1] IMSI,

mSISDN [2] MSISDN,

externalIdentifier [3] NAI,

triggerId [4] TriggerID,

sCSASID [5] SCSASID OPTIONAL,

triggerPayload [6] TriggerPayload OPTIONAL,

validityPeriod [7] INTEGER OPTIONAL,

priorityDT [8] PriorityDT OPTIONAL,

sourcePortId [9] PortNumber OPTIONAL,

destinationPortId [10] PortNumber OPTIONAL

}

-- See clause 7.8.3.1.2 for details of this structure

SCEFDeviceTriggerReplace ::= SEQUENCE

{

iMSI [1] IMSI OPTIONAL,

mSISDN [2] MSISDN OPTIONAL,

externalIdentifier [3] NAI OPTIONAL,

triggerId [4] TriggerID,

sCSASID [5] SCSASID OPTIONAL,

triggerPayload [6] TriggerPayload OPTIONAL,

validityPeriod [7] INTEGER OPTIONAL,

priorityDT [8] PriorityDT OPTIONAL,

sourcePortId [9] PortNumber OPTIONAL,

destinationPortId [10] PortNumber OPTIONAL

}

-- See clause 7.8.3.1.3 for details of this structure

SCEFDeviceTriggerCancellation ::= SEQUENCE

{

iMSI [1] IMSI OPTIONAL,

mSISDN [2] MSISDN OPTIONAL,

externalIdentifier [3] NAI OPTIONAL,

triggerId [4] TriggerID

}

-- See clause 7.8.3.1.4 for details of this structure

SCEFDeviceTriggerReportNotify ::= SEQUENCE

{

iMSI [1] IMSI OPTIONAL,

mSISDN [2] MSISDN OPTIONAL,

externalIdentifier [3] NAI OPTIONAL,

triggerId [4] TriggerID,

deviceTriggerDeliveryResult [5] DeviceTriggerDeliveryResult

}

-- See clause 7.8.4.1.1 for details of this structure

SCEFMSISDNLessMOSMS ::= SEQUENCE

{

iMSI [1] IMSI OPTIONAL,

mSISDN [2] MSISDN OPTIONAL,

externalIdentifie [3] NAI OPTIONAL,

terminatingSMSParty [4] SCSASID,

sMS [5] SMSTPDUData OPTIONAL,

sourcePort [6] PortNumber OPTIONAL,

destinationPort [7] PortNumber OPTIONAL

}

-- See clause 7.8.5.1.1 for details of this structure

SCEFCommunicationPatternUpdate ::= SEQUENCE

{

mSISDN [1] MSISDN OPTIONAL,

externalIdentifier [2] NAI OPTIONAL,

periodicCommunicationIndicator [3] PeriodicCommunicationIndicator OPTIONAL,

communicationDurationTime [4] INTEGER OPTIONAL,

periodicTime [5] INTEGER OPTIONAL,

scheduledCommunicationTime [6] ScheduledCommunicationTime OPTIONAL,

scheduledCommunicationType [7] ScheduledCommunicationType OPTIONAL,

stationaryIndication [8] StationaryIndication OPTIONAL,

batteryIndication [9] BatteryIndication OPTIONAL,

trafficProfile [10] TrafficProfile OPTIONAL,

expectedUEMovingTrajectory [11] SEQUENCE OF UMTLocationArea5G OPTIONAL,

sCSASID [13] SCSASID,

validityTime [14] Timestamp OPTIONAL

}

-- =================

-- SCEF parameters

-- =================

SCEFFailureCause ::= ENUMERATED

{

userUnknown(1),

niddConfigurationNotAvailable(2),

invalidEPSBearer(3),

operationNotAllowed(4),

portNotFree(5),

portNotAssociatedWithSpecifiedApplication(6)

}

SCEFReleaseCause ::= ENUMERATED

{

mMERelease(1),

dNRelease(2),

hSSRelease(3),

localConfigurationPolicy(4),

unknownCause(5)

}

SCSASID ::= UTF8String

SCEFID ::= UTF8String

PeriodicCommunicationIndicator ::= ENUMERATED

{

periodic(1),

nonPeriodic(2)

}

EPSBearerID ::= INTEGER (0..255)

APN ::= UTF8String

-- =======================

-- AKMA AAnF definitions

-- =======================

AAnFAnchorKeyRegister ::= SEQUENCE

{

aKID [1] NAI,

sUPI [2] SUPI,

kAKMA [3] KAKMA OPTIONAL

}

AAnFKAKMAApplicationKeyGet ::= SEQUENCE

{

type [1] KeyGetType,

aKID [2] NAI,

keyInfo [3] AFKeyInfo

}

AAnFStartOfInterceptWithEstablishedAKMAKeyMaterial ::= SEQUENCE

{

aKID [1] NAI,

kAKMA [2] KAKMA OPTIONAL,

aFKeyList [3] SEQUENCE OF AFKeyInfo OPTIONAL

}

AAnFAKMAContextRemovalRecord ::= SEQUENCE

{

aKID [1] NAI,

nFID [2] NFID

}

-- ======================

-- AKMA common parameters

-- ======================

FQDN ::= UTF8String

NFID ::= UTF8String

UAProtocolID ::= OCTET STRING (SIZE(5))

AKMAAFID ::= SEQUENCE

{

aFFQDN [1] FQDN,

uaProtocolID [2] UAProtocolID

}

UAStarParams ::= CHOICE

{

tls12 [1] TLS12UAStarParams,

generic [2] GenericUAStarParams

}

GenericUAStarParams ::= SEQUENCE

{

genericClientParams [1] OCTET STRING,

genericServerParams [2] OCTET STRING

}

-- ===========================================

-- Specific UaStarParmas for TLS 1.2 (RFC5246)

-- ===========================================

TLSCipherType ::= ENUMERATED

{

stream(1),

block(2),

aead(3)

}

TLSCompressionAlgorithm ::= ENUMERATED

{

null(1),

deflate(2)

}

TLSPRFAlgorithm ::= ENUMERATED

{

rfc5246(1)

}

TLSCipherSuite ::= SEQUENCE (SIZE(2)) OF INTEGER (0..255)

TLS12UAStarParams ::= SEQUENCE

{

preMasterSecret [1] OCTET STRING (SIZE(6)) OPTIONAL,

masterSecret [2] OCTET STRING (SIZE(6)),

pRFAlgorithm [3] TLSPRFAlgorithm,

cipherSuite [4] TLSCipherSuite,

cipherType [5] TLSCipherType,

encKeyLength [6] INTEGER (0..255),

blockLength [7] INTEGER (0..255),

fixedIVLength [8] INTEGER (0..255),

recordIVLength [9] INTEGER (0..255),

macLength [10] INTEGER (0..255),

macKeyLength [11] INTEGER (0..255),

compressionAlgorithm [12] TLSCompressionAlgorithm,

clientRandom [13] OCTET STRING (SIZE(4)),

serverRandom [14] OCTET STRING (SIZE(4)),

clientSequenceNumber [15] INTEGER,

serverSequenceNumber [16] INTEGER,

sessionID [17] OCTET STRING (SIZE(0..32)),

tLSExtensions [18] OCTET STRING (SIZE(0..65535))

}

KAF ::= OCTET STRING

KAKMA ::= OCTET STRING

-- ====================

-- AKMA AAnF parameters

-- ====================

KeyGetType ::= ENUMERATED

{

internal(1),

external(2)

}

AFKeyInfo ::= SEQUENCE

{

aFID [1] AKMAAFID,

kAF [2] KAF,

kAFExpTime [3] KAFExpiryTime

}

-- =======================

-- AKMA AF definitions

-- =======================

AFAKMAApplicationKeyRefresh ::= SEQUENCE

{

aFID [1] AFID,

aKID [2] NAI,

kAF [3] KAF,

uaStarParams [4] UAStarParams OPTIONAL

}

AFStartOfInterceptWithEstablishedAKMAApplicationKey ::= SEQUENCE

{

aFID [1] FQDN,

aKID [2] NAI,

kAFParamList [3] SEQUENCE OF AFSecurityParams

}

AFAuxiliarySecurityParameterEstablishment ::= SEQUENCE

{

aFSecurityParams [1] AFSecurityParams

}

AFSecurityParams ::= SEQUENCE

{

aFID [1] AFID,

aKID [2] NAI,

kAF [3] KAF,

uaStarParams [4] UAStarParams

}

AFApplicationKeyRemoval ::= SEQUENCE

{

aFID [1] AFID,

aKID [2] NAI,

removalCause [3] AFKeyRemovalCause

}

-- ===================

-- AKMA AF parameters

-- ===================

KAFParams ::= SEQUENCE

{

aKID [1] NAI,

kAF [2] KAF,

kAFExpTime [3] KAFExpiryTime,

uaStarParams [4] UAStarParams

}

KAFExpiryTime ::= GeneralizedTime

AFKeyRemovalCause ::= ENUMERATED

{

unknown(1),

keyExpiry(2),

applicationSpecific(3)

}

-- ==================

-- 5G AMF definitions

-- ==================

-- See clause 6.2.2.2.2 for details of this structure

AMFRegistration ::= SEQUENCE

{

registrationType [1] AMFRegistrationType,

registrationResult [2] AMFRegistrationResult,

slice [3] Slice OPTIONAL,

sUPI [4] SUPI,

sUCI [5] SUCI OPTIONAL,

pEI [6] PEI OPTIONAL,

gPSI [7] GPSI OPTIONAL,

gUTI [8] FiveGGUTI,

location [9] Location OPTIONAL,

non3GPPAccessEndpoint [10] UEEndpointAddress OPTIONAL,

fiveGSTAIList [11] TAIList OPTIONAL,

sMSOverNasIndicator [12] SMSOverNASIndicator OPTIONAL,

oldGUTI [13] EPS5GGUTI OPTIONAL,

eMM5GRegStatus [14] EMM5GMMStatus OPTIONAL,

nonIMEISVPEI [15] NonIMEISVPEI OPTIONAL,

mACRestIndicator [16] MACRestrictionIndicator OPTIONAL

}

-- See clause 6.2.2.2.3 for details of this structure

AMFDeregistration ::= SEQUENCE

{

deregistrationDirection [1] AMFDirection,

accessType [2] AccessType,

sUPI [3] SUPI OPTIONAL,

sUCI [4] SUCI OPTIONAL,

pEI [5] PEI OPTIONAL,

gPSI [6] GPSI OPTIONAL,

gUTI [7] FiveGGUTI OPTIONAL,

cause [8] FiveGMMCause OPTIONAL,

location [9] Location OPTIONAL,

switchOffIndicator [10] SwitchOffIndicator OPTIONAL,

reRegRequiredIndicator [11] ReRegRequiredIndicator OPTIONAL

}

-- See clause 6.2.2.2.4 for details of this structure

AMFLocationUpdate ::= SEQUENCE

{

sUPI [1] SUPI,

sUCI [2] SUCI OPTIONAL,

pEI [3] PEI OPTIONAL,

gPSI [4] GPSI OPTIONAL,

gUTI [5] FiveGGUTI OPTIONAL,

location [6] Location,

sMSOverNASIndicator [7] SMSOverNASIndicator OPTIONAL,

oldGUTI [8] EPS5GGUTI OPTIONAL

}

-- See clause 6.2.2.2.5 for details of this structure

AMFStartOfInterceptionWithRegisteredUE ::= SEQUENCE

{

registrationResult [1] AMFRegistrationResult,

registrationType [2] AMFRegistrationType OPTIONAL,

slice [3] Slice OPTIONAL,

sUPI [4] SUPI,

sUCI [5] SUCI OPTIONAL,

pEI [6] PEI OPTIONAL,

gPSI [7] GPSI OPTIONAL,

gUTI [8] FiveGGUTI,

location [9] Location OPTIONAL,

non3GPPAccessEndpoint [10] UEEndpointAddress OPTIONAL,

timeOfRegistration [11] Timestamp OPTIONAL,

fiveGSTAIList [12] TAIList OPTIONAL,

sMSOverNASIndicator [13] SMSOverNASIndicator OPTIONAL,

oldGUTI [14] EPS5GGUTI OPTIONAL,

eMM5GRegStatus [15] EMM5GMMStatus OPTIONAL

}

-- See clause 6.2.2.2.6 for details of this structure

AMFUnsuccessfulProcedure ::= SEQUENCE

{

failedProcedureType [1] AMFFailedProcedureType,

failureCause [2] AMFFailureCause,

requestedSlice [3] NSSAI OPTIONAL,

sUPI [4] SUPI OPTIONAL,

sUCI [5] SUCI OPTIONAL,

pEI [6] PEI OPTIONAL,

gPSI [7] GPSI OPTIONAL,

gUTI [8] FiveGGUTI OPTIONAL,

location [9] Location OPTIONAL

}

-- =================

-- 5G AMF parameters

-- =================

AMFID ::= SEQUENCE

{

aMFRegionID [1] AMFRegionID,

aMFSetID [2] AMFSetID,

aMFPointer [3] AMFPointer

}

AMFDirection ::= ENUMERATED

{

networkInitiated(1),

uEInitiated(2)

}

AMFFailedProcedureType ::= ENUMERATED

{

registration(1),

sMS(2),

pDUSessionEstablishment(3)

}

AMFFailureCause ::= CHOICE

{

fiveGMMCause [1] FiveGMMCause,

fiveGSMCause [2] FiveGSMCause

}

AMFPointer ::= INTEGER (0..63)

AMFRegistrationResult ::= ENUMERATED

{

threeGPPAccess(1),

nonThreeGPPAccess(2),

threeGPPAndNonThreeGPPAccess(3)

}

AMFRegionID ::= INTEGER (0..255)

AMFRegistrationType ::= ENUMERATED

{

initial(1),

mobility(2),

periodic(3),

emergency(4)

}

AMFSetID ::= INTEGER (0..1023)

-- ==================

-- 5G SMF definitions

-- ==================

-- See clause 6.2.3.2.2 for details of this structure

SMFPDUSessionEstablishment ::= SEQUENCE

{

sUPI [1] SUPI OPTIONAL,

sUPIUnauthenticated [2] SUPIUnauthenticatedIndication OPTIONAL,

pEI [3] PEI OPTIONAL,

gPSI [4] GPSI OPTIONAL,

pDUSessionID [5] PDUSessionID,

gTPTunnelID [6] FTEID,

pDUSessionType [7] PDUSessionType,

sNSSAI [8] SNSSAI OPTIONAL,

uEEndpoint [9] SEQUENCE OF UEEndpointAddress OPTIONAL,

non3GPPAccessEndpoint [10] UEEndpointAddress OPTIONAL,

location [11] Location OPTIONAL,

dNN [12] DNN,

aMFID [13] AMFID OPTIONAL,

hSMFURI [14] HSMFURI OPTIONAL,

requestType [15] FiveGSMRequestType,

accessType [16] AccessType OPTIONAL,

rATType [17] RATType OPTIONAL,

sMPDUDNRequest [18] SMPDUDNRequest OPTIONAL,

uEEPSPDNConnection [19] UEEPSPDNConnection OPTIONAL,

ePS5GSComboInfo [20] EPS5GSComboInfo OPTIONAL

}

-- See clause 6.2.3.2.3 for details of this structure

SMFPDUSessionModification ::= SEQUENCE

{

sUPI [1] SUPI OPTIONAL,

sUPIUnauthenticated [2] SUPIUnauthenticatedIndication OPTIONAL,

pEI [3] PEI OPTIONAL,

gPSI [4] GPSI OPTIONAL,

sNSSAI [5] SNSSAI OPTIONAL,

non3GPPAccessEndpoint [6] UEEndpointAddress OPTIONAL,

location [7] Location OPTIONAL,

requestType [8] FiveGSMRequestType,

accessType [9] AccessType OPTIONAL,

rATType [10] RATType OPTIONAL,

pDUSessionID [11] PDUSessionID OPTIONAL,

ePS5GSComboInfo [12] EPS5GSComboInfo OPTIONAL

}

-- See clause 6.2.3.2.4 for details of this structure

SMFPDUSessionRelease ::= SEQUENCE

{

sUPI [1] SUPI,

pEI [2] PEI OPTIONAL,

gPSI [3] GPSI OPTIONAL,

pDUSessionID [4] PDUSessionID,

timeOfFirstPacket [5] Timestamp OPTIONAL,

timeOfLastPacket [6] Timestamp OPTIONAL,

uplinkVolume [7] INTEGER OPTIONAL,

downlinkVolume [8] INTEGER OPTIONAL,

location [9] Location OPTIONAL,

cause [10] SMFErrorCodes OPTIONAL,

ePS5GSComboInfo [11] EPS5GSComboInfo OPTIONAL

}

-- See clause 6.2.3.2.5 for details of this structure

SMFStartOfInterceptionWithEstablishedPDUSession ::= SEQUENCE

{

sUPI [1] SUPI OPTIONAL,

sUPIUnauthenticated [2] SUPIUnauthenticatedIndication OPTIONAL,

pEI [3] PEI OPTIONAL,

gPSI [4] GPSI OPTIONAL,

pDUSessionID [5] PDUSessionID,

gTPTunnelID [6] FTEID,

pDUSessionType [7] PDUSessionType,

sNSSAI [8] SNSSAI OPTIONAL,

uEEndpoint [9] SEQUENCE OF UEEndpointAddress,

non3GPPAccessEndpoint [10] UEEndpointAddress OPTIONAL,

location [11] Location OPTIONAL,

dNN [12] DNN,

aMFID [13] AMFID OPTIONAL,

hSMFURI [14] HSMFURI OPTIONAL,

requestType [15] FiveGSMRequestType,

accessType [16] AccessType OPTIONAL,

rATType [17] RATType OPTIONAL,

sMPDUDNRequest [18] SMPDUDNRequest OPTIONAL,

timeOfSessionEstablishment [19] Timestamp OPTIONAL,

ePS5GSComboInfo [20] EPS5GSComboInfo OPTIONAL

}

-- See clause 6.2.3.2.6 for details of this structure

SMFUnsuccessfulProcedure ::= SEQUENCE

{

failedProcedureType [1] SMFFailedProcedureType,

failureCause [2] FiveGSMCause,

initiator [3] Initiator,

requestedSlice [4] NSSAI OPTIONAL,

sUPI [5] SUPI OPTIONAL,

sUPIUnauthenticated [6] SUPIUnauthenticatedIndication OPTIONAL,

pEI [7] PEI OPTIONAL,

gPSI [8] GPSI OPTIONAL,

pDUSessionID [9] PDUSessionID OPTIONAL,

uEEndpoint [10] SEQUENCE OF UEEndpointAddress OPTIONAL,

non3GPPAccessEndpoint [11] UEEndpointAddress OPTIONAL,

dNN [12] DNN OPTIONAL,

aMFID [13] AMFID OPTIONAL,

hSMFURI [14] HSMFURI OPTIONAL,

requestType [15] FiveGSMRequestType OPTIONAL,

accessType [16] AccessType OPTIONAL,

rATType [17] RATType OPTIONAL,

sMPDUDNRequest [18] SMPDUDNRequest OPTIONAL,

location [19] Location OPTIONAL

}

-- See clause 6.2.3.2.8 for details of this structure

SMFPDUtoMAPDUSessionModification ::= SEQUENCE

{

sUPI [1] SUPI OPTIONAL,

sUPIUnauthenticated [2] SUPIUnauthenticatedIndication OPTIONAL,

pEI [3] PEI OPTIONAL,

gPSI [4] GPSI OPTIONAL,

sNSSAI [5] SNSSAI OPTIONAL,

non3GPPAccessEndpoint [6] UEEndpointAddress OPTIONAL,

location [7] Location OPTIONAL,

requestType [8] FiveGSMRequestType,

accessType [9] AccessType OPTIONAL,

rATType [10] RATType OPTIONAL,

pDUSessionID [11] PDUSessionID,

requestIndication [12] RequestIndication,

aTSSSContainer [13] ATSSSContainer

}

-- See clause 6.2.3.2.7.1 for details of this structure

SMFMAPDUSessionEstablishment ::= SEQUENCE

{

sUPI [1] SUPI OPTIONAL,

sUPIUnauthenticated [2] SUPIUnauthenticatedIndication OPTIONAL,

pEI [3] PEI OPTIONAL,

gPSI [4] GPSI OPTIONAL,

pDUSessionID [5] PDUSessionID,

pDUSessionType [6] PDUSessionType,

accessInfo [7] SEQUENCE OF AccessInfo,

sNSSAI [8] SNSSAI OPTIONAL,

uEEndpoint [9] SEQUENCE OF UEEndpointAddress OPTIONAL,

location [10] Location OPTIONAL,

dNN [11] DNN,

aMFID [12] AMFID OPTIONAL,

hSMFURI [13] HSMFURI OPTIONAL,

requestType [14] FiveGSMRequestType,

sMPDUDNRequest [15] SMPDUDNRequest OPTIONAL,

servingNetwork [16] SMFServingNetwork,

oldPDUSessionID [17] PDUSessionID OPTIONAL,

mAUpgradeIndication [18] SMFMAUpgradeIndication OPTIONAL,

ePSPDNCnxInfo [19] SMFEPSPDNCnxInfo OPTIONAL,

mAAcceptedIndication [20] SMFMAAcceptedIndication,

aTSSSContainer [21] ATSSSContainer OPTIONAL

}

-- See clause 6.2.3.2.7.2 for details of this structure

SMFMAPDUSessionModification ::= SEQUENCE

{

sUPI [1] SUPI OPTIONAL,

sUPIUnauthenticated [2] SUPIUnauthenticatedIndication OPTIONAL,

pEI [3] PEI OPTIONAL,

gPSI [4] GPSI OPTIONAL,

pDUSessionID [5] PDUSessionID,

accessInfo [6] SEQUENCE OF AccessInfo OPTIONAL,

sNSSAI [7] SNSSAI OPTIONAL,

location [8] Location OPTIONAL,

requestType [9] FiveGSMRequestType OPTIONAL,

servingNetwork [10] SMFServingNetwork,

oldPDUSessionID [11] PDUSessionID OPTIONAL,

mAUpgradeIndication [12] SMFMAUpgradeIndication OPTIONAL,

ePSPDNCnxInfo [13] SMFEPSPDNCnxInfo OPTIONAL,

mAAcceptedIndication [14] SMFMAAcceptedIndication,

aTSSSContainer [15] ATSSSContainer OPTIONAL

}

-- See clause 6.2.3.2.7.3 for details of this structure

SMFMAPDUSessionRelease ::= SEQUENCE

{

sUPI [1] SUPI,

pEI [2] PEI OPTIONAL,

gPSI [3] GPSI OPTIONAL,

pDUSessionID [4] PDUSessionID,

timeOfFirstPacket [5] Timestamp OPTIONAL,

timeOfLastPacket [6] Timestamp OPTIONAL,

uplinkVolume [7] INTEGER OPTIONAL,

downlinkVolume [8] INTEGER OPTIONAL,

location [9] Location OPTIONAL,

cause [10] SMFErrorCodes OPTIONAL

}

-- See clause 6.2.3.2.7.4 for details of this structure

SMFStartOfInterceptionWithEstablishedMAPDUSession ::= SEQUENCE

{

sUPI [1] SUPI OPTIONAL,

sUPIUnauthenticated [2] SUPIUnauthenticatedIndication OPTIONAL,

pEI [3] PEI OPTIONAL,

gPSI [4] GPSI OPTIONAL,

pDUSessionID [5] PDUSessionID,

pDUSessionType [6] PDUSessionType,

accessInfo [7] SEQUENCE OF AccessInfo,

sNSSAI [8] SNSSAI OPTIONAL,

uEEndpoint [9] SEQUENCE OF UEEndpointAddress OPTIONAL,

location [10] Location OPTIONAL,

dNN [11] DNN,

aMFID [12] AMFID OPTIONAL,

hSMFURI [13] HSMFURI OPTIONAL,

requestType [14] FiveGSMRequestType OPTIONAL,

sMPDUDNRequest [15] SMPDUDNRequest OPTIONAL,

servingNetwork [16] SMFServingNetwork,

oldPDUSessionID [17] PDUSessionID OPTIONAL,

mAUpgradeIndication [18] SMFMAUpgradeIndication OPTIONAL,

ePSPDNCnxInfo [19] SMFEPSPDNCnxInfo OPTIONAL,

mAAcceptedIndication [20] SMFMAAcceptedIndication,

aTSSSContainer [21] ATSSSContainer OPTIONAL

}

-- See clause 6.2.3.2.7.5 for details of this structure

SMFMAUnsuccessfulProcedure ::= SEQUENCE

{

failedProcedureType [1] SMFFailedProcedureType,

failureCause [2] FiveGSMCause,

requestedSlice [3] NSSAI OPTIONAL,

initiator [4] Initiator,

sUPI [5] SUPI OPTIONAL,

sUPIUnauthenticated [6] SUPIUnauthenticatedIndication OPTIONAL,

pEI [7] PEI OPTIONAL,

gPSI [8] GPSI OPTIONAL,

pDUSessionID [9] PDUSessionID OPTIONAL,

accessInfo [10] SEQUENCE OF AccessInfo,

uEEndpoint [11] SEQUENCE OF UEEndpointAddress OPTIONAL,

location [12] Location OPTIONAL,

dNN [13] DNN OPTIONAL,

aMFID [14] AMFID OPTIONAL,

hSMFURI [15] HSMFURI OPTIONAL,

requestType [16] FiveGSMRequestType OPTIONAL,

sMPDUDNRequest [17] SMPDUDNRequest OPTIONAL

}

-- =================

-- 5G SMF parameters

-- =================

SMFID ::= UTF8String

SMFFailedProcedureType ::= ENUMERATED

{

pDUSessionEstablishment(1),

pDUSessionModification(2),

pDUSessionRelease(3)

}

SMFServingNetwork ::= SEQUENCE

{

pLMNID [1] PLMNID,

nID [2] NID OPTIONAL

}

AccessInfo ::= SEQUENCE

{

accessType [1] AccessType,

rATType [2] RATType OPTIONAL,

gTPTunnelID [3] FTEID,

non3GPPAccessEndpoint [4] UEEndpointAddress OPTIONAL,

establishmentStatus [5] EstablishmentStatus,

aNTypeToReactivate [6] AccessType OPTIONAL

}

-- see Clause 6.1.2 of TS 24.193[44] for the details of the ATSSS container contents.

ATSSSContainer ::= OCTET STRING

EstablishmentStatus ::= ENUMERATED

{

established(0),

released(1)

}

SMFMAUpgradeIndication ::= BOOLEAN

-- Given in YAML encoding as defined in clause 6.1.6.2.31 of TS 29.502[16]

SMFEPSPDNCnxInfo ::= UTF8String

SMFMAAcceptedIndication ::= BOOLEAN

-- see Clause 6.1.6.3.8 of TS 29.502[16] for the details of this structure.

SMFErrorCodes ::= UTF8String

-- see Clause 6.1.6.3.2 of TS 29.502[16] for details of this structure.

UEEPSPDNConnection ::= OCTET STRING

-- see Clause 6.1.6.3.6 of TS 29.502[16] for the details of this structure.

RequestIndication ::= ENUMERATED

{

uEREQPDUSESMOD(0),

uEREQPDUSESREL(1),

pDUSESMOB(2),

nWREQPDUSESAUTH(3),

nWREQPDUSESMOD(4),

nWREQPDUSESREL(5),

eBIASSIGNMENTREQ(6),

rELDUETO5GANREQUEST(7)

}

-- ======================

-- PGW-C + SMF Parameters

-- ======================

EPS5GSComboInfo ::= SEQUENCE

{

ePSInterworkingIndication [1] EPSInterworkingIndication,

ePSSubscriberIDs [2] EPSSubscriberIDs,

ePSPDNCnxInfo [3] EPSPDNCnxInfo OPTIONAL,

ePSBearerInfo [4] EPSBearerInfo OPTIONAL

}

EPSInterworkingIndication ::= ENUMERATED

{

none(1),

withN26(2),

withoutN26(3),

iwkNon3GPP(4)

}

EPSSubscriberIDs ::= SEQUENCE

{

iMSI [1] IMSI OPTIONAL,

mSISDN [2] MSISDN OPTIONAL,

iMEI [3] IMEI OPTIONAL

}

EPSPDNCnxInfo ::= SEQUENCE

{

pGWS8ControlPlaneFTEID [1] FTEID,

linkedBearerID [2] EPSBearerID OPTIONAL

}

EPSBearerInfo ::= SEQUENCE OF EPSBearers

EPSBearers ::= SEQUENCE

{

ePSBearerID [1] EPSBearerID,

pGWS8UserPlaneFTEID [2] FTEID,

qCI [3] QCI

}

QCI ::= INTEGER (0..255)

-- ==================

-- 5G UPF definitions

-- ==================

UPFCCPDU ::= OCTET STRING

-- See clause 6.2.3.8 for the details of this structure

ExtendedUPFCCPDU ::= SEQUENCE

{

payload [1] UPFCCPDUPayload,

qFI [2] QFI OPTIONAL

}

-- =================

-- 5G UPF parameters

-- =================

UPFCCPDUPayload ::= CHOICE

{

uPFIPCC [1] OCTET STRING,

uPFEthernetCC [2] OCTET STRING,

uPFUnstructuredCC [3] OCTET STRING

}

QFI ::= INTEGER (0..63)

-- ==================

-- 5G UDM definitions

-- ==================

UDMServingSystemMessage ::= SEQUENCE

{

sUPI [1] SUPI,

pEI [2] PEI OPTIONAL,

gPSI [3] GPSI OPTIONAL,

gUAMI [4] GUAMI OPTIONAL,

gUMMEI [5] GUMMEI OPTIONAL,

pLMNID [6] PLMNID OPTIONAL,

servingSystemMethod [7] UDMServingSystemMethod,

serviceID [8] ServiceID OPTIONAL

}

UDMSubscriberRecordChangeMessage ::= SEQUENCE

{

sUPI [1] SUPI OPTIONAL,

pEI [2] PEI OPTIONAL,

gPSI [3] GPSI OPTIONAL,

oldPEI [4] PEI OPTIONAL,

oldSUPI [5] SUPI OPTIONAL,

oldGPSI [6] GPSI OPTIONAL,

oldserviceID [7] ServiceID OPTIONAL,

subscriberRecordChangeMethod [8] UDMSubscriberRecordChangeMethod,

serviceID [9] ServiceID OPTIONAL

}

UDMCancelLocationMessage ::= SEQUENCE

{

sUPI [1] SUPI,

pEI [2] PEI OPTIONAL,

gPSI [3] GPSI OPTIONAL,

gUAMI [4] GUAMI OPTIONAL,

pLMNID [5] PLMNID OPTIONAL,

cancelLocationMethod [6] UDMCancelLocationMethod

}

UDMLocationInformationResult ::= SEQUENCE

{

sUPI [1] SUPI,

pEI [2] PEI OPTIONAL,

gPSI [3] GPSI OPTIONAL,

locationInfoRequest [4] UDMLocationInfoRequest,

vPLMNID [5] PLMNID OPTIONAL,

currentLocationIndicator [6] BOOLEAN OPTIONAL,

aMFInstanceID [7] NFID OPTIONAL,

sMSFInstanceID [8] NFID OPTIONAL,

location [9] Location OPTIONAL,

rATType [10] RATType OPTIONAL,

problemDetails [11] UDMProblemDetails OPTIONAL

}

UDMUEInformationResponse ::= SEQUENCE

{

sUPI [1] SUPI,

tADSInfo [2] UEContextInfo OPTIONAL,

fiveGSUserStateInfo [3] FiveGSUserStateInfo OPTIONAL,

fiveGSRVCCInfo [4] FiveGSRVCCInfo OPTIONAL,

problemDetails [5] UDMProblemDetails OPTIONAL

}

UDMUEAuthenticationResponse ::= SEQUENCE

{

sUPI [1] SUPI,

authenticationInfoRequest [2] UDMAuthenticationInfoRequest,

aKMAIndicator [3] BOOLEAN OPTIONAL,

problemDetails [4] UDMProblemDetails OPTIONAL

}

-- =================

-- 5G UDM parameters

-- =================

UDMServingSystemMethod ::= ENUMERATED

{

amf3GPPAccessRegistration(0),

amfNon3GPPAccessRegistration(1),

unknown(2)

}

UDMSubscriberRecordChangeMethod ::= ENUMERATED

{

pEIChange(1),

sUPIChange(2),

gPSIChange(3),

uEDeprovisioning(4),

unknown(5),

serviceIDChange(6)

}

UDMCancelLocationMethod ::= ENUMERATED

{

aMF3GPPAccessDeregistration(1),

aMFNon3GPPAccessDeregistration(2),

uDMDeregistration(3),

unknown(4)

}

ServiceID ::= SEQUENCE

{

nSSAI [1] NSSAI OPTIONAL,

cAGID [2] SEQUENCE OF CAGID OPTIONAL

}

CAGID ::= UTF8String

UDMAuthenticationInfoRequest ::= SEQUENCE

{

infoRequestType [1] UDMInfoRequestType,

rGAuthCtx [2] SEQUENCE SIZE(1..MAX) OF SubscriberIdentifier,

authType [3] PrimaryAuthenticationType,

servingNetworkName [4] PLMNID,

aUSFInstanceID [5] NFID OPTIONAL,

cellCAGInfo [6] CAGID OPTIONAL,

n5GCIndicator [7] BOOLEAN OPTIONAL

}

UDMLocationInfoRequest ::= SEQUENCE

{

requested5GSLocation [1] BOOLEAN OPTIONAL,

requestedCurrentLocation [2] BOOLEAN OPTIONAL,

requestedRATType [3] BOOLEAN OPTIONAL,

requestedTimeZone [4] BOOLEAN OPTIONAL,

requestedServingNode [5] BOOLEAN OPTIONAL

}

UDMProblemDetails ::= SEQUENCE

{

cause [1] UDMProblemDetailsCause OPTIONAL

}

UDMProblemDetailsCause ::= CHOICE

{

uDMDefinedCause [1] UDMDefinedCause,

otherCause [2] UDMProblemDetailsOtherCause

}

UDMDefinedCause ::= ENUMERATED

{

userNotFound(1),

dataNotFound(2),

contextNotFound(3),

subscriptionNotFound(4),

other(5)

}

UDMInfoRequestType ::= ENUMERATED

{

hSS(1),

aUSF(2),

other(3)

}

UDMProblemDetailsOtherCause ::= SEQUENCE

{

problemDetailsType [1] UTF8String OPTIONAL,

title [2] UTF8String OPTIONAL,

status [3] INTEGER OPTIONAL,

detail [4] UTF8String OPTIONAL,

instance [5] UTF8String OPTIONAL,

cause [6] UTF8String OPTIONAL,

uDMInvalidParameters [7] UDMInvalidParameters,

uDMSupportedFeatures [8] UTF8String

}

UDMInvalidParameters ::= SEQUENCE

{

parameter [1] UTF8String OPTIONAL,

reason [2] UTF8String OPTIONAL

}

-- ===================

-- 5G SMSF definitions

-- ===================

-- See clause 6.2.5.3 for details of this structure

SMSMessage ::= SEQUENCE

{

originatingSMSParty [1] SMSParty,

terminatingSMSParty [2] SMSParty,

direction [3] Direction,

linkTransferStatus [4] SMSTransferStatus,

otherMessage [5] SMSOtherMessageIndication OPTIONAL,

location [6] Location OPTIONAL,

peerNFAddress [7] SMSNFAddress OPTIONAL,

peerNFType [8] SMSNFType OPTIONAL,

sMSTPDUData [9] SMSTPDUData OPTIONAL,

messageType [10] SMSMessageType OPTIONAL,

rPMessageReference [11] SMSRPMessageReference OPTIONAL

}

SMSReport ::= SEQUENCE

{

location [1] Location OPTIONAL,

sMSTPDUData [2] SMSTPDUData,

messageType [3] SMSMessageType,

rPMessageReference [4] SMSRPMessageReference

}

-- ==================

-- 5G SMSF parameters

-- ==================

SMSAddress ::= OCTET STRING(SIZE(2..12))

SMSMessageType ::= ENUMERATED

{

deliver(1),

deliverReportAck(2),

deliverReportError(3),

statusReport(4),

command(5),

submit(6),

submitReportAck(7),

submitReportError(8),

reserved(9)

}

SMSParty ::= SEQUENCE

{

sUPI [1] SUPI OPTIONAL,

pEI [2] PEI OPTIONAL,

gPSI [3] GPSI OPTIONAL,

sMSAddress [4] SMSAddress OPTIONAL

}

SMSTransferStatus ::= ENUMERATED

{

transferSucceeded(1),

transferFailed(2),

undefined(3)

}

SMSOtherMessageIndication ::= BOOLEAN

SMSNFAddress ::= CHOICE

{

iPAddress [1] IPAddress,

e164Number [2] E164Number

}

SMSNFType ::= ENUMERATED

{

sMSGMSC(1),

iWMSC(2),

sMSRouter(3)

}

SMSRPMessageReference ::= INTEGER (0..255)

SMSTPDUData ::= CHOICE

{

sMSTPDU [1] SMSTPDU,

truncatedSMSTPDU [2] TruncatedSMSTPDU

}

SMSTPDU ::= OCTET STRING (SIZE(1..270))

TruncatedSMSTPDU ::= OCTET STRING (SIZE(1..130))

-- ===============

-- MMS definitions

-- ===============

MMSSend ::= SEQUENCE

{

transactionID [1] UTF8String,

version [2] MMSVersion,

dateTime [3] Timestamp,

originatingMMSParty [4] MMSParty,

terminatingMMSParty [5] SEQUENCE OF MMSParty OPTIONAL,

cCRecipients [6] SEQUENCE OF MMSParty OPTIONAL,

bCCRecipients [7] SEQUENCE OF MMSParty OPTIONAL,

direction [8] MMSDirection,

subject [9] MMSSubject OPTIONAL,

messageClass [10] MMSMessageClass OPTIONAL,

expiry [11] MMSExpiry,

desiredDeliveryTime [12] Timestamp OPTIONAL,

priority [13] MMSPriority OPTIONAL,

senderVisibility [14] BOOLEAN OPTIONAL,

deliveryReport [15] BOOLEAN OPTIONAL,

readReport [16] BOOLEAN OPTIONAL,

store [17] BOOLEAN OPTIONAL,

state [18] MMState OPTIONAL,

flags [19] MMFlags OPTIONAL,

replyCharging [20] MMSReplyCharging OPTIONAL,

applicID [21] UTF8String OPTIONAL,

replyApplicID [22] UTF8String OPTIONAL,

auxApplicInfo [23] UTF8String OPTIONAL,

contentClass [24] MMSContentClass OPTIONAL,

dRMContent [25] BOOLEAN OPTIONAL,

adaptationAllowed [26] MMSAdaptation OPTIONAL,

contentType [27] MMSContentType,

responseStatus [28] MMSResponseStatus,

responseStatusText [29] UTF8String OPTIONAL,

messageID [30] UTF8String

}

MMSSendByNonLocalTarget ::= SEQUENCE

{

version [1] MMSVersion,

transactionID [2] UTF8String,

messageID [3] UTF8String,

terminatingMMSParty [4] SEQUENCE OF MMSParty,

originatingMMSParty [5] MMSParty,

direction [6] MMSDirection,

contentType [7] MMSContentType,

messageClass [8] MMSMessageClass OPTIONAL,

dateTime [9] Timestamp,

expiry [10] MMSExpiry OPTIONAL,

deliveryReport [11] BOOLEAN OPTIONAL,

priority [12] MMSPriority OPTIONAL,

senderVisibility [13] BOOLEAN OPTIONAL,

readReport [14] BOOLEAN OPTIONAL,

subject [15] MMSSubject OPTIONAL,

forwardCount [16] INTEGER OPTIONAL,

previouslySentBy [17] MMSPreviouslySentBy OPTIONAL,

prevSentByDateTime [18] Timestamp OPTIONAL,

applicID [19] UTF8String OPTIONAL,

replyApplicID [20] UTF8String OPTIONAL,

auxApplicInfo [21] UTF8String OPTIONAL,

contentClass [22] MMSContentClass OPTIONAL,

dRMContent [23] BOOLEAN OPTIONAL,

adaptationAllowed [24] MMSAdaptation OPTIONAL

}

MMSNotification ::= SEQUENCE

{

transactionID [1] UTF8String,

version [2] MMSVersion,

originatingMMSParty [3] MMSParty OPTIONAL,

direction [4] MMSDirection,

subject [5] MMSSubject OPTIONAL,

deliveryReportRequested [6] BOOLEAN OPTIONAL,

stored [7] BOOLEAN OPTIONAL,

messageClass [8] MMSMessageClass,

priority [9] MMSPriority OPTIONAL,

messageSize [10] INTEGER,

expiry [11] MMSExpiry,

replyCharging [12] MMSReplyCharging OPTIONAL

}

MMSSendToNonLocalTarget ::= SEQUENCE

{

version [1] MMSVersion,

transactionID [2] UTF8String,

messageID [3] UTF8String,

terminatingMMSParty [4] SEQUENCE OF MMSParty,

originatingMMSParty [5] MMSParty,

direction [6] MMSDirection,

contentType [7] MMSContentType,

messageClass [8] MMSMessageClass OPTIONAL,

dateTime [9] Timestamp,

expiry [10] MMSExpiry OPTIONAL,

deliveryReport [11] BOOLEAN OPTIONAL,

priority [12] MMSPriority OPTIONAL,

senderVisibility [13] BOOLEAN OPTIONAL,

readReport [14] BOOLEAN OPTIONAL,

subject [15] MMSSubject OPTIONAL,

forwardCount [16] INTEGER OPTIONAL,

previouslySentBy [17] MMSPreviouslySentBy OPTIONAL,

prevSentByDateTime [18] Timestamp OPTIONAL,

applicID [19] UTF8String OPTIONAL,

replyApplicID [20] UTF8String OPTIONAL,

auxApplicInfo [21] UTF8String OPTIONAL,

contentClass [22] MMSContentClass OPTIONAL,

dRMContent [23] BOOLEAN OPTIONAL,

adaptationAllowed [24] MMSAdaptation OPTIONAL

}

MMSNotificationResponse ::= SEQUENCE

{

transactionID [1] UTF8String,

version [2] MMSVersion,

direction [3] MMSDirection,

status [4] MMStatus,

reportAllowed [5] BOOLEAN OPTIONAL

}

MMSRetrieval ::= SEQUENCE

{

transactionID [1] UTF8String,

version [2] MMSVersion,

messageID [3] UTF8String,

dateTime [4] Timestamp,

originatingMMSParty [5] MMSParty OPTIONAL,

previouslySentBy [6] MMSPreviouslySentBy OPTIONAL,

prevSentByDateTime [7] Timestamp OPTIONAL,

terminatingMMSParty [8] SEQUENCE OF MMSParty OPTIONAL,

cCRecipients [9] SEQUENCE OF MMSParty OPTIONAL,

direction [10] MMSDirection,

subject [11] MMSSubject OPTIONAL,

state [12] MMState OPTIONAL,

flags [13] MMFlags OPTIONAL,

messageClass [14] MMSMessageClass OPTIONAL,

priority [15] MMSPriority,

deliveryReport [16] BOOLEAN OPTIONAL,

readReport [17] BOOLEAN OPTIONAL,

replyCharging [18] MMSReplyCharging OPTIONAL,

retrieveStatus [19] MMSRetrieveStatus OPTIONAL,

retrieveStatusText [20] UTF8String OPTIONAL,

applicID [21] UTF8String OPTIONAL,

replyApplicID [22] UTF8String OPTIONAL,

auxApplicInfo [23] UTF8String OPTIONAL,

contentClass [24] MMSContentClass OPTIONAL,

dRMContent [25] BOOLEAN OPTIONAL,

replaceID [26] UTF8String OPTIONAL,

contentType [27] UTF8String OPTIONAL

}

MMSDeliveryAck ::= SEQUENCE

{

transactionID [1] UTF8String,

version [2] MMSVersion,

reportAllowed [3] BOOLEAN OPTIONAL,

status [4] MMStatus,

direction [5] MMSDirection

}

MMSForward ::= SEQUENCE

{

transactionID [1] UTF8String,

version [2] MMSVersion,

dateTime [3] Timestamp OPTIONAL,

originatingMMSParty [4] MMSParty,

terminatingMMSParty [5] SEQUENCE OF MMSParty OPTIONAL,

cCRecipients [6] SEQUENCE OF MMSParty OPTIONAL,

bCCRecipients [7] SEQUENCE OF MMSParty OPTIONAL,

direction [8] MMSDirection,

expiry [9] MMSExpiry OPTIONAL,

desiredDeliveryTime [10] Timestamp OPTIONAL,

deliveryReportAllowed [11] BOOLEAN OPTIONAL,

deliveryReport [12] BOOLEAN OPTIONAL,

store [13] BOOLEAN OPTIONAL,

state [14] MMState OPTIONAL,

flags [15] MMFlags OPTIONAL,

contentLocationReq [16] UTF8String,

replyCharging [17] MMSReplyCharging OPTIONAL,

responseStatus [18] MMSResponseStatus,

responseStatusText [19] UTF8String OPTIONAL,

messageID [20] UTF8String OPTIONAL,

contentLocationConf [21] UTF8String OPTIONAL,

storeStatus [22] MMSStoreStatus OPTIONAL,

storeStatusText [23] UTF8String OPTIONAL

}

MMSDeleteFromRelay ::= SEQUENCE

{

transactionID [1] UTF8String,

version [2] MMSVersion,

direction [3] MMSDirection,

contentLocationReq [4] SEQUENCE OF UTF8String,

contentLocationConf [5] SEQUENCE OF UTF8String,

deleteResponseStatus [6] MMSDeleteResponseStatus,

deleteResponseText [7] SEQUENCE OF UTF8String

}

MMSMBoxStore ::= SEQUENCE

{

transactionID [1] UTF8String,

version [2] MMSVersion,

direction [3] MMSDirection,

contentLocationReq [4] UTF8String,

state [5] MMState OPTIONAL,

flags [6] MMFlags OPTIONAL,

contentLocationConf [7] UTF8String OPTIONAL,

storeStatus [8] MMSStoreStatus,

storeStatusText [9] UTF8String OPTIONAL

}

MMSMBoxUpload ::= SEQUENCE

{

transactionID [1] UTF8String,

version [2] MMSVersion,

direction [3] MMSDirection,

state [4] MMState OPTIONAL,

flags [5] MMFlags OPTIONAL,

contentType [6] UTF8String,

contentLocation [7] UTF8String OPTIONAL,

storeStatus [8] MMSStoreStatus,

storeStatusText [9] UTF8String OPTIONAL,

mMessages [10] SEQUENCE OF MMBoxDescription

}

MMSMBoxDelete ::= SEQUENCE

{

transactionID [1] UTF8String,

version [2] MMSVersion,

direction [3] MMSDirection,

contentLocationReq [4] SEQUENCE OF UTF8String,

contentLocationConf [5] SEQUENCE OF UTF8String OPTIONAL,

responseStatus [6] MMSDeleteResponseStatus,

responseStatusText [7] UTF8String OPTIONAL

}

MMSDeliveryReport ::= SEQUENCE

{

version [1] MMSVersion,

messageID [2] UTF8String,

terminatingMMSParty [3] SEQUENCE OF MMSParty,

mMSDateTime [4] Timestamp,

responseStatus [5] MMSResponseStatus,

responseStatusText [6] UTF8String OPTIONAL,

applicID [7] UTF8String OPTIONAL,

replyApplicID [8] UTF8String OPTIONAL,

auxApplicInfo [9] UTF8String OPTIONAL

}

MMSDeliveryReportNonLocalTarget ::= SEQUENCE

{

version [1] MMSVersion,

transactionID [2] UTF8String,

messageID [3] UTF8String,

terminatingMMSParty [4] SEQUENCE OF MMSParty,

originatingMMSParty [5] MMSParty,

direction [6] MMSDirection,

mMSDateTime [7] Timestamp,

forwardToOriginator [8] BOOLEAN OPTIONAL,

status [9] MMStatus,

statusExtension [10] MMStatusExtension,

statusText [11] MMStatusText,

applicID [12] UTF8String OPTIONAL,

replyApplicID [13] UTF8String OPTIONAL,

auxApplicInfo [14] UTF8String OPTIONAL

}

MMSReadReport ::= SEQUENCE

{

version [1] MMSVersion,

messageID [2] UTF8String,

terminatingMMSParty [3] SEQUENCE OF MMSParty,

originatingMMSParty [4] SEQUENCE OF MMSParty,

direction [5] MMSDirection,

mMSDateTime [6] Timestamp,

readStatus [7] MMSReadStatus,

applicID [8] UTF8String OPTIONAL,

replyApplicID [9] UTF8String OPTIONAL,

auxApplicInfo [10] UTF8String OPTIONAL

}

MMSReadReportNonLocalTarget ::= SEQUENCE

{

version [1] MMSVersion,

transactionID [2] UTF8String,

terminatingMMSParty [3] SEQUENCE OF MMSParty,

originatingMMSParty [4] SEQUENCE OF MMSParty,

direction [5] MMSDirection,

messageID [6] UTF8String,

mMSDateTime [7] Timestamp,

readStatus [8] MMSReadStatus,

readStatusText [9] MMSReadStatusText OPTIONAL,

applicID [10] UTF8String OPTIONAL,

replyApplicID [11] UTF8String OPTIONAL,

auxApplicInfo [12] UTF8String OPTIONAL

}

MMSCancel ::= SEQUENCE

{

transactionID [1] UTF8String,

version [2] MMSVersion,

cancelID [3] UTF8String,

direction [4] MMSDirection

}

MMSMBoxViewRequest ::= SEQUENCE

{

transactionID [1] UTF8String,

version [2] MMSVersion,

contentLocation [3] UTF8String OPTIONAL,

state [4] SEQUENCE OF MMState OPTIONAL,

flags [5] SEQUENCE OF MMFlags OPTIONAL,

start [6] INTEGER OPTIONAL,

limit [7] INTEGER OPTIONAL,

attributes [8] SEQUENCE OF UTF8String OPTIONAL,

totals [9] INTEGER OPTIONAL,

quotas [10] MMSQuota OPTIONAL

}

MMSMBoxViewResponse ::= SEQUENCE

{

transactionID [1] UTF8String,

version [2] MMSVersion,

contentLocation [3] UTF8String OPTIONAL,

state [4] SEQUENCE OF MMState OPTIONAL,

flags [5] SEQUENCE OF MMFlags OPTIONAL,

start [6] INTEGER OPTIONAL,

limit [7] INTEGER OPTIONAL,

attributes [8] SEQUENCE OF UTF8String OPTIONAL,

mMSTotals [9] BOOLEAN OPTIONAL,

mMSQuotas [10] BOOLEAN OPTIONAL,

mMessages [11] SEQUENCE OF MMBoxDescription

}

MMBoxDescription ::= SEQUENCE

{

contentLocation [1] UTF8String OPTIONAL,

messageID [2] UTF8String OPTIONAL,

state [3] MMState OPTIONAL,

flags [4] SEQUENCE OF MMFlags OPTIONAL,

dateTime [5] Timestamp OPTIONAL,

originatingMMSParty [6] MMSParty OPTIONAL,

terminatingMMSParty [7] SEQUENCE OF MMSParty OPTIONAL,

cCRecipients [8] SEQUENCE OF MMSParty OPTIONAL,

bCCRecipients [9] SEQUENCE OF MMSParty OPTIONAL,

messageClass [10] MMSMessageClass OPTIONAL,

subject [11] MMSSubject OPTIONAL,

priority [12] MMSPriority OPTIONAL,

deliveryTime [13] Timestamp OPTIONAL,

readReport [14] BOOLEAN OPTIONAL,

messageSize [15] INTEGER OPTIONAL,

replyCharging [16] MMSReplyCharging OPTIONAL,

previouslySentBy [17] MMSPreviouslySentBy OPTIONAL,

previouslySentByDateTime [18] Timestamp OPTIONAL,

contentType [19] UTF8String OPTIONAL

}

-- =========

-- MMS CCPDU

-- =========

MMSCCPDU ::= SEQUENCE

{

version [1] MMSVersion,

transactionID [2] UTF8String,

mMSContent [3] OCTET STRING

}

-- ==============

-- MMS parameters

-- ==============

MMSAdaptation ::= SEQUENCE

{

allowed [1] BOOLEAN,

overriden [2] BOOLEAN

}

MMSCancelStatus ::= ENUMERATED

{

cancelRequestSuccessfullyReceived(1),

cancelRequestCorrupted(2)

}

MMSContentClass ::= ENUMERATED

{

text(1),

imageBasic(2),

imageRich(3),

videoBasic(4),

videoRich(5),

megaPixel(6),

contentBasic(7),

contentRich(8)

}

MMSContentType ::= UTF8String

MMSDeleteResponseStatus ::= ENUMERATED

{

ok(1),

errorUnspecified(2),

errorServiceDenied(3),

errorMessageFormatCorrupt(4),

errorSendingAddressUnresolved(5),

errorMessageNotFound(6),

errorNetworkProblem(7),

errorContentNotAccepted(8),

errorUnsupportedMessage(9),

errorTransientFailure(10),

errorTransientSendingAddressUnresolved(11),

errorTransientMessageNotFound(12),

errorTransientNetworkProblem(13),

errorTransientPartialSuccess(14),

errorPermanentFailure(15),

errorPermanentServiceDenied(16),

errorPermanentMessageFormatCorrupt(17),

errorPermanentSendingAddressUnresolved(18),

errorPermanentMessageNotFound(19),

errorPermanentContentNotAccepted(20),

errorPermanentReplyChargingLimitationsNotMet(21),

errorPermanentReplyChargingRequestNotAccepted(22),

errorPermanentReplyChargingForwardingDenied(23),

errorPermanentReplyChargingNotSupported(24),

errorPermanentAddressHidingNotSupported(25),

errorPermanentLackOfPrepaid(26)

}

MMSDirection ::= ENUMERATED

{

fromTarget(0),

toTarget(1)

}

MMSElementDescriptor ::= SEQUENCE

{

reference [1] UTF8String,

parameter [2] UTF8String OPTIONAL,

value [3] UTF8String OPTIONAL

}

MMSExpiry ::= SEQUENCE

{

expiryPeriod [1] INTEGER,

periodFormat [2] MMSPeriodFormat

}

MMFlags ::= SEQUENCE

{

length [1] INTEGER,

flag [2] MMStateFlag,

flagString [3] UTF8String

}

MMSMessageClass ::= ENUMERATED

{

personal(1),

advertisement(2),

informational(3),

auto(4)

}

MMSParty ::= SEQUENCE

{

mMSPartyIDs [1] SEQUENCE OF MMSPartyID,

nonLocalID [2] NonLocalID

}

MMSPartyID ::= CHOICE

{

e164Number [1] E164Number,

emailAddress [2] EmailAddress,

iMSI [3] IMSI,

iMPU [4] IMPU,

iMPI [5] IMPI,

sUPI [6] SUPI,

gPSI [7] GPSI

}

MMSPeriodFormat ::= ENUMERATED

{

absolute(1),

relative(2)

}

MMSPreviouslySent ::= SEQUENCE

{

previouslySentByParty [1] MMSParty,

sequenceNumber [2] INTEGER,

previousSendDateTime [3] Timestamp

}

MMSPreviouslySentBy ::= SEQUENCE OF MMSPreviouslySent

MMSPriority ::= ENUMERATED

{

low(1),

normal(2),

high(3)

}

MMSQuota ::= SEQUENCE

{

quota [1] INTEGER,

quotaUnit [2] MMSQuotaUnit

}

MMSQuotaUnit ::= ENUMERATED

{

numMessages(1),

bytes(2)

}

MMSReadStatus ::= ENUMERATED

{

read(1),

deletedWithoutBeingRead(2)

}

MMSReadStatusText ::= UTF8String

MMSReplyCharging ::= ENUMERATED

{

requested(0),

requestedTextOnly(1),

accepted(2),

acceptedTextOnly(3)

}

MMSResponseStatus ::= ENUMERATED

{

ok(1),

errorUnspecified(2),

errorServiceDenied(3),

errorMessageFormatCorrupt(4),

errorSendingAddressUnresolved(5),

errorMessageNotFound(6),

errorNetworkProblem(7),

errorContentNotAccepted(8),

errorUnsupportedMessage(9),

errorTransientFailure(10),

errorTransientSendingAddressUnresolved(11),

errorTransientMessageNotFound(12),

errorTransientNetworkProblem(13),

errorTransientPartialSuccess(14),

errorPermanentFailure(15),

errorPermanentServiceDenied(16),

errorPermanentMessageFormatCorrupt(17),

errorPermanentSendingAddressUnresolved(18),

errorPermanentMessageNotFound(19),

errorPermanentContentNotAccepted(20),

errorPermanentReplyChargingLimitationsNotMet(21),

errorPermanentReplyChargingRequestNotAccepted(22),

errorPermanentReplyChargingForwardingDenied(23),

errorPermanentReplyChargingNotSupported(24),

errorPermanentAddressHidingNotSupported(25),

errorPermanentLackOfPrepaid(26)

}

MMSRetrieveStatus ::= ENUMERATED

{

success(1),

errorTransientFailure(2),

errorTransientMessageNotFound(3),

errorTransientNetworkProblem(4),

errorPermanentFailure(5),

errorPermanentServiceDenied(6),

errorPermanentMessageNotFound(7),

errorPermanentContentUnsupported(8)

}

MMSStoreStatus ::= ENUMERATED

{

success(1),

errorTransientFailure(2),

errorTransientNetworkProblem(3),

errorPermanentFailure(4),

errorPermanentServiceDenied(5),

errorPermanentMessageFormatCorrupt(6),

errorPermanentMessageNotFound(7),

errorMMBoxFull(8)

}

MMState ::= ENUMERATED

{

draft(1),

sent(2),

new(3),

retrieved(4),

forwarded(5)

}

MMStateFlag ::= ENUMERATED

{

add(1),

remove(2),

filter(3)

}

MMStatus ::= ENUMERATED

{

expired(1),

retrieved(2),

rejected(3),

deferred(4),

unrecognized(5),

indeterminate(6),

forwarded(7),

unreachable(8)

}

MMStatusExtension ::= ENUMERATED

{

rejectionByMMSRecipient(0),

rejectionByOtherRS(1)

}

MMStatusText ::= UTF8String

MMSSubject ::= UTF8String

MMSVersion ::= SEQUENCE

{

majorVersion [1] INTEGER,

minorVersion [2] INTEGER

}

-- ==================

-- 5G PTC definitions

-- ==================

PTCRegistration ::= SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCServerURI [2] UTF8String,

pTCRegistrationRequest [3] PTCRegistrationRequest,

pTCRegistrationOutcome [4] PTCRegistrationOutcome

}

PTCSessionInitiation ::= SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCDirection [2] Direction,

pTCServerURI [3] UTF8String,

pTCSessionInfo [4] PTCSessionInfo,

pTCOriginatingID [5] PTCTargetInformation,

pTCParticipants [6] SEQUENCE OF PTCTargetInformation OPTIONAL,

pTCParticipantPresenceStatus [7] MultipleParticipantPresenceStatus OPTIONAL,

location [8] Location OPTIONAL,

pTCBearerCapability [9] UTF8String OPTIONAL,

pTCHost [10] PTCTargetInformation OPTIONAL

}

PTCSessionAbandon ::= SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCDirection [2] Direction,

pTCSessionInfo [3] PTCSessionInfo,

location [4] Location OPTIONAL,

pTCAbandonCause [5] INTEGER

}

PTCSessionStart ::= SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCDirection [2] Direction,

pTCServerURI [3] UTF8String,

pTCSessionInfo [4] PTCSessionInfo,

pTCOriginatingID [5] PTCTargetInformation,

pTCParticipants [6] SEQUENCE OF PTCTargetInformation OPTIONAL,

pTCParticipantPresenceStatus [7] MultipleParticipantPresenceStatus OPTIONAL,

location [8] Location OPTIONAL,

pTCHost [9] PTCTargetInformation OPTIONAL,

pTCBearerCapability [10] UTF8String OPTIONAL

}

PTCSessionEnd ::= SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCDirection [2] Direction,

pTCServerURI [3] UTF8String,

pTCSessionInfo [4] PTCSessionInfo,

pTCParticipants [5] SEQUENCE OF PTCTargetInformation OPTIONAL,

location [6] Location OPTIONAL,

pTCSessionEndCause [7] PTCSessionEndCause

}

PTCStartOfInterception ::= SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCDirection [2] Direction,

preEstSessionID [3] PTCSessionInfo OPTIONAL,

pTCOriginatingID [4] PTCTargetInformation,

pTCSessionInfo [5] PTCSessionInfo OPTIONAL,

pTCHost [6] PTCTargetInformation OPTIONAL,

pTCParticipants [7] SEQUENCE OF PTCTargetInformation OPTIONAL,

pTCMediaStreamAvail [8] BOOLEAN OPTIONAL,

pTCBearerCapability [9] UTF8String OPTIONAL

}

PTCPreEstablishedSession ::= SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCServerURI [2] UTF8String,

rTPSetting [3] RTPSetting,

pTCMediaCapability [4] UTF8String,

pTCPreEstSessionID [5] PTCSessionInfo,

pTCPreEstStatus [6] PTCPreEstStatus,

pTCMediaStreamAvail [7] BOOLEAN OPTIONAL,

location [8] Location OPTIONAL,

pTCFailureCode [9] PTCFailureCode OPTIONAL

}

PTCInstantPersonalAlert ::= SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCIPAPartyID [2] PTCTargetInformation,

pTCIPADirection [3] Direction

}

PTCPartyJoin ::= SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCDirection [2] Direction,

pTCSessionInfo [3] PTCSessionInfo,

pTCParticipants [4] SEQUENCE OF PTCTargetInformation OPTIONAL,

pTCParticipantPresenceStatus [5] MultipleParticipantPresenceStatus OPTIONAL,

pTCMediaStreamAvail [6] BOOLEAN OPTIONAL,

pTCBearerCapability [7] UTF8String OPTIONAL

}

PTCPartyDrop ::= SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCDirection [2] Direction,

pTCSessionInfo [3] PTCSessionInfo,

pTCPartyDrop [4] PTCTargetInformation,

pTCParticipantPresenceStatus [5] PTCParticipantPresenceStatus OPTIONAL

}

PTCPartyHold ::= SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCDirection [2] Direction,

pTCSessionInfo [3] PTCSessionInfo,

pTCParticipants [4] SEQUENCE OF PTCTargetInformation OPTIONAL,

pTCHoldID [5] SEQUENCE OF PTCTargetInformation,

pTCHoldRetrieveInd [6] BOOLEAN

}

PTCMediaModification ::= SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCDirection [2] Direction,

pTCSessionInfo [3] PTCSessionInfo,

pTCMediaStreamAvail [4] BOOLEAN OPTIONAL,

pTCBearerCapability [5] UTF8String

}

PTCGroupAdvertisement ::=SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCDirection [2] Direction,

pTCIDList [3] SEQUENCE OF PTCTargetInformation OPTIONAL,

pTCGroupAuthRule [4] PTCGroupAuthRule OPTIONAL,

pTCGroupAdSender [5] PTCTargetInformation,

pTCGroupNickname [6] UTF8String OPTIONAL

}

PTCFloorControl ::= SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCDirection [2] Direction,

pTCSessioninfo [3] PTCSessionInfo,

pTCFloorActivity [4] SEQUENCE OF PTCFloorActivity,

pTCFloorSpeakerID [5] PTCTargetInformation OPTIONAL,

pTCMaxTBTime [6] INTEGER OPTIONAL,

pTCQueuedFloorControl [7] BOOLEAN OPTIONAL,

pTCQueuedPosition [8] INTEGER OPTIONAL,

pTCTalkBurstPriority [9] PTCTBPriorityLevel OPTIONAL,

pTCTalkBurstReason [10] PTCTBReasonCode OPTIONAL

}

PTCTargetPresence ::= SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCTargetPresenceStatus [2] PTCParticipantPresenceStatus

}

PTCParticipantPresence ::= SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCParticipantPresenceStatus [2] PTCParticipantPresenceStatus

}

PTCListManagement ::= SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCDirection [2] Direction,

pTCListManagementType [3] PTCListManagementType OPTIONAL,

pTCListManagementAction [4] PTCListManagementAction OPTIONAL,

pTCListManagementFailure [5] PTCListManagementFailure OPTIONAL,

pTCContactID [6] PTCTargetInformation OPTIONAL,

pTCIDList [7] SEQUENCE OF PTCIDList OPTIONAL,

pTCHost [8] PTCTargetInformation OPTIONAL

}

PTCAccessPolicy ::= SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCDirection [2] Direction,

pTCAccessPolicyType [3] PTCAccessPolicyType OPTIONAL,

pTCUserAccessPolicy [4] PTCUserAccessPolicy OPTIONAL,

pTCGroupAuthRule [5] PTCGroupAuthRule OPTIONAL,

pTCContactID [6] PTCTargetInformation OPTIONAL,

pTCAccessPolicyFailure [7] PTCAccessPolicyFailure OPTIONAL

}

-- =========

-- PTC CCPDU

-- =========

PTCCCPDU ::= OCTET STRING

-- =================

-- 5G PTC parameters

-- =================

PTCRegistrationRequest ::= ENUMERATED

{

register(1),

reRegister(2),

deRegister(3)

}

PTCRegistrationOutcome ::= ENUMERATED

{

success(1),

failure(2)

}

PTCSessionEndCause ::= ENUMERATED

{

initiaterLeavesSession(1),

definedParticipantLeaves(2),

numberOfParticipants(3),

sessionTimerExpired(4),

pTCSpeechInactive(5),

allMediaTypesInactive(6)

}

PTCTargetInformation ::= SEQUENCE

{

identifiers [1] SEQUENCE SIZE(1..MAX) OF PTCIdentifiers

}

PTCIdentifiers ::= CHOICE

{

mCPTTID [1] UTF8String,

instanceIdentifierURN [2] UTF8String,

pTCChatGroupID [3] PTCChatGroupID,

iMPU [4] IMPU,

iMPI [5] IMPI

}

PTCSessionInfo ::= SEQUENCE

{

pTCSessionURI [1] UTF8String,

pTCSessionType [2] PTCSessionType

}

PTCSessionType ::= ENUMERATED

{

ondemand(1),

preEstablished(2),

adhoc(3),

prearranged(4),

groupSession(5)

}

MultipleParticipantPresenceStatus ::= SEQUENCE OF PTCParticipantPresenceStatus

PTCParticipantPresenceStatus ::= SEQUENCE

{

presenceID [1] PTCTargetInformation,

presenceType [2] PTCPresenceType,

presenceStatus [3] BOOLEAN

}

PTCPresenceType ::= ENUMERATED

{

pTCClient(1),

pTCGroup(2)

}

PTCPreEstStatus ::= ENUMERATED

{

established(1),

modified(2),

released(3)

}

RTPSetting ::= SEQUENCE

{

iPAddress [1] IPAddress,

portNumber [2] PortNumber

}

PTCIDList ::= SEQUENCE

{

pTCPartyID [1] PTCTargetInformation,

pTCChatGroupID [2] PTCChatGroupID

}

PTCChatGroupID ::= SEQUENCE

{

groupIdentity [1] UTF8String

}

PTCFloorActivity ::= ENUMERATED

{

tBCPRequest(1),

tBCPGranted(2),

tBCPDeny(3),

tBCPIdle(4),

tBCPTaken(5),

tBCPRevoke(6),

tBCPQueued(7),

tBCPRelease(8)

}

PTCTBPriorityLevel ::= ENUMERATED

{

preEmptive(1),

highPriority(2),

normalPriority(3),

listenOnly(4)

}

PTCTBReasonCode ::= ENUMERATED

{

noQueuingAllowed(1),

oneParticipantSession(2),

listenOnly(3),

exceededMaxDuration(4),

tBPrevented(5)

}

PTCListManagementType ::= ENUMERATED

{

contactListManagementAttempt(1),

groupListManagementAttempt(2),

contactListManagementResult(3),

groupListManagementResult(4),

requestUnsuccessful(5)

}

PTCListManagementAction ::= ENUMERATED

{

create(1),

modify(2),

retrieve(3),

delete(4),

notify(5)

}

PTCAccessPolicyType ::= ENUMERATED

{

pTCUserAccessPolicyAttempt(1),

groupAuthorizationRulesAttempt(2),

pTCUserAccessPolicyQuery(3),

groupAuthorizationRulesQuery(4),

pTCUserAccessPolicyResult(5),

groupAuthorizationRulesResult(6),

requestUnsuccessful(7)

}

PTCUserAccessPolicy ::= ENUMERATED

{

allowIncomingPTCSessionRequest(1),

blockIncomingPTCSessionRequest(2),

allowAutoAnswerMode(3),

allowOverrideManualAnswerMode(4)

}

PTCGroupAuthRule ::= ENUMERATED

{

allowInitiatingPTCSession(1),

blockInitiatingPTCSession(2),

allowJoiningPTCSession(3),

blockJoiningPTCSession(4),

allowAddParticipants(5),

blockAddParticipants(6),

allowSubscriptionPTCSessionState(7),

blockSubscriptionPTCSessionState(8),

allowAnonymity(9),

forbidAnonymity(10)

}

PTCFailureCode ::= ENUMERATED

{

sessionCannotBeEstablished(1),

sessionCannotBeModified(2)

}

PTCListManagementFailure ::= ENUMERATED

{

requestUnsuccessful(1),

requestUnknown(2)

}

PTCAccessPolicyFailure ::= ENUMERATED

{

requestUnsuccessful(1),

requestUnknown(2)

}

-- ===============

-- IMS definitions

-- ===============

-- See clause 7.12.4.2.1 for details of this structure

IMSMessage ::= SEQUENCE

{

payload [1] IMSPayload,

sessionDirection [2] SessionDirection,

voIPRoamingIndication [3] VoIPRoamingIndication OPTIONAL,

location [6] Location OPTIONAL

}

-- See clause 7.12.4.2.3 for details of this structure

StartOfInterceptionForActiveIMSSession ::= SEQUENCE

{

originatingId [1] SEQUENCE OF IMPU,

terminatingId [2] IMPU,

sDPState [3] SEQUENCE OF OCTET STRING OPTIONAL,

diversionIdentity [4] IMPU OPTIONAL,

voIPRoamingIndication [5] VoIPRoamingIndication OPTIONAL,

location [7] Location OPTIONAL

}

-- ==============

-- IMS parameters

-- ==============

IMSPayload ::= CHOICE

{

encapsulatedSIPMessage [1] SIPMessage

}

SIPMessage ::= SEQUENCE

{

iPSourceAddress [1] IPAddress,

iPDestinationAddress [2] IPAddress,

sIPContent [3] OCTET STRING

}

VoIPRoamingIndication ::= ENUMERATED

{

roamingLBO(1),

roamingS8HR(2),

roamingN9HR(3)

}

SessionDirection ::= ENUMERATED

{

fromTarget(1),

toTarget(2),

combined(3),

indeterminate(4)

}

HeaderOnlyIndication ::= BOOLEAN

-- =================================

-- STIR/SHAKEN/RCD/eCNAM definitions

-- =================================

-- See clause 7.11.2.1.2 for details of this structure

STIRSHAKENSignatureGeneration ::= SEQUENCE

{

pASSporTs [1] SEQUENCE OF PASSporT

}

-- See clause 7.11.2.1.3 for details of this structure

STIRSHAKENSignatureValidation ::= SEQUENCE

{

pASSporTs [1] SEQUENCE OF PASSporT OPTIONAL,

rCDTerminalDisplayInfo [2] RCDDisplayInfo OPTIONAL,

eCNAMTerminalDisplayInfo [3] ECNAMDisplayInfo OPTIONAL,

sHAKENValidationResult [4] SHAKENValidationResult,

sHAKENFailureStatusCode [5] SHAKENFailureStatusCode OPTIONAL

}

-- ================================

-- STIR/SHAKEN/RCD/eCNAM parameters

-- ================================

PASSporT ::= SEQUENCE

{

pASSporTHeader [1] PASSporTHeader,

pASSporTPayload [2] PASSporTPayload,

pASSporTSignature [3] OCTET STRING

}

PASSporTHeader ::= SEQUENCE

{

type [1] JWSTokenType,

algorithm [2] UTF8String,

ppt [3] UTF8String OPTIONAL,

x5u [4] UTF8String

}

JWSTokenType ::= ENUMERATED

{

passport(1)

}

PASSporTPayload ::= SEQUENCE

{

issuedAtTime [1] GeneralizedTime,

originator [2] STIRSHAKENOriginator,

destination [3] STIRSHAKENDestinations,

attestation [4] Attestation,

origId [5] UTF8String,

diversion [6] STIRSHAKENDestination

}

STIRSHAKENOriginator ::= CHOICE

{

telephoneNumber [1] STIRSHAKENTN,

sTIRSHAKENURI [2] UTF8String

}

STIRSHAKENDestinations ::= SEQUENCE OF STIRSHAKENDestination

STIRSHAKENDestination ::= CHOICE

{

telephoneNumber [1] STIRSHAKENTN,

sTIRSHAKENURI [2] UTF8String

}

STIRSHAKENTN ::= CHOICE

{

mSISDN [1] MSISDN

}

Attestation ::= ENUMERATED

{

attestationA(1),

attestationB(2),

attestationC(3)

}

SHAKENValidationResult ::= ENUMERATED

{

tNValidationPassed(1),

tNValidationFailed(2),

noTNValidation(3)

}

SHAKENFailureStatusCode ::= INTEGER

ECNAMDisplayInfo ::= SEQUENCE

{

name [1] UTF8String,

additionalInfo [2] OCTET STRING OPTIONAL

}

RCDDisplayInfo ::= SEQUENCE

{

name [1] UTF8String,

jcd [2] OCTET STRING OPTIONAL,

jcl [3] OCTET STRING OPTIONAL

}

-- ===================

-- 5G LALS definitions

-- ===================

LALSReport ::= SEQUENCE

{

sUPI [1] SUPI OPTIONAL,

-- pEI [2] PEI OPTIONAL, deprecated in Release-16, do not re-use this tag number

gPSI [3] GPSI OPTIONAL,

location [4] Location OPTIONAL,

iMPU [5] IMPU OPTIONAL,

iMSI [7] IMSI OPTIONAL,

mSISDN [8] MSISDN OPTIONAL

}

-- =====================

-- PDHR/PDSR definitions

-- =====================

PDHeaderReport ::= SEQUENCE

{

pDUSessionID [1] PDUSessionID,

sourceIPAddress [2] IPAddress,

sourcePort [3] PortNumber OPTIONAL,

destinationIPAddress [4] IPAddress,

destinationPort [5] PortNumber OPTIONAL,

nextLayerProtocol [6] NextLayerProtocol,

iPv6flowLabel [7] IPv6FlowLabel OPTIONAL,

direction [8] Direction,

packetSize [9] INTEGER

}

PDSummaryReport ::= SEQUENCE

{

pDUSessionID [1] PDUSessionID,

sourceIPAddress [2] IPAddress,

sourcePort [3] PortNumber OPTIONAL,

destinationIPAddress [4] IPAddress,

destinationPort [5] PortNumber OPTIONAL,

nextLayerProtocol [6] NextLayerProtocol,

iPv6flowLabel [7] IPv6FlowLabel OPTIONAL,

direction [8] Direction,

pDSRSummaryTrigger [9] PDSRSummaryTrigger,

firstPacketTimestamp [10] Timestamp,

lastPacketTimestamp [11] Timestamp,

packetCount [12] INTEGER,

byteCount [13] INTEGER

}

-- ====================

-- PDHR/PDSR parameters

-- ====================

PDSRSummaryTrigger ::= ENUMERATED

{

timerExpiry(1),

packetCount(2),

byteCount(3),

startOfFlow(4),

endOfFlow(5)

}

-- ==================================

-- Identifier Association definitions

-- ==================================

AMFIdentifierAssociation ::= SEQUENCE

{

sUPI [1] SUPI,

sUCI [2] SUCI OPTIONAL,

pEI [3] PEI OPTIONAL,

gPSI [4] GPSI OPTIONAL,

gUTI [5] FiveGGUTI,

location [6] Location,

fiveGSTAIList [7] TAIList OPTIONAL

}

MMEIdentifierAssociation ::= SEQUENCE

{

iMSI [1] IMSI,

iMEI [2] IMEI OPTIONAL,

mSISDN [3] MSISDN OPTIONAL,

gUTI [4] GUTI,

location [5] Location,

tAIList [6] TAIList OPTIONAL

}

-- =================================

-- Identifier Association parameters

-- =================================

MMEGroupID ::= OCTET STRING (SIZE(2))

MMECode ::= OCTET STRING (SIZE(1))

TMSI ::= OCTET STRING (SIZE(4))

-- ===================

-- EPS MME definitions

-- ===================

MMEAttach ::= SEQUENCE

{

attachType [1] EPSAttachType,

attachResult [2] EPSAttachResult,

iMSI [3] IMSI,

iMEI [4] IMEI OPTIONAL,

mSISDN [5] MSISDN OPTIONAL,

gUTI [6] GUTI OPTIONAL,

location [7] Location OPTIONAL,

ePSTAIList [8] TAIList OPTIONAL,

sMSServiceStatus [9] EPSSMSServiceStatus OPTIONAL,

oldGUTI [10] GUTI OPTIONAL,

eMM5GRegStatus [11] EMM5GMMStatus OPTIONAL

}

MMEDetach ::= SEQUENCE

{

detachDirection [1] MMEDirection,

detachType [2] EPSDetachType,

iMSI [3] IMSI,

iMEI [4] IMEI OPTIONAL,

mSISDN [5] MSISDN OPTIONAL,

gUTI [6] GUTI OPTIONAL,

cause [7] EMMCause OPTIONAL,

location [8] Location OPTIONAL,

switchOffIndicator [9] SwitchOffIndicator OPTIONAL

}

MMELocationUpdate ::= SEQUENCE

{

iMSI [1] IMSI,

iMEI [2] IMEI OPTIONAL,

mSISDN [3] MSISDN OPTIONAL,

gUTI [4] GUTI OPTIONAL,

location [5] Location OPTIONAL,

oldGUTI [6] GUTI OPTIONAL,

sMSServiceStatus [7] EPSSMSServiceStatus OPTIONAL

}

MMEStartOfInterceptionWithEPSAttachedUE ::= SEQUENCE

{

attachType [1] EPSAttachType,

attachResult [2] EPSAttachResult,

iMSI [3] IMSI,

iMEI [4] IMEI OPTIONAL,

mSISDN [5] MSISDN OPTIONAL,

gUTI [6] GUTI OPTIONAL,

location [7] Location OPTIONAL,

ePSTAIList [9] TAIList OPTIONAL,

sMSServiceStatus [10] EPSSMSServiceStatus OPTIONAL,

eMM5GRegStatus [12] EMM5GMMStatus OPTIONAL

}

MMEUnsuccessfulProcedure ::= SEQUENCE

{

failedProcedureType [1] MMEFailedProcedureType,

failureCause [2] MMEFailureCause,

iMSI [3] IMSI OPTIONAL,

iMEI [4] IMEI OPTIONAL,

mSISDN [5] MSISDN OPTIONAL,

gUTI [6] GUTI OPTIONAL,

location [7] Location OPTIONAL

}

-- ==================

-- EPS MME parameters

-- ==================

EMMCause ::= INTEGER (0..255)

ESMCause ::= INTEGER (0..255)

EPSAttachType ::= ENUMERATED

{

ePSAttach(1),

combinedEPSIMSIAttach(2),

ePSRLOSAttach(3),

ePSEmergencyAttach(4),

reserved(5)

}

EPSAttachResult ::= ENUMERATED

{

ePSOnly(1),

combinedEPSIMSI(2)

}

EPSDetachType ::= ENUMERATED

{

ePSDetach(1),

iMSIDetach(2),

combinedEPSIMSIDetach(3),

reAttachRequired(4),

reAttachNotRequired(5),

reserved(6)

}

EPSSMSServiceStatus ::= ENUMERATED

{

sMSServicesNotAvailable(1),

sMSServicesNotAvailableInThisPLMN(2),

networkFailure(3),

congestion(4)

}

MMEDirection ::= ENUMERATED

{

networkInitiated(1),

uEInitiated(2)

}

MMEFailedProcedureType ::= ENUMERATED

{

attachReject(1),

authenticationReject(2),

securityModeReject(3),

serviceReject(4),

trackingAreaUpdateReject(5),

activateDedicatedEPSBearerContextReject(6),

activateDefaultEPSBearerContextReject(7),

bearerResourceAllocationReject(8),

bearerResourceModificationReject(9),

modifyEPSBearerContectReject(10),

pDNConnectivityReject(11),

pDNDisconnectReject(12)

}

MMEFailureCause ::= CHOICE

{

eMMCause [1] EMMCause,

eSMCause [2] ESMCause

}

-- ===========================

-- LI Notification definitions

-- ===========================

LINotification ::= SEQUENCE

{

notificationType [1] LINotificationType,

appliedTargetID [2] TargetIdentifier OPTIONAL,

appliedDeliveryInformation [3] SEQUENCE OF LIAppliedDeliveryInformation OPTIONAL,

appliedStartTime [4] Timestamp OPTIONAL,

appliedEndTime [5] Timestamp OPTIONAL

}

-- ==========================

-- LI Notification parameters

-- ==========================

LINotificationType ::= ENUMERATED

{

activation(1),

deactivation(2),

modification(3)

}

LIAppliedDeliveryInformation ::= SEQUENCE

{

hI2DeliveryIPAddress [1] IPAddress OPTIONAL,

hI2DeliveryPortNumber [2] PortNumber OPTIONAL,

hI3DeliveryIPAddress [3] IPAddress OPTIONAL,

hI3DeliveryPortNumber [4] PortNumber OPTIONAL

}

-- ===============

-- MDF definitions

-- ===============

MDFCellSiteReport ::= SEQUENCE OF CellInformation

-- ==============================

-- 5G EPS Interworking Parameters

-- ==============================

EMM5GMMStatus ::= SEQUENCE

{

eMMRegStatus [1] EMMRegStatus OPTIONAL,

fiveGMMStatus [2] FiveGMMStatus OPTIONAL

}

EPS5GGUTI ::= CHOICE

{

gUTI [1] GUTI,

fiveGGUTI [2] FiveGGUTI

}

EMMRegStatus ::= ENUMERATED

{

uEEMMRegistered(1),

uENotEMMRegistered(2)

}

FiveGMMStatus ::= ENUMERATED

{

uE5GMMRegistered(1),

uENot5GMMRegistered(2)

}

-- ========================================

-- Separated Location Reporting definitions

-- ========================================

SeparatedLocationReporting ::= SEQUENCE

{

sUPI [1] SUPI,

sUCI [2] SUCI OPTIONAL,

pEI [3] PEI OPTIONAL,

gPSI [4] GPSI OPTIONAL,

gUTI [5] FiveGGUTI OPTIONAL,

location [6] Location,

non3GPPAccessEndpoint [7] UEEndpointAddress OPTIONAL,

rATType [8] RATType OPTIONAL

}

-- =================

-- Common Parameters

-- =================

AccessType ::= ENUMERATED

{

threeGPPAccess(1),

nonThreeGPPAccess(2),

threeGPPandNonThreeGPPAccess(3)

}

Direction ::= ENUMERATED

{

fromTarget(1),

toTarget(2)

}

DNN ::= UTF8String

E164Number ::= NumericString (SIZE(1..15))

EmailAddress ::= UTF8String

EUI64 ::= OCTET STRING (SIZE(8))

FiveGGUTI ::= SEQUENCE

{

mCC [1] MCC,

mNC [2] MNC,

aMFRegionID [3] AMFRegionID,

aMFSetID [4] AMFSetID,

aMFPointer [5] AMFPointer,

fiveGTMSI [6] FiveGTMSI

}

FiveGMMCause ::= INTEGER (0..255)

FiveGSMRequestType ::= ENUMERATED

{

initialRequest(1),

existingPDUSession(2),

initialEmergencyRequest(3),

existingEmergencyPDUSession(4),

modificationRequest(5),

reserved(6),

mAPDURequest(7)

}

FiveGSMCause ::= INTEGER (0..255)

FiveGTMSI ::= INTEGER (0..4294967295)

FiveGSRVCCInfo ::= SEQUENCE

{

uE5GSRVCCCapability [1] BOOLEAN,

sessionTransferNumber [2] UTF8String OPTIONAL,

correlationMSISDN [3] MSISDN OPTIONAL

}

FiveGSUserStateInfo ::= SEQUENCE

{

fiveGSUserState [1] FiveGSUserState,

accessType [2] AccessType

}

FiveGSUserState ::= ENUMERATED

{

deregistered(1),

registeredNotReachableForPaging(2),

registeredReachableForPaging(3),

connectedNotReachableForPaging(4),

connectedReachableForPaging(5),

notProvidedFromAMF(6)

}

FTEID ::= SEQUENCE

{

tEID [1] INTEGER (0.. 4294967295),

iPv4Address [2] IPv4Address OPTIONAL,

iPv6Address [3] IPv6Address OPTIONAL

}

GPSI ::= CHOICE

{

mSISDN [1] MSISDN,

nAI [2] NAI

}

GUAMI ::= SEQUENCE

{

aMFID [1] AMFID,

pLMNID [2] PLMNID

}

GUMMEI ::= SEQUENCE

{

mMEID [1] MMEID,

mCC [2] MCC,

mNC [3] MNC

}

GUTI ::= SEQUENCE

{

mCC [1] MCC,

mNC [2] MNC,

mMEGroupID [3] MMEGroupID,

mMECode [4] MMECode,

mTMSI [5] TMSI

}

HomeNetworkPublicKeyID ::= OCTET STRING

HSMFURI ::= UTF8String

IMEI ::= NumericString (SIZE(14))

IMEISV ::= NumericString (SIZE(16))

IMPI ::= NAI

IMPU ::= CHOICE

{

sIPURI [1] SIPURI,

tELURI [2] TELURI

}

IMSI ::= NumericString (SIZE(6..15))

Initiator ::= ENUMERATED

{

uE(1),

network(2),

unknown(3)

}

IPAddress ::= CHOICE

{

iPv4Address [1] IPv4Address,

iPv6Address [2] IPv6Address

}

IPv4Address ::= OCTET STRING (SIZE(4))

IPv6Address ::= OCTET STRING (SIZE(16))

IPv6FlowLabel ::= INTEGER(0..1048575)

MACAddress ::= OCTET STRING (SIZE(6))

MACRestrictionIndicator ::= ENUMERATED

{

noResrictions(1),

mACAddressNotUseableAsEquipmentIdentifier(2),

unknown(3)

}

MCC ::= NumericString (SIZE(3))

MNC ::= NumericString (SIZE(2..3))

MMEID ::= SEQUENCE

{

mMEGI [1] MMEGI,

mMEC [2] MMEC

}

MMEC ::= NumericString

MMEGI ::= NumericString

MSISDN ::= NumericString (SIZE(1..15))

NAI ::= UTF8String

NextLayerProtocol ::= INTEGER(0..255)

NonLocalID ::= ENUMERATED

{

local(1),

nonLocal(2)

}

NonIMEISVPEI ::= CHOICE

{

mACAddress [1] MACAddress

}

NSSAI ::= SEQUENCE OF SNSSAI

PLMNID ::= SEQUENCE

{

mCC [1] MCC,

mNC [2] MNC

}

PDUSessionID ::= INTEGER (0..255)

PDUSessionType ::= ENUMERATED

{

iPv4(1),

iPv6(2),

iPv4v6(3),

unstructured(4),

ethernet(5)

}

PEI ::= CHOICE

{

iMEI [1] IMEI,

iMEISV [2] IMEISV,

mACAddress [3] MACAddress,

eUI64 [4] EUI64

}

PortNumber ::= INTEGER(0..65535)

PrimaryAuthenticationType ::= ENUMERATED

{

eAPAKAPrime(1),

fiveGAKA(2),

eAPTLS(3),

none(4),

ePSAKA(5),

eAPAKA(6),

iMSAKA(7),

gBAAKA(8),

uMTSAKA(9)

}

ProtectionSchemeID ::= INTEGER (0..15)

RATType ::= ENUMERATED

{

nR(1),

eUTRA(2),

wLAN(3),

virtual(4),

nBIOT(5),

wireline(6),

wirelineCable(7),

wirelineBBF(8),

lTEM(9),

nRU(10),

eUTRAU(11),

trustedN3GA(12),

trustedWLAN(13),

uTRA(14),

gERA(15)

}

RejectedNSSAI ::= SEQUENCE OF RejectedSNSSAI

RejectedSNSSAI ::= SEQUENCE

{

causeValue [1] RejectedSliceCauseValue,

sNSSAI [2] SNSSAI

}

RejectedSliceCauseValue ::= INTEGER (0..255)

ReRegRequiredIndicator ::= ENUMERATED

{

reRegistrationRequired(1),

reRegistrationNotRequired(2)

}

RoutingIndicator ::= INTEGER (0..9999)

SchemeOutput ::= OCTET STRING

SIPURI ::= UTF8String

Slice ::= SEQUENCE

{

allowedNSSAI [1] NSSAI OPTIONAL,

configuredNSSAI [2] NSSAI OPTIONAL,

rejectedNSSAI [3] RejectedNSSAI OPTIONAL

}

SMPDUDNRequest ::= OCTET STRING

-- TS 24.501 [13], clause 9.11.3.6.1

SMSOverNASIndicator ::= ENUMERATED

{

sMSOverNASNotAllowed(1),

sMSOverNASAllowed(2)

}

SNSSAI ::= SEQUENCE

{

sliceServiceType [1] INTEGER (0..255),

sliceDifferentiator [2] OCTET STRING (SIZE(3)) OPTIONAL

}

SubscriberIdentifier ::= CHOICE

{

sUCI [1] SUCI,

sUPI [2] SUPI

}

SUCI ::= SEQUENCE

{

mCC [1] MCC,

mNC [2] MNC,

routingIndicator [3] RoutingIndicator,

protectionSchemeID [4] ProtectionSchemeID,

homeNetworkPublicKeyID [5] HomeNetworkPublicKeyID,

schemeOutput [6] SchemeOutput

}

SUPI ::= CHOICE

{

iMSI [1] IMSI,

nAI [2] NAI

}

SUPIUnauthenticatedIndication ::= BOOLEAN

SwitchOffIndicator ::= ENUMERATED

{

normalDetach(1),

switchOff(2)

}

TargetIdentifier ::= CHOICE

{

sUPI [1] SUPI,

iMSI [2] IMSI,

pEI [3] PEI,

iMEI [4] IMEI,

gPSI [5] GPSI,

mSISDN [6] MSISDN,

nAI [7] NAI,

iPv4Address [8] IPv4Address,

iPv6Address [9] IPv6Address,

ethernetAddress [10] MACAddress

}

TargetIdentifierProvenance ::= ENUMERATED

{

lEAProvided(1),

observed(2),

matchedOn(3),

other(4)

}

TELURI ::= UTF8String

Timestamp ::= GeneralizedTime

UEContextInfo ::= SEQUENCE

{

supportVoPS [1] BOOLEAN OPTIONAL,

supportVoPSNon3GPP [2] BOOLEAN OPTIONAL,

lastActiveTime [3] Timestamp OPTIONAL,

accessType [4] AccessType OPTIONAL,

rATType [5] RATType OPTIONAL

}

UEEndpointAddress ::= CHOICE

{

iPv4Address [1] IPv4Address,

iPv6Address [2] IPv6Address,

ethernetAddress [3] MACAddress

}

-- ===================

-- Location parameters

-- ===================

Location ::= SEQUENCE

{

locationInfo [1] LocationInfo OPTIONAL,

positioningInfo [2] PositioningInfo OPTIONAL,

locationPresenceReport [3] LocationPresenceReport OPTIONAL,

ePSLocationInfo [4] EPSLocationInfo OPTIONAL

}

CellSiteInformation ::= SEQUENCE

{

geographicalCoordinates [1] GeographicalCoordinates,

azimuth [2] INTEGER (0..359) OPTIONAL,

operatorSpecificInformation [3] UTF8String OPTIONAL

}

-- TS 29.518 [22], clause 6.4.6.2.6

LocationInfo ::= SEQUENCE

{

userLocation [1] UserLocation OPTIONAL,

currentLoc [2] BOOLEAN OPTIONAL,

geoInfo [3] GeographicArea OPTIONAL,

rATType [4] RATType OPTIONAL,

timeZone [5] TimeZone OPTIONAL,

additionalCellIDs [6] SEQUENCE OF CellInformation OPTIONAL

}

-- TS 29.571 [17], clause 5.4.4.7

UserLocation ::= SEQUENCE

{

eUTRALocation [1] EUTRALocation OPTIONAL,

nRLocation [2] NRLocation OPTIONAL,

n3GALocation [3] N3GALocation OPTIONAL

}

-- TS 29.571 [17], clause 5.4.4.8

EUTRALocation ::= SEQUENCE

{

tAI [1] TAI,

eCGI [2] ECGI,

ageOfLocationInfo [3] INTEGER OPTIONAL,

uELocationTimestamp [4] Timestamp OPTIONAL,

geographicalInformation [5] UTF8String OPTIONAL,

geodeticInformation [6] UTF8String OPTIONAL,

globalNGENbID [7] GlobalRANNodeID OPTIONAL,

cellSiteInformation [8] CellSiteInformation OPTIONAL,

globalENbID [9] GlobalRANNodeID OPTIONAL

}

-- TS 29.571 [17], clause 5.4.4.9

NRLocation ::= SEQUENCE

{

tAI [1] TAI,

nCGI [2] NCGI,

ageOfLocationInfo [3] INTEGER OPTIONAL,

uELocationTimestamp [4] Timestamp OPTIONAL,

geographicalInformation [5] UTF8String OPTIONAL,

geodeticInformation [6] UTF8String OPTIONAL,

globalGNbID [7] GlobalRANNodeID OPTIONAL,

cellSiteInformation [8] CellSiteInformation OPTIONAL

}

-- TS 29.571 [17], clause 5.4.4.10

N3GALocation ::= SEQUENCE

{

tAI [1] TAI OPTIONAL,

n3IWFID [2] N3IWFIDNGAP OPTIONAL,

uEIPAddr [3] IPAddr OPTIONAL,

portNumber [4] INTEGER OPTIONAL,

tNAPID [5] TNAPID OPTIONAL,

tWAPID [6] TWAPID OPTIONAL,

hFCNodeID [7] HFCNodeID OPTIONAL,

gLI [8] GLI OPTIONAL,

w5GBANLineType [9] W5GBANLineType OPTIONAL,

gCI [10] GCI OPTIONAL,

ageOfLocationInfo [11] INTEGER OPTIONAL,

uELocationTimestamp [12] Timestamp OPTIONAL

}

-- TS 38.413 [23], clause 9.3.2.4

IPAddr ::= SEQUENCE

{

iPv4Addr [1] IPv4Address OPTIONAL,

iPv6Addr [2] IPv6Address OPTIONAL

}

-- TS 29.571 [17], clause 5.4.4.28

GlobalRANNodeID ::= SEQUENCE

{

pLMNID [1] PLMNID,

aNNodeID [2] ANNodeID,

nID [3] NID OPTIONAL

}

ANNodeID ::= CHOICE

{

n3IWFID [1] N3IWFIDSBI,

gNbID [2] GNbID,

nGENbID [3] NGENbID,

eNbID [4] ENbID,

wAGFID [5] WAGFID,

tNGFID [6] TNGFID

}

-- TS 38.413 [23], clause 9.3.1.6

GNbID ::= BIT STRING(SIZE(22..32))

-- TS 29.571 [17], clause 5.4.4.4

TAI ::= SEQUENCE

{

pLMNID [1] PLMNID,

tAC [2] TAC,

nID [3] NID OPTIONAL

}

CGI ::= SEQUENCE

{

lAI [1] LAI,

cellID [2] CellID

}

LAI ::= SEQUENCE

{

pLMNID [1] PLMNID,

lAC [2] LAC

}

LAC ::= OCTET STRING (SIZE(2))

CellID ::= OCTET STRING (SIZE(2))

SAI ::= SEQUENCE

{

pLMNID [1] PLMNID,

lAC [2] LAC,

sAC [3] SAC

}

SAC ::= OCTET STRING (SIZE(2))

-- TS 29.571 [17], clause 5.4.4.5

ECGI ::= SEQUENCE

{

pLMNID [1] PLMNID,

eUTRACellID [2] EUTRACellID,

nID [3] NID OPTIONAL

}

TAIList ::= SEQUENCE OF TAI

-- TS 29.571 [17], clause 5.4.4.6

NCGI ::= SEQUENCE

{

pLMNID [1] PLMNID,

nRCellID [2] NRCellID,

nID [3] NID OPTIONAL

}

RANCGI ::= CHOICE

{

eCGI [1] ECGI,

nCGI [2] NCGI

}

CellInformation ::= SEQUENCE

{

rANCGI [1] RANCGI,

cellSiteinformation [2] CellSiteInformation OPTIONAL,

timeOfLocation [3] Timestamp OPTIONAL

}

-- TS 38.413 [23], clause 9.3.1.57

N3IWFIDNGAP ::= BIT STRING (SIZE(16))

-- TS 29.571 [17], clause 5.4.4.28

N3IWFIDSBI ::= UTF8String

-- TS 29.571 [17], clause 5.4.4.28 and table 5.4.2-1

TNGFID ::= UTF8String

-- TS 29.571 [17], clause 5.4.4.28 and table 5.4.2-1

WAGFID ::= UTF8String

-- TS 29.571 [17], clause 5.4.4.62

TNAPID ::= SEQUENCE

{

sSID [1] SSID OPTIONAL,

bSSID [2] BSSID OPTIONAL,

civicAddress [3] CivicAddressBytes OPTIONAL

}

-- TS 29.571 [17], clause 5.4.4.64

TWAPID ::= SEQUENCE

{

sSID [1] SSID OPTIONAL,

bSSID [2] BSSID OPTIONAL,

civicAddress [3] CivicAddressBytes OPTIONAL

}

-- TS 29.571 [17], clause 5.4.4.62 and clause 5.4.4.64

SSID ::= UTF8String

-- TS 29.571 [17], clause 5.4.4.62 and clause 5.4.4.64

BSSID ::= UTF8String

-- TS 29.571 [17], clause 5.4.4.36 and table 5.4.2-1

HFCNodeID ::= UTF8String

-- TS 29.571 [17], clause 5.4.4.10 and table 5.4.2-1

-- Contains the original binary data i.e. value of the YAML field after base64 encoding is removed

GLI ::= OCTET STRING (SIZE(0..150))

-- TS 29.571 [17], clause 5.4.4.10 and table 5.4.2-1

GCI ::= UTF8String

-- TS 29.571 [17], clause 5.4.4.10 and clause 5.4.3.33

W5GBANLineType ::= ENUMERATED

{

dSL(1),

pON(2)

}

-- TS 29.571 [17], table 5.4.2-1

TAC ::= OCTET STRING (SIZE(2..3))

-- TS 38.413 [23], clause 9.3.1.9

EUTRACellID ::= BIT STRING (SIZE(28))

-- TS 38.413 [23], clause 9.3.1.7

NRCellID ::= BIT STRING (SIZE(36))

-- TS 38.413 [23], clause 9.3.1.8

NGENbID ::= CHOICE

{

macroNGENbID [1] BIT STRING (SIZE(20)),

shortMacroNGENbID [2] BIT STRING (SIZE(18)),

longMacroNGENbID [3] BIT STRING (SIZE(21))

}

-- TS 23.003 [19], clause 12.7.1 encoded as per TS 29.571 [17], clause 5.4.2

NID ::= UTF8String (SIZE(11))

-- TS 36.413 [38], clause 9.2.1.37

ENbID ::= CHOICE

{

macroENbID [1] BIT STRING (SIZE(20)),

homeENbID [2] BIT STRING (SIZE(28)),

shortMacroENbID [3] BIT STRING (SIZE(18)),

longMacroENbID [4] BIT STRING (SIZE(21))

}

-- TS 29.518 [22], clause 6.4.6.2.3

PositioningInfo ::= SEQUENCE

{

positionInfo [1] LocationData OPTIONAL,

rawMLPResponse [2] RawMLPResponse OPTIONAL

}

RawMLPResponse ::= CHOICE

{

-- The following parameter contains a copy of unparsed XML code of the

-- MLP response message, i.e. the entire XML document containing

-- a <slia> (described in OMA-TS-MLP-V3\_5-20181211-C [20], clause 5.2.3.2.2) or

-- a <slirep> (described in OMA-TS-MLP-V3\_5-20181211-C [20], clause 5.2.3.2.3) MLP message.

mLPPositionData [1] UTF8String,

-- OMA MLP result id, defined in OMA-TS-MLP-V3\_5-20181211-C [20], Clause 5.4

mLPErrorCode [2] INTEGER (1..699)

}

-- TS 29.572 [24], clause 6.1.6.2.3

LocationData ::= SEQUENCE

{

locationEstimate [1] GeographicArea,

accuracyFulfilmentIndicator [2] AccuracyFulfilmentIndicator OPTIONAL,

ageOfLocationEstimate [3] AgeOfLocationEstimate OPTIONAL,

velocityEstimate [4] VelocityEstimate OPTIONAL,

civicAddress [5] CivicAddress OPTIONAL,

positioningDataList [6] SET OF PositioningMethodAndUsage OPTIONAL,

gNSSPositioningDataList [7] SET OF GNSSPositioningMethodAndUsage OPTIONAL,

eCGI [8] ECGI OPTIONAL,

nCGI [9] NCGI OPTIONAL,

altitude [10] Altitude OPTIONAL,

barometricPressure [11] BarometricPressure OPTIONAL

}

-- TS 29.172 [53], table 6.2.2-2

EPSLocationInfo ::= SEQUENCE

{

locationData [1] LocationData,

cGI [2] CGI OPTIONAL,

sAI [3] SAI OPTIONAL,

eSMLCCellInfo [4] ESMLCCellInfo OPTIONAL

}

-- TS 29.172 [53], clause 7.4.57

ESMLCCellInfo ::= SEQUENCE

{

eCGI [1] ECGI,

cellPortionID [2] CellPortionID

}

-- TS 29.171 [54], clause 7.4.31

CellPortionID ::= INTEGER (0..4095)

-- TS 29.518 [22], clause 6.2.6.2.5

LocationPresenceReport ::= SEQUENCE

{

type [1] AMFEventType,

timestamp [2] Timestamp,

areaList [3] SET OF AMFEventArea OPTIONAL,

timeZone [4] TimeZone OPTIONAL,

accessTypes [5] SET OF AccessType OPTIONAL,

rMInfoList [6] SET OF RMInfo OPTIONAL,

cMInfoList [7] SET OF CMInfo OPTIONAL,

reachability [8] UEReachability OPTIONAL,

location [9] UserLocation OPTIONAL,

additionalCellIDs [10] SEQUENCE OF CellInformation OPTIONAL

}

-- TS 29.518 [22], clause 6.2.6.3.3

AMFEventType ::= ENUMERATED

{

locationReport(1),

presenceInAOIReport(2)

}

-- TS 29.518 [22], clause 6.2.6.2.16

AMFEventArea ::= SEQUENCE

{

presenceInfo [1] PresenceInfo OPTIONAL,

lADNInfo [2] LADNInfo OPTIONAL

}

-- TS 29.571 [17], clause 5.4.4.27

PresenceInfo ::= SEQUENCE

{

presenceState [1] PresenceState OPTIONAL,

trackingAreaList [2] SET OF TAI OPTIONAL,

eCGIList [3] SET OF ECGI OPTIONAL,

nCGIList [4] SET OF NCGI OPTIONAL,

globalRANNodeIDList [5] SET OF GlobalRANNodeID OPTIONAL,

globalENbIDList [6] SET OF GlobalRANNodeID OPTIONAL

}

-- TS 29.518 [22], clause 6.2.6.2.17

LADNInfo ::= SEQUENCE

{

lADN [1] UTF8String,

presence [2] PresenceState OPTIONAL

}

-- TS 29.571 [17], clause 5.4.3.20

PresenceState ::= ENUMERATED

{

inArea(1),

outOfArea(2),

unknown(3),

inactive(4)

}

-- TS 29.518 [22], clause 6.2.6.2.8

RMInfo ::= SEQUENCE

{

rMState [1] RMState,

accessType [2] AccessType

}

-- TS 29.518 [22], clause 6.2.6.2.9

CMInfo ::= SEQUENCE

{

cMState [1] CMState,

accessType [2] AccessType

}

-- TS 29.518 [22], clause 6.2.6.3.7

UEReachability ::= ENUMERATED

{

unreachable(1),

reachable(2),

regulatoryOnly(3)

}

-- TS 29.518 [22], clause 6.2.6.3.9

RMState ::= ENUMERATED

{

registered(1),

deregistered(2)

}

-- TS 29.518 [22], clause 6.2.6.3.10

CMState ::= ENUMERATED

{

idle(1),

connected(2)

}

-- TS 29.572 [24], clause 6.1.6.2.5

GeographicArea ::= CHOICE

{

point [1] Point,

pointUncertaintyCircle [2] PointUncertaintyCircle,

pointUncertaintyEllipse [3] PointUncertaintyEllipse,

polygon [4] Polygon,

pointAltitude [5] PointAltitude,

pointAltitudeUncertainty [6] PointAltitudeUncertainty,

ellipsoidArc [7] EllipsoidArc

}

-- TS 29.572 [24], clause 6.1.6.3.12

AccuracyFulfilmentIndicator ::= ENUMERATED

{

requestedAccuracyFulfilled(1),

requestedAccuracyNotFulfilled(2)

}

-- TS 29.572 [24], clause 6.1.6.2.17

VelocityEstimate ::= CHOICE

{

horVelocity [1] HorizontalVelocity,

horWithVertVelocity [2] HorizontalWithVerticalVelocity,

horVelocityWithUncertainty [3] HorizontalVelocityWithUncertainty,

horWithVertVelocityAndUncertainty [4] HorizontalWithVerticalVelocityAndUncertainty

}

-- TS 29.572 [24], clause 6.1.6.2.14

CivicAddress ::= SEQUENCE

{

country [1] UTF8String,

a1 [2] UTF8String OPTIONAL,

a2 [3] UTF8String OPTIONAL,

a3 [4] UTF8String OPTIONAL,

a4 [5] UTF8String OPTIONAL,

a5 [6] UTF8String OPTIONAL,

a6 [7] UTF8String OPTIONAL,

prd [8] UTF8String OPTIONAL,

pod [9] UTF8String OPTIONAL,

sts [10] UTF8String OPTIONAL,

hno [11] UTF8String OPTIONAL,

hns [12] UTF8String OPTIONAL,

lmk [13] UTF8String OPTIONAL,

loc [14] UTF8String OPTIONAL,

nam [15] UTF8String OPTIONAL,

pc [16] UTF8String OPTIONAL,

bld [17] UTF8String OPTIONAL,

unit [18] UTF8String OPTIONAL,

flr [19] UTF8String OPTIONAL,

room [20] UTF8String OPTIONAL,

plc [21] UTF8String OPTIONAL,

pcn [22] UTF8String OPTIONAL,

pobox [23] UTF8String OPTIONAL,

addcode [24] UTF8String OPTIONAL,

seat [25] UTF8String OPTIONAL,

rd [26] UTF8String OPTIONAL,

rdsec [27] UTF8String OPTIONAL,

rdbr [28] UTF8String OPTIONAL,

rdsubbr [29] UTF8String OPTIONAL,

prm [30] UTF8String OPTIONAL,

pom [31] UTF8String OPTIONAL

}

-- TS 29.571 [17], clauses 5.4.4.62 and 5.4.4.64

-- Contains the original binary data i.e. value of the YAML field after base64 encoding is removed

CivicAddressBytes ::= OCTET STRING

-- TS 29.572 [24], clause 6.1.6.2.15

PositioningMethodAndUsage ::= SEQUENCE

{

method [1] PositioningMethod,

mode [2] PositioningMode,

usage [3] Usage,

methodCode [4] MethodCode OPTIONAL

}

-- TS 29.572 [24], clause 6.1.6.2.16

GNSSPositioningMethodAndUsage ::= SEQUENCE

{

mode [1] PositioningMode,

gNSS [2] GNSSID,

usage [3] Usage

}

-- TS 29.572 [24], clause 6.1.6.2.6

Point ::= SEQUENCE

{

geographicalCoordinates [1] GeographicalCoordinates

}

-- TS 29.572 [24], clause 6.1.6.2.7

PointUncertaintyCircle ::= SEQUENCE

{

geographicalCoordinates [1] GeographicalCoordinates,

uncertainty [2] Uncertainty

}

-- TS 29.572 [24], clause 6.1.6.2.8

PointUncertaintyEllipse ::= SEQUENCE

{

geographicalCoordinates [1] GeographicalCoordinates,

uncertainty [2] UncertaintyEllipse,

confidence [3] Confidence

}

-- TS 29.572 [24], clause 6.1.6.2.9

Polygon ::= SEQUENCE

{

pointList [1] SET SIZE (3..15) OF GeographicalCoordinates

}

-- TS 29.572 [24], clause 6.1.6.2.10

PointAltitude ::= SEQUENCE

{

point [1] GeographicalCoordinates,

altitude [2] Altitude

}

-- TS 29.572 [24], clause 6.1.6.2.11

PointAltitudeUncertainty ::= SEQUENCE

{

point [1] GeographicalCoordinates,

altitude [2] Altitude,

uncertaintyEllipse [3] UncertaintyEllipse,

uncertaintyAltitude [4] Uncertainty,

confidence [5] Confidence

}

-- TS 29.572 [24], clause 6.1.6.2.12

EllipsoidArc ::= SEQUENCE

{

point [1] GeographicalCoordinates,

innerRadius [2] InnerRadius,

uncertaintyRadius [3] Uncertainty,

offsetAngle [4] Angle,

includedAngle [5] Angle,

confidence [6] Confidence

}

-- TS 29.572 [24], clause 6.1.6.2.4

GeographicalCoordinates ::= SEQUENCE

{

latitude [1] UTF8String,

longitude [2] UTF8String,

mapDatumInformation [3] OGCURN OPTIONAL

}

-- TS 29.572 [24], clause 6.1.6.2.22

UncertaintyEllipse ::= SEQUENCE

{

semiMajor [1] Uncertainty,

semiMinor [2] Uncertainty,

orientationMajor [3] Orientation

}

-- TS 29.572 [24], clause 6.1.6.2.18

HorizontalVelocity ::= SEQUENCE

{

hSpeed [1] HorizontalSpeed,

bearing [2] Angle

}

-- TS 29.572 [24], clause 6.1.6.2.19

HorizontalWithVerticalVelocity ::= SEQUENCE

{

hSpeed [1] HorizontalSpeed,

bearing [2] Angle,

vSpeed [3] VerticalSpeed,

vDirection [4] VerticalDirection

}

-- TS 29.572 [24], clause 6.1.6.2.20

HorizontalVelocityWithUncertainty ::= SEQUENCE

{

hSpeed [1] HorizontalSpeed,

bearing [2] Angle,

uncertainty [3] SpeedUncertainty

}

-- TS 29.572 [24], clause 6.1.6.2.21

HorizontalWithVerticalVelocityAndUncertainty ::= SEQUENCE

{

hSpeed [1] HorizontalSpeed,

bearing [2] Angle,

vSpeed [3] VerticalSpeed,

vDirection [4] VerticalDirection,

hUncertainty [5] SpeedUncertainty,

vUncertainty [6] SpeedUncertainty

}

-- The following types are described in TS 29.572 [24], table 6.1.6.3.2-1

Altitude ::= UTF8String

Angle ::= INTEGER (0..360)

Uncertainty ::= INTEGER (0..127)

Orientation ::= INTEGER (0..180)

Confidence ::= INTEGER (0..100)

InnerRadius ::= INTEGER (0..65535)

AgeOfLocationEstimate ::= INTEGER (0..32767)

HorizontalSpeed ::= UTF8String

VerticalSpeed ::= UTF8String

SpeedUncertainty ::= UTF8String

BarometricPressure ::= INTEGER (30000..155000)

-- TS 29.572 [24], clause 6.1.6.3.13

VerticalDirection ::= ENUMERATED

{

upward(1),

downward(2)

}

-- TS 29.572 [24], clause 6.1.6.3.6

PositioningMethod ::= ENUMERATED

{

cellID(1),

eCID(2),

oTDOA(3),

barometricPressure(4),

wLAN(5),

bluetooth(6),

mBS(7),

motionSensor(8),

dLTDOA(9),

dLAOD(10),

multiRTT(11),

nRECID(12),

uLTDOA(13),

uLAOA(14),

networkSpecific(15)

}

-- TS 29.572 [24], clause 6.1.6.3.7

PositioningMode ::= ENUMERATED

{

uEBased(1),

uEAssisted(2),

conventional(3)

}

-- TS 29.572 [24], clause 6.1.6.3.8

GNSSID ::= ENUMERATED

{

gPS(1),

galileo(2),

sBAS(3),

modernizedGPS(4),

qZSS(5),

gLONASS(6),

bDS(7),

nAVIC(8)

}

-- TS 29.572 [24], clause 6.1.6.3.9

Usage ::= ENUMERATED

{

unsuccess(1),

successResultsNotUsed(2),

successResultsUsedToVerifyLocation(3),

successResultsUsedToGenerateLocation(4),

successMethodNotDetermined(5)

}

-- TS 29.571 [17], table 5.2.2-1

TimeZone ::= UTF8String

-- Open Geospatial Consortium URN [35]

OGCURN ::= UTF8String

-- TS 29.572 [24], clause 6.1.6.2.15

MethodCode ::= INTEGER (16..31)

END

\*\*\*END OF SECOND CHANGE \*\*\*

\*\*\*END OF ALL CHANGES \*\*\*