**3GPP SA3#95-LI S3i240713**

**Las Vegas; October 29-November 1, 2024**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **33.127** | **CR** | **0257**  | **rev** | **2** | **Current version:** | **18.9.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | GPSI Missing from IEF Event Parameters at Stage 2 |
|  |  |
| ***Source to WG:*** | SA3-LI (Rogers Communications Canada) |
| ***Source to TSG:*** | SA3 |
|  |  |
| ***Work item code:*** | LI17 |  | ***Date:*** | 2024-10-29 |
|  |  |  |  |  |
| ***Category:*** | ***A*** |  | ***Release:*** | Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | GPSI parameter is missing from the list of IEF reportable parameters.  |
|  |  |
| ***Summary of change:*** | GPSI parameter is added to the list of IEF reportable parameters.  |
|  |  |
| ***Consequences if not approved:*** | Misalignment between Stage 2 and Stage 3 Identity Association Caching specifications.  |
|  |  |
| ***Clauses affected:*** |  6.2.2A.3 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  S3i240679, S3i240683 |

### \*\* First Change \*\*

#### 6.2.2A.3 IEF Event parameters

The list of event parameters is specified in TS 33.128 [15]. Each event shall include at the minimum the following information:

- Subscription permanent identifier.

- Observed temporary identifier(s).

- Cell identity (see clause 7.3).

- Time stamp of event.

- AMF identifier (including Region and Set Identifiers).

- Tracking area identifier.

- Registration area (including tracking area identifier list).

The following additional information shall be included if it is available in the AMF when the event is reported to the ICF:

- Permanent Equipment Identifier (PEI).

- Generic Public Subscription Identifier (GPSI).

### \*\* End of all Changes \*\*