**3GPP TSG- Meeting #**

**, , –**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.3* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **33.128** | **CR** |  | **rev** | **1** | **Current version:** |  |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Correction on table 6.2.2.2.12-1: Payload for AMFUEPolicyTransfer record | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | SA3-LI (Ministere de l’économie et des finances France, Nokia) | | | | | | | | | |
| ***Source to TSG:*** | SA3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | LI18 | | | | |  | ***Date:*** | | | 2024 10 31 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | A |  | | | | | ***Release:*** | | |  |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)  Rel-20 (Release 20)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Based on TS 29.518 and TS 24.501 on UE policy transfer, this table of “6.2.2.2.12 UE policy transfer” has mistakes. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Changes in Description fields | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Regulatory issues as LI system related to AMF may not work | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 6.2.2.2.12 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | | s3i240649 | | | | | | | | |

\*\*\*\* FIRST CHANGE \*\*\*\*

6.2.2.2.12 UE policy transfer

The IRI-POI present in the AMF shall generate an xIRI containing an AMFUEPolicyTransfer record when the IRI-POI present in the AMF detects the following event:

- AMF sends a Namf\_Communication\_N1MessageNotify Request (See TS 29.518 [22] clause 5.2.2.3) related to the target UE containing the N1 NAS message MANAGE UE POLICY COMPLETE. It confirms that UE policies forwarded by AMF to the target UE in the N1 NAS message MANAGE UE POLICY COMMAND have been accepted by the UE.

**Table 6.2.2.2.12-1: Payload for AMFUEPolicyTransfer record**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Field name** | **Type** | **Cardinality** | **Description** | **M/C/O** |
| sUPI | SUPI | 1 | SUPI associated with the procedure (see NOTE). | M |
| sUCI | SUCI | 0..1 | SUCI used in the procedure, if applicable and if available (see NOTE). | C |
| pEI | PEI | 0..1 | PEI used in the procedure, if available (see NOTE). | C |
| gPSI | GPSI | 0..1 | GPSI used in the procedure, if available (see NOTE). | C |
| gUTI | FiveGGUTI | 0..1 | 5G-GUTI used in the procedure, see TS 24.501 [13] clause 9.11.3.4 (see NOTE). | C |
| uePolicy | UEPolicy | 1 | Content of the N1 NAS message MANAGE UE POLICY COMMAND, as defined in TS 24.501 [13] table D.5.1.1.1 (see NOTE). | M |
| NOTE:    SUPI shall always be provided, in addition to the warrant target identifier if different to SUPI. Other identifiers shall be provided if available. | | | | |

\*\*\*\* END OF FIRST CHANGE \*\*\*\*

\*\*\*\* END OF ALL CHANGES \*\*\*\*