**3GPP TSG- Meeting #**

**, , -**

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** | **0253** | **rev** | **1** | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **\*** |

|  |
| --- |
|  |
| ***Title:***  |  |
|  |  |
| ***Source to WG:*** | SA3LI (Ministère Economie et Finances) |
| ***Source to TSG:*** | SA3 |
|  |  |
| ***Work item code:*** |  |  | ***Date:*** |  |
|  |  |  |  |  |
| ***Category:*** |  |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19) Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | Lack of VN Group information related to a specific target by NEF PoI |
|  |  |
| ***Summary of change:*** | Add 5G LAN Parameter provisioning (VN Group) and related events for an LI system |
|  |  |
| ***Consequences if not approved:*** | Regulatory issues |
|  |  |
| ***Clauses affected:*** | 3.3; 7.9.X;  |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **\*** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **\*** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **\*** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** | s3i240650 |

 START OF FIRST CHANGE

## 3.3 Abbreviations

For the purposes of the present document, the abbreviations given in 3GPP TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in 3GPP TR 21.905 [1].

5GC 5G Core Network

5GMS 5G Media Streaming

5GS 5G System

AAnF AKMA Anchor Function

AC Application Client

ACR Application Context Relocation

ADMF LI Administration Function

AF Application Function

AF\_ID Application Function Identity

AKA Authentication and Key Agreement

A-KID AKMA Key IDentifier

AKMA Authentication and Key Management for Applications

AMF Access and Mobility Management Function

AS Application Server

AUSF Authentication Server Function

BBIFF Bearer Binding Intercept and Forward Function

BSS Business Support System

CAG Closed Access Group

CC Content of Communication

CP Control Plane

CPIM Common Presence and Instant Messaging

CPS Call Placement Service

CSI Cell Supplemental Information

CSP Communication Service Provider

CSR Cell Site Report

CUPS Control and User Plane Separation

DC-AS Data Channel Application Server

DCSF Data Channel Signalling Function

DN Data Network

DNAI Data Network Access Identifier

DoNAS Data over NAS

EAP Extensible Authentication Protocol

EAS Edge Application Server

ECGI E-UTRAN Cell Global Identifier

eCNAM Enhanced Calling Name

ECSP Edge Computing Service Provider

E-CSCF Emergency – Call Session Control Function

EDN Edge Data Network

EEC Edge Enabler Client

EECID Edge Enabler Client IDentifier

EES Edge Enabler Server

GPSI Generic Public Subscription Identifier

HMEE Hardware Mediated Execution Enclave

HR Home Routed

IBCF Interconnection Border Control Functions

ICF Identity Caching Function

IEF Identity Event Function

IMS-AGW IMS Access Gateway

IM-MGW IM Media Gateway

IP Interception Product

IPPR Internet Protocol Packet Reporting

IQF Identity Query Function

IRI Intercept Related Information

KAF AKMA Application Key

KAKMA AKMA Anchor Key

KID Key IDentifier

KLI Decryption key(s) for services encrypted by CSP-provided keys

KSF Key Server Function

LAF Location Acquisition Function

LALS Lawful Access Location Services

LARF Location Acquisition Requesting Function

LBO Local Break Out

LEA Law Enforcement Agency

LEMF Law Enforcement Monitoring Facility

LI Lawful Interception

LI CA Lawful Interception Certificate Authority

LICF Lawful Interception Control Function

LI\_HI1 Lawful Interception Handover Interface 1

LI\_HI2 Lawful Interception Handover Interface 2

LI\_HI3 Lawful Interception Handover Interface 3

LI\_HI4 Lawful Interception Handover Interface 4

LI\_HILA Lawful Interception Handover Interface Location Acquisition

LI\_HIQR Lawful Interception Handover Interface Query Response

LIID Lawful Interception Identifier

LIPF Lawful Interception Provisioning Function

LIR Location Immediate Request

LI\_SI Lawful Interception System Information Interface

LISSF Lawful Interception State Storage Function

LI\_ST Lawful Interception State Transfer Interface

LI\_T1 Lawful Interception Internal Triggering Interface 1

LI\_T2 Lawful Interception Internal Triggering Interface 2

LI\_T3 Lawful Interception Internal Triggering Interface 3

LI\_X0 Lawful Interception Internal Interface 0

LI\_X1 Lawful Interception Internal Interface 1

LI\_X2 Lawful Interception Internal Interface 2

LI\_X2\_LA Lawful Interception Internal Interface 2 Location Acquisition

LI\_X3 Lawful Interception Internal Interface 3

LI\_X3A Lawful Interception Internal Interface 3 Aggregator

LI\_XEM1 Lawful Interception Internal Interface Event Management Interface 1

LI\_XER Lawful Interception Internal Interface Event Record

LI\_XLA Lawful Interception Internal Interface Location Acquisition

LI\_XQR Lawful Interception Internal Interface Query Response

LMF Location Management Function

LMISF LI Mirror IMS State Function

LMISF-CC LMISF for the handling of CC

LMISF-IRI LMISF for the handling of IRI

LTF Location Triggering Function

MA Multi-Access

MANO Management and Orchestration

MDF Mediation and Delivery Function

MDF2 Mediation and Delivery Function 2

MDF3 Mediation and Delivery Function 3

MF Media Function

MRFP Multimedia Resource Function Processor

MSRP Message Session Relay Protocol

N3A Non-3GPP Access

N3IWF Non 3GPP Inter Working Function

N9HR N9 Home Routed

NAS Non-Access Stratum

NCGI NR Cell Global Identity

NEF Network Exposure Function

NFV Network Function Virtualisation

NFVI Network Function Virtualisation Infrastructure

NFVO Network Function Virtualisation Orchestrator

NIDD Non-IP Data Delivery

NNI Network to Network Interfaces

NPLI Network Provided Location Information

NR New Radio

NRF Network Repository Function

NSSF Network Slice Selection Function

NWDAF Network Data Analytics Function

OSS Operations Support System

PAG POI Aggregator

PCF Policy Control Function

P-CSCF Proxy - Call Session Control Function

PEI Permanent Equipment Identifier

PGW PDN Gateway

PGW-C PDN Gateway Control Plane

PGW-U PDN Gateway User Plane

POI Point Of Interception

PLMN Public Land Mobile Network

PTC Push to Talk over Cellular

RCD Rich Call Data

RCS Rich Communication Suite

S8HR S8 Home Routed

SCEF Service Capability Exposure Function

SCS Service Capability Server

SGW Serving Gateway

SGW-C Serving Gateway Control Plane

SGW-U Serving Gateway User Plane

SHAKEN Signature-based Handling of Asserted information using toKENs

SIRF System Information Retrieval Function

S-CSCF Serving - Call Session Control Function

SIP Session Initiation Protocol

SMF Session Management Function

SMSF SMS-Function

STF Security Terminating Function

STIR Secure Telephony Identity Revisited

SUCI Subscriber Concealed Identifier

SUPI Subscriber Permanent Identifier

TAI Tracking Area Identity

TF Triggering Function

TLS Transport Layer Security

TNGF Trusted Non-3GPP Gateway Function

TrGW Transit Gateway

TWIF Trusted WLAN Interworking Function

UDM Unified Data Management

UDR Unified Data Repository

UDSF Unstructured Data Storage Function

UPF User Plane Function

VN Group Virtual Network Group

VNF Virtual Network Function

VNFC Virtual Network Function Component

W-AFG Wireline Access Gateway Function

xCC LI\_X3 Content of Communication

xIRI LI\_X2 Intercept Related Information

 END OF FIRST CHANGE

 START OF SECOND CHANGE

### 7.9.X LI for 5G LAN parameter provisioning

#### 7.9.X.1 Background

5G LAN Parameter provisioning is a provisioning capability exposed by NEF to AF (see TS 23.502 [4] clause 4.15.6 and TS 29.522 [31] clause 4.4.15). The AF can use this capability to create, update, delete and query 5G VN group and its information. The AF provides the 5G LAN parameter provisioning data specified in TS 29.522 [31] clause 5.7.2 to NEF and NEF updates the 5G VN group information towards UDM as described in figure 7.9.X-1.



Figure 7.9.X-1: 5GS architecture for 5G LAN parameter provisioning

#### 7.9.X.2 Architecture

Figure 7.9-1 provides the LI architecture for 5G LAN parameter provisioning. The CC-POI is not shown in figure 7.9-1.

#### 7.9.X.3 Target identities

The LIPF present in the ADMF provisions the intercept information associated with the following target identity to the IRI-POI present in the NEF:

- GPSI.

#### 7.9.X.4 IRI events

The IRI-POI present in the NEF shall generate the following xIRIs for 5G LAN parameter provisioning:

- 5G VN group creation.

- 5G VN group update.

- 5G VN group deletion.

- 5G VN group query.

The 5G VN group creation xIRI is generated when the IRI-POI present in the NEF detects that an AF sent a request to create a 5G VN group the target UE belongs to.

The 5G VN group update xIRI is generated when the IRI-POI present in the NEF detects that an AF sent a request to update a 5G VN group the target UE belongs to.

The 5G VN group deletion xIRI is generated when the IRI-POI present in the NEF detects that an AF sent a request to delete a 5G VN group the target UE belongs to.

The 5G VN group query xIRI is generated when the IRI-POI present in the NEF detects that an AF sent a request to query a 5G VN group the target UE belongs to.

 END OF SECOND CHANGE

 END OF LAST CHANGE