**3GPP TSG SA WG4#119e S4-220592**

**E-meeting, 11th – 20th May 2022 revision of S4-220547**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.0* | | | | | | | | |
| **DRAFT CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **26**.**348** | **CR** | draft | **rev** |  | **Current version:** | **16.3.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | **[5MBP3] 5GMS Protocol Extensions for 5GMS via eMBMS** | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Qualcomm Incorporated | | | | | | | | | |
| ***Source to TSG:*** | S4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | 5MBP3 | | | | |  | ***Date:*** | | | 30/03/2022 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | | 17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) Rel-12 (Release 12)* *Rel-13 (Release 13) Rel-14 (Release 14) Rel-15 (Release 15) Rel-16 (Release 16)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | See work item | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Add 5GMS via eMBMS | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Work Item objectives not complete | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | See attached | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | | **X** |  | Other core specifications | | | | TS/TR ... CR | | |
| ***affected:*** | |  |  | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  |  | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | Serves as baseline for future work | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

**===== CHANGE =====**

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 26.501: "5G Media Streaming (5GMS); General description and architecture".

[3] DASH Industry Forum, "Specification of Live Media Ingest",   
<https://dashif-documents.azurewebsites.net/Ingest/master/DASH-IF-Ingest.pdf>

[4] 3GPP TS 26.247: "Transparent end-to-end Packet-switched Streaming Service (PSS); Progressive Download and Dynamic Adaptive Streaming over HTTP (3GP-DASH)".

[5] Standard ECMA-262, 5.1 Edition: "ECMAScript Language Specification", June 2011.

[6] IETF RFC 6234: "US Secure Hash Algorithms (SHA and SHA-based HMAC and HKDF)".

[7] 3GPP TS 23.003: "Numbering, addressing and identification".

[8] ITU-T Recommendation X.509 (2005) | ISO/IEC 9594-8:2005: "Information Technology – Open Systems Interconnection – The Directory: Public-key and attribute certificate frameworks".

[9] IETF RFC 7230: "Hypertext-Transfer Protocol (HTTP/1.1): Message Syntax and Routing".

[10] IETF RFC 4648: "The Base16, Base32, and Base64 Data Encodings".

[11] IEEE Standard 1003.1™, Issue 7: "The Open Group Base Specifications", 2018.  
<https://pubs.opengroup.org/onlinepubs/9699919799/>

[12] 3GPP TS 29.571: "Common Data Types for Service Based Interfaces; Stage 3".

[13] 3GPP TS 38.321: "NR; Medium Access Control (MAC) protocol specification".

[14] 3GPP TS 36.321: "Evolved Universal Terrestrial Radio Access (E-UTRA); Medium Access Control (MAC) protocol specification".

[15] 3GPP TS 27.007: "AT Command set for User Equipment (UE)".

[16] IETF RFC 8446: "The Transport Layer Security (TLS) Protocol Version 1.3", August 2018.

[17] IETF RFC 7468: "Textual Encodings of PKIX, PKCS, and CMS Structures", April 2015.

[18] ISO 3166‑1: "Codes for the representation of names of countries and their subdivisions — Part 1: Country codes".

[19] ISO 3166‑2: "Codes for the representation of names of countries and their subdivisions — Part 2: Country subdivision code".

[20] IETF RFC 5280: "Internet X.509 Public Key Infrastructure Certificate and Certificate Revocation List (CRL) Profile", May 2008.

[21] 3GPP TS 29.500: "5G System; Technical Realization of Service Based Architecture; Stage 3".

[22] 3GPP TS 29.501: "5G System; Principles and Guidelines for Services Definition; Stage 3".

[23] OpenAPI: "OpenAPI 3.0.0 Specification", <https://github.com/OAI/OpenAPI-Specification/blob/master/versions/3.0.0.md>.

[24] IETF RFC 7230: "Hypertext Transfer Protocol (HTTP/1.1): Message Syntax and Routing".

[25] IETF RFC 7231: "Hypertext Transfer Protocol (HTTP/1.1): Semantics and Content".

[26] IETF RFC 7232: "Hypertext Transfer Protocol (HTTP/1.1): Conditional Requests".

[27] IETF RFC 7233: "Hypertext Transfer Protocol (HTTP/1.1): Range Requests".

[28] IETF RFC 7234: "Hypertext Transfer Protocol (HTTP/1.1): Caching".

[29] IETF RFC 7235: "Hypertext Transfer Protocol (HTTP/1.1): Authentication".

[30] IETF RFC 5246: "The Transport Layer Security (TLS) Protocol V8rsion 1.2".

[31] IETF RFC 7540: "Hypertext Transfer Protocol Version 2 (HTTP/2)".

[32] ISO/IEC 23009-1: "Information technology; Dynamic adaptive streaming over HTTP (DASH) — Part 1: Media presentation description and segment formats".

[33] 3GPP TS 23.503: "Policy and charging control framework for the 5G System (5GS); Stage 2".

[34] 3GPP TS 29.514: "5G System; Policy Authorization Service; Stage 3".

[35] 3GPP TS 26.511: "5G Media Streaming (5GMS); Profiles, codecs and formats".

[36] Void.

[37] 3GPP TS 26.244: "Transparent end-to-end packet switched streaming service (PSS); 3GPP file format (3GP)".

[38] IETF RFC 8259: "The JavaScript Object Notation (JSON) Data Interchange Format", December 2017.

[39] ISO 14496-12: "Information technology – Coding of audio-visual objects – Part 12: ISO base media file format".

[40] ISO 23000-19: "Information technology – Coding of audio-visual objects – Part 19: Common media application format (CMAF) for segmented media".

[41] IETF RFC 3986: "URI Generic Syntax".

[42] 3GPP TS 26.118: "Virtual Reality (VR) profiles for streaming applications".

[43] 3GPP TS 26.346: "Multimedia Broadcast/Multicast Service (MBMS); Protocols and codecs".

[44] 3GPP TS 26.347: "Multimedia Broadcast/Multicast Service (MBMS); Application Programming Interface and URL".

**===== CHANGE =====**

## 3.3 Abbreviations

For the purposes of the present document, the abbreviations given in 3GPP TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in 3GPP TR 21.905 [1].

5GMS 5G Media Streaming

5GMSd 5GMS downlink

5GMSu 5GMS uplink

5GMSA 5GMS Architecture

BMFF (ISO) Base Media File Format

ABR Adaptive Bit Rate

AF Application Function

ANBR Access Network Bit rate Recommendation

AS Application Server

CDN Content Delivery Network / Content Distribution Network

CGI Cell Global Identifier

CMAF Common Media Application Format

CRUD Create, Read, Update, Delete

CNAME Canonical Name

CORS Cross-Origin Resource Sharing

CRL Certificate Revocation List

DASH Dynamic Adaptive Streaming over HTTP

DER Distinguished Encoding Rule

DNN Domain Name News

DNS Domain Name Server

ECGI E-UTRAN Cell Global Identifier

ECMA European Computer Manufacturers Association

eMBMS enhanced Multimedia Broadcast Multicast Services

FQDN Fully Qualified Domain Name

GPSI Generic Public Subscription Identifier

HLS HTTP Live Streaming

ISO International Organization for Standardization

JSON JavaScript Object Notation

LCID Logical Channel IDentifier

MFBR Maximum Flow Bit Rate

MIME Multipurpose Internet Mail Extensions

MNO Mobile Network Operator

MPD Media Presentation Description

MSISDN Mobile Subscriber ISDN number

NCGI NR Cell Global Identifier

NEF Network Exposure Function

OAM Operations, Administration and Maintenance

PCC Policy Control and Charging

PCF Policy Control Function

PEM Privacy-Enhanced Mail

PFD Packet Flow Description

PFDF Packet Flow Description Function

QoE Quality of Experience

QoS Quality of Service

SDF Service Data Flow

SHA Secure Hash Algorithm

TLS Transport Layer Security

URI Uniform Resource Identifier

URL Uniform Resource Locator

UTC Coordinated Universal Time

**===== CHANGE =====**

## 4.2 APIs relevant to Downlink Media Streaming

Table 4.2‑1 summarises the APIs used to provision and use the various downlink media streaming features specified in TS 26.501 [2].

Table 4.2‑1: Summary of APIs relevant to downlink media streaming features

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| 5GMSd feature | Abstract | Relevant APIs | | | |
| Interface | API name | | Clause |
| Content protocols discovery | Used by the 5GMSd Application Provider to interrogate which content ingest protocols are supported by 5GMSd AS(s). | M1d | Content Protocols Discovery API | | 7.5 |
| Content hosting | Content is ingested, hosted and distributed by the 5GMSd AS according to a Content Hosting Configuration associated with a Provisioning Session. | M1d | Provisioning Sessions API | | 7.2 |
| Server Certificates Provisioning API | | 7.3 |
| Content Preparation Templates Provisioning API | | 7.4 |
| Content Hosting Provisioning API | | 7.6 |
| M2d | HTTP-pull based content ingest protocol | | 8.2 |
| DASH-IF push based content ingest protocol | | 8.3 |
| M4d | DASH [4] or 3GP [37] | | 10 |
| M5d | Service Access Information API | | 11.2 |
| Metrics reporting | The 5GMSd Client uploads metrics reports to the 5GMSd AF according to a provisioned Metrics Reporting Configuration it obtains from the Service Access Information for its Provisioning Session. | M1d | Provisioning Sessions API | | 7.2 |
| Metrics Reporting Provisioning API | | 7.8 |
| M5d | Service Access Information API | | 11.2 |
| Metrics Reporting API | | 11.4 |
| Consumption reporting | The 5GMSd Client provides feedback reports on currently consumed content according to a provisioned Consumption Reporting Configuration it obtains from the Service Access Information for its Provisioning Session. | M1d | Provisioning Sessions API | | 7.2 |
| Consumption Reporting Provisioning API | | 7.7 |
| M5d | Service Access Information API | | 11.2 |
| Consumption Reporting API | | 11.3 |
| Dynamic Policy invocation | The 5GMSd Client activates different traffic treatment policies selected from a set of Policy Templates configured in its Provisioning Session. | M1d | Provisioning Sessions API | | 7.2 |
| Policy Templates Provisioning API | | 7.9 |
| M5d | Service Access Information API | | 11.2 |
| Dynamic Policies API | | 11.5 |
| Network Assistance | The 5GMSd Client requests bit rate recommendations and delivery boosts from the 5GMSd AF. | M5d | Service Access Information API | | 11.2 |
| Network Assistance API | | 11.6 |
| 5GMS via eMBMS | The 5GMSd AF provisions the delivery of content via eMBMS. | M1d | | Provisioning Sessions API | X.X |
| M5d | | Service Access Information API | X.X |
| M4d | | DASH [4] or 3GP [37] or HLS | X.X |

**===== CHANGE =====**

### 4.3.1 General

A 5GMS Application Provider may use the procedures in this clause to provision the network for media streaming sessions that are operated by that 5GMS Application Provider. For downlink media streaming, these sessions may be DASH streaming sessions, progressive download sessions, or any other type of media streaming or distribution (e.g. HLS) sessions. For uplink media streaming, the content format and delivery protocol are defined by the 5GMSu Application Provider, and may be either non-fully standardized or employ standardized HTTP-based streaming of ISO BMFF content fragments as profiled by CMAF [39].

The M1 interface offers three different sets of procedures:

- For downlink media streaming, configuration of content ingest at M2d for onward distribution by the 5GMSd AS over M4d or via other distribution systems such as eMBMS: designed as an API that is equivalent to the functionality of a public CDN. For uplink media streaming, configuration of content egest at M2u for the media content received by the 5GMSu AS from the 5GMSu Client over M4u. The resource types involved in content hosting configuration are provisioning session (see clause 4.3.2), content hosting procedures (see clause 4.3.3), ingest protocols (see clause 4.3.4), content preparation template (see clause 4.3.5), and server certificates (see clause 4.3.6).

- Configuration of dynamic policies: allows the configuration of Policy Templates at M5 that can be applied to M4 downlink/uplink media streaming sessions.

- Configuration of reporting: permits the MNO to collect, at M5, QoE metrics and consumption reports about M4 downlink sessions, as well as permits the MNO to collect, at M5, QoE metrics reports about M4 uplink sessions.

A 5GMS Application Provider may use any of these procedures, in any combination, to support its media streaming sessions.

**===== CHANGE =====**

#### 4.3.6.1 General

Each X.509 server certificate [8] presented by the 5GMSd AS at reference point M4d or at reference point xMB-U is represented by a Server Certificate resource at M1d. The Server Certificates Provisioning API as specified in clause 7.3 enables a Server Certificate resource to be created within the scope of a Provisioning Session, and subsequently referenced by a Content Hosting Configuration created in the scope of the same Provisioning Session. That API supports two alternative provisioning methods for Server Certificate resources: one in which a certificate is generated by the 5GMS System operator on behalf of the 5GMSd Application Provider; the other in which a certificate is generated by the 5GMSd Application Provider from a Certificate Signing Request solicited from the 5GMSd AF. Both methods shall be supported by implementations of the 5GMSd AF.

**===== CHANGE =====**

#### 4.7.2.1 General

Service Access Information is the set of parameters and addresses needed by the 5GMSd Client to activate reception of a downlink media streaming session or by a 5GMSu Client to activate an uplink media streaming session for contribution. The data model of the ServiceAccessInformation resource acquired by the Media Session Handler of the 5GMS Client is shown in clause 11.2.3. Service Access Information additionally includes configuration information to allow the Media Session Handler to invoke procedures for dynamic policy (see clause 4.7.3), consumption reporting (clause 4.7.4), metrics reporting (clause 4.7.5) and network assistance (clause 4.7.6).

- For downlink media streaming, the Media Session Handler may obtain Service Access Information from either the 5GMSd-Aware Application (via M6d) or the 5GMSd AF (via M5d). In the former case, the Service Access Information is initially acquired by the 5GMSd-Aware Application from the 5GMSd Application Provider via M8d. In the latter case, the Service Access Information is derived by the 5GMSd AF from the Provisioning Session established via M1d.

Typically, the Service Access Information for downlink media streaming includes a media entry point (e.g. a URL to a DASH MPD or a URL to a progressive download file) that can be consumed by the Media Player and is handed to the Media Player through M7d.

For downlink media streaming exclusively via eMBMS and for hybrid 5GMSd/eMBMS services as defined in clauses 5.10.2 and 5.10.5 respectively of TS 26.501 [2], the Service Access Information indicates that the 5GMSd Client acts as an MBMS-Aware Application.

For dynamically provisioned downlink media streaming via eMBMS as defined in clause 5.10.6 of TS 26.501 [2], the Service Access Information is updated dynamically by the 5GMSd AF to reflect whether or not the eMBMS service is currently active, and this determines whether the 5GMSd Client acts as an MBMS-Aware Application or not.- For uplink media streaming, the 5GMSu Client may obtain Service Access Information from either the 5GMSu-Aware Application (via M6u/M7u) or the 5GMSu AF (via M5u). In the former case, the Service Access Information is initially acquired by the 5GMSu-Aware Application from the 5GMSu Application Provider via M8u. In the latter case, the Service Access Information is derived by the 5GMSu AF from the Provisioning Session established via M1u.

This clause specifies the procedures whereby the 5GMS Client fetches Service Access Information from the 5GMS AF.

**===== CHANGE =====**

### 4.7.4 Procedures for consumption reporting

These procedures are used by the Media Session Handler and the Consumption Reporting functions of the 5GMSd Client to submit a consumption report via the M5d interface if Consumption Reporting is applied for a downlink streaming session.

The Service Access Information indicating whether Consumption Reporting is provisioned for downlink streaming sessions is described in clause 11.2.3. When the ClientConsumptionReportingConfiguration.samplePercentage value is 100, the Media Session Handler shall activate the consumption reporting procedure. If the samplePercentage is less than 100, the Media Session Handler shall generate a random number which is uniformly distributed in the range of 0 to 100, and the Media Session Handler shall activate the consumption report procedure when the generated random number is of a lower value than the samplePercentage value.

If the consumption reporting procedure is activated, the Media Session Handler shall submit a consumption report to the 5GMSd AF when any of the following conditions occur:

- Start of consumption of a downlink streaming session;

- Stop of consumption of a downlink streaming session;

- Upon determining the need to report ongoing 5GMS consumption at periodic intervals determined by the ClientConsumptionReportingConfiguration.reportingInterval property.

- Upon determining a location change, if the ClientConsumptionReportingConfiguration.locationReporting property is set to True.

- Upon determining an access network change (e.g. 5GMSd to eMBMS, or *vice versa*), if the ClientConsumptionReportingConfiguration.accessReporting property is set to True.

Whenever a consumption report is sent, the Media Session Handler shall reset its reporting interval timer to the value of the reportingInterval property and it shall begin countdown of the timer again. Whenever the Media Session Handler stops the consumption of a downlink streaming session, it shall disable its reporting interval timer.

In order to submit a consumption report, the Media Session Handler shall send an HTTP POST message to the 5GMSd AF. If several 5GMSd AF addresses are listed in the ClientConsumptionReportingConfiguration.‌serverAddresses array (see table 11.2.3.1-1), the Media Session Handler shall choose one and send the message to the selected. The request body shall be a ConsumptionReport structure, as specified in clause 11.3.3.1.The server shall respond with a 200 (OK) message to acknowledge successful processing of the consumption report.

The Consumption Reporting API, defining the data formats and structures and related procedures for consumption reporting, is described in clause 11.3.

A reporting client identifier shall be included in the consumption report. If available to the Media Session Handler, its value should be a GPSI value as defined by TS 23.003 [7]. Otherwise, the reporting client identifier should be represented by a stable and globally unique string.

**===== CHANGE =====**

### 4.7.5 Procedures for metrics reporting

The M5 procedures for QoE metrics reporting pertain to the combination of the provisioning of metrics collection and reporting in the Media Session Handler using relevant Service Access Information, and the sending of collected metrics by the Media Session Handler to the 5GMS AF in accordance with the configured metrics scheme(s). A metrics scheme may be 3GPP-defined or non-3GPP-defined.

When the metrics collection and reporting feature is activated for a downlink media streaming session, one or more metrics configuration sets, each associated with a metrics scheme, may be provided to the 5GMS Client. A given metrics configuration set contains information such as the 5GMS AF address(es) to which metrics are to be sent by the Media Session Handler, metrics reporting interval, target percentage of media streaming sessions for which reports should be sent, and the set of metrics to be collected and reported. See TS 26.501 [2] for additional details.

For progressive download and DASH streaming services, the listed metrics in a given metrics configuration set are associated with the 3GPP metrics scheme and shall correspond to one or more of the metrics as specified in clauses 10.3 and 10.4, respectively, of TS 26.247 [4]. Metrics related to virtual reality media, as specified in clause 9.3 of TS 26.118 [42], may also be listed in the metrics configuration. Metrics related to eMBMS delivery, as specified in clause 9.4.6 of TS 26.346 [43], may also be listed in the metrics configuration.

Details of the metrics reporting API are provided in clause 11.4, and for 3GP-DASH based downlink media streaming services, the 3GPP-defined metrics reporting scheme and metrics report format are defined in clause 11.4.3.

A reporting client identifier may be included in the metrics report. If available to the Media Session Handler, its value should be a GPSI value as defined by TS 23.003 [7]. Otherwise, the reporting client identifier should be represented by a stable and globally unique string.

**===== CHANGE =====**

## 4.X Procedures for downlink media streaming via eMBMS

This procedure is used by a 5GMSd Client to establish a 5GMSd session either completely, or at least partially, through eMBMS.

- For downlink media streaming exclusively via eMBMS and for hybrid 5GMSd/eMBMS services, as defined in clauses 5.10.2 and 5.10.5 respectively of TS 26.501 [2]:

- The MBMS Client shall host an MPD as defined in ISO/IEC 23009‑1 [32] or in TS 26.247 [4], or any other presentation manifest as the 5GMSd Media Entry Point.

- The URL of this presentation manifest shall be signalled to the 5GMSd Client through the 5GMSd session establishment procedure.

- The MBMS Client shall be invoked by the Media Session Handler via reference point MBMS-API-C using the procedures defined in TS 26.347 [44].

- For dynamically provisioned downlink media streaming via eMBMS as defined in clause 5.10.6 TS 26.501 [2]L

- The 5GMSd AS shall host an MPD as defined in ISO/IEC 23009‑1 [32] or in TS 26.247 [4], or any other presentation manifest as the 5GMSd Media Entry Point.

- The URL of this presentation manifest shall be signalled to the 5GMSd Client through the 5GMSd session establishment procedure. The manifest request shall be proxied through the Media Session Handler and, if the 5GMSd service is currently available as an MBMS User Service, the Media Session Handler forwards the manifest request to the MBMS Client; otherwise, it forwards the request to the 5GMSd AS via reference point M4d.

- The MBMS Client shall be invoked dynamically, paused or destroyed by the Media Session Handler via reference point MBMS-API-C using the procedures defined in TS 26.347 [44].

Additional procedures for reactions to different HTTP status codes are provided in clause A.7 of TS 26.247 [4] and clause A.7 of ISO/IEC 23009‑1 [32].

Additional procedures for handling partial file responses are provided in clause A.9 of TS 26.247 [4].

**===== CHANGE =====**

#### 11.2.3.1 ServiceAccessInformation resource type

The data model for the ServiceAccessInformtion resource is specified in table 11.2.3.1-1 below. Different properties are present in the resource depending on the type of Provisioning Session from which the Service Access Information is derived (as indicated in the provisioningSessionType property) and this is specified in the Applicability column.

Table 11.2.3.1‑1: Definition of ServiceAccessInformation resource

| Property name | Type | Cardinality | Usage | Description | Applicability |
| --- | --- | --- | --- | --- | --- |
| provisioningSessionId | ResourceId | 1..1 | RO | Unique identification of the M1 Provisioning Session. | All types |
| provisioningSession‌Type | Provisioning‌Session‌Type | 1..1 | RO | The type of Provisioning Session. | All types. |
| StreamingAccess | Object | 0..1 | RO |  | downlink |
| mediaPlayerEntry | Url | 0..1 | RO | A document or a pointer to a document that defines a media presentation e.g. MPD for DASH content or URL to a video clip file. |
| eMBMS‌Service‌Announcement‌Locator | Url | 0..1 | RO | A pointer to a document that defines a user service announcement for eMBMS where the service announcement file is available. | downlink |
| ClientConsumptionReporting‌Configuration | Object | 0..1 | RO |  | downlink |
| reportingInterval | DurationSec | 0..1 | RO | The time interval, expressed in seconds, between consumption report messages being sent by the Media Session Handler. The value shall be greater than zero.  When this property is omitted, a single final report shall be sent immediately after the media streaming session has ended. |
| serverAddresses | Array(Url) | 1..1 | RO | A list of 5GMSd AF addresses (URLs) where the consumption reporting messages are sent by the Media Session Handler. See NOTE.  (Opaque URL, following the 5GMS URL format.) |
| locationReporting | Boolean | 1..1 | RO | Stipulates whether the Media Session Handler is required to provide location data to the 5GMSd AF in consumption reporting messages (in case of MNO or trusted third parties). |
| accessReporting | Boolean | 1..1 | RO | Stipulates whether the Media Session Handler is required to provide consumption reporting messages to the 5GMSd AF when the access network changes during a media streaming session. |
| samplePercentage | Percentage | 1..1 | RO | The percentage of media streaming sessions that shall send consumption reports, expressed as a floating point value between 0.0 and 100.0. |
| DynamicPolicyInvocation‌Configuration | Object | 0..1 | RO |  | downlink,  uplink |
| serverAddresses | Array(Url) | 1..1 | RO | A list of 5GMSd AF addresses (URLs) which offer the APIs for dynamic policy invocation sent by the Media Session Handler. See NOTE.  (Opaque URL, following the 5GMS URL format.) |
| scheme | Uri | 1..1 | RO | The metrics reporting scheme that metrics reports shall use (see clause 4.7.5). |
| validPolicyTemplateIds | Array(ResourceId) | 1..1 | RO | A list of Policy Template identifiers which the 5GMS Client is authorized to use. |
| sdfMethods | Array(SdfMethod) | 1..1 | RO | A list of recommended service data flow description methods (descriptors), e.g. 5-Tuple, ToS, 2-Tuple, etc., which should be used by the Media Session Handler to describe the service data flows for the traffic to be policed. |
| externalReferences | Array(String) | 0..1 | RO | Additional identifier for this Policy Template, unique within the scope of its Provisioning Session, that can be cross-referenced with external metadata about the media streaming session.  Example: "HD\_Premium". |
| ClientMetricsReporting‌Configurations | Array(Object) | 0..1 | RO |  | downlink,  uplink |
| serverAddresses | Array(Url) | 1..1 | RO | A list of 5GMS AF addresses to which metrics reports shall be sent. See NOTE.  (Opaque URL, following the 5GMS URL format.) |
| dataNetworkName | Dnn | 0..1 | RO | The DNN which shall be used when sending metrics reports. If not specified, the name of the default DN shall be used. |
| reportingInterval | DurationSec | 0..1 | RO | The time interval, expressed in seconds, between metrics reports being sent by the Media Session Handler. The value shall be greater than zero.  When this property is omitted, a single final report shall be sent immediately after the media streaming session has ended. |
| samplePercentage | Percentage | 1..1 | RO | The percentage of media streaming sessions that shall report metrics, expressed as a floating point value between 0.0 and 100.0. |
| urlFilters | Array(String) | 0..1 | RO | A non-empty list of URL patterns for which metrics reporting shall be done. The format of each pattern shall be a regular expression as specified in [5].  If not specified, reporting shall be done for all sessions. |
| metrics | Array(String) | 1..1 | RO | A list of metrics which shall be reported. |
| NetworkAssistanceConfiguration | Object | 0..1 | RO |  | downlink,  uplink |
| serverAddress | Url | 1..1 | RO | Address of the 5GMS AF that offers the APIs for 5GMS AF-based Network Assistance, for access by the 5GMSd Media Session Handler. See NOTE.  This address shall be an opaque URL, following the 5GMS URL format. |
| NOTE: In deployments where multiple instances of the 5GMSd AF expose the Media Session Handling APIs at M5, the 5G System may use a suitable mechanism (e.g. HTTP load balancing or DNS resolution) to direct requests to a suitable AF instance. | | | | | |

**===== CHANGE =====**

#### 11.3.3.2 ConsumptionReportingUnit type

This type represents a single consumption reporting unit.

Table 11.3.3.2-1: Definition of type ConsumptionReportingUnit

|  |  |  |  |
| --- | --- | --- | --- |
| Property name | Data type | Cardinality | Description |
| mediaConsumed | string | 1..1 | Identifies the media consumed.  In the case of DASH, the value of the **Representation**@id attribute shall be quoted. |
| mediaBaseURL | Url | 0..1 | The Base URL used to access the media consumed, indicating whether 5GMSd or eMBMS was used to acquire the media during the period of this consumption reporting unit.  Property present only if access reporting is enabled in the Consumption Reporting Configuration. |
| startTime | DateTime | 1..1 | The time when this consumption reporting unit started. |
| duration | DurationSec | 1..1 | The duration of this consumption reporting unit. |
| locations | Array(TypedLocation) | 0..1 | A time-ordered list of UE location(s) where the media was consumed during the period of this consumption reporting unit.  Property present only if location reporting is enabled in the Consumption Reporting Configuration (only for trusted AF).  The cardinality of objects in this array is 1..N. |

**===== CHANGE =====**

## C.4.1 M5\_ServiceAccessInformation API

|  |
| --- |
| openapi: 3.0.0  info:    title: M5\_ServiceAccessInformation    version: 2.0.0    description: |      5GMS AF M5 Service Access Information API      © 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).      All rights reserved.  tags:    - name: M5\_ServiceAccessInformation      description: '5G Media Streaming: Media Session Handling (M5) APIs: Service Access Information'  externalDocs:    description: 'TS 26.512 V17.1.0; 5G Media Streaming (5GMS); Protocols'    url: 'https://www.3gpp.org/ftp/Specs/archive/26\_series/26.512/'  servers:    - url: '{apiRoot}/3gpp-m5/v2'      variables:        apiRoot:          default: https://example.com          description: See 3GPP TS 29.512 clause 6.1.  paths:    /service-access-information/{provisioningSessionId}:      parameters:        - name: provisioningSessionId          description: 'The resource identifier of an existing Provisioning Session.'          in: path          required: true          schema:            $ref: 'TS26512\_CommonData.yaml#/components/schemas/ResourceId'      get:        operationId: retrieveServiceAccessInformation        summary: 'Retrieve the Service Access Information resource'        responses:          '200':            description: 'Success'            content:              application/json:                schema:                    $ref: '#/components/schemas/ServiceAccessInformationResource'          '404':            description: 'Not Found'  components:    schemas:      ServerAddresses:        type: array        items:          $ref: 'TS26512\_CommonData.yaml#/components/schemas/Url'        minItems: 1      ServiceAccessInformationResource:        type: object        required:        - provisioningSessionId        - provisioningSessionType        properties:          provisioningSessionId:            $ref: 'TS26512\_CommonData.yaml#/components/schemas/ResourceId'          provisioningSessionType:            $ref: 'TS26512\_CommonData.yaml#/components/schemas/ProvisioningSessionType'          StreamingAccess:            type: object            properties:              mediaPlayerEntry:                $ref: 'TS26512\_CommonData.yaml#/components/schemas/Url'              eMBMSServiceAnnouncementLocator:                $ref: 'TS26512\_CommonData.yaml#/components/schemas/Url'          ClientConsumptionReportingConfiguration:            type: object            required:              - serverAddresses              - locationReporting              - samplePercentage            properties:              reportingInterval:                $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'              serverAddresses:                $ref: '#/components/schemas/ServerAddresses'              locationReporting:                type: boolean              accessReporting:                type: boolean              samplePercentage:                $ref: 'TS26512\_CommonData.yaml#/components/schemas/Percentage'          DynamicPolicyInvocationConfiguration:            type: object            required:              - serverAddresses              - validPolicyTemplateIds              - sdfMethods            properties:              serverAddresses:                $ref: '#/components/schemas/ServerAddresses'              validPolicyTemplateIds:                type: array                items:                  $ref: 'TS26512\_CommonData.yaml#/components/schemas/ResourceId'                minItems: 0              sdfMethods:                type: array                items:                  $ref: 'TS26512\_CommonData.yaml#/components/schemas/SdfMethod'                minItems: 0              externalReferences:                type: array                items:                  type: string                minItems: 1          ClientMetricsReportingConfiguration:            type: array            items:              type: object              required:              - serverAddresses              - scheme              - samplePercentage              - urlFilters              - metrics              properties:                serverAddresses:                  $ref: '#/components/schemas/ServerAddresses'                scheme:                  $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'                dataNetworkName:                  $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'                reportingInterval:                  $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'                samplePercentage:                  $ref: 'TS26512\_CommonData.yaml#/components/schemas/Percentage'                urlFilters:                  type: array                  items:                    type: string                  minItems: 0                metrics:                  type: array                  items:                    type: string          NetworkAssistanceConfiguration:            type: object            required:              - serverAddress            properties:              serverAddress:                $ref: 'TS26512\_CommonData.yaml#/components/schemas/Url' |

**===== CHANGE =====**

## C.4.2 M5\_ConsumptionReporting API

|  |
| --- |
| openapi: 3.0.0  info:    title: M5\_ConsumptionReporting    version: 2.0.0    description: |      5GMS AF M5 Consumption Reporting API      © 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).      All rights reserved.  tags:    - name: M5\_ConsumptionReporting      description: '5G Media Streaming: Media Session Handling (M5) APIs: Consumption Reporting'  externalDocs:    description: 'TS 26.512 V17.1.0; 5G Media Streaming (5GMS); Protocols'    url: 'https://www.3gpp.org/ftp/Specs/archive/26\_series/26.512/'  servers:    - url: '{apiRoot}/3gpp-m5/v2'      variables:        apiRoot:          default: https://example.com          description: See 3GPP TS 29.512 clause 6.1.  paths:    /consumption-reporting/{aspId}:      parameters:        - name: aspId          in: path          required: true          schema:            $ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/AspId'          description: 'See 3GPP TS 26.512 clause 11.3.2.'      post:        operationId: submitConsumptionReport        summary: 'Submit a Consumption Report'        requestBody:          description: 'A Consumption Report'          required: true          content:            application/json:              schema:                $ref: '#/components/schemas/ConsumptionReport'        responses:          '204':            description: 'Consumption Report Accepted'          '400':            description: 'Bad Request'          '415':            description: 'Unsupported Media Type'  components:    schemas:      ConsumptionReport:        type: object        required:          - mediaPlayerEntry          - reportingClientId          - consumptionReportingUnits        properties:          mediaPlayerEntry:            type: string          reportingClientId:            type: string          consumptionReportingUnits:            type: array            items:              $ref: '#/components/schemas/ConsumptionReportingUnit'      ConsumptionReportingUnit:        type: object        required:          - mediaConsumed          - startTime          - duration        properties:          mediaConsumed:            type: string          mediaBaseURL:            $ref: 'TS26512\_CommonData.yaml#/components/schemas/Url'          startTime:            $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'          duration:            $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'          locations:            type: array            items:              $ref: 'TS26512\_CommonData.yaml#/components/schemas/TypedLocation'            minItems: 1 |