|  |
| --- |
| 3GPP TS 26.517 V1.2.0 (2022-05) |
| Technical Specification |
| 3rd Generation Partnership Project;Technical Specification Group Systems and Services Aspects;5G Multicast–Broadcast User Services;Protocols and Formats(Release 17) |
|  |
|  |  |
|  |
| The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP.The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented.This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification.Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices. |

|  |
| --- |
|  |
| ***3GPP***Postal address3GPP support office address650 Route des Lucioles - Sophia AntipolisValbonne - FRANCETel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16Internethttp://www.3gpp.org |
| ***Copyright Notification***No part may be reproduced except as authorized by written permission.The copyright and the foregoing restriction extend to reproduction in all media.© 2021, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).All rights reserved.UMTS™ is a Trade Mark of ETSI registered for the benefit of its members3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational PartnersLTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational PartnersGSM® and the GSM logo are registered and owned by the GSM Association |

Contents

Foreword 5

1 Scope 7

2 References 7

3 Definitions of terms, symbols and abbreviations 7

3.1 Terms 7

3.2 Symbols 7

3.3 Abbreviations 8

4 System overview 8

5 User Service Announcement 8

5.1 Data model 8

5.1.1 General 8

5.2 Semantics 11

5.2.1 General 11

5.2.2 MBS User Service Bundle Description metadata unit 11

5.2.3 MBS User Service Description metadata unit 11

5.2.4 MBS Distribution Session Description metadata unit 11

5.2.5 Session Description metadata unit 12

5.2.6 MBS Application Service Description metadata unit 12

5.2.7 MBS Schedule Description metadata unit 13

5.2.8 MBS Object Repair Parameters metadata unit 15

5.3 Delivery of Service Announcement 16

6 Object Delivery Method 16

6.1 General 16

6.2 Usage of FLUTE for Object Distribution Method 16

6.2.1 General 16

6.2.2 Session Description metadata unit 16

6.2.2.1 General 16

6.2.2.2 MBS service type of MBS Session 17

6.2.2.3 SDP examples for FLUTE Session 18

6.2.3 Operating modes for Object Distribution Method 18

6.2.3.1 Introduction 18

6.2.3.2 Single object operating mode 18

6.2.3.3 Object collection operating mode 18

6.2.3.4 Object carousel operating mode 19

6.2.3.5 Segment streaming operating mode 19

7 Packet Delivery Method 20

7.1 General 20

7.2 Re-using MBMS Delivery Method as Packet Distribution Method 20

7.2.1 General 20

7.2.3 Session Description 20

7.2.3.1 General 20

7.2.3.2 SDP examples for Packet Distribution Method 21

Annex A (normative) Syntax for Service Announcement 22

A.1 XML-based representation 22

A.1.1 MBS User Service Description schema 22

A.1.2 Object Repair Parameters schema 24

A.1.3 Schedule Description schema 24

A.2 JSON-based representation 26

A.2.1 MBS User Service Bundle Description schema 26

Annex B (informative) Service Announcement examples 31

B.1 XML-based representation 31

B.2 JSON-based representation 31

Annex C (normative) Controlled vocabulary of conformance profiles 33

Annex <X> (informative): Change history 34

# Foreword

This Technical Specification has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

In the present document, modal verbs have the following meanings:

**shall** indicates a mandatory requirement to do something

**shall not** indicates an interdiction (prohibition) to do something

The constructions "shall" and "shall not" are confined to the context of normative provisions, and do not appear in Technical Reports.

The constructions "must" and "must not" are not used as substitutes for "shall" and "shall not". Their use is avoided insofar as possible, and they are not used in a normative context except in a direct citation from an external, referenced, non-3GPP document, or so as to maintain continuity of style when extending or modifying the provisions of such a referenced document.

**should** indicates a recommendation to do something

**should not** indicates a recommendation not to do something

**may** indicates permission to do something

**need not** indicates permission not to do something

The construction "may not" is ambiguous and is not used in normative elements. The unambiguous constructions "might not" or "shall not" are used instead, depending upon the meaning intended.

**can** indicates that something is possible

**cannot** indicates that something is impossible

The constructions "can" and "cannot" are not substitutes for "may" and "need not".

**will** indicates that something is certain or expected to happen as a result of action taken by an agency the behaviour of which is outside the scope of the present document

**will not** indicates that something is certain or expected not to happen as a result of action taken by an agency the behaviour of which is outside the scope of the present document

**might** indicates a likelihood that something will happen as a result of action taken by some agency the behaviour of which is outside the scope of the present document

**might not** indicates a likelihood that something will not happen as a result of action taken by some agency the behaviour of which is outside the scope of the present document

In addition:

**is** (or any other verb in the indicative mood) indicates a statement of fact

**is not** (or any other negative verb in the indicative mood) indicates a statement of fact

The constructions "is" and "is not" do not indicate requirements.

# 1 Scope

The present document defines protocols and formats for User Services as defined in TS 26.502 [6] and conveyed using the 5G multicast–broadcast capabilities of the 5G System defined in TS 23.501 [2], TS 23.502 [3] and TS 23.247 [5].

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 23.501: "System architecture for the 5G System (5GS)".

[3] 3GPP TS 23.502: "Procedures for the 5G System (5GS)".

[4] 3GPP TS 23.503: "Policy and charging control framework for the 5G System (5GS); Stage 2".

[5] 3GPP TS 23.247: "Architectural enhancements for 5G multicast-broadcast services; Stage 2".

[6] 3GPP TS 26.502: "5G multicast–broadcast services; User Service architecture".

[7] 3GPP TS 26.346: “MBMS; Protocols and Codecs".

[8] IETF RFC 8866: "Session Description Protocol".

[9] W3C: "XML Schema Part 2: Datatypes".

[10] 3GPP TS 23.003: "Numbering, addressing and identification".

[11] 3GPP TS 24.008: "Mobile radio interface Layer 3 specification; Core network protocols; Stage 3".

[12] IETF RFC 3926: "FLUTE - File Delivery over Unidirectional Transport".

[13] IETF RFC 2616: "Hypertext Transfer Protocol -- HTTP/1.1".

# 3 Definitions of terms, symbols and abbreviations

## 3.1 Terms

For the purposes of the present document, the terms given in 3GPP TR 21.905 [1], TS 23.501 [2], TS 23.502 [3], TS 23.247 [5], TS 26.502 [6] and the following apply. A term defined in the present document takes precedence over the definition of the same term, if any, in 3GPP TR 21.905 [1].

## 3.2 Symbols

Void.

## 3.3 Abbreviations

For the purposes of the present document, the abbreviations given in 3GPP TR 21.905 [1], TS 23.501 [2], TS 23.502 [3], TS 23.247 [4] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in 3GPP TR 21.905 [1].

CMAF Common Media Application Format

FLUTE File Delivery over Unidirectional Transport

MBS Multicast–Broadcast Services

MB‑SMF Multicast–Broadcast Session Management Function

MB‑UPF Multicast–Broadcast User Plane Function

MBSF Multicast–Broadcast Service Function

MBSTF Multicast–Broadcast Service Transport Function

PCF Policy and Charging Function

NEF Network Exposure Function

SDP Session Description Protocol

TMGI Temporary Mobile Group Identity

UE User Equipment

UML Unified Markup Language

XML eXtensible Markup Language

# 4 System overview

# 5 User Service Announcement

## 5.1 Data model

### 5.1.1 General

MBS User Service Announcement is needed in order to advertise MBS User Services in advance of, and potentially during, the MBS User Service Sessions described. The MBS User Service Sessions are described by a set of metadata documents that are delivered as described in clause 4.3.2 of TS 23.502 [3].

Each metadata document is divided into *metadata units*. A metadata unit is a single uniquely identifiable block of metadata. The metadata itself describes details of services. An obvious example of a metadata unit would be a single SDP document [8].

The metadata consists of:

- An *MBS User Service Bundle Description* metadata unit (see clause 5.2.2) describing a bundle of one or more MBS User Services, and containing one or more:

- *MBS User Service Description* metadata unit (see clause 5.2.3) describing an MBS User Service Session that is associated with:

- One or more *MBS Distribution Session Description* metadata units (see clause 5.2.4), each of which references a Session Description document [8] that may be packaged with the MBS User Service Bundle Description, and each of which may optionally reference an Object Repair Parameters document (see clause 5.2.7) describing the object repair parameters for the MBS Distribution Session.

- Zero or more *MBS Application Service Description* metadata units (see clause 5.2.5), each of which references an Application Service Entry Point document that may be packaged with the MBS User Service Bundle Description. Additional resources referenced by the entry point document may also be packaged with the MBS User Service Bundle Description.

- Zero or one *MBS Schedule Description* metadata unit (see clause 5.2.6) advertising the delivery schedule for the MBS User Service Session.

Figure 5.1‑1 illustrates the relationships between these metadata units using UML for a single MBS User Service Bundle.



NOTE: “N” means any number in each instance.

Figure 5.1-1: User Service Data Model simple description

An MBS User Service Bundle Description document shall contain one or more instances of the MBS User Service Description metadata unit, each of which describes a single MBS User Service Session within the MBS User Service Bundle.

Each instance of the MBS User Service Description metadata unit shall include at least one *MBS Distribution Service Description* metadata unit describing the set of MBS Distribution Sessions currently associated with the MBS User Service Session.

- The MBS Distribution Session Description metadata unit shall refer to one *Session Description document*.

- Each MBS Distribution Session Description metadata unit may contain a reference to an *Object Repair Parameters document*.

Each instance of the MBS User Service Description metadata unit may include zero or more *MBS Application Service Description* metadata units, each one referencing an Application Service Entry Point document (e.g. a DASH MPD, HLS Master Playlist or HTML document) which describes the root of the Application Service associated with this MBS User Service. When multiple Application Service Entry Point documents are referenced, an MBS Client shall select only one on the basis of a distinct MIME content type indicated in the Application Service Description.

Each instance of the MBS User Service Description metadata unit may include an *MBS Schedule Description* metadata unit. If included, the MBS Schedule Description shall refer to a *Schedule Description document*, and the UE can expect to receive MBS User Service data during the time periods described in the Schedule Description document.

In the case of the Object Distribution Method, the Schedule Description document may include an object transmission schedule for objects associated with the MBS User Service Session. The UE may select which objects to receive based on the object transmission schedule information published in the Schedule Description document.

## 5.2 Semantics

### 5.2.1 General

The following description in this clause presumes XML encoding of the metadata units comprising the MBS User Service Announcement.

### 5.2.2 MBS User Service Bundle Description metadata unit

The root element of the MBS User Service Bundle Description metadata unit is bundleDescription. This element is of type *bundleDescriptionType*. The bundleDescription element contains one or several userService‌Description child elements.

### 5.2.3 MBS User Service Description metadata unit

The root element of the MBS User Servive Description metadata unit is the userServiceDescription element. Each userServiceDescription element shall signal a unique identifier in its @serviceIdattribute and this shall be of URI format.

The userServiceDescription element may contain one or more name child elements. The purpose of a nameelement is to communicate a human-readable title of the MBS User Service. For each name element, the language shall be specified according to XML datatypes (XML Schema Part 2 [9]).

The userServiceDescription element may contain one or more serviceLanguage child elements. Each serviceLanguageelement represents the available languages of the MBS User Service. The language shall be specified according to XML datatypes (XML Schema Part 2 [9]) using the xml:lang attribute.

### 5.2.4 MBS Distribution Session Description metadata unit

Each MBS User Service Description metadata unit shall reference at least one MBS Distribution Session Description. The distributionSessionDescription element shall contain a @sessionDescriptionURI attribute which references a Session Description document. The element may also contain an @objectRepairParametersURIattribute referencing an Object Repair Parameters document.

ThedistributionSessionDescription element shall contain a @conformanceProfileattribute indicating the set of features that the MBS Distribution Session conforms to and which the MBS Client needs to support in order to fully receive the MBS Distribution Session. The value of this attribute shall be a fully-qualified term identifier URI from the controlled vocabulary defined in annex C.

ThedistributionSessionDescription element may contain a @dataNetworkNameattribute indicating a Data Network Name (DNN) as defined in TS 23.003 [10]. When this attribute is present, the MBS Client shall use the given DNN for interactions with the MBSF at reference point MBS‑5 and with the MBS AS at reference point MBS‑4‑UC. If this attribute is not present, the MBS UE shall use a default PDU Session for these network interactions.

The userServiceDescription element may include an availabilityInfo child element providing additional information pertaining to the availability of the MBS Distribution Session within the 5G Network. If present, the availabilityInfo element shall include one or more infoBinding child elements. The infoBinding element shall contain the child elements serviceArea and radiofrequency:

- The serviceArea element declares the one or more service areas in which the MBS Session corresponding to this MBS Distribution Session is currently available.

- The radioFrequencyelement indicates the one or more radio frequencies in the NG-RAN downlink which transmit the MBS Session corresponding to this MBS Distribution Session in the service area(s) identified by the serviceArea element.

### 5.2.5 Session Description metadata unit

The @sessionDescriptionURI attribute of the MBS User Service Bundle Description references a Session Description metadata unit. Each Session Description metadata unit shall describe one MBS Distribution Session. The Session Description metadata unit is conveyed in a Session Description document that shall be formatted according to RFC 8866 [8]. The Session Description document may be packaged in the same MBS User Service Bundle.

- The session description for the MBS Object Distribution Method is specified in clause 6.2.3

- The session description for the MBS Packet Distribution Method is specified in clause 7.2.3.

### 5.2.6 MBS Application Service Description metadata unit

In order to support application services in MBS, the MBS User Service Bundle Description metadata unit shall contain an appServiceDescription element referencing an *Application Service Entry Point* document which contains the descriptive information of the resources delivered via MBS and/or unicast distribution. That Application Service Entry Point document shall be formatted according to the value of the @mimeType attribute.

If the MBS User Service Description contains a reference to an Application Service Entry Point document, then:

1) At least one MBS Distribution Session Description of type Object Distribution Method shall be present, i.e. the MBS User Service Description shall include at least one distributionSessionDescription element referencing a Session Description Document that describes an Object Distribution Method as defined in clause 7.

2) When multiple MBS Distribution Session Descriptions of type Object Distribution Method are present, the appServiceDescription element shall define a mapping between the Application Service Entry Point document and the associated MBS Distribution Session.

3) The MBS Distribution Session described by the Session Description document shall deliver objects that are directly or indirectly referenced by the Application Service Entry Point document.

4) When the Application Service Entry Point document is a DASH MPD, then all of the following shall hold:

a) The MBS Distribution Session shall deliver the objects such that the last packet of the delivered object is available to the MBS Client by no later than its availability time as announced in the DASH MPD.

b) The Content-Location element in the FLUTE File Delivery Table for the delivered object shall match the URL in the DASH MPD.

Editor’s Note: Bullets 4 and 5 should be moved to Clause 7.

4) If an update to the Application Service Entry Point document is delivered as a FLUTE transmission object then the Content-Location element in the FLUTE File Delivery Table for the delivered object shall match the URL of the referenced Application Service Entry Point document.

In the case of 3GP-DASH formatted content, the appServiceDescription element may refer to a unified media manifest document which describes Representations available for both MBS reception and unicast retrieval, and this shall be used by MBS Clients compliant with this specification. In practical deployments, different subsets of the Representations described by the unified manifest document and referenced by such appServiceDescription may be specified for:

- Availability via MBS delivery only,

- Availability via both unicast and MBS delivery,

- Availability via unicast only, and the Representation is redundant in MBS area coverage, i.e. the usage of these resources does not provide an improved user experience. As an example, this may be a lower bitrate Representation of a media component for which a higher bitrate is available over MBS distribution, and

- Availability always via unicast, and the Representation is supplementary in MBS area coverage, i.e. even in MBS area coverage these resources provide an improved user experience. As an example, this may be a secondary language that is only accessible over unicast.

All resources that are directly or indirectly referenced in the Application Service Entry Point document of this metadata unit that are expected to be retrieved by HTTP GET shall be delivered by at least one of the MBS Distribution Sessions associated with the MBS User Service Description.

### 5.2.7 MBS Schedule Description metadata unit

Availability of the Schedule Description metadata unit is indicated by the presence of the scheduleDescription element in the MBS User Service Bundle Description metadata unit. The URI of the Schedule Description instance document is provided by the @scheduleDescriptionURI attribute in the scheduleDescription element.

A Schedule Description instance document describes the distribution schedule of the MBS Distribution Session and the availability of content via unicast delivery for an MBS User Service in terms of:

- Start/stop lists,

- Recurrence information,

- The service ID or service class to which the schedule may apply,

An MBS User Service containing multiple content components may be carried on a single MBS Distribution Session, or on multiple MBS Distribution Sessions. The MBS Client can expect to receive MBS data during the described time period(s) when at least one of the MBS Distribution Sessions for the MBS User Service is active.

A Schedule Description instance document may also include a schedule of when the objects are intended to be transmitted as part of an MBS Distribution Session using the Object Distribution Method. The object schedule information is defined in terms of:

- The service ID or service class to which the object schedule applies,

- An object transmission schedule listing for each object:

- Object URI,

- A list of start and end times for distribution of the object via MBS,

A Schedule Description instance document may be delivered to the MBS Client:

- prior to the MBS Distribution Session as part of the MBS User Service Announcement along with the Session Description metadata unit (out-of-band of that session); or

- in band within an MBS Distribution Session; or

- via an MBS Distribution Session dedicated to the transport of Schedule Description instance documents.

The most recently delivered Schedule Description instance document shall take priority, such that schedule parameters received prior to – and out-of-band of – the MBS Distribution Session they apply to are regarded as "initial defaults", and schedule parameters received in-band with the MBS Distribution Session overwrite the earlier received schedule parameters.

The Schedule Description instance document is clearly identified using a URI, to enable cross-referencing by the MBS Client of instance documents delivered in band and out of band.

The session schedule and object transmission schedule are described in the Schedule Description instance document respectively by the sessionSchedule and objectSchedule elements.

- The start and stop time of a single sessionSchedule is specified by the start and stop elements.

- The start and stop time of a single objectSchedule is specified by the @start and @endattributes.

In both cases the time is specified as the absolute date and UTC time. The duration may be determined by subtracting the start time from the stop time.

The MBS Distribution Session shall be available to the MBS Client during the time interval(s) announced by the session schedule (i.e. scheduleDescription/serviceSchedule/sessionSchedule element of the Schedule Description instance document), for either unicast or MBS reception. In particular, for unicast reception, the Schedule Description is indicative of the time availability for unicast access of an MBS User Service while the TMGI for the MBS Distribution Session is not activated, as well as for unicast fallback reception when the MBS Client is not located in the MBS coverage area for the service.

The MBS Client may activate reception of that MBS Distribution Session only within the sessionSchedule (and the objectSchedule if present) time window.

When an objectSchedule element is present in a serviceSchedule element, then:

- The MBS Client should not expect that an object described by an objectSchedule will be updated during a time window instance, defined by @start and @end attributes, within a deliveryInfo element of that objectSchedule.

- There shall be only one object version (as defined in the @File-ETag attribute in the FLUTE File Delivery Table) transmitted in a time window defined by the @start and @end attributes within a deliveryInfo element for a given objectSchedule element.

- If objectETag attribute is not present, the objects transmitted in the time windows from different deliveryInfo elements in an objectSchedule should not be expected to be the same object version.

- If the @objectETag attribute is present, there shall be only one object version transmitted in all of the time windows delimited by the start and end attributes of each of the one or more deliveryInfo elements.

- In-band Schedule Description instance document updates can be used to provide a dynamic schedule update to override the existing delivery schedule, such as using the @cancelled attribute mechanism specified in this clause.

- A sessionSchedule element in the same serviceSchedule element shall be present, and its start and stop elements shall specify a time window that completely overlaps the time windows specified in each of the objectSchedule elements of the same serviceSchedule.

When a sessionSchedule is present and there are no objectSchedule child elements in a serviceSchedule, then the MBS Client should download each new object, independently of whether the MBS Distribution Session uses the MBS Object Distribution Method or the MBS Packet Distribution Method.

The objectSchedule element specifies details about the objects to be delivered during an MBS Distribution Session. The @sessionId attribute, if present, identifies the MBS Distribution Session for each object. If not present, an MBS Client shall instead determine the MBS Distribution Session by examining the Session Description metadata unit for the MBS Distribution Session. The @objectETag attribute of the objectSchedule element is the version identifier of the object. If present, the purpose of this entity tag is to enable an MBS Client to determine if an object has changed since a prior reception without having to download the object.

The scheduleUpdate element specifies a time after which MBS Client shall seek to update its schedule information by acquiring the latest available Schedule Description instance document.

An @index attribute is included as a child of the sessionSchedule element. If the sessionSchedule does not describe any session reoccurrence, then the index corresponds to the single session occurrence. If the sessionSchedule describes one or more reoccurrences the @index is the starting index of the first session occurrence with the index value increased by one for each session reoccurrence.

A @cancelled attribute is defined as a child of the objectSchedule/objectURI element.

- If the @cancelled attribute is set to "true" or "1", then the transmission of the object identified by the objectURI element is cancelled, and the MBS Client shall cancel any applicable repair and/or reception reporting procedures for that object.

If this object schedule-level cancellation indication in the updated schedule description is received after the associated object has already been delivered, then any related repair or reception reporting for that object (associated with its parent service), either in progress or yet to occur, shall be aborted.

- If the @cancelled attribute is set to "false" or "0" or is absent, then normal object transmission and associated delivery procedures, if applicable, shall occur.

A sessionScheduleOverride element is defined as a child of the serviceSchedule element. If present, the sessionScheduleOverride element indicates either the cancellation of the session occurrence, or schedule override, as follows:

- If the @cancelled attribute (a child of sessionScheduleOverrideelement) is set to "true" or "1", then the transmission of the MBS Distribution Session identified by the index attribute (a child of sessionScheduleOverrideelement) is cancelled, and the MBS Client shall cancel any applicable repair and/or reception reporting for all objects belonging to that MBS Distribution Session.

If this session schedule-level cancellation indication in the updated schedule description is received after any of the associated objects have already been delivered, then any related repair or reception reporting for those objects (associated with their parent service(s)), either in progress or yet to occur, shall be aborted.

- If the @cancelled attribute (a child of sessionScheduleOverrideelement) is set to "false" or "0" or is absent, then the start and stop time elements (children of sessionScheduleOverrideelement) shall override the nominal start and stop time of the transmission schedule of the session as identified by the @index attribute (a child of sessionScheduleOverrideelement).

The value of the @index attribute in the sessionScheduleOverride element corresponds to any of the value of the index element in the reoccurenceStartStopType in the sessionSchedule element.

Schedule information received in the Schedule Description metadata unit shall take precedence over timing information that may have been received in the Session Description metadata unit (t and/or r lines in the SDP).

### 5.2.8 MBS Object Repair Parameters metadata unit

An Object Repair Parameters document for the object repair procedures may be delivered to MBS Clients:

- Prior to the MBS Distribution Session becoming active, along with the MBS Distribution Session Description metadata unit (out of band of that session); or

- in band within an MBS Distribution Session.

The most recently delivered Object Repair Parameters document shall take priority, such that configuration parameters received prior to – and out-of-band of – the MBS Distribution Session they apply to are regarded as "initial defaults", and configuration parameters received during – and in band with – the MBS Distribution Session, override the earlier received parameters. Thus, a method to update parameters dynamically on a short timescale is provided but, as would be desirable where dynamics are minimal, is not mandatory.

During the User Service Discovery/Announcement Procedure, the Object Repair Parameters document is clearly identified using a URI, to enable UE cross-referencing by the MBS Client of instance documents delivered in band and out of band.

## 5.3 Delivery of Service Announcement

Editor’s Note: Specify delivery envelope for User Service Bundles.

The MBS User Service Announcement provides information needed by the MBS Client to discover and activate the reception of one or more MBS User Services. User Service Announcement information may be delivered via MBS Distribution Sessions or via a regular PDU Session.

# 6 Object Delivery Method

## 6.1 General

The Object Distribution Method supports the transmission of media segments, e.g. CMAF media segments [7] and also non-real-time objects.

The MBS Distribution Session shall be provisioned to accommodate the bit rate of the aggregated object flow, accounting for in-band carriage of metadata units, protocol header overheads, and FEC redundancy (if configured).

## 6.2 Usage of FLUTE for Object Distribution Method

### 6.2.1 General

If FLUTE [12] is used to realise the Object Distribution Method, the MBS Distribution Session shall conform to the MBMS Download Profile as defined in clause L.4 of TS 26.346 [7] with the additional requirements in clause 6.2 of the present document.

The usage of this distribution method is identified in the MBS Session Description metadata unit as defined in clause 6.2.3, in particular by the indication of the protocol FLUTE/UDP in combination with the MBS service type.

The MBSTF shall use the Profiled FDT Schema according to clause L.6 of TS 26.346 [7] to describe the object list currently being transmitted in the MBS Distribution Session.

Generally, the end of transmission of an object is the expiry time for the latest FDT instance describing the object. Objects shall be described in an FDT Instance with the Expires attribute. Depending on the operating mode (clause 6.2.4), different settings of the expiry time and different numbers of objects per FDT Instance are recommended.

Inclusion of the @Content-MD5 and @File-ETag FDT Instance attributes is optional.

- The @File-ETag represents the value of the HTTP entity tag as defined in section 3.11 of RFC 2616 [13] which may also serve as the version identifier of the File object described by the FDT Instance.

In order to fetch missing portions of an object, the MBS Client may use the Object Repair services. The Object Repair service is realized as a Byte-Range based File Repair, as specified in clause 9.3.6.2 of TS 26.346 [7].

NOTE: The use of Alternate-Content-Location-1 and Alternate-Content-Location-2 is not supported.

### 6.2.2 Session Description metadata unit

#### 6.2.2.1 General

The Session Description metadata unit contains the needed information to activate the reception of an Object Distribution Method. The Session Description metadata unit is formatted according to the Session Description Protocol [8]. The Session Description metadata unit for the Object Distribution Method is based on the Session Description parameters as defined in clause 7.3 of TS 26.346 [7] with the following restrictions and extensions.

Restrictions:

- The *Mode of MBMS bearer per media* parameter (clause 7.3.2.7 of [7]) shall not be used.

- The *QoE Metrics* (as defined in clauses 7.3.2.0 of [7]) shall not be used

- The *Service-language(s) per media* (clause 7.3.2.9 of [7]) shall not be used. It is assumed that the service languages are described within an application manifest.

- The *Alternative TMGI* (clause 7.3.2.12 of [7]) shall not be used.

- The *Start time* and *End time* of the session (SDP t-line) shall indicate a superset of the active times specified in the MBS Schedule Description metadata unit, if present. If there is no schedule specified, both values should be set to zero indicating undefined times.

Extensions:

- When an MBS Session is of MBS Service Type *Broadcast* or when the Multicast MBS Session Type uses a TMGI as MBS Session ID, the *MBS service type of MBS Session* declaration attribute as defined in clause 6.2.2.2 shall be present in the Session Description.

#### 6.2.2.2 MBS service type of MBS Session

A new MBS service type declaration attribute is defined which results in, e.g.:

- a=mbs-servicetype:broadcast 123869108302929

or:

- a=mbs-servicetype:multicast 123869108302929

The MBS service type declaration attribute shall be used in Session Description metadatato indicate the type of the corresponding MBS Distribution Session as defined in table 6.2.2.2‑1.

Table 6.2.2.2‑1: Assignment of mbs-servicetype attribute value

|  |  |
| --- | --- |
| Attribute value | Meaning |
| multicast | The MBS Distribution Session is delivered using a Multicast MBS Session. |
| broadcast | The MBS Distribution Session is delivered using a Broadcast MBS Session. |

The MBS service type attribute shall be declared at session level in the Session Description metadata unit. The session level attribute applies to all media entries without a media-level occurrence of the mbs-servicetype attribute. The Session Description metadata unit shall include only a single instance of MBS service type declaration attribute.

Definition:

- mbs-service-type-declaration-line = "a=mbs-servicetype:" ("broadcast"/"multicast" SP tmgi) CRLF

- tmgi = 1\*15DIGIT

EXAMPLE:

UK MCC = 234 *(MCC Digit 1 = 2; MCC Digit 2 = 3 and MCC Digit 3 = 4)*

Vodafone UK MNC = 15

and, with padding, Vodafone UK MNC = 15F *(MNC Digit 1 = 1; MNC Digit 2 = 5 and MNC Digit 3 = F)*

MBS Service ID = 70A886

Therefore, TMGI = 70A886 32F451 (Hex) or 123869108302929 (Decimal)

The Temporary Mobile Group Identity (tmgi) information element is defined in TS 24.008 [11] including the coding of the fields. Octets 3 to 8 (MBS Service ID, MCC and MNC) shall be placed in the tmgi attribute of the MBS service type declaration line, and are encoded as a decimal number. Octet 3 is the most significant octet. Because this is encoded as a decimal number, leading zeros of the MBS Service ID field may be omitted.

#### 6.2.2.3 SDP examples for FLUTE Session

Listing 6.2.2.3‑1 provides a full example of an SDP description describing a FLUTE-based MBS Distribution Session using the Object Distribution Method with a TMGI as MBS Session Id:

Listing 6.2.2.3‑1: Session Description metadata unit for
FLUTE-based MBS Distribution Session with TMGI

|  |
| --- |
| v=0o=user123 2890844526 2890842807 IN IP6 2201:056D::112E:144A:1E24s=Object Distribution session examplei=More informationt=2873397496 2873404696a=mbs-servicetype:broadcast 123869108302929a=FEC-declaration:0 encoding-id=1a=source-filter: incl IN IP6 \* 2001:210:1:2:240:96FF:FE25:8EC9a=flute-tsi:3m=application 12345 FLUTE/UDP 0c=IN IP6 FF1E:03AD::7F2E:172A:1E24/1b=1000a=lang:ENa=FEC:0 |

Listing 6.2.2.3‑2 provides a second example of an SDP description describing a FLUTE-based MBS Distribution Session using the Object Distribution Method and which indicates that 25% redundant FEC protection is applied to the FEC encoding of the video Segments of the associated DASH-formatted content:

Listing 6.2.2.3‑2: Session Description metadata unit for
FLUTE-based MBS Distribution Session with TMGI and 25% FEC redundancy

|  |
| --- |
| v=0o=user123 2890844526 2890842807 IN IP6 2201:056D::112E:144A:1E24s=Object Distribution session carrying 2-hour DASH-packaged programmei=More informationt=3615124600 3615131800a=mbs-servicetype:broadcast 123869108302929a=FEC-declaration:0 encoding-id=1a=FEC-redundancy-level:0 redundancy-level=25a=source-filter: incl IN IP6 \* 2001:210:1:2:240:96FF:FE25:8EC9a=flute-tsi:5m=video 10111 FLUTE/UDP 0c=IN IP6 FF1E:03AD::7F2E:172A:1E24/1b=2048a=lang:EN |

|  |
| --- |
|  |

### 6.2.3 Operating modes for Object Distribution Method

#### 6.2.3.1 Introduction

The operating modes for the Object Distribution Method are defined in clause 6.1 of TS 26.502 [6]. Operating modes primarily describe the operation of the MBSTF to convert ingest data into an MBS Distribution Session. The following clauses specify how FLUTE is used for each operating mode.

#### 6.2.3.2 Single object operating mode

Single object operating mode (OBJECT\_SINGLE) refers to the case in which a single object is distributed via the Object Distribution Method.

No specific aspects beyond the general provisions in clauses 6.1, 6.2.1 and 6.2.2 apply to this operating mode.

#### 6.2.3.3 Object collection operating mode

Object collection operating mode (OBJECT\_COLLECTION) refers to the case in which multiple objects are distributed via the Object Distribution Method.

In this operating mode, the FDT Instance should describe all objects that are part of the collection.

#### 6.2.3.4 Object carousel operating mode

Object carousel operating mode (OBJECT\_CAROUSEL) refers to the case in which one or multiple objects are distributed via the Object Distribution Method in a repeated fashion.

The list of objects described in the manifest may be updated over time.

In this operating mode, the FDT Instance should describe all objects that are currently available in the FLUTE Session, considering the potential object update interval.

#### 6.2.3.5 Segment streaming operating mode

Segment streaming operating mode (OBJECT\_STREAMING) refers to the case for which a sequence of objects, typically representing timed segments from a timed presentation, are distributed using the Object Distribution Method. The sequence of objects is referred to as an *object flow*. This operating mode is recommended for streaming DASH or HLS content to a Media Player in the UE using MBS User Services.

NOTE: This operating mode may also be used for non-media object flows, e.g. in the absence of an Application Service Description.

For each object associated with the object flow to be delivered in the MBS distribution session the following information shall be maintained by the MBSTF in an object list:

- The URL used by the MBS-Aware Application to request the object, derived from the object ingest URL.

- The object’s *latest availability start time* at the MBS Client. After this time, the MBS-Aware Application may request the full object from the MBSTF Client by using the URL of the object.

This valueis determined for each object based on an availability start time at the point of ingest (i.e. reception of first byte of the object) combined with a configured distribution offset.

- The object’s *availability end time* from the MBSTF Client. After this time, the object may no longer be requested by the MBS-Aware Application.

This valueis determined for each object based on an availability start time at the point of ingest (i.e. reception of first byte of the object) combined with a configured clean-up time.

The object list is typically extended over time, for example as new objects (e.g. media segments) become available.

The object list may, for example, be provided by an explicit object distribution manifest.

NOTE: An object distribution manifest format is not defined in the present document.

The object list may also be defined by a presentation manifest (e.g. DASH MPD), for example in the case of an Application Service, for which the manifest is provided as part of the User Service Description.

When the Application Service Entry Point document is a DASH MPD, this document is used by the MBSTF to update the object list. The DASH MPD may itself be included in the object list, and hence be delivered in band with the media segment objects it describes on the same MBS Distribution Session. If the content of the Application Service Entry Point document changes during an MBS User Data Ingest Session the updated document shall be reflected in the MBS Distribution Session at the soonest opportunity.

For the segment streaming operating mode, the MBSTF acts as follows based on the object list:

* The MBSTF shall transmit each object in the object list such that the last packet of the delivered FLUTE transmission object (including any FEC recovery packets, when configured) is available at the MBSTF Client latest at its latest availability start time.
* An FDT Instance object should be sent frequently by the MBSTF, describing all objects of the object list that are not yet fully transmitted.
* The Content-Location element in the FDT Instance shall match the URL of the corresponding object in the object list. The URL may be rewritten by the MBSTF using the Object distribution base URL property of the MBS Distribution Session.
* The File@Expires attribute for each object shall be set such that it is equal to or earlier than its *latest availability start time*.
* The Cache-Control@Expires attribute shall be used to indicate the *availability end time of the object.*
* Content-MD5 and File-ETag may optionally be used.

# 7 Packet Delivery Method

## 7.1 General

The Packet Distribution Method reuses different delivery concepts from TS 26.346. Additional distribution methods may be defined in future.

## 7.2 Re-using MBMS Delivery Method as Packet Distribution Method

### 7.2.1 General

The Packet Distribution Method combines three different delivery methods of TS 26.346 [7] (namely the MBMS Streaming Delivery Method, Group Communication Delivery Method and Transparent Delivery Method) into a single distribution method, with a set of modifications.

For the Packet Distribution Method, the MBSTF may handle the ingested content on three different protocol layers according to the operating mode provisioned for the MBS Distribution Session:

- *Proxy mode:* The MBSTF handles UDP packet payloads and forwards UDP packet payloads from ingest into the MBS Distribution Session. The MBSTF may use different UDP ports for the MBS Distribution Session. The MBSTF re-uses the Proxy Mode of the Transparent Delivery Method as defined in clause 8B of [7].

- *Forward-only mode:* The MBS receives complete IP packets and forwards the ingested packets as MBS PDUs. The MBSTF re-uses the Group Communication Delivery Method as defined in clause 8A of [7] and the Forward-Only Mode of the Transparent Delivery Method as defined in clause 8B of [7].

### 7.2.3 Session Description

#### 7.2.3.1 General

The Session Description metadata unit contains the needed information to activate the reception of a Packet Distribution Method. The Session Description metadata unit is formatted according to the Session Description Protocol [8]. The Session Description metadata unit for the Packet Distribution Method is based on the Session Description parameters as defined in clauses 8.3, 8A.3 and 8B.3 of TS 26.346 [7] with the following restrictions and extensions.

Restrictions:

- The *Mode of MBMS bearer per media* parameter (clauses 8.3.1.5 and 8B.3.2 of [7]) shall not be used.

- The *QoE Metrics* (as defined in clauses 8.3.2.1 and 8.4 of [7]) shall not be used.

- ROHC header compression (as defined in clauses 8A.4 and 8B.4 of [7]) shall not be used.

NOTE: ROHC is handled by RAN in 5MBS.

- The *Alternative TMGI* (clause 7.3.2.12 of [7]) shall not be used.

- The *Start time* and *End time* of the session (SDP t line) shall indicate a superset of the active times specified in the MBS Schedule Description metadata unit, if present. If there is no schedule specified, both values should be set to zero indicating undefined times.

Extensions:

- When the MBS User Service is of MBS Service Type *Broadcast* or when an MBS User Service of type *Multicast* uses a TMGI as its MBS Session ID, the *MBS service type of MBS Session* declaration attribute as defined in clause 6.2.3.2 shall be present in the Session Description.

#### 7.2.3.2 SDP examples for Packet Distribution Method

Below is a full example of SDP description describing the media streams part of an MBS Packet Distribution session for RTP streaming:

Listing 7.2.3.2‑1: Session description for RTP streaming

|  |
| --- |
| v=0o=ghost 2890844526 2890842807 IN IP4 192.168.10.10s=3GPP MBS Packet Distribution SDP Examplei=Example of MBS Packet Distribution SDP fileu=http://www.infoserver.example.com/ae600e=ghost@mailserver.example.com*c=IN IP6 FF1E:03AD::7F2E:172A:1E24*t=0 0b=AS:77a=mbs-mode:broadcast 123869108302929a=source-filter: incl IN IP6 \* 2001:210:1:2:240:96FF:FE25:8EC9m=video 4002 RTP/AVP 96b=TIAS:62000b=RR:0b=RS:600a=maxprate:17a=rtpmap:96 H264/90000a=fmtp:96 profile-level-id=42A01E; packetization-mode=1; sprop-parameter-sets=Z0IACpZTBYmI,aMljiA== |

The following is a full example of SDP description for transparent streaming with two MPEG-2 Transport Streams:

Listing 7.2.3.2‑2: Session description for MPEG‑2 Transport Stream

|  |
| --- |
| v=0o=ghost 2890844526 2890842807 IN IP4 192.168.10.10s=3GPP MBS Transport-only SDP Examplei=Example of MBS transport-only SDP fileu=http://www.infoserver.example.com/ae600e=ghost@mailserver.example.com*c=IN IP6 FF1E:03AD::7F2E:172A:1E24*t=3034423619 3042462419b=AS:8000000a=mbs-mode:broadcast 123869108302929a=source-filter: incl IN IP6 \* 2001:210:1:2:240:96FF:FE25:8EC9m=video 4002 UDP/RTP/AVP 96b=TIAS:4000000a=mms-framing-header:0 2 a=rtpmap:100 MP2T/90000m=video 4002 RTP/AVP 98b=TIAS:4000000a=rtpmap:100 MP2T/90000a=MBS-framing-trailer:0 2 |

Annex A (normative)
Syntax for Service Announcement

# A.1 XML-based representation

### A.1.1 MBS User Service Description schema

|  |
| --- |
| <?xml version="1.0" encoding="UTF-8"?><xs:schema xmlns="urn:3GPP:metadata:2022:MBS:userServiceDescription" xmlns:xs="http://www.w3.org/2001/XMLSchema" targetNamespace="urn:3GPP:metadata:2022:MBS:userServiceDescription" elementFormDefault="qualified"> <xs:element name="bundleDescription" type="bundleDescriptionType"/> <xs:complexType name="bundleDescriptionType"> <xs:sequence> <xs:element name="userServiceDescription" type="userServiceDescriptionType" maxOccurs="unbounded"/> <xs:any namespace="##other" minOccurs="0" maxOccurs="unbounded" processContents="lax"/> </xs:sequence> <xs:anyAttribute processContents="skip"/> </xs:complexType> <xs:complexType name="userServiceDescriptionType"> <xs:sequence> <xs:element name="name" type="nameType" minOccurs="0" maxOccurs="unbounded"/> <xs:element name="serviceLanguage" type="xs:language" minOccurs="0" maxOccurs="unbounded"/> <xs:element name="distributionSessionDescription" type="distributionSessionDescriptionType" maxOccurs="unbounded"/> <xs:element ref="appService" minOccurs="0" maxOccurs="unbounded"/> <xs:element ref="availabilityInfo" minOccurs="0"/> <xs:any namespace="##other" minOccurs="0" maxOccurs="unbounded" processContents="lax"/> </xs:sequence> <xs:attribute name="serviceId" type="xs:anyURI" use="required"/> <xs:anyAttribute processContents="skip"/> </xs:complexType> <xs:complexType name="distributionSessionDescriptionType"> <xs:sequence> <xs:element ref="mbsAppService" minOccurs="0" maxOccurs="unbounded"/> <xs:element ref="unicastAppService" minOccurs="0"/> <xs:any namespace="##other" minOccurs="0" maxOccurs="unbounded" processContents="lax"/> </xs:sequence>  <xs:attribute name="associatedProcedureDescriptionURI" type="xs:anyURI" use="optional"/> <xs:attribute name="sessionDescriptionURI" type="xs:anyURI" use="required"/> <xs:attribute name="dataNetworkName" type="xs:anyURI" use="optional" /> <xs:anyAttribute processContents="skip"/> </xs:complexType> <xs:complexType name="nameType"> <xs:simpleContent> <xs:extension base="xs:string"> <xs:attribute name="lang" type="xs:language" use="optional"/> </xs:extension> </xs:simpleContent> </xs:complexType> <xs:element name="appService" type="appServiceType"/> <xs:complexType name="appServiceType"> <xs:sequence> <xs:element name="identicalContent" minOccurs="0" maxOccurs="unbounded"> <xs:complexType> <xs:sequence> <xs:element name="basePattern" type="xs:anyURI" minOccurs="2" maxOccurs="unbounded"/> <xs:any namespace="##other" processContents="lax" minOccurs="0" maxOccurs="unbounded"/> </xs:sequence> <xs:anyAttribute processContents="skip"/> </xs:complexType> </xs:element> <xs:element name="alternativeContent" minOccurs="0" maxOccurs="unbounded"> <xs:complexType> <xs:sequence> <xs:element name="basePattern" type="xs:anyURI" minOccurs="2" maxOccurs="unbounded"/> <xs:any namespace="##other" processContents="lax" minOccurs="0" maxOccurs="unbounded"/> </xs:sequence> <xs:anyAttribute processContents="skip"/> </xs:complexType> </xs:element> <xs:any namespace="##other" processContents="lax" minOccurs="0" maxOccurs="unbounded"/> </xs:sequence> <xs:attribute name="mediaManifestDescriptionURI" type="xs:anyURI" use="required"/> <xs:attribute name="mimeType" type="xs:string" use="required"/> <xs:anyAttribute processContents="skip"/> </xs:complexType> <xs:element name="mbsAppService"> <xs:complexType> <xs:sequence> <xs:element name="basePattern" type="xs:anyURI" maxOccurs="unbounded"/> <xs:element name="serviceArea" type="xs:unsignedShort" minOccurs="0" maxOccurs="unbounded"/> <xs:any namespace="##other" processContents="lax" minOccurs="0" maxOccurs="unbounded"/> </xs:sequence> <xs:anyAttribute processContents="skip"/> </xs:complexType> </xs:element> <xs:element name="unicastAppService"> <xs:complexType> <xs:sequence> <xs:element name="basePattern" type="xs:anyURI" maxOccurs="unbounded"/> <xs:any namespace="##other" processContents="lax" minOccurs="0" maxOccurs="unbounded"/> </xs:sequence> <xs:anyAttribute processContents="skip"/> </xs:complexType> </xs:element> <xs:element name="availabilityInfo"> <xs:complexType> <xs:sequence> <xs:element name="infoBinding" maxOccurs="unbounded"> <xs:complexType> <xs:sequence> <xs:element ref="mbsServiceArea" minOccurs="0" maxOccurs="unbounded"/> <xs:element name="radioFrequency" type="xs:unsignedInt" maxOccurs="unbounded"/> </xs:sequence> </xs:complexType> </xs:element> </xs:sequence> </xs:complexType> <xs:element name="mbsServiceArea"> <xs:complexType> <xs:sequence> <xs:element name="taiList" minOccurs="0" maxOccurs="unbounded"> <xs:complexType> <xs:sequence> <xs:element ref="tai" maxOccurs="unbounded"/> </xs:sequence> </xs:complexType> </xs:element> <xs:element name="ncgiList" minOccurs="0" maxOccurs="unbounded"> <xs:complexType> <xs:sequence> <xs:element ref="ncgiTai" maxOccurs="unbounded"> </xs:sequence> </xs:complexType> </xs:element> </xs:sequence> </xs:complexType> <xs:element name="tai"> <xs:complexType> <xs:sequence> <xs:element name="plmnId"> <xs:complexType> <xs:sequence> <xs:element name="mcc" type="xs:string"/> <xs:element name="mnc" type="xs:string"/> </xs:sequence> </xs:complexType> </xs:element> <xs:element name="tac" type="xs:string"/> <xs:element name="nid" type="xs:string" minOccurs="0"/> </xs:sequence> </xs:complexType> <xs:element name="ncgiTai"> <xs:complexType> <xs:sequence> <xs:element ref="tai"/> <xs:element ref="ncgi"/> </xs:sequence> </xs:complexType> <xs:element name="ncgi"> <xs:complexType> <xs:sequence> <xs:element name="plmnId"> <xs:complexType> <xs:sequence> <xs:element name="mcc" type="xs:string"/> <xs:element name="mnc" type="xs:string"/> </xs:sequence> </xs:complexType> </xs:element> <xs:element name="nrCellId" type="xs:string"/> <xs:element name="nid" type="xs:string" minOccurs="0"/> </xs:sequence> </xs:complexType></xs:schema> |

### A.1.2 Object Repair Parameters schema

Below is the formal XML syntax of associated distribution procedure description instances. Documents following this schema can be identified with the MIME type "application/mbs‑object-repair-parameters+xml". The schema filename of distribution procedure description is objectrepairparameters.xsd.

|  |
| --- |
| <?xml version="1.0" encoding="UTF-8"?><xs:schema  xmlns="urn:3gpp:metadata:2020:MBS:associatedProcedure" xmlns:xs="http://www.w3.org/2001/XMLSchema"  targetNamespace="urn:3gpp:metadata:2022:MBS:associatedProcedure" elementFormDefault="qualified" version="1"> <xs:element name="associatedProcedureDescription" type="associatedProcedureType"/> <xs:complexType name="associatedProcedureType"> <xs:sequence> <xs:element name="postFileRepair" type="basicProcedureType" minOccurs="0"/> <xs:element name="mbsFileRepair" type="mbsFileRepairType" minOccurs="0"/> <xs:any namespace="##other" processContents="skip" minOccurs="0" maxOccurs="unbounded"/> </xs:sequence> </xs:complexType> <xs:complexType name="basicProcedureType"> <xs:sequence> <xs:element name="serviceURI" type="xs:anyURI" maxOccurs="unbounded"/> </xs:sequence> <xs:attribute name="offsetTime" type="xs:unsignedLong" use="optional"/> <xs:attribute name="randomTimePeriod" type="xs:unsignedLong" use="required"/> </xs:complexType> <xs:complexType name="mbsFileRepairType"> <xs:attribute name="sessionDescriptionURI" type="xs:anyURI" use="required"/> </xs:complexType></xs:schema> |

## A.1.3 Schedule Description schema

Below is the formal XML syntax of schedule information procedure. Documents following this schema can be identified with the MIME type "application/mbms‑schedule+xml". The file name of XML schema for schedule description is Schedule-Description.xsd.

|  |
| --- |
| <?xml version="1.0" encoding="UTF-8"?><xs:schema xmlns="urn:3gpp:metadata:2022:MBS:scheduleDescription" xmlns:xs="http://www.w3.org/2001/XMLSchema" targetNamespace="urn:3gpp:metadata:2022:MBS:scheduleDescription" elementFormDefault="qualified" version="1"> <xs:complexType name="scheduleDescriptionType"> <xs:sequence><xs:element name="serviceSchedule" maxOccurs="unbounded"> <xs:complexType> <xs:sequence> <xs:element name="sessionSchedule" type="reoccurenceStartStopType" minOccurs="0" maxOccurs="unbounded"/> <xs:element name="sessionScheduleOverride" minOccurs="0" maxOccurs="unbounded"> <xs:complexType> <xs:sequence minOccurs="0"> <xs:element name="start" type="xs:dateTime"/> <xs:element name="stop" type="xs:dateTime"/> </xs:sequence> <xs:attribute name="index" type="xs:unsignedInt" use="required"/> <xs:attribute name="cancelled" type="xs:boolean"/> </xs:complexType> </xs:element> <xs:element name="objectSchedule" minOccurs="0" maxOccurs="unbounded"> <xs:complexType> <xs:sequence> <xs:element name="objectURI"> <xs:complexType> <xs:simpleContent> <xs:extension base="xs:anyURI"> <xs:attribute name="cancelled" type="xs:boolean"/> </xs:extension> </xs:simpleContent> </xs:complexType> </xs:element> <xs:element name="deliveryInfo" minOccurs="0" maxOccurs="unbounded"> <xs:complexType> <xs:attribute name="start" type="xs:dateTime"/> <xs:attribute name="end" type="xs:dateTime"/> <xs:anyAttribute processContents="skip"/> </xs:complexType> </xs:element> <xs:any namespace="##other" processContents="lax" minOccurs="0" maxOccurs="unbounded"/> </xs:sequence> <xs:attribute name="sessionId" type="xs:string" use="optional"/> <xs:attribute name="objectEtag" type="xs:string" use="optional"/> <xs:attribute name="unicastOnly" type="xs:boolean" use="optional" default="false"/> <xs:anyAttribute processContents="skip"/> </xs:complexType> </xs:element> <xs:any namespace="##other" processContents="lax" minOccurs="0" maxOccurs="unbounded"/> </xs:sequence> <xs:attribute name="serviceId" type="xs:anyURI"/> <xs:attribute name="serviceClass" type="xs:string" use="optional"/> <xs:anyAttribute processContents="skip"/> </xs:complexType> </xs:element> <xs:any namespace="##other" processContents="lax" minOccurs="0" maxOccurs="unbounded"/> </xs:sequence> <xs:attribute name="scheduleUpdate" type="xs:dateTime"/> <xs:anyAttribute processContents="skip"/> </xs:complexType> <xs:complexType name="reoccurenceStartStopType"> <xs:sequence> <xs:element name="start" type="xs:dateTime"/> <xs:element name="stop" type="xs:dateTime"/> <xs:element name="reoccurencePattern" type="xs:string" minOccurs="0"/> <xs:element name="numberOfTimes" type="xs:unsignedInt" minOccurs="0"/> <xs:element name="reoccurenceStopTime" type="xs:dateTime" minOccurs="0"/> <xs:element name="index" type="xs:unsignedInt" minOccurs="0"/> <xs:element name="FDTInstanceURI" type="xs:anyURI" minOccurs="0"/> <xs:any namespace="##other" processContents="lax" minOccurs="0" maxOccurs="unbounded"/> </xs:sequence> <xs:attribute name="sessionDescriptionURI" type="xs:anyURI" use="optional"/> <xs:anyAttribute processContents="skip"/> </xs:complexType> <xs:element name="scheduleDescription" type="scheduleDescriptionType"/></xs:schema> |

## A.2 JSON-based representation

### A.2.1 MBS User Service Bundle Description schema

|  |
| --- |
| openapi: 3.0.0info: title: 'MBS User Service Announcement Element units’ definition' version: 1.0.0 description: | MBS User Service Announcement Element units. © 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC). All rights reserved.externalDocs: description: 3GPP TS 26.517 V0.1.0; 5G System; 5G MBSF; Stage 3. url: http://www.3gpp.org/ftp/Specs/archive/26\_series/26.517/paths: {}components: schemas:  bundleDescription: type: array items: $ref: '#/components/schemas/userServiceDescription' minItems: 1  userServiceDescription: type: object properties: name: type: array items:  type: string serviceLanguage: type: array items:  type: string serviceId:  type: string distributionSessionDescription: $ref: '#/components/schemas/distributionMethod' appService: $ref: '#/components/schemas/mbsAppService' availabilityInfo: $ref: '#/components/schemas/availabilityInfo' required: - distributionMethod - serviceId distributionSessionDescription: type: object  properties: sessionDescriptionURI: type: string associatedProcedureDescriptionURI: type: string dataNetworkName: type: string mbsAppService: type: array items: $ref: '#/components/schemas/appService' unicastAppServices: type: array items: unicastAppService: type: object properties: $ref: '#/components/schemas/appService' required: - sessionDescriptionURI mbsAppService:  type: object properties:  MediaManifestDescriptionURI: type: string mimeType: type: string identicalContents: type: array items: identicalContent: type: array items: $ref: '#/components/schemas/appService' alternativeContents: type: array items:  alternativeContent: type: array items: $ref: '#/components/schemas/appService'  appService: type: object properties: basePattern: type: string required: - basePattern  MbsServiceArea: description: MBS Service Area type: object properties: ncgiList: type: array items: $ref: '#/components/schemas/NcgiTai' minItems: 1 description: List of NR cell Ids  taiList: type: array items: $ref: '#/components/schemas/Tai' minItems: 1 description: List of tracking area Ids NcgiTai: description: List of NR cell ids, with their pertaining TAIs type: object properties: tai: $ref: '#/components/schemas/Tai' cellList: type: array items: $ref: '#/components/schemas/Ncgi' minItems: 1 description: List of List of NR cell ids required: - tai - cellList Tai: description: Contains the tracking area identity as described in 3GPP 23.003 type: object properties: plmnId: $ref: '#/components/schemas/PlmnId' tac: $ref: '#/components/schemas/Tac' nid: $ref: '#/components/schemas/Nid' required: - plmnId - tac Ncgi: description: Contains the NCGI (NR Cell Global Identity), as described in 3GPP 23.003 type: object properties: plmnId: $ref: '#/components/schemas/PlmnId' nrCellId: $ref: '#/components/schemas/NrCellId' nid: $ref: '#/components/schemas/Nid' required: - plmnId - nrCellId PlmnId: type: object properties: mcc: $ref: '#/components/schemas/Mcc' mnc: $ref: '#/components/schemas/Mnc' description: When PlmnId needs to be converted to string (e.g. when used in maps as key), the string shall be composed of three digits "mcc" followed by "-" and two or three digits "mnc". required: - mcc - mnc Mcc: type: string pattern: '^\d{3}$' description: Mobile Country Code part of the PLMN, comprising 3 digits, as defined in clause 9.3.3.5 of 3GPP TS 38.413. Mnc: type: string pattern: '^\d{2,3}$' description: Mobile Network Code part of the PLMN, comprising 2 or 3 digits, as defined in clause 9.3.3.5 of 3GPP TS 38.413. Tac: type: string pattern: '(^[A-Fa-f0-9]{4}$)|(^[A-Fa-f0-9]{6}$)' description: 2 or 3-octet string identifying a tracking area code as specified in clause 9.3.3.10 of 3GPP TS 38.413, in hexadecimal representation. Each character in the string shall take a value of "0" to "9", "a" to "f" or "A" to "F" and shall represent 4 bits. The most significant character representing the 4 most significant bits of the TAC shall appear first in the string, and the character representing the 4 least significant bit of the TAC shall appear last in the string. Nid: type: string pattern: '^[A-Fa-f0-9]{11}$' description: This represents the Network Identifier, which together with a PLMN ID is used to identify an SNPN (see 3GPP TS 23.003 and 3GPP TS 23.501 clause 5.30.2.1). NrCellId: type: string pattern: '^[A-Fa-f0-9]{9}$' description: 36-bit string identifying an NR Cell Id as specified in clause 9.3.1.7 of 3GPP TS 38.413, in hexadecimal representation. Each character in the string shall take a value of "0" to "9", "a" to "f" or "A" to "F" and shall represent 4 bits. The most significant character representing the 4 most significant bits of the Cell Id shall appear first in the string, and the character representing the 4 least significant bit of the Cell Id shall appear last in the string. availabilityInfo: type: array properties: $ref: '#/components/schemas/infoBinding' infoBinding: type: object properties: mbsServiceArea: type: array items: $ref: '#/components/schemas/MbsServiceArea' radioFrequency: type: array items: type: integer minimum: 0  associatedProcedureDescription: type: object properties: postFileRepair:  $ref: '#/components/schemas/postFileRepair' mbsFileRepair: $ref: '#/components/schemas/mbsFileRepair' postFileRepair: type: object items: serviceURI: type: array items: type: string offsetTime: type: integer randomTimePeriod: type: integer mbsFileRepair: type: object properties: "sessionDescriptionURI": type: string  scheduleDescription: type: array items: $ref: '#/components/schemas/serviceSchedule'  serviceSchedule: type: object properties: sessionSchedule:  $ref: '#/components/schemas/sessionSchedule' sessionScheduleOverride:  $ref: '#/components/schemas/sessionScheduleOverride' fileSchedule: $ref: '#/components/schemas/fileSchedule' serviceId:  type: string serviceClass: type: string required: - serviceId - serviceClass - serviceSchedule sessionSchedule: type: array items: type: object properties: start: type: string stop: type: string reoccurencePattern: type: string numberOfTimes: type: integer reoccurenceStopTime: type: string index: type: integer FDTInstanceURI: type: string required: - start - stop sessionScheduleOverride: type: array items:  type: object properties: start: type: string stop: type: string index: type: integer cancelled: type: boolean sessionDescriptionURI: type: string  fileSchedule: type: array items: type:object properties:  fileURI:  type: string sessionId: type: string fileEtag: type: string unicastOnly: type: boolean deliveryInfo: type: array items: type: object properties: start: type: string stop: type: string |

Annex B (informative)
Service Announcement examples

# B.1 XML-based representation

# B.2 JSON-based representation

|  |
| --- |
| { "bundleDescription":[ { "userServiceDescription":{ "name":[ "test1" ], "serviceLanguage":[ "en-us" ], "serviceId":"urn:test:test:D4-Service:D4-SB:D4-US", "distributionSessionDescription":{ "sessionDescriptionURI":"http://www.test.com/D4-Service/D4-SB/D4-US.sdp", "dataNetworkName":"media-dnn", "mbsAppService":[ {"basePattern":"http://www.test.com/D4-Service/D4-SB/D4-US/video/2048/"}, {"basePattern":"http://www.test.com/D4-Service/D4-SB/D4-US/audio/1/"} ], "unicastAppServices":[ {"unicastAppService":[ {"basePattern":"http://www.test.com/D4-Service/D4-SB/D4-US/video/1024/"}, {"basePattern":"http://www.test.com/D4-Service/D4-SB/D4-US/audio/1/"}] }, {"unicastAppService":[ {"basePattern":"http://www.test.com/D4-Service/D4-SB/D4-US/video/2048/"}, {"basePattern":"http://www.test.com/D4-Service/D4-SB/D4-US/audio/1/"}] }  ]  }, "appService":{ "MediaManifestDescriptionURI":"http://www.test.com/D4-Service/D4-SB/D4-US/adpd.xml", "mimeType":"application/dash+xml;profiles=urn:3GPP:PSS:profile:DASH10", "identicalContents":[ { "identicalContent":[ {"basePattern":"http://www.test.com/D4-Service/D4-SB/D4-US/video/1024/"}, {"basePattern":"http://www.test.com/D4-Service/D4-SB/D4-US/video/2048/"} ], },{ "identicalContent":[ {"basePattern":"http://www.test.com/D4-Service/D4-SB/D4-US/audio/1/"} ]  }] }, "availabilityInfo":[ { "infoBinding":{ "mbsServiceArea":[ { "ncgiList":[ { "NcgiTai":{ "tai":{ "plmnId":{ "mcc":"860", "mnc":"15" }, "tac":"0fa0" }, "cellList":[ { "Ncgi":{ "plmnId":{ "mcc":"860", "mnc":"15" }, "nrCellId":"999999999" } }, { "Ncgi":{ "plmnId":{ "mcc":"860", "mnc":"15" }, "nrCellId":"999999998" } } ] } } ], "taiList":[ { "tai":{ "plmnId":{ "mcc":"860", "mnc":"15" }, "tac":"0fa0" } }, { "tai":{ "plmnId":{ "mcc":"860", "mnc":"15" }, "tac":"0fa0" } } ] } ], "radioFrequency":[ "9410" ] } } ] } } ]} |

Annex C (normative)
Controlled vocabulary of conformance profiles

The controlled vocabulary is for future study.

Annex <X> (informative):
Change history

|  |
| --- |
| **Change history** |
| **Date** | **Meeting** | **TDoc** | **CR** | **Rev** | **Cat** | **Subject/Comment** | **New version** |
| 2022-02 | SA4#117-e | S4-200141 |  |  |  | Initial skeleton document. | 0.0.1 |
| S4-220285 |  |  |  | Revised skeleton document | 0.1.0 |
| 2022-03 | SA4#117-e | SP-220249 |  |  |  | Presentation for information at SA#95-e  | 1.0.0 |
| 2022-04 | SA4#118-e | S4-220521 |  |  |  | S4-220570: Service Announcement specification and schemas.S4-220470: Packet Distribution Method initial specification.S4-220471: Object Distribution Method initial specification | 1.1.0 |
| 2022-05 | SA4#119-e | S4-220867 |  |  |  | S4-220864: Service Announcement corrections.S4-220865: Object Distribution Method updates.S4-220866: Packet Distribution Method updates. | 1.2.0 |