**3GPP TSG-SA5 Meeting #129-e *S5-201259***

**Online, , 24th Feb 2020 - 4th Mar 2020**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.0* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **28.541** | **CR** | **0245** | **rev** | **-** | **Current version:** | **16.3.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **x** | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** |  | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Huawei | | | | | | | | | |
| ***Source to TSG:*** | S5 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | eNRM | | | | |  | ***Date:*** | | | 2020-02-14 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | | Rel-16 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) Rel-12 (Release 12)* *Rel-13 (Release 13) Rel-14 (Release 14) Rel-15 (Release 15) Rel-16 (Release 16)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | According to the received LS S5-201166 R3-197540, OAM needs to provide the relationship between set ID and backhaul addresses (gNB ID+TAI) to the gNB CU-CP.  According to R1-1903833, set ID value is defined as rim-RS-SetId-of-RS1 for RIM-RS type1 and rim-RS-SetId-of-RS2 for RIM-RS type2. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Add mapping relationship between set ID and backhaul address of gNBs (gNB ID+TAI) to the GBNCUCPFunction. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | The function of Remote Interference Management(RIM) can not be applicable for all NG-RAN deployment scenarios. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 4.3.2.2, 4.3.X (new), 4.4.1,D.4.3 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **x** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **x** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **x** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

|  |
| --- |
| **First of Changes** |

### 4.3.1 GNBDUFunction

#### 4.3.1.1 Definition

For non-split NG-RAN deployment scenario, this IOC together with GNBCUCPFunction IOC and GNBCUUPFunction IOC provide the management of gNB defined in clause 6.1.1 in 3GPP TS 38.401 [4].

For 2-split and 3-split NG-RAN architecture, this IOC provides the management representation of tgNB-DU defined in clause 6.1.1 in 3GPP TS 38.401 [4].

The following table identifies the necessary end points required for the representation of gNB and en-gNB, of all deployment scenarios.

|  |  |  |  |
| --- | --- | --- | --- |
| Req  Role | End point requirement for 3-split deployment scenario | End point requirement for 2-split deployment scenario | End point requirement for Non-split deployment scenario |
| gNB | <<IOC>>EP\_F1C, <<IOC>>EP\_F1U | <<IOC>>EP\_F1C, <<IOC>>EP\_F1U | None. |
| en-gNB | <<IOC>>EP\_F1C, <<IOC>>EP\_F1U | <<IOC>>EP\_F1C, <<IOC>>EP\_F1U | None. |

#### 4.3.1.2 Attributes

The GNBDUFunction IOC includes attributes inherited from ManagedFunction IOC (defined in TS 28.622[30]) and the following attributes:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| gNB­DUId | M | T | T | F | T |
| gNBDUName | O | T | T | F | T |
| gNBId | M | T | F | F | T |
| gNBIdLength | M | T | T | F | T |
| aggressorSetID | CM | T | F | T | T |
| victimSetID | CM | T | F | T | T |

#### 4.3.1.3 Attribute constraints

|  |  |
| --- | --- |
| Name | Definition |
| aggressorSetID | Condition: Remote Interference Management function is supported. |
| victimSetID | Condition: Remote Interference Management function is supported. |

#### 4.3.1.4 Notifications

The common notifications defined in subclause 4.5 are valid for this IOC, without exceptions or additions.

|  |
| --- |
| **Second of Changes** |

### 4.3.2 GNBCUCPFunction

#### 4.3.2.1 Definition

For non-split NG-RAN deployment scenario, this IOC together with GNBCUUPFunction IOC and GNBDUFunction IOC provide the management representation of gNB defined in clause 6.1.1 in 3GPP TS 38.401 [4].

For 2-split NG-RAN deployment scenario, this IOC together with GNBCUUPFunction IOC provide management representation of the gNB-CU defined in clause 6.1.1 in 3GPP TS 38.401 [4].

For 3-split NG-RAN deployment scenario, this IOC provides management representation of gNB-CU-CP defined in clause 6.1.2 in 3GPP TS 38.401 [4].

The following table identifies the necessary end points required for the representation of gNB and en-gNB, of all deployment scenarios.

|  |  |  |  |
| --- | --- | --- | --- |
| Req  **Role** | End point requirement for 3-split deployment scenario | End point requirement for 2-split deployment scenario | End point requirement for Non-split deployment scenario |
| gNB | <<IOC>>EP\_XnC, <<IOC>>EP\_NgC, <<IOC>>EP\_F1C,  <<IOC>>EP\_E1. | <<IOC>>EP\_XnC, <<IOC>>EP\_NgC, <<IOC>>EP\_F1C  <<IOC>>EP\_F1U. | <<IOC>>EP\_XnC, <<IOC>>EP\_NgC. |
| en-gNB | <<IOC>>EP\_X2C, <<IOC>>EP\_F1C, <<IOC>>EP\_E1. | <<IOC>>EP\_X2C, <<IOC>>EP\_F1C. | <<IOC>>EP\_X2C. |

#### 4.3.2.2 Attributes

The GNBCUCPFunction IOC includes attributes inherited from ManagedFunction IOC (defined in TS 28.622[30]) and the following attributes:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| gNBId | M | T | T | F | T |
| gNBIdLength | M | T | T | F | T |
| gNBCUName | O | T | T | F | T |
| pLMNId | M | T | T | T | T |
| x2BlackList | CM | T | T | F | T |
| x2WhiteList | CM | T | T | F | T |
| xnBlackList | CM | T | T | F | T |
| xnWhiteList | CM | T | T | F | T |
| x2XnHOBlackList | CM | T | T | F | T |
| mappingSetIDBackhaulAddressList | CM | T | T | F | T |

#### 4.3.2.3 Attribute constraints

|  |  |
| --- | --- |
| Name | Definition |
| x2BlackList | Condition: ANR function is supported *AND* Multi-Radio Dual Connectivity with the EPC (see TS 37.340 [9] clause 4.1.2) is supported. |
| x2WhiteList | Condition: ANR function is supported *AND* Multi-Radio Dual Connectivity with the EPC (see TS 37.340 [9] clause 4.1.2) is supported. |
| xnBlackList | Condition: ANR function is supported. |
| xnWhiteList | Condition: ANR function is supported. |
| x2XnHOBlackList | Condition: ANR function is supported. |
| mappingSetIDBackhaulAddressList | Condition: Remote Interference Management function is supported. |

#### 4.3.2.4 Notifications

The common notifications defined in subclause 4.5 are valid for this IOC, without exceptions or additions.

|  |
| --- |
| **Third of Changes** |

### 4.3.X MappingSetIDBackhaulAddress <<dataType>>

#### 4.3.X.1 Definition

This data type represents the properties describing the mapping relationship between set ID and backhaul address of gNB.

#### 4.3.X.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| setID | M | T | T | F | T |
| backhaulAddress | M | T | T | F | T |

#### 4.3.X.3 Attribute constraints

None.

#### 4.3.X.4 Notifications

The subclause 4.5 of the <<IOC>> using this <<dataType>> as one of its attributes, shall be applicable.

### 4.3.X1 BackhaulAddress <<dataType>>

#### 4.3.X1.1 Definition

This data type represents the properties describing the backhaul address of gNB.

#### 4.3.X1.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| gNBId | M | T | T | F | T |
| tAI | M | T | T | F | T |

#### 4.3.X1.3 Attribute constraints

None.

#### 4.3.X1.4 Notifications

The subclause 4.5 of the <<IOC>> using this <<dataType>> as one of its attributes, shall be applicable.

### 4.3.X2 TAI <<dataType>>

#### 4.3.X2.1 Definition

This data type represents the properties describing the TAI of gNB, which is used to uniquely identify a Tracking Area.

#### 4.3.X2.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| pLMNId | M | T | T | F | T |
| nRTAC | M | T | T | F | T |

#### 4.3.X2.3 Attribute constraints

None.

#### 4.3.X2.4 Notifications

The subclause 4.5 of the <<IOC>> using this <<dataType>> as one of its attributes, shall be applicable.

|  |
| --- |
| **Fourth of Changes** |

### 4.4.1 Attribute properties

| Attribute Name | Documentation and Allowed Values | Properties |
| --- | --- | --- |
| administrativeState | It indicates the administrative state of the NRCellDU. It describes the permission to use or prohibition against using the cell, imposed through the OAM services.  allowedValues: LOCKED, SHUTTING DOWN, UNLOCKED.  The meaning of these values is as defined in ITU‑T Recommendation X.731 [18].  See Annex A for Relation between the "Pre-operation state of the gNB-DU Cell" and administrative state relevant in case of 2-split and 3-split deployment scenarios. | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: LOCKED  isNullable: False |
| operationalState | It indicates the operational state of the NRCellDU instance. It describes whether the resource is installed and partially or fully operable (Enabled) or the resource is not installed or not operable (Disabled).  allowedValues: ENABLED, DISABLED. | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| cellState | It indicates the usage state of the NRCellDU instance. It describes whether the cell is not currently in use (Idle), or currently in use but not configured to carry traffic (Inactive) or is currently in use and is configured to carry traffic (Active).  The Inactive and Active definitions are in accordance with TS 38.401 [4]:  "Inactive: the cell is known by both the gNB-DU and the gNB-CU. The cell shall not serve UEs;  Active: the cell is known by both the gNB-DU and the gNB-CU. The cell should be able to serve UEs."  "allowedValues: IDLE, INACTIVE, ACTIVE. | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| arfcnDL | NR Absolute Radio Frequency Channel Number (NR-ARFCN) for downlink  allowedValues:  See TS 38.104 [12] subclause 5.4.2. Note that allowed values of NR-ARFCN are specified for each band in subclause 5.4.2.3. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| arfcnUL | NR Absolute Radio Frequency Channel Number (NR-ARFCN) for uplink  allowedValues:  See TS 38.104 [12] subclause 5.4.2. Note that allowed values of NR-ARFCN are specified for each band in subclause 5.4.2.3. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| arfcnSUL | NR Absolute Radio Frequency Channel Number (NR-ARFCN) for supplementary uplink  allowedValues:  See TS 38.104 [12] subclause 5.4.2. Note that allowed values of NR-ARFCN are specified for each band in subclause 5.4.2.3. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| beamAzimuth | The azimuth of a beam transmission, which means the horizontal beamforming pointing angle (beam peak direction) in the (Phi) φ-axis in 1/10th degree resolution. See subclauses 3.2 in TS 38.104 [12] and 7.3 in TS 38.901 [53] as well as TS 28.662 [11]. The pointing angle is the direction equal to the geometric centre of the half-power contour of the beam relative to the reference plane. Zero degree implies explicit antenna bearing (boresight). Positive angle implies clockwise from the antenna bearing.  allowedValues: [-1800 ..1800] 0.1 degree | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: Null  isNullable: True |
| beamHorizWidth | The Horizontal beamWidth of a beam transmission, which means the horizontal beamforming half-power (3dB down) beamwidth in the (Phi) φ-axis in 1/10th degree resolution. See subclauses 3.2 in TS 38.104 [12] and 7.3 in TS 38.901 [53].  allowedValues: [0..3599] 0.1 degree | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: Null  isNullable: True |
| beamIndex | Index of the beam.  For example, please see subclause 6.6.2 of TS 38.331 [54] where the ssb-Index in the rsIndexResults element of MeasResultNR is defined. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: Null  isNullable: True |
| beamTilt | The tilt of a beam transmission, which means the vertical beamforming pointing angle (beam peak direction) in the (Theta) θ-axis in 1/10th degree resolution. See subclauses 3.2 in TS 38.104 [12] and 7.3 in TS 38.901 [53] as well as TS 28.662 [11]. The pointing angle is the direction equal to the geometric centre of the half-power contour of the beam relative to the reference plane. Positive value implies downtilt.  allowedValues: [-900..900] 0.1 degree | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: Null  isNullable: True |
| beamType | The type of the beam.  allowedValues: "SSB-BEAM" | type: string  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: Null  isNullable: True |
| beamVertWidth | The Vertical beamWidth of a beam transmission, which means the vertical beamforming half-power (3dB down) beamwidth in the (Theta) θ-axis in 1/10th degree resolution. See subclauses 3.2 in TS 38.104 [12] and 7.3 in TS 38.901 [53].  allowedValues: [0...1800] 0.1 degree | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: Null  isNullable: True |
| bSChannelBwDL | BS Channel BW in MHz. for downlink  allowedValues:  See BS Channel BW in TS 38.104 [12], subclause 5.3.​ | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| bSChannelBwUL | BS Channel BW in MHz.for uplink  allowedValues:  See BS Channel BW in TS 38.104 [12], subclause 5.3.​ | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| bSChannelBwSUL | BS Channel BW in MHz.for supplementary uplink  allowedValues:  See BS Channel BW in TS 38.104 [12], subclause 5.3.​ | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| configuredMaxTxPower | This is the maximum possible for all downlink channels, used simultaneously in a cell, added together.  allowedValues:TBD | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| coverageShape | Identifies the sector carrier coverage shape described by the envelope of the contained SSB beams. The coverage shape is implementation dependent.  allowedValues: 0 : 65535 | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| digitalTilt | Digitally-controlled tilt through beamforming. It represents the vertical pointing direction of the antenna relative to the antenna bore sight, representing the total non-mechanical vertical tilt of the selected coverageShape. Positive value gives downwards tilt and negative value gives upwards tilt.  allowedValues: [-900..900] 0.1 degree | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| digitalAzimuth | Digitally-controlled azimuth through beamforming. It represents the horizontal pointing direction of the antenna relative to the antenna bore sight, representing the total non-mechanical horizontal pan of the selected coverageShape. Positive value gives azimuth to the right and negative value gives an azimuth to the left.  allowedValues: [-1800 ..1800] 0.1 degree | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| cyclicPrefix | Cyclic prefix as defined in TS 38.211 [32], subclause 4.2.  allowedValues:  NORMAL, EXTENDED. | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| localAddress | This parameter specifies the localAddress including IP address and VLAN ID used for initialization of the underlying transport.  First string is IP address, IP address can be an IPv4 address (See RFC 791 [37]) or an IPv6 address (See RFC 2373 [38]).  Second string is VLAN Id. (See IEEE 802.1Q [39]), | type: String  multiplicity: 2  isOrdered: True  isUnique: N/A  defaultValue: None  isNullable: False |
| remoteAddress | Remote address including IP address used for initialization of the underlying transport.  IP address can be an IPv4 address (See RFC 791 [37]) or an IPv6 address (See RFC 2373 [38]). | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| gNBId | It identifies a gNB within a PLMN. The gNB ID is part of the NR Cell Identifier (NCI) of the gNB cells.  See "gNB Identifier (gNB ID)" of subclause 8.2 of TS 38.300 [3]). See "Global gNB ID" in subclause 9.3.1.6 of TS 38.413 [5].  allowedValues: 0..4294967295 | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| gNBIdLength | This indicates the number of bits for encoding the gNB ID. See "Global gNB ID" in subclause 9.3.1.6 of TS 38.413 [5].  allowedValues: 22 .. 32. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| gNB­DUId | It uniquely identifies the DU at least within a gNB-CU. See 'gNB-DU ID' in subclause 9.3.1.9 of 3GPP TS 38.473 [8].  allowedValues: 0..236-1 | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| gNB­CUUPId | It uniquely identifies the gNB-CU-UP at least within a gNB-CU-CP. See 'gNB-CU-UP ID' in subclause 9.3.1.15 of 3GPP TS 38.463 [48].  allowedValues: 0..236-1 | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| gNBCUName | It identifies the Central Entity of a NR node, see subclause 9.2.1.4 of 3GPP TS 38.473 [8].  allowedValues: Not applicable | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| gNBDUName | It identifies the Distributed Entity of a NR node, see subclause 9.2.1.5 of 3GPP TS 38.473 [8].  allowedValues: Not applicable | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| cellLocalId | It identifies a NR cell of a gNB.  It, together with the gNB Identifier (using gNBId of the parent GNBCUCPFunction or GNBDUFunction or ExternalCUCPFunction), identifies a NR cell within a PLMN. This is the NR Cell Identity (NCI). See subclause 8.2 of TS 38.300 [3]),  The NCI can be constructed by encoding the gNB Identifier using gNBId (of the parent GNBCUCPFunction or GNBDUFunction or ExternalCUCPFunction) and cellLocalId where the gNB Identifier field is of length specified by gNBIdLength (of the parent GNBCUCPFunction or GNBDUFunction or ExternalCUCPFunction). See "Global gNB ID" in subclause 9.3.1.6 of TS 38.413 [5].  The NR Cell Global identifier (NCGI) is constructed from the PLMN identity the cell belongs to and the NR Cell Identifier (NCI) of the cell.  See relation between NCI and NCGI subclause 8.2 of TS 38.300 [3].  allowedValues: Not applicable | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: True  defaultValue: None  isNullable: False |
| nRPCI | This holds the Physical Cell Identity (PCI) of the NR cell.  allowedValues:  See 3GPP TS 36.211 subclause 6.11 for legal values of pci. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| nRTAC | This holds the identity of the common Tracking Area Code for the PLMNs.  allowedValues:  a) It is the TAC or Extended-TAC.  b) A cell can only broadcast one TAC or Extended-TAC. See TS 36.300, subclause 10.1.7 (PLMNID and TAC relation).  c) TAC is defined in subclause 19.4.2.3 of 3GPP TS 23.003  [13] and Extended-TAC is defined in subclause 9.3.1.29 of 3GPP TS 38.473 [8].  d) For a 5G SA (Stand Alone), it has a non-null value. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: NULL  isNullable: True |
| GNBCUCPFunction.pLMNId | It specifies the PLMN identifier to be used as part of the global RAN node identity.  allowedValues: Not applicable. | Type: PLMNId  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| GNBCUUPFunction.pLMNIdList | This is a list of PLMN identifiers. It defines from which set of PLMNs an UE must have as its serving PLMN to be allowed to use the GNB-CU-UP.  allowedValues: Not applicable. | type: PLMNId  multiplicity: 1..12  isOrdered: N/A  isUnique: True  defaultValue: None  isNullable: False |
| NRCellCU.pLMNIdList | This is a list of PLMN identifiers. It defines from which set of PLMNs an UE must have as its serving PLMN to be allowed to use the GNB-CU-UP.  allowedValues: Not applicable. | type: PLMNId  multiplicity: 1..12  isOrdered: N/A  isUnique: True  defaultValue: None  isNullable: False |
| NRCellDU.pLMNIdList | It defines which PLMNs that can be served by the NR cell. The first entry of the list is the PLMN used to construct the nCGI for the NR cell.  allowedValues: Not applicable. | type: PLMNId  multiplicity: 1..12  isOrdered: N/A  isUnique: True  defaultValue: None  isNullable: False |
| ExternalNRCellCU.pLMNIdList | It defines which PLMNs that are assumed to be served by the NR Cell in another gNB-CU-CP. This list is either updated by the managed element itself (e.g. due to ANR, signalling over Xn etc) or by consumer over the standard interface.  allowedValues: Not applicable. | Type: PLMNId  multiplicity: 1..12  isOrdered: N/A  isUnique: True  defaultValue: None  isNullable: False |
| sNSSAIList | It represents the list of S-NSSAI the managed object is supporting. The S-NSSAI is defined in 3GPP TS 23.003 [13].  allowedValues: See 3GPP TS 23.003 [13] | type: S-NSSAI  multiplicity: \*  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| sST | This attribute specifies the Slice/Service type (SST) of the network slice.  See clause 5.15.2 of 3GPP TS 23.501 [2]. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| sD | This attribute specifies the Slice Differentiator (SD), which is optional information that complements the slice/service type(s) to differentiate amongst multiple Network Slices.  See clause 5.15.2 of 3GPP TS 23.501 [2]. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| rRMPolicyType | Type of the RRM policy.  The value 0 denotes use of the rRMPolicy.  The value 1 denotes use of the rRMPolicyNSSIId, rRMPolicyRatio  The value 2 denotes use of the rRMPolicyRatio2.  allowedValues: 0 : 65535. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| rRMPolicyNSSIId | The list of S-NSSAIs for which a rRMPolicyRatio value is specified  allowedValues: Not applicable. | type: DN  multiplicity: 1..\*  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| rRMPolicyRatio | The RRM policy setting the ratio for the split of the Radio resources between the supported S-NSSAI lists A S-NSSAI list is defined in rRMPolicyNSSIId. rRMPolicyRatio is the list of target percentage values assigned to the corresponding rRMPolicyNSSIId values. Every value specifies the percentage of PRBs to be allocated to the corresponding S-NSSAIs, in average over time. The sum of the values shall be less or equal 100.  allowedValues:  0 : 100  See NOTE 3 and NOTE 4. | type: Integer  multiplicity: 1..\*  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| rRMPolicyRatio2List | The attribute specifies a list of RRMPolicyRatio2 which is defined as a datatype. The attribute is used to set the ratios for the split of the Radio resources between the sNSSAILists for radio resources (e.g. RRC connected users, PDCP resource, etc.) in average time (see NOTE 2 and NOTE 3).  The sum of the values included in the item of rRMPolicyRatio2 shall be less or equal 100 (see NOTE 4).  allowedValues: Not applicable. | type: RRMPolicyRatio2  multiplicity: 1..\*  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| groupId | The attribute identifies one sNSSAIList group inside NRCellCU. The rRMPolicyRatio2 is configured for each group. The value of the groupId is unique inside one NRCellCU instance | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| quotaType | The attribute indicates the type of the quota which allows to allocate resources as strictly usable for defined slice(s) ( “strict quota”) or allows that resources to be used by other slice(s) when defined slice(s) do not need them ( “float quota”).  allowedValues: STRICT, FLOAT. | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| rRMPolicyMaxRatio | The RRM policy setting the maximum percentage of radio resources to be allocated to the corresponding S-NSSAIList.  This quota can be strict or float quota. Strict quota means resources are not allowed for other sNSSAIs even when they are not used by the defined sNSSAIList. Float quota resources can be used by other sNSSAIs when the defined sNSSAIList do not need them.  Value 0 indicates that there is no maximum limit.  allowedValues:  0 : 100 | type: Integer  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| rRMPolicyMarginMaxRatio | Maximum quota margin ratio is applicable when maximum quota policy ratio is of type “float quota”. It defines the resource quota within maximum quota to reserve buffers for new resource requirements for the specified S-NSSAIList. With the margin ratio, unused resources of the maximum resource quota can be allocated to other S-NSSAIs when the free resources are more than resource amount indicated by the margin. The margin resource quota can only be used for the specific S-NSSAIList. Value 0 indicates that no margin is used.  allowedValues:  0 : 100 | type: Integer  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| rRMPolicyMinRatio | The RRM policy setting the minimum percentage of radio resources to be allocated to the corresponding S-NSSAIList.  This quota can be strict or float quota. Strict quota means resources are not allowed for other sNSSAIs even when they are not used by the defined sNSSAIList. Float quota resources can be used by other sNSSAIs when the defined sNSSAIList do not need them.  Value 0 indicates that there is no minimum limit.  allowedValues:  0 : 100  NOTE: The averaging time interval is implementation dependent. | type: Integer  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| rRMPolicyMarginMinRatio | Minimum quota margin ratio is applicable when minimum quota policy ratio is of type “float quota”. It defines the resource quota within minimum quota to reserve buffers for new resource requirements for the specified S-NSSAIList. With the margin ratio, unused resources of the minimum resource quota can be allocated to other S-NSSAIs when the free resources are more than resource amount indicated by the margin. The margin resource quota can only be used for the specific S-NSSAIList. Value 0 indicates that no margin is used.  allowedValues:  0 : 100 | type: Integer  multiplicity: 0..1  isOrdered: N/A  isUnique: N/A  defaultValue: None  allowedValues: N/A  isNullable: False |
| rRMPolicy | It represents RRM policy which includes guidance for split of radio resources between the S-NSSAIs that the cell supports in case when the rRMPolicyType is absent or equal to 0. The RRM policy is implementation dependent.  allowedValues: Not applicable | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| subCarrierSpacing | Subcarrier spacing configuration for a BWP. See subclause 5 in TS 38.104 [12].  AllowedValues: [15, 30, 60, 120] depending on the frequency range FR1 or FR2. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| txDirection | Indicates if the transmission direction is downlink (DL), uplink (UL) or both downlink and uplink (DL and UL).  allowedValues:  DL, UL, DL and UL | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| bwpContext | It identifies whether the object is used for downlink, uplink or supplementary uplink.  allowedValues:  DL, UL, SUL | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| isInitialBwp | It identifies whether the object is used for initial or other BWP.  allowedValues:  INITIAL, OTHER | type: ENUM  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| startRB | Offset in common resource blocks to common resource block 0 for the applicable subcarrier spacing for a BWP. This corresponds to N\_BWP\_start, see subclause 4.4.5 in TS 38.211 [32].  allowedValues:  0 to N\_grid\_size – 1, where N\_grid\_size equals the number of resource blocks for the BS channel bandwidth, given the subcarrier spacing of the BWP. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| numberOfRBs | Number of physical resource blocks for a BWP. This corresponds to N\_BWP\_size, see subclause 4.4.5 in TS 38.211 [32].  allowedValues:  1 to N\_grid\_size – startRB of the BWP. Se startRB for definition of N\_grid\_size. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| nRTCI | This is the Target NR Cell Identifier. It consists of NR Cell Identifier (NCI) and Physical Cell Identifier of the target NR cell (nRPCI).  The NRRelation.nRTCI identifies the target cell from the perspective of the NRCell, the name-containing instance of the subject NRCellCU instance.  allowedValues: Not applicable. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| adjacentCellRef | This attribute contains the DN of an adjacentNRCell (NRCellCU or ExternalNRCellCU)  allowedValues: Not applicable. | type: DN  multiplicity: 1  isOrdered: N/A  isUnique: True  defaultValue: None  isNullable: False |
| ssbFrequency | Indicates cell defining SSB frequency domain position  Frequency of the cell defining SSB transmission. The frequency provided in this attribute identifies the position of resource element RE=#0 (subcarrier #0) of resource block RB#10 of the SS block. The frequency must be positioned on the NR global frequency raster, as defined in TS 38.101 [42] subclause 5.4.2. and within bSChannelBwDL.  allowedValues: 0..3279165 | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| nRFrequencyRef | This attribute contains the DN of the referenced NRFrequency.  allowedValues: Not applicable. | type: DN  multiplicity: 1  isOrdered: N/A  isUnique: True  defaultValue: None  isNullable: False |
| nRSectorCarrierRef | This attribute contains the DN of the referenced NRSectorCarrier.  allowedValues: Not applicable. | type: DN  multiplicity: 1  isOrdered: N/A  isUnique: True  defaultValue: None  isNullable: False |
| bWPRef | This attribute contains the DN of the referenced BWP.  allowedValues: Not applicable. | type: DN  multiplicity: 1  isOrdered: N/A  isUnique: True  defaultValue: None  isNullable: False |
| sectorEquipmentFunctionRef | This attribute contains the DN of the referenced NSectorEquipmentFunction.  allowedValues: Not applicable. | type: DN  multiplicity: 1  isOrdered: N/A  isUnique: True  defaultValue: None  isNullable: False |
| offsetMO | It is a list of offset values applicable to all measured cells with reference signal(s) indicated in this *MeasObjectNR*. See offsetMO of subclause 5.5.4 of TS 38.331 [31].  allowedValues: Not applicable. | type: QOffsetRangeList  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: N/A  isNullable: False |
| cellIndividualOffset | It is a list of offset values for the neighbour cell. Used when UE is in connected mode. The unit is 1dB. It is defined for rsrpOffsetSSB, rsrqOffsetSSB, sinrOffsetSSB, rsrpOffsetCSI-RS, rsrqOffsetCSI-RS and sinrOffsetCSI-RS. See TS 38.331 [31].  allowedValues: Not applicable. | type: Integer  multiplicity: 6  isOrdered: True  isUnique: N/A  defaultValue: 0  isNullable: False |
| blackListEntry | It specifies a list of PCI (physical cell identity) that are blacklisted in EUTRAN measurements as described in 3GPP TS 38.331 [31].  allowedValues: { 0…1007 } | type: Integer  multiplicity: \*  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| blackListEntryIdleMode | It specifies a list of PCI (physical cell identity) that are blacklisted in SIB4 and SIB5.  allowedValues: { 0…1007 } | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| cellReselectionPriority | It is the absolute priority of the carrier frequency used by the cell reselection procedure. See *CellReselectionPriority* IE in TS 38.331 [31].  It corresponds to the parameter priority in 3GPP TS 38.304 [49].  Value 0 means lowest priority. The UE behaviour when no value is entered is specified in subclause 5.2.4.1 of 3GPP TS 38.304 [49].  The value must not already used by other RAT, i.e. equal priorities between RATs are not supported.  allowedValues: N/A | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: 0None  isNullable: False |
| cellReselectionSubPriority | It indicates a fractional value to be added to the value of cellReselectionPriority to obtain the absolute priority of the concerned carrier frequency for E-UTRA and NR. See *CellReselectionSubPriority* IE in TS 38.331 [31].  allowedValues: { 0.2, 0.4, 0.6, 0.8 }. | type: Short  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| pMax | It calculates the parameter Pcompensation (defined in 3GPP TS 38.304 [49]), at cell reselection to an Cell. Its unit is 1 dBm. It corresponds to parameter PEMAX in 3GPP TS 38.101 [??].  allowedValues: { -30..33 }. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| qOffsetFreq | It is the frequency specific offset applied when evaluating candidates for cell reselection. See TS 38.331 [49]. Its unit is 1 dB.  allowedValues:  { -24, -22, -20, -18, -16, -14, -12, -10, -8, -6, -5, -4, -3, -2, -1, 0, 1, 2, 3, 4, 5, 6, 8, 10, 12, 14, 16, 20, 22, 24 } | type: Real  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: 0  isNullable: False |
| qOffsetRangeList | It is used to indicate a cell, beam or measurement object specific offset to be applied when evaluating candidates for cell re-selection or when evaluating triggering conditions for measurement reporting. The value in dB. Value dB-24 corresponds to -24 dB, dB-22 corresponds to -22 dB and so on.  This is a list of enum values representing, in sequence: rsrpOffsetSSB, rsrqOffsetSSB, sinrOffsetSSB, rsrpOffsetCSI-RS, srqOffsetCSI-RS, sinrOffsetCSI-RS.  See Q-OffsetRangeList in subclause of subclause 6.3.1 of TS 38.311 [31].  allowedValues:  { -24, -22, -20, -18, -16, -14, -12, -10, -8, -6, -5, -4, -3, -2, -1, 0, 1, 2, 3, 4, 5, 6, 8, 10, 12, 14, 16, 18, 20, 22, 24 } | type: ENUM  multiplicity: 6  isOrdered: True  isUnique: N/A  defaultValue: 0  isNullable: False |
| qQualMin | It indicates the minimum required quality level in the cell (dB). See qQualMin in TS 38.304 [49]. Unit is 1 dB.  Value 0 means that it is not sent and UE applies in such case the (default) value of negative infinity for Qqualmin. Sent in SIB3 or SIB5.  allowedValues: { -34..-3, 0 } | type: Real  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| qRxLevMin | It indicates the required minimum received Reference Symbol Received Power (RSRP) level in the (E-UTRA) frequency for cell reselection. It corresponds to Qrxlevmin defined in 3GPP TS 38.304 [49]. It is broadcast in SIB3 or SIB5, depending on whether the related frequency is intra- or inter-frequency. Its unit is 1 dBm and resolution is 2.  allowedValues: { -140..-44 }. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| threshXHighP | This specifies the Srxlev threshold (in dB) used by the UE when reselecting towards a higher priority RAT/ frequency than the current serving frequency. Each frequency of NR and E-UTRAN might have a specific threshold. It corresponds to the ThreshX, HighPin 3GPP TS 38.304 [49]. Its unit is 1 dB and resolution is 2**.**  allowedValues: { 0..62 } | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| threshXHighQ | This specifies the Squal threshold (in dB) used by the UE when reselecting towards a higher priority RAT/ frequency than the current serving frequency. Each frequency of NR and E-UTRAN might have a specific threshold. It corresponds to the ThreshX, HighQ in TS 38.304 [49]. Its unit is 1 dB.  allowedValues: { 0..31 } | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| threshXLowP | This specifies the Srxlev threshold (in dB) used by the UE when reselecting towards a lower priority RAT/ frequency than the current serving frequency. Each frequency of NR might have a specific threshold. It corresponds to ThreshX,LowP in 3GPP TS 38.304 [49]. Its unit is 1 dB. Its resolution is 2.  allowedValues: { 0..62 } | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| threshXLowQ | This specifies the Squal threshold (in dB) used by the UE when reselecting towards a lower priority RAT/ frequency than the current serving frequency. Each frequency of NR might have a specific threshold. It corresponds to ThreshX,Low in TS 38.304 [49]. Its unit is 1 dB.  allowedValues: {0..31}. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| tReselectionNr | It is the cell reselection timer and corresponds to parameter TreselectionRAT for NR defined in 38.331 [4]. Its unit is in seconds.   allowedValues: {0..7}. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| tReselectionNRSfHigh | The attribute t-ReselectionNr (a parameter TreselectionNR in TS 38.304 [49]) is multiplied with this factor if the UE is in high mobility state. It corresponds to the parameter Speed dependent ScalingFactor for TreselectionNr for medium high state in 3GPP TS 38.304 [49]. The unit is one %.  Value mapping: 25 = 0.25 50 = 0.5 75 = 0.75 100 = 1.0  allowedValues: {25, 50, 75, 100}. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| tReselectionNRSfMedium | The attribute t-ReselectionNR (a parameter "TreselectionNR in TS 38.304 [49]”) is multiplied with this factor if the UE is in medium mobility state. It corresponds to the parameter Speed dependent ScalingFactor for TreselectionNr for medium mobility state in 3GPP TS 38.304 [49]. Its unit is one %.  Value mapping: 25 = 0.25 50 = 0.5 75 = 0.75 100 = 1.0   allowedValues: {25, 50, 75, 100}. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| absoluteFrequencySSB | The absolute frequency applicable for a downlink NR carrier frequency associated with the SSB.  allowedValues: {0.. 3279165}. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| sSBSubCarrierSpacing | This SSB is used for for synchronization. See subclause 5 in TS 38.104 [12]. Its units are in kHz.  allowedValues: {15, 30, 120, 240}.  Note that the allowed values of SSB used for representing data, by e.g. a BWP, are: 15, 30, 60 and 120 in units of kHz. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| multiFrequencyBandListNR | It is a list of additional frequency bands the frequency belongs to. The list is automatically set by the gNB.  allowedValues: {1..256 } | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| ssbPeriodicity | Indicates cell defined SSB periodicity in number of subframes (ms).  The SSB periodicity in msec is used for the rate matching purpose.  allowedValues: 5, 10, 20, 40, 80, 160. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| ssbOffset   |  | | --- | |  | | Indicates cell defining SSB time domain position. Defined as the offset of the measurement window, in number of subframes (ms), in which to receive SS/PBCH blocks, where allowed values depend on the ssbPeriodicity.  allowedValues:  ssbPeriodicity5 ms 0..4,  ssbPeriodicity10 ms 0..9,  ssbPeriodicity20 ms 0..19,  ssbPeriodicity40 ms 0..39,  ssbPeriodicity80 ms 0..79,  ssbPeriodicity160 ms 0..159. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| ssbDuration   |  | | --- | |  | | Duration of the measurement window in which to receive SS/PBCH blocks. It is given in number of subframes (ms) (see 38.213 [41], subclause 4.1.  allowedValues: 1, 2, 3, 4, 5. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| rimRSMonitoringStartTime | This field configures the UTC time when the gNB attempts to start RIM-RS monitoring.  allowedValues: containing the information same with xsd: dateTime. | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| rimRSMonitoringStopTime | This field configures the UTC time when the gNB stops RIM-RS monitoring.  allowedValues: containing the information same with xsd: dateTime. | type: String  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| aggressorSetID | This attributer indicates the associated aggressor gNB Set ID of the cell. (See subclause 7.4.1.6 in TS 38.211 [32]). Editor's Note: The definition of aggressorSetID needs further clarification with RAN1.  allowedValues:  The bit length of the set ID is maximum 22bit. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| victimSetID | This attributer indicates the associated Victim gNB Set ID of the cell. (See subclause 7.4.1.6 in TS 38.211 [32]). Editor's Note: The definition of victimSetID needs further clarification with RAN1.  allowedValues:  The bit length of the set ID is maximum 22bit. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| mappingSetIDBackhaulAddressList | The attribute specifies a list of mappingSetIDBackhaulAddress which is defined as a datatype (see clause 4.3.X). Which is used to retrieve the backhaul address of the victim set.  allowedValues: Not applicable | type: MappingSetIDBackhaulAddress  multiplicity: 1..\*  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| backhaulAddress | The attribute specifies backhaulAddress which is defined as a datatype (see clause 4.3.X1).  allowedValues: Not applicable | type: BackhaulAddress  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| setID | This specifies the set ID. (See subclause 7.4.1.6 in TS 38.211 [32]).  allowedValues:  The bit length of the set ID is maximum 22bit. | type: Integer  multiplicity: 1  isOrdered: N/A  isUnique: N/A  defaultValue: None  isNullable: False |
| NOTE 1: Void  NOTE 2: The radio resource can be signaling resources (e.g. RRC connected users) or user plane resources (e.g. PDCP). The detail resource and how to map the ratio to exact number of resources is implementation dependant.  NOTE 3: The averaging time interval is implementation dependent.  NOTE 4: How to calculate the sum of the ratio is implementation dependent. | | |

|  |
| --- |
| **Fifth of Changes** |

## D.4.3 JSON schema "nrNrm.json"

{

"openapi": "3.0.1",

"info": {

"title": "3GPP NR NRM",

"version": "16.1.0",

"description": "OAS 3.0.1 specification compatible schema for 3GPP NR NRM"

},

"paths": {},

"components": {

"schemas": {

"GnbId": {

"type": "string"

},

"GnbIdLength": {

"type": "integer",

"minimum": 22,

"maximum": 32

},

"GnbName": {

"type": "string",

"maxLength": 150

},

"GnbDuId": {

"type": "number",

"minimum": 0,

"maximum": 68719476735

},

"GnbCuUpId": {

"type": "number",

"minimum": 0,

"maximum": 68719476735

},

"NCi": {

"type": "object",

"properties": {

"plmnId": {

"$ref": "#/components/schemas/PlmnId"

},

"nCI": {

"$ref": "#/components/schemas/NrCellId"

}

}

},

"SnssaiList": {

"type": "array",

"items": {

"$ref": "#/components/schemas/Snssai"

}

},

"RrmPolicy": {

"type": "string"

},

"NrPci": {

"type": "integer",

"maximum": 503

},

"NrTac": {

"type": "integer",

"maximum": 16777215

},

"NrCellId": {

"type": "integer",

"maximum": 68719476735

},

"Sst": {

"type": "integer",

"maximum": 255

},

"Snssai": {

"type": "object",

"properties": {

"sst": {

"$ref": "#/components/schemas/Sst"

},

"sd": {

"type": "string"

}

}

},

"CellState": {

"type": "string",

"enum": [

"IDLE",

"INACTIVE",

"ACTIVE"

]

},

"CyclicPrefix": {

"type": "string",

"enum": [

"15",

"30",

"60",

"120"

]

},

"TxDirection": {

"type": "string",

"enum": [

"DL",

"UL",

"DL and UL"

]

},

"BwpContext": {

"type": "string",

"enum": [

"DL",

"UL",

"SUL"

]

},

"IsInitialBwp": {

"type": "string",

"enum": [

"INITIAL",

"OTHER",

"SUL"

]

},

"QuotaType": {

"type": "string",

"enum": [

"STRICT",

"FLOAT"

]

},

"RrmPolicyRatio2": {

"type": "object",

"properties": {

"groupId": {

"type": "integer"

},

"sNSSAIList": {

"$ref": "#/components/schemas/SnssaiList"

},

"quotaType": {

"$ref": "#/components/schemas/QuotaType"

},

"rRMPolicyMaxRation": {

"type": "integer"

},

"rRMPolicyMarginMaxRation": {

"type": "integer"

},

"rRMPolicyMinRation": {

"type": "integer"

},

"rRMPolicyMarginMinRation": {

"type": "integer"

}

}

},

"Mnc": {

"type": "string",

"pattern": "[0-9]{3}|[0-9]{2}"

},

"PlmnId": {

"type": "object",

"properties": {

"mcc": {

"$ref": "genericNrm.json#/components/schemas/Mcc"

},

"mnc": {

"$ref": "#/components/schemas/Mnc"

}

}

},

"PlmnIdList": {

"type": "array",

"items": {

"$ref": "#/components/schemas/PlmnId"

}

},

"LocalAddress": {

"type": "object",

"properties": {

"ipv4Address": {

"$ref": "genericNrm.json#/components/schemas/Ipv4Addr"

},

"ipv6Address": {

"$ref": "genericNrm.json#/components/schemas/Ipv6Addr"

},

"vlanId": {

"type": "integer",

"minimum": 0,

"maximum": 4096

},

"port": {

"type": "integer",

"minimum": 0,

"maximum": 65535

}

}

},

"RemoteAddress": {

"type": "object",

"properties": {

"ipv4Address": {

"$ref": "genericNrm.json#/components/schemas/Ipv4Addr"

},

"ipv6Address": {

"$ref": "genericNrm.json#/components/schemas/Ipv6Addr"

}

}

},

"CellIndividualOffset": {

"type": "object",

"properties": {

"rsrpOffsetSSB": {

"type": "integer"

},

"rsrqOffsetSSB": {

"type": "integer"

},

"sinrOffsetSSB": {

"type": "integer"

},

"rsrpOffsetCSI-RS": {

"type": "integer"

},

"rsrqOffsetCSI-RS": {

"type": "integer"

},

"sinrOffsetCSI-RS": {

"type": "integer"

}

}

},

"QOffsetRange": {

"type": "integer",

"enum": [

-24,

-22,

-20,

-18,

-16,

-14,

-12,

-10,

-8,

-6,

-5,

-4,

-3,

-2,

-1,

0,

24,

22,

20,

18,

16,

14,

12,

10,

8,

6,

5,

4,

3,

2,

1

]

},

"QOffsetRangeList": {

"type": "object",

"properties": {

"rsrpOffsetSSB": {

"$ref": "#/components/schemas/QOffsetRange"

},

"rsrqOffsetSSB": {

"$ref": "#/components/schemas/QOffsetRange"

},

"sinrOffsetSSB": {

"$ref": "#/components/schemas/QOffsetRange"

},

"rsrpOffsetCSI-RS": {

"$ref": "#/components/schemas/QOffsetRange"

},

"rsrqOffsetCSI-RS": {

"$ref": "#/components/schemas/QOffsetRange"

},

"sinrOffsetCSI-RS": {

"$ref": "#/components/schemas/QOffsetRange"

}

}

},

"QOffsetFreq": {

"type": "number"

},

"TReselectionNRSf": {

"type": "integer",

"enum": [

25,

50,

75,

100

]

},

"SsbPeriodicity": {

"type": "integer",

"enum": [

5,

10,

20,

40,

80,

160

]

},

"SsbDuration": {

"type": "integer",

"enum": [

1,

2,

3,

4,

5

]

},

"SsbSubCarrierSpacing": {

"type": "integer",

"enum": [

15,

30,

120,

240

]

},

"coverageShape": {

"type": "integer",

"maximum": 65535

},

"digitalTilt": {

"type": "integer",

"minimum": -900,

"maximum": 900

},

"digitalAzimuth": {

"type": "integer",

"minimum": -1800,

"maximum": 1800

},

"GnbDuFunction": {

"allOf": [

{

"$ref": "genericNrm.json#/components/schemas/Top-Attributes"

},

{

"type": "object",

"properties": {

"attributes": {

"allOf": [

{

"$ref": "genericNrm.json#/components/schemas/ManagedFunction-Attributes"

},

{

"type": "object",

"properties": {

"gnbDuId": {

"$ref": "#/components/schemas/GnbDuId"

},

"gnbDuName": {

"$ref": "#/components/schemas/GnbName"

},

"gnbId": {

"$ref": "#/components/schemas/GnbId"

},

"gnbIdLength": {

"$ref": "#/components/schemas/GnbIdLength"

}

}

}

]

}

}

},

{

"$ref": "genericNrm.json#/components/schemas/ManagedFunction-ContainingObjects"

},

{

"type": "object",

"properties": {

"EP\_F1C": {

"$ref": "#/components/schemas/EP\_F1C"

},

"EP\_F1U": {

"type": "array",

"items": {

"$ref": "#/components/schemas/EP\_F1U"

}

},

"NrCellDu": {

"type": "array",

"items": {

"$ref": "#/components/schemas/NrCellDu"

}

},

"NrSectorCarrier": {

"type": "array",

"items": {

"$ref": "#/components/schemas/NrSectorCarrier"

}

},

"Bwp": {

"type": "array",

"items": {

"$ref": "#/components/schemas/Bwp"

}

},

"CommonBeamformingFunction": {

"type": "array",

"items": {

"$ref": "#/components/schemas/CommonBeamformingFunction"

}

},

"Beam": {

"type": "array",

"items": {

"$ref": "#/components/schemas/Beam"

}

}

}

}

]

},

"GnbCuCpFunction": {

"allOf": [

{

"$ref": "genericNrm.json#/components/schemas/Top-Attributes"

},

{

"type": "object",

"properties": {

"attributes": {

"allOf": [

{

"$ref": "genericNrm.json#/components/schemas/ManagedFunction-Attributes"

},

{

"type": "object",

"properties": {

"gnbId": {

"$ref": "#/components/schemas/GnbId"

},

"gnbIdLength": {

"$ref": "#/components/schemas/GnbIdLength"

},

"gnbCuName": {

"$ref": "#/components/schemas/GnbName"

},

"plmnId": {

"$ref": "#/components/schemas/PlmnId"

},

"x2BlackList": {

"$ref": "genericNrm.json#/components/schemas/DnList"

},

"xnWhiteList": {

"$ref": "genericNrm.json#/components/schemas/DnList"

},

"x2BlackList": {

"$ref": "genericNrm.json#/components/schemas/DnList"

},

"xnWhiteList": {

"$ref": "genericNrm.json#/components/schemas/DnList"

},

"x2XnHOBlackList": {

"$ref": "genericNrm.json#/components/schemas/DnList"

},

"mappingSetIDBackhaulAddress": {

"$ref": "#/components/schemas/MappingSetIDBackhaulAddress"

}

}

}

]

}

}

},

{

"$ref": "genericNrm.json#/components/schemas/ManagedFunction-ContainingObjects"

},

{

"type": "object",

"properties": {

"EP\_F1C": {

"type": "array",

"items": {

"$ref": "#/components/schemas/EP\_F1C"

}

},

"EP\_E1": {

"type": "array",

"items": {

"$ref": "#/components/schemas/EP\_E1"

}

},

"EP\_XnC": {

"type": "array",

"items": {

"$ref": "#/components/schemas/EP\_XnC"

}

},

"EP\_X2C": {

"type": "array",

"items": {

"$ref": "#/components/schemas/EP\_X2C"

}

},

"EP\_NgC": {

"type": "array",

"items": {

"$ref": "#/components/schemas/EP\_NgC"

}

},

"NrCellCu": {

"type": "array",

"items": {

"$ref": "#/components/schemas/NrCellCu"

}

}

}

}

]

},

"GnbCuUpFunction": {

"allOf": [

{

"$ref": "genericNrm.json#/components/schemas/Top-Attributes"

},

{

"type": "object",

"properties": {

"attributes": {

"allOf": [

{

"$ref": "genericNrm.json#/components/schemas/ManagedFunction-Attributes"

},

{

"type": "object",

"properties": {

"gnbId": {

"$ref": "#/components/schemas/GnbId"

},

"gnbIdLength": {

"$ref": "#/components/schemas/GnbIdLength"

},

"gnbCuUpId": {

"$ref": "#/components/schemas/GnbCuUpId"

},

"plmnIdList": {

"$ref": "#/components/schemas/PlmnIdList"

}

}

}

]

}

}

},

{

"$ref": "genericNrm.json#/components/schemas/ManagedFunction-ContainingObjects"

},

{

"type": "object",

"properties": {

"EP\_E1": {

"$ref": "#/components/schemas/EP\_E1"

},

"EP\_F1U": {

"type": "array",

"items": {

"$ref": "#/components/schemas/EP\_F1U"

}

},

"EP\_XnU": {

"type": "array",

"items": {

"$ref": "#/components/schemas/EP\_XnU"

}

},

"EP\_NgU": {

"type": "array",

"items": {

"$ref": "#/components/schemas/EP\_NgU"

}

},

"EP\_X2U": {

"type": "array",

"items": {

"$ref": "#/components/schemas/EP\_X2U"

}

},

"EP\_S1U": {

"type": "array",

"items": {

"$ref": "#/components/schemas/EP\_S1U"

}

}

}

}

]

},

"NrCellCu": {

"allOf": [

{

"$ref": "genericNrm.json#/components/schemas/Top-Attributes"

},

{

"type": "object",

"properties": {

"attributes": {

"allOf": [

{

"$ref": "genericNrm.json#/components/schemas/ManagedFunction-Attributes"

},

{

"type": "object",

"properties": {

"cellLocalId": {

"type": "integer"

},

"plmnIdList": {

"$ref": "#/components/schemas/PlmnIdList"

},

"snssaiList": {

"$ref": "#/components/schemas/SnssaiList"

},

"rrmPolicyType": {

"type": "integer"

},

"rrmPolicyNSSIId": {

"$ref": "genericNrm.json#/components/schemas/Dn"

},

"rrmPolicyRatio": {

"type": "integer"

},

"rrmPolicy": {

"$ref": "#/components/schemas/RrmPolicy"

},

"rrmPolicyRatio2": {

"$ref": "#/components/schemas/RrmPolicyRatio2"

},

"nRFrequencyRef": {

"$ref": "genericNrm.json#/components/schemas/Dn"

}

}

}

]

}

}

},

{

"$ref": "genericNrm.json#/components/schemas/ManagedFunction-ContainingObjects"

},

{

"type": "object",

"properties": {

"NRCellRelation": {

"type": "array",

"items": {

"$ref": "#/components/schemas/NRCellRelation"

}

},

"NRFreqRelation": {

"type": "array",

"items": {

"$ref": "#/components/schemas/NRFreqRelation"

}

},

"EUtranCellRelation": {

"type": "array",

"items": {

"$ref": "#/components/schemas/EUtranCellRelation"

}

},

"EUtranFreqRelation": {

"type": "array",

"items": {

"$ref": "#/components/schemas/EUtranFreqRelation"

}

}

}

}

]

},

"NrCellDu": {

"allOf": [

{

"$ref": "genericNrm.json#/components/schemas/Top-Attributes"

},

{

"type": "object",

"properties": {

"attributes": {

"allOf": [

{

"$ref": "genericNrm.json#/components/schemas/ManagedFunction-Attributes"

},

{

"type": "object",

"properties": {

"administrativeState": {

"$ref": "genericNrm.json#/components/schemas/AdministrativeState"

},

"operationalState": {

"$ref": "genericNrm.json#/components/schemas/OperationalState"

},

"cellLocalId": {

"type": "integer"

},

"cellState": {

"$ref": "#/components/schemas/CellState"

},

"plmnIdList": {

"$ref": "#/components/schemas/PlmnIdList"

},

"snssaiList": {

"$ref": "#/components/schemas/SnssaiList"

},

"nrPci": {

"$ref": "#/components/schemas/NrPci"

},

"nrTac": {

"$ref": "#/components/schemas/NrTac"

},

"arfcnDL": {

"type": "integer"

},

"arfcnUL": {

"type": "integer"

},

"arfcnSUL": {

"type": "integer"

},

"bSChannelBwDL": {

"type": "integer"

},

"bSChannelBwUL": {

"type": "integer"

},

"bSChannelBwSUL": {

"type": "integer"

},

"ssbFrequency": {

"type": "integer",

"minimum": 0,

"maximum": 3279165

},

"ssbPeriodicity": {

"$ref": "#/components/schemas/SsbPeriodicity"

},

"ssbSubCarrierSpacing": {

"$ref": "#/components/schemas/SsbSubCarrierSpacing"

},

"ssbOffset": {

"type": "integer",

"minimum": 0,

"maximum": 159

},

"ssbDuration": {

"$ref": "#/components/schemas/SsbDuration"

},

"nrSectorCarrierRef": {

"type": "array",

"items": {

"$ref": "genericNrm.json#/components/schemas/Dn"

}

},

"bwpRef": {

"type": "array",

"items": {

"$ref": "genericNrm.json#/components/schemas/Dn"

}

},

"nRFrequencyRef": {

"$ref": "genericNrm.json#/components/schemas/Dn"

}

}

}

]

}

}

},

{

"$ref": "genericNrm.json#/components/schemas/ManagedFunction-ContainingObjects"

}

]

},

"NrSectorCarrier": {

"allOf": [

{

"$ref": "genericNrm.json#/components/schemas/Top-Attributes"

},

{

"type": "object",

"properties": {

"attributes": {

"allOf": [

{

"$ref": "genericNrm.json#/components/schemas/ManagedFunction-Attributes"

},

{

"type": "object",

"properties": {

"txDirection": {

"$ref": "#/components/schemas/TxDirection"

},

"configuredMaxTxPower": {

"type": "integer"

},

"arfcnDL": {

"type": "integer"

},

"arfcnUL": {

"type": "integer"

},

"bSChannelBwDL": {

"type": "integer"

},

"bSChannelBwUL": {

"type": "integer"

},

"sectorEquipmentFunctionRef": {

"$ref": "genericNrm.json#/components/schemas/Dn"

}

}

}

]

}

}

},

{

"$ref": "genericNrm.json#/components/schemas/ManagedFunction-ContainingObjects"

}

]

},

"Bwp": {

"allOf": [

{

"$ref": "genericNrm.json#/components/schemas/Top-Attributes"

},

{

"type": "object",

"properties": {

"attributes": {

"allOf": [

{

"$ref": "genericNrm.json#/components/schemas/ManagedFunction-Attributes"

},

{

"type": "object",

"properties": {

"bwpContext": {

"$ref": "#/components/schemas/BwpContext"

},

"isInitialBwp": {

"$ref": "#/components/schemas/IsInitialBwp"

},

"subCarrierSpacing": {

"type": "integer"

},

"cyclicPrefix": {

"$ref": "#/components/schemas/CyclicPrefix"

},

"startRB": {

"type": "integer"

},

"numberOfRBs": {

"type": "integer"

}

}

}

]

}

}

},

{

"$ref": "genericNrm.json#/components/schemas/ManagedFunction-ContainingObjects"

}

]

},

"CommonBeamformingFunction": {

"allOf": [

{

"$ref": "genericNrm.json#/components/schemas/Top-Attributes"

},

{

"type": "object",

"properties": {

"attributes": {

"allOf": [

{

"type": "object",

"properties": {

"coverageShape": {

"type": "#/components/schemas/coverageShape"

},

"digitalAzimuth": {

"type": "#/components/schemas/digitalAzimuth"

},

"digitalTilt": {

"type": "#/components/schemas/digitalTilt"

}

}

}

]

}

}

},

{

"$ref": "genericNrm.json#/components/schemas/ManagedFunction-ContainingObjects"

}

]

},

"Beam": {

"allOf": [

{

"$ref": "genericNrm.json#/components/schemas/Top-Attributes"

},

{

"type": "object",

"properties": {

"attributes": {

"allOf": [

{

"type": "object",

"properties": {

"beamIndex": {

"type": "integer"

},

"beamType": {

"type": "string",

"enum": [

"SSB-BEAM"

]

},

"beamAzimuth": {

"type": "integer",

"minimum": -1800,

"maximum": 1800

},

"beamTilt": {

"type": "integer",

"minimum": -900,

"maximum": 900

},

"beamHorizWidth": {

"type": "integer",

"minimum": 0,

"maximum": 3599

},

"beamVertWidth": {

"type": "integer",

"minimum": 0,

"maximum": 1800

}

}

}

]

}

}

}

]

},

"ExternalGnbDuFunction": {

"allOf": [

{

"$ref": "genericNrm.json#/components/schemas/Top-Attributes"

},

{

"type": "object",

"properties": {

"attributes": {

"allOf": [

{

"$ref": "genericNrm.json#/components/schemas/ManagedFunction-Attributes"

},

{

"type": "object",

"properties": {

"gnbId": {

"$ref": "#/components/schemas/GnbId"

},

"gnbIdLength": {

"$ref": "#/components/schemas/GnbIdLength"

}

}

}

]

}

}

},

{

"$ref": "genericNrm.json#/components/schemas/ManagedFunction-ContainingObjects"

},

{

"type": "object",

"properties": {

"EP\_F1C": {

"type": "array",

"items": {

"$ref": "#/components/schemas/EP\_F1C"

}

},

"EP\_F1U": {

"type": "array",

"items": {

"$ref": "#/components/schemas/EP\_F1U"

}

}

}

}

]

},

"ExternalGnbCuCpFunction": {

"allOf": [

{

"$ref": "genericNrm.json#/components/schemas/Top-Attributes"

},

{

"type": "object",

"properties": {

"attributes": {

"allOf": [

{

"$ref": "genericNrm.json#/components/schemas/ManagedFunction-Attributes"

},

{

"type": "object",

"properties": {

"gnbId": {

"$ref": "#/components/schemas/GnbId"

},

"gnbIdLength": {

"$ref": "#/components/schemas/GnbIdLength"

},

"plmnId": {

"$ref": "#/components/schemas/PlmnId"

}

}

}

]

}

}

},

{

"$ref": "genericNrm.json#/components/schemas/ManagedFunction-ContainingObjects"

},

{

"type": "object",

"properties": {

"ExternalNrCellCu": {

"type": "array",

"items": {

"$ref": "#/components/schemas/ExternalNrCellCu"

}

},

"EP\_F1C": {

"type": "array",

"items": {

"$ref": "#/components/schemas/EP\_F1C"

}

},

"EP\_E1": {

"type": "array",

"items": {

"$ref": "#/components/schemas/EP\_E1"

}

},

"EP\_XnC": {

"type": "array",

"items": {

"$ref": "#/components/schemas/EP\_XnC"

}

}

}

}

]

},

"ExternalGnbCuUpFunction": {

"allOf": [

{

"$ref": "genericNrm.json#/components/schemas/Top-Attributes"

},

{

"type": "object",

"properties": {

"attributes": {

"allOf": [

{

"$ref": "genericNrm.json#/components/schemas/ManagedFunction-Attributes"

},

{

"type": "object",

"properties": {

"gnbId": {

"$ref": "#/components/schemas/GnbId"

},

"gnbIdLength": {

"$ref": "#/components/schemas/GnbIdLength"

}

}

}

]

}

}

},

{

"$ref": "genericNrm.json#/components/schemas/ManagedFunction-ContainingObjects"

},

{

"type": "object",

"properties": {

"EP\_E1": {

"type": "array",

"items": {

"$ref": "#/components/schemas/EP\_E1"

}

},

"EP\_F1U": {

"type": "array",

"items": {

"$ref": "#/components/schemas/EP\_F1U"

}

},

"EP\_XnU": {

"type": "array",

"items": {

"$ref": "#/components/schemas/EP\_XnU"

}

}

}

}

]

},

"ExternalAmfFunction": {

"allOf": [

{

"$ref": "genericNrm.json#/components/schemas/Top-Attributes"

},

{

"type": "object",

"properties": {

"attributes": {

"allOf": [

{

"$ref": "genericNrm.json#/components/schemas/ManagedFunction-Attributes"

}

]

}

}

},

{

"$ref": "genericNrm.json#/components/schemas/ManagedFunction-ContainingObjects"

},

{

"type": "object",

"properties": {

"EP\_NgC": {

"type": "array",

"items": {

"$ref": "#/components/schemas/EP\_NgC"

}

}

}

}

]

},

"ExternalUpfFunction": {

"allOf": [

{

"$ref": "genericNrm.json#/components/schemas/Top-Attributes"

},

{

"type": "object",

"properties": {

"attributes": {

"allOf": [

{

"$ref": "genericNrm.json#/components/schemas/ManagedFunction-Attributes"

}

]

}

}

},

{

"$ref": "genericNrm.json#/components/schemas/ManagedFunction-ContainingObjects"

},

{

"type": "object",

"properties": {

"EP\_NgU": {

"type": "array",

"items": {

"$ref": "#/components/schemas/EP\_NgU"

}

}

}

}

]

},

"ExternalNrCellCu": {

"allOf": [

{

"$ref": "genericNrm.json#/components/schemas/Top-Attributes"

},

{

"type": "object",

"properties": {

"attributes": {

"allOf": [

{

"$ref": "genericNrm.json#/components/schemas/ManagedFunction-Attributes"

},

{

"type": "object",

"properties": {

"cellLocalId": {

"type": "integer"

},

"nrPci": {

"$ref": "#/components/schemas/NrPci"

},

"plmnIdList": {

"$ref": "#/components/schemas/PlmnIdList"

},

"nRFrequencyRef": {

"$ref": "genericNrm.json#/components/schemas/Dn"

}

}

}

]

}

}

},

{

"$ref": "genericNrm.json#/components/schemas/ManagedFunction-ContainingObjects"

}

]

},

"NRCellRelation": {

"allOf": [

{

"$ref": "genericNrm.json#/components/schemas/Top-Attributes"

},

{

"type": "object",

"properties": {

"attributes": {

"allOf": [

{

"$ref": "genericNrm.json#/components/schemas/ManagedFunction-Attributes"

},

{

"type": "object",

"properties": {

"nRTCI": {

"type": "integer"

},

"cellIndividualOffset": {

"$ref": "#/components/schemas/CellIndividualOffset"

},

"adjacentNRCellRef": {

"$ref": "genericNrm.json#/components/schemas/Dn"

},

"nRFrequencyRef": {

"$ref": "genericNrm.json#/components/schemas/Dn"

},

"isRemoveAllowed": {

"type": "boolean"

},

"isHOAllowed": {

"type": "boolean"

}

}

}

]

}

}

},

{

"$ref": "genericNrm.json#/components/schemas/ManagedFunction-ContainingObjects"

}

]

},

"NRFreqRelation": {

"allOf": [

{

"$ref": "genericNrm.json#/components/schemas/Top-Attributes"

},

{

"type": "object",

"properties": {

"attributes": {

"allOf": [

{

"$ref": "genericNrm.json#/components/schemas/ManagedFunction-Attributes"

},

{

"type": "object",

"properties": {

"offsetMO": {

"$ref": "#/components/schemas/QOffsetRangeList"

},

"blackListEntry": {

"type": "array",

"items": {

"type": "integer",

"minimum": 0,

"maximum": 1007

}

},

"blackListEntryIdleMode": {

"type": "integer"

},

"cellReselectionPriority": {

"type": "integer"

},

"cellReselectionSubPriority": {

"type": "number",

"minimum": 0.2,

"maximum": 0.8,

"multipleOf": 0.2

},

"pMax": {

"type": "integer",

"minimum": -30,

"maximum": 33

},

"qOffsetFreq": {

"$ref": "#/components/schemas/QOffsetFreq"

},

"qQualMin": {

"type": "number"

},

"qRxLevMin": {

"type": "integer",

"minimum": -140,

"maximum": -44

},

"threshXHighP": {

"type": "integer",

"minimum": 0,

"maximum": 62

},

"threshXHighQ": {

"type": "integer",

"minimum": 0,

"maximum": 31

},

"threshXLowP": {

"type": "integer",

"minimum": 0,

"maximum": 62

},

"threshXLowQ": {

"type": "integer",

"minimum": 0,

"maximum": 31

},

"tReselectionNr": {

"type": "integer",

"minimum": 0,

"maximum": 7

},

"tReselectionNRSfHigh": {

"$ref": "#/components/schemas/TReselectionNRSf"

},

"tReselectionNRSfMedium": {

"$ref": "#/components/schemas/TReselectionNRSf"

},

"nRFrequencyRef": {

"$ref": "genericNrm.json#/components/schemas/Dn"

}

}

}

]

}

}

},

{

"$ref": "genericNrm.json#/components/schemas/ManagedFunction-ContainingObjects"

}

]

},

"NRFrequency": {

"allOf": [

{

"$ref": "genericNrm.json#/components/schemas/Top-Attributes"

},

{

"type": "object",

"properties": {

"attributes": {

"allOf": [

{

"$ref": "genericNrm.json#/components/schemas/ManagedFunction-Attributes"

},

{

"type": "object",

"properties": {

"absoluteFrequencySSB": {

"type": "integer",

"minimum": 0,

"maximum": 3279165

},

"ssbSubCarrierSpacing": {

"$ref": "#/components/schemas/SsbSubCarrierSpacing"

},

"multiFrequencyBandListNR": {

"type": "integer",

"minimum": 1,

"maximum": 256

}

}

}

]

}

}

},

{

"$ref": "genericNrm.json#/components/schemas/ManagedFunction-ContainingObjects"

}

]

},

"ExternalENBFunction": {

"allOf": [

{

"$ref": "genericNrm.json#/components/schemas/Top-Attributes"

},

{

"type": "object",

"properties": {

"attributes": {

"allOf": [

{

"$ref": "genericNrm.json#/components/schemas/ManagedFunction-Attributes"

},

{

"type": "object",

"properties": {

"eNBId": {

"type": "integer"

}

}

}

]

}

}

},

{

"$ref": "genericNrm.json#/components/schemas/ManagedFunction-ContainingObjects"

},

{

"type": "object",

"properties": {

"ExternalEUTranCell": {

"type": "array",

"items": {

"$ref": "#/components/schemas/ExternalEUTranCell"

}

}

}

}

]

},

"ExternalEUTranCell": {

"allOf": [

{

"$ref": "genericNrm.json#/components/schemas/Top-Attributes"

},

{

"type": "object",

"properties": {

"attributes": {

"allOf": [

{

"$ref": "genericNrm.json#/components/schemas/ManagedFunction-Attributes"

},

{

"type": "object",

"properties": {

"EUtranFrequencyRef": {

"$ref": "genericNrm.json#/components/schemas/Dn"

}

}

}

]

}

}

},

{

"$ref": "genericNrm.json#/components/schemas/ManagedFunction-ContainingObjects"

}

]

},

"EUtranCellRelation": {

"allOf": [

{

"$ref": "genericNrm.json#/components/schemas/Top-Attributes"

},

{

"type": "object",

"properties": {

"attributes": {

"allOf": [

{

"$ref": "genericNrm.json#/components/schemas/ManagedFunction-Attributes"

},

{

"type": "object",

"properties": {

"adjacentEUtranCellRef": {

"$ref": "genericNrm.json#/components/schemas/Dn"

}

}

}

]

}

}

},

{

"$ref": "genericNrm.json#/components/schemas/ManagedFunction-ContainingObjects"

}

]

},

"EUtranFreqRelation": {

"allOf": [

{

"$ref": "genericNrm.json#/components/schemas/Top-Attributes"

},

{

"type": "object",

"properties": {

"attributes": {

"allOf": [

{

"$ref": "genericNrm.json#/components/schemas/ManagedFunction-Attributes"

},

{

"type": "object",

"properties": {

"eUTranFrequencyRef": {

"$ref": "genericNrm.json#/components/schemas/Dn"

}

}

}

]

}

}

},

{

"$ref": "genericNrm.json#/components/schemas/ManagedFunction-ContainingObjects"

}

]

},

"EUtranFrequency": {

"allOf": [

{

"$ref": "genericNrm.json#/components/schemas/Top-Attributes"

},

{

"type": "object",

"properties": {

"attributes": {

"allOf": [

{

"$ref": "genericNrm.json#/components/schemas/ManagedFunction-Attributes"

},

{

"type": "object",

"properties": {}

}

]

}

}

},

{

"$ref": "genericNrm.json#/components/schemas/ManagedFunction-ContainingObjects"

}

]

},

"ManagedElement-Single": {

"allOf": [

{

"$ref": "genericNrm.json#/components/schemas/Top-Attributes"

},

{

"type": "object",

"properties": {

"attributes": {

"allOf": [

{

"$ref": "genericNrm.json#/components/schemas/ManagedElement-Attributes"

}

]

}

}

},

{

"$ref": "genericNrm.json#/components/schemas/ManagedElement-ContainingObjects"

},

{

"type": "object",

"properties": {

"GnbDuFunction": {

"type": "array",

"items": {

"$ref": "#/components/schemas/GnbDuFunction"

}

},

"GnbCuCpFunction": {

"type": "array",

"items": {

"$ref": "#/components/schemas/GnbCuCpFunction"

}

},

"GnbCuUpFunction": {

"type": "array",

"items": {

"$ref": "#/components/schemas/GnbCuUpFunction"

}

}

}

}

]

},

"ManagedElement-Multiple": {

"type": "array",

"items": {

"$ref": "#/components/schemas/ManagedElement-Single"

}

},

"SubNetwork-Single": {

"allOf": [

{

"$ref": "genericNrm.json#/components/schemas/Top-Attributes"

},

{

"type": "object",

"properties": {

"attributes": {

"allOf": [

{

"$ref": "genericNrm.json#/components/schemas/SubNetwork-Attributes"

}

]

}

}

},

{

"$ref": "genericNrm.json#/components/schemas/SubNetwork-ContainingObjects"

},

{

"type": "object",

"properties": {

"SubNetwork": {

"$ref": "#/components/schemas/SubNetwork-Multiple"

},

"ManagedElement": {

"$ref": "#/components/schemas/ManagedElement-Multiple"

},

"ExternalGnbCuCpFunction": {

"type": "array",

"items": {

"$ref": "#/components/schemas/ExternalGnbCuCpFunction"

}

},

"ExternalENBFunction": {

"type": "array",

"items": {

"$ref": "#/components/schemas/ExternalENBFunction"

}

},

"NRFrequency": {

"type": "array",

"items": {

"$ref": "#/components/schemas/NRFrequency"

}

},

"EUtranFrequency": {

"type": "array",

"items": {

"$ref": "#/components/schemas/EUtranFrequency"

}

}

}

}

]

},

"SubNetwork-Multiple": {

"type": "array",

"items": {

"$ref": "#/components/schemas/SubNetwork-Single"

}

},

"EP\_RP": {

"allOf": [

{

"$ref": "genericNrm.json#/components/schemas/Top-Attributes"

},

{

"type": "object",

"properties": {

"attributes": {

"type": "object",

"properties": {

"userLabel": {

"type": "string"

},

"farEndEntity": {

"type": "string"

},

"localAddress": {

"$ref": "#/components/schemas/LocalAddress"

},

"remoteAddress": {

"$ref": "#/components/schemas/RemoteAddress"

}

}

}

}

}

]

},

"EP\_E1": {

"$ref": "#/components/schemas/EP\_RP"

},

"EP\_XnC": {

"$ref": "#/components/schemas/EP\_RP"

},

"EP\_XnU": {

"$ref": "#/components/schemas/EP\_RP"

},

"EP\_NgC": {

"$ref": "#/components/schemas/EP\_RP"

},

"EP\_NgU": {

"$ref": "#/components/schemas/EP\_RP"

},

"EP\_F1C": {

"$ref": "#/components/schemas/EP\_RP"

},

"EP\_F1U": {

"$ref": "#/components/schemas/EP\_RP"

},

"EP\_S1U": {

"$ref": "#/components/schemas/EP\_RP"

},

"EP\_X2C": {

"$ref": "#/components/schemas/EP\_RP"

},

"EP\_X2U": {

"$ref": "#/components/schemas/EP\_RP"

},

"MappingSetIDBackhaulAddress": {

"type": "object",

"properties": {

"SetID": {

"type": "string"

},

"GnbId": {

"type": "string"

},

"Tai": {

"type": "string"

}

}

}

}

}

}

|  |
| --- |
| **End of Changes** |