**3GPP TSG-SA5 Meeting #132e *S5-204237rev1***

**e-meeting 17th 28th August 2020**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **32.255** | **CR** | **0247** | **rev** | **1** | **Current version:** | **16.5.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Add PDU Address in for IPv6 multi-homing  |
|  |  |
| ***Source to WG:*** | Huawei  |
| ***Source to TSG:*** | S5 |
|  |  |
| ***Work item code:*** | TEI16, 5GS\_Ph1-DCH |  | ***Date:*** | 2020-08-7 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | 16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | The PDU Addresses per PSA for IPv6 multi-homing is not specified in TS 32.255. |
|  |  |
| ***Summary of change:*** | This contribution is to add PDU Addresses per PSA in Multiple Unit Usage for IPv6 multi-homing, including in the charging data request/response and CDR. |
|  |  |
| ***Consequences if not approved:*** | In IPv6 multi-homing scenario, only one PDU address is reported to CHF, and other PDU addresses are droped by SMF. |
|  |  |
| ***Clauses affected:*** | 6.1.1.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

|  |
| --- |
| **First change to TS 32.255** |

#### 6.1.1.2 Charging Data Request message

Table 6.1.1.2.1 illustrates the basic structure of a Charging Data Request message from the SMF as used for 5G data connectivity converged charging.

Table 6.1.1.2.1: Charging Data Request message contents

| **Information Element** | **Category for converged charging** | **Category for offline only charging** | **Description** |
| --- | --- | --- | --- |
| Session Identifier | OC | OC | Described in TS 32.290 [57] |
| Subscriber Identifier | OM | M | Described in TS 32.290 [57]In case SUPI is not present (for emergency service), the User Equipment Info in table 6.2.1.2.1. shall be present for identifying the user. |
| NF Consumer Identification | M | M | Described in TS 32.290 [57] |
| NF Functionality | M | OC | Described in TS 32.290 [57] |
| NF Name | OC | OC | Described in TS 32.290 [57] |
| NF Address | OC | OC | Described in TS 32.290 [57] |
| NF PLMN ID | OC | OC | Described in TS 32.290 [57] |
| Invocation Timestamp | M | M | Described in TS 32.290 [57] |
| Invocation Sequence Number | M | M | Described in TS 32.290 [57] |
| Notify URI | OC | OC | Described in TS 32.290 [57] |
| Service Specification Information | OC | OC | Described in TS 32.290 [57] |
| Triggers | OC | OC | This field is described in TS 32.290 [57] and holds the 5G data connectivity specific triggers described in clause 5.2.1. |
| Multiple Unit Usage  | OC | OC | Described in TS 32.290 [57]This field is not applicable to QBC. |
| Rating Group | M | M | Described in TS 32.290 [57] |
| Requested Unit | OC | - | Described in TS 32.290 [57] |
| Used Unit Container | OC | OC | Described in TS 32.290 [57] |
| Triggers | OC | OC | This field is described in TS 32.290 [57] and holds the 5G data connectivity specific triggers described in clause 5.2.1.  |
| PDU Container Information  | OC | OC | This field holds the 5G data connectivity PDU session container specific information described in clause 6.2. |
| UPF ID | OC | OC | This field holds the UPF identifier used to identify the UPF.These fields shall only be included when either quota is requested per UPF, or used units are reported per UPF |
| Used multi-homing address | Oc | Oc | This field holds the IPv6 prefix used by PSA to transfer service data flow for the IPv6 multi-homed PDU session. This field presents when UPF ID is presented for multihomed PDU session.This field is included in case of used units report for multi-homing address. |
| PDU Session Charging Information | OM | OM | This field holds the 5G data connectivity specific information described in clause 6.2. |
| Roaming QBC information | OM | OM | This field holds the roaming QBC specific information defined in clause 6.2.1.4This field is not applicable to FBC. |

|  |
| --- |
| **End of Change** |