**3GPP TSG-SA5 Meeting #133e *S5-205141rev4***

**e-meeting 12th – 21st October 2020**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** |  | **rev** |  | **Current version:** | **16.0.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Correct Distributed PCI optimization  |
|  |  |
| ***Source to WG:*** |  Ericsson |
| ***Source to TSG:*** | S5 |
|  |  |
| ***Work item code:*** | SON\_5G |  | ***Date:*** | 2020-10-03 |
|  |  |  |  |  |
| ***Category:*** |  |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | The Use Case and Management Services descriptions for D-SON PCI optimization do not confirm to RAN3 agreements.The PCI reconfiguration is controlled by the CU, as evident from TS 38.473 clause 9.2.1.10, Information Element *NR PCI* |
|  |  |
| ***Summary of change:*** | Correct Use Case and Management Services descriptions for D-SON PCI optimization |
|  |  |
| ***Consequences if not approved:*** | Misalignment with this specification and Stage 2 and Stage 3 in TS 28.541. |
|  |  |
| ***Clauses affected:*** |  6.1.1.4, 6.4.1.4.1, 6.4.1.4.2, 7.1.3.3, 7.1.3.3.1, 8.2.3.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  |  |
| ***affected:*** |  | **X** |  Test specifications |  |
| ***(show related CRs)*** | **X** |  |  O&M Specifications | CR 0385, CR 0386 |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

**First change**

#### 6.1.1.4 PCI configuration and re-configuration

**REQ-DPCI-CONFIG-FUN-1** producer of provisioning MnS should have a capability allowing an authorized consumer to set or update the list(s) of PCI value(s) for NR cell(s).

**REQ-DPCI-CONFIG-FUN-2** producer of provisioning MnS should have a capability allowing an authorized consumer to enable or disable the PCI configuration function.

**REQ-DPCI-CONFIG-FUN-3** producer of provisioning MnS should have a capability to notify the authorized consumer with the PCI value(s) being selected for NR cell(s).

**REQ-DPCI-CONFIG-FUN-4** producer of provisioning MnS should have a capability to notify the authorized consumer about the resolution of PCI collision or PCI confusion problems for NR cells.

**REQ-DPCI-CONFIG-FUN-5** producer of provisioning MnS should have a capability allowing an authorized consumer to configure or re-configure the PCI list at the PCI configuration function.

**Next change**

##### 6.4.1.4.1 Initial PCI configuration

| Use case stage | Evolution/Specification | <<Uses>>Related use |
| --- | --- | --- |
| **Goal**  | To automatically configure the PCI for a NR cell that have not been assigned any PCI. |  |
| **Actors and Roles** | D-SON management function to support initial PCI configuration. |  |
| **Telecom resources** | * gNB;
* The producer of provisioning MnS
 |  |
| **Assumptions** | N/A |  |
| **Pre-conditions** | * The NR cell is not in operation.
* No PCI value has been assigned to the NR cell.
 |  |
| **Begins when**  | The D-SON management function decides to configure the PCI list for a NR cell. |  |
| **Step 1 (M)** | The D-SON management function configures a PCI list to the PCI configuration function using the producer of provisioning MnS. |  |
| **Step 2 (M)** | The D-SON management function requests the producer of provisioning MnS to enable the PCI configuration function for the NR cell. |  |
| **Step 3 (M)** | The PCI configuration function selects a PCI value from the list of PCI values provided by the consumer of provisioning MnS, and configures the NR cell to use this PCI. |  |
| **Step 4 (M)** | The producer of provisioning MnS notifies the consumer about the PCI value assigned to the NR cell.  |  |
| **Ends when**  | All the steps identified above are successfully completed. |  |
| **Exceptions** | One of the steps identified above fails. |  |
| **Post-conditions** | The PCI value of a NR cell has been configured. |  |
| **Traceability**  | **REQ-DPCI-CONFIG-FUN-1, REQ-DPCI-CONFIG-FUN-2, REQ-DPCI-CONFIG-FUN-3, REQ-DPCI-CONFIG-FUN-5** |  |

##### 6.4.1.4.2 PCI re-configuration

| Use case stage | Evolution/Specification | <<Uses>>Related use |
| --- | --- | --- |
| **Goal**  | To automatically re-configure the PCI of an NR cell, due to PCI collision or PCI confusion problems. |  |
| **Actors and Roles** | D-SON management function to support PCI re-configuration. |  |
| **Telecom resources** | * gNB;
* The producer of provisioning MnS
 |  |
| **Assumptions** | N/A |  |
| **Pre-conditions** | * A NR cell has been assigned a PCI value.
* The PCI configuration function is in operation and enabled.
 |  |
| **Begins when**  | The PCI configuration function has detected the PCI problem of a PCI collision or a PCI confusion for an NR cell. |  |
|  |  |  |
| **Step 1 (M)** | The D-SON PCI configuration function re-configures the PCI of that cell using one of the PCI values in the PCI list. |  |
|  |  |  |
| **Step 2 (M)** | The producer of provisioning MnS notifies the consumer about the new PCI value of the NR cell.  |  |
|  |  |  |
| **Ends when**  | All the steps identified above are successfully completed. |  |
| **Exceptions** | One of the steps identified above fails. |  |
| **Post-conditions** | The PCI collision or PCI confusion have been resolved. |  |
| **Traceability**  | **REQ-DPCI-CONFIG-FUN-3, REQ-DPCI-CONFIG-FUN-4, REQ-DPCI-CONFIG-FUN-5** |  |

**Next change**

#### 7.1.3.3 MnS Component Type C definition

No performance management or alarms are available for this service.

##### 7.1.3.3.1 Notification information

The table below lists the notifications related to D-SON PCI configuration.

|  |  |  |
| --- | --- | --- |
| Notifications | Description | Note |
| PCI change notification | When the PCI configuration function changes the PCI of a cell, this change is reported using a notifyMOIAttributeValueChanges notification |  |
| PCI collision notification | The collision notification is used to indicate two neighbouring cells of a serving cell are using the same PCIs. |  |
| PCI confusion notification | The confusion notification is used to indicate that a serving cell has 2 neighbouring cells that are using the same PCI value. |  |

**Next change**

#### 8.2.3.2 PCI re-configuration

Figure 8.2.3.2-1 depicts a procedure that describes how D-SON management function can re-configure the PCI list for NR cell(s) when PCI collision or PCI confusion issues were detected.

**D-SON management consumer**

**Producer of provisioning MnS**

3. *notifyMOIAttributeChange*
 to indicate new PCI value

**PCI configuration function**

2. Indicate that PCI attribute is changed.

1. Detect and correct PCI collision or confusion

Figure 8.2.3.2-1: PCI re-configuration procedure

1. The PCI configuration (D-SON) function detects and corrects the PCI collision or PCI confusion problem for a NR cell. This is done by selecting one PCI value from the PCI list and reconfigure the cell using that PCI value.

2. The PCI configuration (D-SON) function indicates the attribute change to the Producer of provisioning MnS. (NOTE).

3. The Producer of provisioning MnS sends a notification *notifyMOIAttributeValueChange* to the D-SON management function to indicate the new PCI value being assigned to NR cell.

NOTE: The interface between Producer of provisioning MnS and PCI configuration (D-SON) function is not subject to standardization.

**End of changes**