3GPP TSG SA WG5 Meeting 137-e TDoc S5-213126

electronic meeting, online, 10 - 19 May 2021

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **28.623** | **CR** | **0126** | **rev** |  | **Current version:** | **16.7.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **x** | Core Network | **x** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Add IOC for discovery of management services | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | S5 | | | | | | | | | |
| ***Source to TSG:*** | Huawei | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | 5GDMS | | | | |  | ***Date:*** | | | 2021-05-10 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | B |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | As described in 28.533 clause 4.7, MnS data should be stored in the Network Resource Model to allow discovery of management services. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | New IOC and related DataType are added. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | NRM does not support discovery of management services. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | C.4.3 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | Forge link  https://forge.3gpp.org/rep/sa5/MnS/commits/S5-213126\_Rel-17\_CR\_28.623\_Add\_IOC\_for\_discovery\_of\_management\_services | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

|  |
| --- |
| **1st change** |

## C.4.3 OpenAPI document "genericNrm.yaml"

openapi: 3.0.1

info:

title: Generic NRM

version: 16.7.0

description: >-

OAS 3.0.1 definition of the Generic NRM

© 2020, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: 3GPP TS 28.623 V16.7.0; Generic NRM

url: http://www.3gpp.org/ftp/Specs/archive/28\_series/28.623/

paths: {}

components:

schemas:

#-------- Definition of types-----------------------------------------------------

RegistrationState:

type: string

enum:

- REGISTERED

- DEREGISTERED

VnfParameter:

type: object

properties:

vnfInstanceId:

type: string

vnfdId:

type: string

flavourId:

type: string

autoScalable:

type: boolean

SiteLatitude:

type: number

format: float

minimum: -90

maximum: 90

SiteLongitude:

type: number

format: float

minimum: -180

maximum: 180

PeeParameter:

type: object

properties:

siteIdentification:

type: string

siteDescription:

type: string

siteLatitude:

$ref: '#/components/schemas/SiteLatitude'

siteLongitude:

$ref: '#/components/schemas/SiteLongitude'

equipmentType:

type: string

environmentType:

type: string

powerInterface:

type: string

ThresholdInfo:

type: object

properties:

thresholdDirection:

type: string

enum:

- UP

- DOWN

- UP\_AND\_DOWN

thresholdValue:

oneOf:

- type: integer

- $ref: 'comDefs.yaml#/components/schemas/Float'

hysteresis:

oneOf:

- type: integer

minimum: 0

- type: number

format: float

minimum: 0

Operation:

type: object

properties:

name:

type: string

allowedNFTypes:

$ref: '#/components/schemas/NFType'

operationSemantics:

$ref: '#/components/schemas/OperationSemantics'

NFType:

type: string

description: ' NF name defined in TS 23.501'

enum:

- NRF

- UDM

- AMF

- SMF

- AUSF

- NEF

- PCF

- SMSF

- NSSF

- UDR

- LMF

- GMLC

- 5G\_EIR

- SEPP

- UPF

- N3IWF

- AF

- UDSF

- DN

Fqdn:

type: string

OperationSemantics:

type: string

enum:

- REQUEST\_RESPONSE

- SUBSCRIBE\_NOTIFY

SAP:

type: object

properties:

host:

$ref: '#/components/schemas/HostAddr'

port:

type: integer

NFServiceType:

type: string

enum:

- Namf\_Communication

- Namf\_EventExposure

- Namf\_MT

- Namf\_Location

- Nsmf\_PDUSession

- Nsmf\_EventExposure

- Others

HostAddr:

oneOf:

- $ref: '#/components/schemas/Ipv4Addr'

- $ref: '#/components/schemas/Ipv6Addr'

- $ref: '#/components/schemas/Fqdn'

Ipv4Addr:

type: string

pattern: '^(([0-9]|[1-9][0-9]|1[0-9][0-9]|2[0-4][0-9]|25[0-5])\.){3}([0-9]|[1-9][0-9]|1[0-9][0-9]|2[0-4][0-9]|25[0-5])$'

example: '198.51.100.1'

Ipv6Addr:

type: string

allOf:

- pattern: '^((:|(0?|([1-9a-f][0-9a-f]{0,3}))):)((0?|([1-9a-f][0-9a-f]{0,3})):){0,6}(:|(0?|([1-9a-f][0-9a-f]{0,3})))$'

- pattern: '^((([^:]+:){7}([^:]+))|((([^:]+:)\*[^:]+)?::(([^:]+:)\*[^:]+)?))$'

example: '2001:db8:85a3::8a2e:370:7334'

Ipv6Prefix:

type: string

allOf:

- pattern: '^((:|(0?|([1-9a-f][0-9a-f]{0,3}))):)((0?|([1-9a-f][0-9a-f]{0,3})):){0,6}(:|(0?|([1-9a-f][0-9a-f]{0,3})))(\/(([0-9])|([0-9]{2})|(1[0-1][0-9])|(12[0-8])))$'

- pattern: '^((([^:]+:){7}([^:]+))|((([^:]+:)\*[^:]+)?::(([^:]+:)\*[^:]+)?))(\/.+)$'

example: '2001:db8:abcd:12::0/64'

TransportProtocol:

anyOf:

- type: string

enum:

- TCP

- type: string

SupportedPerfMetricGroup:

type: object

properties:

performanceMetrics:

type: array

items:

type: string

granularityPeriods:

type: array

items:

type: integer

minimum: 1

reportingMethods:

type: array

items:

type: string

enum:

- FILE\_BASED\_LOC\_SET\_BY\_PRODUCER

- FILE\_BASED\_LOC\_SET\_BY\_CONSUMER

- STREAM\_BASED

monitorGranularityPeriods:

type: array

items:

type: integer

minimum: 1

ReportingCtrl:

oneOf:

- type: object

properties:

fileReportingPeriod:

type: integer

- type: object

properties:

fileReportingPeriod:

type: integer

fileLocation:

$ref: 'comDefs.yaml#/components/schemas/Uri'

- type: object

properties:

streamTarget:

$ref: 'comDefs.yaml#/components/schemas/Uri'

Scope:

type: object

properties:

scopeType:

type: string

enum:

- BASE\_ONLY

- BASE\_ALL

- BASE\_NTH\_LEVEL

- BASE\_SUBTREE

scopeLevel:

type: integer

#-------- Definition of types used in Trace control NRM fragment------------------

tjJobType-Type:

type: string

description: Specifies whether the TraceJob represents only MDT, Logged MBSFN MDT, Trace or a combined Trace and MDT job. Applicable for Trace, MDT, RCEF and RLF reporting. See 3GPP TS 32.422 clause 5.9a for additional details.

enum:

- IMMEDIATE\_MDT\_ONLY

- LOGGED\_MDT\_ONLY

- TRACE\_ONLY

- IMMEDIATE\_MDT AND TRACE

- RLF\_REPORT\_ONLY

- RCEF\_REPORT\_ONLY

- LOGGED\_MBSFN\_MDT

tjListOfInterfaces-Type:

description: The interfaces to be recorded in the Network Element. See 3GPP TS 32.422 clause 5.5 for additional details.

type: object

properties:

MSCServerInterfaces:

type: array

items:

type: string

enum:

- A

- Iu-CS

- Mc

- MAP-G

- MAP-B

- MAP-E

- MAP-F

- MAP-D

- MAP-C

- CAP

MGWInterfaces:

type: array

items:

type: string

enum:

- Mc

- Nb-UP

- Iu-UP

RNCInterfaces:

type: array

items:

type: string

enum:

- Iu-CS

- Iu-PS

- Iur

- Iub

- Uu

SGSNInterfaces:

type: array

items:

type: string

enum:

- Gb

- Iu-PS

- Gn

- MAP-Gr

- MAP-Gd

- MAP-Gf

- Ge

- Gs

- S6d

- S4

- S3

- S13

GGSNInterfaces:

type: array

items:

type: string

enum:

- Gn

- Gi

- Gmb

S-CSCFInterfaces:

type: array

items:

type: string

enum:

- Mw

- Mg

- Mr

- Mi

P-CSCFInterfaces:

type: array

items:

type: string

enum:

- Gm

- Mw

I-CSCFInterfaces:

type: array

items:

type: string

enum:

- Cx

- Dx

- Mg

- Mw

MRFCInterfaces:

type: array

items:

type: string

enum:

- Mp

- Mr

MGCFInterfaces:

type: array

items:

type: string

enum:

- Mg

- Mj

- Mn

IBCFInterfaces:

type: array

items:

type: string

enum:

- Ix

- Mx

E-CSCFInterfaces:

type: array

items:

type: string

enum:

- Mw

- Ml

- Mm

- Mi/Mg

BGCFInterfaces:

type: array

items:

type: string

enum:

- Mi

- Mj

- Mk

ASInterfaces:

type: array

items:

type: string

enum:

- Dh

- Sh

- ISC

- Ut

HSSInterfaces:

type: array

items:

type: string

enum:

- MAP-C

- MAP-D

- Gc

- Gr

- Cx

- S6d

- S6a

- Sh

EIRInterfaces:

type: array

items:

type: string

enum:

- MAP-F

- S13

- MAP-Gf

BM-SCInterfaces:

type: array

items:

type: string

enum:

- Gmb

MMEInterfaces:

type: array

items:

type: string

enum:

- S1-MME

- S3

- S6a

- S10

- S11

- S13

SGWInterfaces:

type: array

items:

type: string

enum:

- S4

- S5

- S8

- S11

- Gxc

PDN\_GWInterfaces:

type: array

items:

type: string

enum:

- S2a

- S2b

- S2c

- S5

- S6b

- Gx

- S8

- SGi

eNBInterfaces:

type: array

items:

type: string

enum:

- S1-MME

- X2

en-gNBInterfaces:

type: array

items:

type: string

enum:

- S1-MME

- X2

- Uu

- F1-C

- E1

AMFInterfaces:

type: array

items:

type: string

enum:

- N1

- N2

- N8

- N11

- N12

- N14

- N15

- N20

- N22

- N26

AUSFInterfaces:

type: array

items:

type: string

enum:

- N12

- N13

NEFInterfaces:

type: array

items:

type: string

enum:

- N29

- N30

- N33

NRFInterfaces:

type: array

items:

type: string

enum:

- N27

NSSFInterfaces:

type: array

items:

type: string

enum:

- N22

- N31

PCFInterfaces:

type: array

items:

type: string

enum:

- N5

- N7

- N15

SMFInterfaces:

type: array

items:

type: string

enum:

- N4

- N7

- N10

- N11

- S5-C

SMSFInterfaces:

type: array

items:

type: string

enum:

- N20

- N21

UDMInterfaces:

type: array

items:

type: string

enum:

- N8

- N10

- N13

- N21

UPFInterfaces:

type: array

items:

type: string

enum:

- N4

ng-eNBInterfaces:

type: array

items:

type: string

enum:

- NG-C

- Xn-C

- Uu

gNB-CU-CPInterfaces:

type: array

items:

type: string

enum:

- NG-C

- Xn-C

- Uu

- F1-C

- E1

- X2-C

gNB-CU-UPInterfaces:

type: array

items:

type: string

enum:

- E1

gNB-DUInterfaces:

type: array

items:

type: string

enum:

- F1-C

tjListOfNeTypes-Type:

description: The Network Element types where Trace Session activation is needed. See 3GPP TS 32.422 clause 5.4 for additional details.

type: array

items:

type: string

enum:

- MSC\_SERVER

- SGSN

- MGW

- GGSN

- RNC

- BM\_SC

- MME

- SGW

- PGW

- ENB

- EN\_GNB

- GNB\_CU\_CP

- GNB\_CU\_UP

- GNB\_DU

tjPLMNTaget-Type:

type: object

description: The PLMN for which sessions shall be selected in the Trace Session in case of management based activation when several PLMNs are supported in the RAN (this means that shared cells and not shared cells are allowed for the specified PLMN. Note that the PLMN Target might differ from the PLMN specified in the Trace Reference, as that specifies the PLMN that is containing the management system requesting the Trace Session from the NE. See 3GPP TS 32.422 clause 5.9b for additional details.

properties:

mcc:

$ref: 'comDefs.yaml#/components/schemas/Mcc'

mnc:

$ref: 'comDefs.yaml#/components/schemas/Mnc'

required:

- mcc

- mnc

tjStreamingTraceConsumerURI-Type:

type: string

description: The URI of the Trace Reporting MnS consumer (see 3GPP TS 28.532) to which the Trace records shall be sent. See 3GPP TS 32.422 clause 5.9 for additional details.

format: uri

tjTraceCollectionEntityAddress-Type:

description: The IP address to which the Trace records shall be transferred. See 3GPP TS 32.422 clause 5.9 for additional details.

oneOf:

- $ref: '#/components/schemas/Ipv4Addr'

- $ref: '#/components/schemas/Ipv6Addr'

tjTraceDepth-Type:

description: Specifies how detailed information should be recorded in the Network Element. The Trace Depth is a paremeter for Trace Session level, i.e., the Trace Depth is the same for all of the NEs to be traced in the same Trace Session. See 3GPP TS 32.422 clause 5.3 for additional details.

type: string

enum:

- MINIMUM

- MEDIUM

- MAXIMUM

- VENDORMINIMUM

- VENDORMEDIUM

- VENDORMAXIMUM

tjTraceReference-Type:

type: object

description: The Trace Reference parameter shall be globally unique, therefore the Trace Reference shall compose as follows - MCC+MNC+Trace ID, where the MCC and MNC are coming with the Trace activation request from the management system to identify one PLMN containing the management system, and Trace ID is a 3 byte Octet String. See 3GPP TS 32.422 clause 5.6 for additional details.

properties:

mcc:

$ref: 'comDefs.yaml#/components/schemas/Mcc'

mnc:

$ref: 'comDefs.yaml#/components/schemas/Mnc'

traceId:

type: integer

required:

- mcc

- mnc

- traceId

tjTraceReportingFormat-Type:

type: string

description: Specifies whether file-based or streaming reporting shall be used for this Trace Session. See 3GPP TS 32.422 clause 5.11 for additional details.

enum:

- FILE-BASED

- STREAMING

tjTraceTarget-Type:

type: object

description: Trace target conveying both the type and value of the target ID. For additional details see 3GPP TS 32.422

properties:

TargetIdType:

type: string

enum:

- IMSI

- IMEI

- IMEISV

- PUBLIC\_ID

- UTRAN\_CELL

- E-UTRAN\_CELL

- NG-RAN\_CELL

- eNB

- RNC

- gNB

- SUPI

TargetIdValue:

type: string

required:

- TargetIdType

- TargetIdValue

tjTriggeringEvent-Type:

type: object

description: Specifies when to start a Trace Recording Session and which message shall be recorded first, when to stop a Trace Recording Session and which message shall be recorded last respectively. See 3GPP TS 32.422 clause 5.1 for additional detials.

properties:

NetworkElement:

type: string

enum:

- MSC\_SERVER

- SGSN

- MGW

- GGSN

- BM\_SC

- MME

- SGW

- PGW

- AMF

- SMF

- PCF

- UPF

EventBitmap:

type: integer

required:

- NetworkElement

- EventBitmap

tjMDTAnonymizationOfData-Type:

description: Specifies level of MDT anonymization. For additional details see 3GPP TS 32.422 clause 5.10.12.

type: string

enum:

- NO\_IDENTITY

- TAC\_OF\_IMEI

tjMDTAreaConfigurationForNeighCell-Type:

description: Used for logged NR MDT and defines the area for which UE is requested to perform measurement logging for neighbour cells which have list of frequencies. For additional details see 3GPP TS 32.422 clause 5.10.26.

type: array

items:

type: object

properties:

frequency:

type: string

cell:

type: string

tjMDTAreaScope-Type:

description: defines the area in terms or Cells or Tracking Area/Routing Area/Location Area where the MDT data collection shall take place. For additional details see 3GPP TS 32.422 clause 5.10.2.

allOf:

- $ref: 'comDefs.yaml#/components/schemas/DnList'

tjMDTCollectionPeriodRrmLte-Type:

description: See details in 3GPP TS 32.422 clause 5.10.20.

type: string

enum:

- 250ms

- 500ms

- 1000ms

- 2000ms

- 3000ms

- 4000ms

- 6000ms

- 8000ms

- 12000ms

- 16000ms

- 20000ms

- 24000ms

- 28000ms

- 32000ms

- 64000ms

tjMDTCollectionPeriodRrmUmts-Type:

description: See details in 3GPP TS 32.422 clause 5.10.21.

type: string

enum:

- 1024ms

- 1280ms

- 2048ms

- 2560ms

- 5120ms

- 10240ms

- 1min

tjMDTCollectionPeriodRrmNR-Type:

description: See details in 3GPP TS 32.422 clause 5.10.30.

type: string

enum:

- 1024ms

- 1280ms

- 2048ms

- 5120ms

- 10240ms

- 60000ms

tjMDTEventListForTriggeredMeasurement-Type:

description: See details in 3GPP TS 32.422 clause 5.10.28.

type: string

enum:

- OUT\_OF\_COVERAGE

- A2\_EVENT

tjMDTEventThreshold-Type:

description: See details in 3GPP TS 32.422 clause 5.10.7, 5.10.7a, 5.10.13 and 5.10.14.

type: object

properties:

EventThresholdRSRP:

type: integer

minimum: 0

maximum: 97

EventThresholdRSRQ:

type: integer

minimum: 0

maximum: 34

EventThreshold1F:

type: object

properties:

CPICH\_RSCP:

type: integer

minimum: -120

maximum: 25

CPICH\_EcNo:

type: integer

minimum: -24

maximum: 0

PathLoss:

type: integer

minimum: 30

maximum: 165

EventThreshold1I:

type: integer

minimum: -120

maximum: 25

tjMDTListOfMeasurements-Type:

description: See details in 3GPP TS 32.422 clause 5.10.3 for details.

type: object

properties:

UMTS:

type: array

items:

type: string

enum:

- M1

- M2

- M3

- M4

- M5

- M6\_DL

- M6\_UL

- M7\_DL

- M7\_UL

LTE:

type: array

items:

type: string

enum:

- M1

- M2

- M3

- M4

- M5

- M1\_EVENT\_TRIGGERED

- M6

- M7

- M8

- M9

NR:

type: array

items:

type: string

enum:

- M1

- M2

- M3

- M4

- M5

- M6

- M7

- M8

- M9

tjMDTLoggingDuration-Type:

description: See details in 3GPP TS 32.422 clause 5.10.9.

type: string

enum:

- 600s

- 1200s

- 2400s

- 3600s

- 5400s

- 7200s

tjMDTLoggingInterval-Type:

description: See details in 3GPP TS 32.422 clause 5.10.8.

type: string

enum:

- 1.28s

- 2.56s

- 5.12s

- 10.24s

- 20.48s

- 30.72s

- 40.96s

- 61.44s

tjMDTMBSFNAreaList-Type:

description: See details in 3GPP TS 32.422 clause 5.10.25.

type: array

items:

type: object

properties:

mbsfnAreaId:

type: integer

minimum: 1

earfcn:

type: integer

minimum: 1

required:

- mbsfnAreaId

- earfcn

tjMDTMeasurementPeriodLTE-Type:

description: See details in 3GPP TS 32.422 clause 5.10.23.

type: string

enum:

- 1024ms

- 1280ms

- 2048ms

- 2560ms

- 5120ms

- 10240ms

- 1min

tjMDTMeasurementPeriodUMTS-Type:

description: See details in 3GPP TS 32.422 clause 5.10.22.

type: string

enum:

- 250ms

- 500ms

- 1000ms

- 2000ms

- 3000ms

- 4000ms

- 6000ms

- 8000ms

- 12000ms

- 16000ms

- 20000ms

- 24000ms

- 28000ms

- 32000ms

- 64000ms

tjMDTMeasurementQuantity-Type:

description: See details in 3GPP TS 32.422 clause 5.10.15.

type: string

enum:

- CPICH\_EcNo

- CPICH\_RSCP

- PathLoss

tjMDTPLMList-Type:

description: See details in 3GPP TS 32.422 clause 5.10.24.

type: array

items:

type: object

properties:

mcc:

$ref: 'comDefs.yaml#/components/schemas/Mcc'

mnc:

$ref: 'comDefs.yaml#/components/schemas/Mnc'

required:

- mcc

- mnc

maxItems: 16

tjMDTPositioningMethod-Type:

description: See details in 3GPP TS 32.422 clause 5.10.19.

type: string

enum:

- GNSS

- E-CELL\_ID

tjMDTReportAmount-Type:

description: See details in 3GPP TS 32.422 clause 5.10.6.

type: string

enum:

- 1

- 2

- 4

- 8

- 16

- 32

- 64

- INFINITY

tjMDTReportingTrigger-Type:

description: See details in 3GPP TS 32.422 clause 5.10.4.

type: array

items:

type: string

enum:

- PERIODICAL

- A2\_FOR\_LTE

- 1F\_FOR\_UMTS

- 1I\_FOR\_UMTS\_MCPS\_TDD

- A2\_TRIGGERED\_PERIODIC\_FOR\_LTE

- ALL\_CONFIGURED\_RRM\_FOR\_LTE

- ALL\_CONFIGURED\_RRM\_FOR\_UMTS

tjMDTReportInterval-Type:

description: See details in 3GPP TS 32.422 clause 5.10.5.

type: string

enum:

- 250ms

- 500ms

- 1000ms

- 2000ms

- 3000ms

- 4000ms

- 6000ms

- 8000ms

- 12000ms

- 16000ms

- 20000ms

- 24000ms

- 28000ms

- 32000ms

- 64000ms

- 120ms

- 240ms

- 480ms

- 640ms

- 1024ms

- 2048ms

- 5120ms

- 10240ms

- 60000ms

- 360000ms

- 720000ms

- 1800000ms

- 3600000ms

tjMDTReportType-Type:

description: Report type for logged NR MDT. See details in 3GPP TS 32.422 clause 5.10.27.

type: string

enum:

- PERIODICAL

- EVENT\_TRIGGERED

tjMDTSensorInformation-Type:

description: See details in 3GPP TS 32.422 clause 5.10.29.

type: array

items:

type: string

enum:

- BAROMETRIC\_PRESSURE

- UE\_SPEED

- UE\_ORIENTATION

tjMDTTraceCollectionEntityID-Type:

description: See details in 3GPP TS 32.422 clause 5.10.11. Only tceID value may be sent over the air to the UE being configured for Logged MDT.

type: object

properties:

tceID:

type: integer

tcePLMN:

type: object

properties:

mcc:

$ref: 'comDefs.yaml#/components/schemas/Mcc'

mnc:

$ref: 'comDefs.yaml#/components/schemas/Mnc'

required:

- mcc

- mnc

tceAddress:

oneOf:

- $ref: '#/components/schemas/tjTraceCollectionEntityAddress-Type'

- $ref: '#/components/schemas/tjStreamingTraceConsumerURI-Type'

required:

- tceID

- tcePLMN

- tceAddress

#-------- end of Definition of types used in Trace control NRM fragment ----------

#-------- Definition of abstract IOC Top -----------------------------------------

Top-Attr:

# This definition will be deprecated, when all occurances of Top-Attr

# are replaced by Top.

type: object

properties:

id:

type: string

VsDataContainer:

$ref: '#/components/schemas/VsDataContainer-Multiple'

Top:

type: object

properties:

id:

type: string

VsDataContainer:

$ref: '#/components/schemas/VsDataContainer-Multiple'

#-------- Definition of IOCs with new name-containments defined in other TS ------

SubNetwork-Attr:

type: object

properties:

dnPrefix:

type: string

userLabel:

type: string

userDefinedNetworkType:

type: string

setOfMcc:

type: array

items:

$ref: 'comDefs.yaml#/components/schemas/Mcc'

priorityLabel:

type: integer

supportedPerfMetricGroups:

type: array

items:

$ref: '#/components/schemas/SupportedPerfMetricGroup'

ManagedElement-Attr:

type: object

properties:

dnPrefix:

type: string

managedElementTypeList:

type: array

items:

type: string

userLabel:

type: string

locationName:

type: string

managedBy:

$ref: 'comDefs.yaml#/components/schemas/DnList'

vendorName:

type: string

userDefinedState:

type: string

swVersion:

type: string

priorityLabel:

type: integer

supportedPerfMetricGroups:

type: array

items:

$ref: '#/components/schemas/SupportedPerfMetricGroup'

SubNetwork-ncO:

type: object

properties:

ManagementNode:

$ref: '#/components/schemas/ManagementNode-Multiple'

MeContext:

$ref: '#/components/schemas/MeContext-Multiple'

PerfMetricJob:

$ref: '#/components/schemas/PerfMetricJob-Multiple'

ThresholdMonitor:

$ref: '#/components/schemas/ThresholdMonitor-Multiple'

NtfSubscriptionControl:

$ref: '#/components/schemas/NtfSubscriptionControl-Multiple'

TraceJob:

$ref: '#/components/schemas/TraceJob-Multiple'

AlarmList:

$ref: '#/components/schemas/AlarmList-Single'

MnsRegistry:

$ref: '#/components/schemas/MnsRegistry'

ManagedElement-ncO:

type: object

properties:

PerfMetricJob:

$ref: '#/components/schemas/PerfMetricJob-Multiple'

ThresholdMonitor:

$ref: '#/components/schemas/ThresholdMonitor-Multiple'

NtfSubscriptionControl:

$ref: '#/components/schemas/NtfSubscriptionControl-Multiple'

TraceJob:

$ref: '#/components/schemas/TraceJob-Multiple'

AlarmList:

$ref: '#/components/schemas/AlarmList-Single'

#-------- Definition of abstract IOCs --------------------------------------------

ManagedFunction-Attr:

type: object

properties:

userLabel:

type: string

vnfParametersList:

type: array

items:

$ref: '#/components/schemas/VnfParameter'

peeParametersList:

type: array

items:

$ref: '#/components/schemas/PeeParameter'

priorityLabel:

type: integer

supportedPerfMetricGroups:

type: array

items:

$ref: '#/components/schemas/SupportedPerfMetricGroup'

EP\_RP-Attr:

type: object

properties:

userLabel:

type: string

farEndEntity:

type: string

supportedPerfMetricGroups:

type: array

items:

$ref: '#/components/schemas/SupportedPerfMetricGroup'

TraceJob-Attr:

type: object

description: abstract class used as a container of all TraceJob attributes

properties:

tjJobType:

$ref: '#/components/schemas/tjJobType-Type'

tjListOfInterfaces:

$ref: '#/components/schemas/tjListOfInterfaces-Type'

tjListOfNeTypes:

$ref: '#/components/schemas/tjListOfNeTypes-Type'

tjPLMNTarget:

$ref: '#/components/schemas/tjPLMNTaget-Type'

tjTraceConsumer:

oneOf:

- $ref: '#/components/schemas/tjStreamingTraceConsumerURI-Type'

- $ref: '#/components/schemas/tjTraceCollectionEntityAddress-Type'

tjTraceDepth:

$ref: '#/components/schemas/tjTraceDepth-Type'

tjTraceReference:

$ref: '#/components/schemas/tjTraceReference-Type'

tjTraceReportingFormat:

$ref: '#/components/schemas/tjTraceReportingFormat-Type'

tjTraceTarget:

$ref: '#/components/schemas/tjTraceTarget-Type'

tjTriggeringEvent:

$ref: '#/components/schemas/tjTriggeringEvent-Type'

tjMDTAnonymizationOfData:

$ref: '#/components/schemas/tjMDTAnonymizationOfData-Type'

tjMDTAreaConfigurationForNeighCell:

$ref: '#/components/schemas/tjMDTAreaConfigurationForNeighCell-Type'

tjMDTAreaScope:

$ref: '#/components/schemas/tjMDTAreaScope-Type'

tjMDTCollectionPeriodRrmLte:

$ref: '#/components/schemas/tjMDTCollectionPeriodRrmLte-Type'

tjMDTCollectionPeriodRrmUmts:

$ref: '#/components/schemas/tjMDTCollectionPeriodRrmUmts-Type'

tjMDTCollectionPeriodRrmNR:

$ref: '#/components/schemas/tjMDTCollectionPeriodRrmNR-Type'

tjMDTEventListForTriggeredMeasurement:

$ref: '#/components/schemas/tjMDTEventListForTriggeredMeasurement-Type'

tjMDTEventThreshold:

$ref: '#/components/schemas/tjMDTEventThreshold-Type'

tjMDTListOfMeasurements:

$ref: '#/components/schemas/tjMDTListOfMeasurements-Type'

tjMDTLoggingDuration:

$ref: '#/components/schemas/tjMDTLoggingDuration-Type'

tjMDTLoggingInterval:

$ref: '#/components/schemas/tjMDTLoggingInterval-Type'

tjMDTMBSFNAreaList:

$ref: '#/components/schemas/tjMDTMBSFNAreaList-Type'

tjMDTMeasurementPeriodLTE:

$ref: '#/components/schemas/tjMDTMeasurementPeriodLTE-Type'

tjMDTMeasurementPeriodUMTS:

$ref: '#/components/schemas/tjMDTMeasurementPeriodUMTS-Type'

tjMDTMeasurementQuantity:

$ref: '#/components/schemas/tjMDTMeasurementQuantity-Type'

tjMDTPLMList:

$ref: '#/components/schemas/tjMDTPLMList-Type'

tjMDTPositioningMethod:

$ref: '#/components/schemas/tjMDTPositioningMethod-Type'

tjMDTReportAmount:

$ref: '#/components/schemas/tjMDTReportAmount-Type'

tjMDTReportingTrigger:

$ref: '#/components/schemas/tjMDTReportingTrigger-Type'

tjMDTReportInterval:

$ref: '#/components/schemas/tjMDTReportInterval-Type'

tjMDTReportType:

$ref: '#/components/schemas/tjMDTReportType-Type'

tjMDTSensorInformation:

$ref: '#/components/schemas/tjMDTSensorInformation-Type'

tjMDTTraceCollectionEntityID:

$ref: '#/components/schemas/tjMDTTraceCollectionEntityID-Type'

required:

- tjJobType

- tjTraceReference

- tjTraceConsumer

- tjTraceReportingFormat

- tjTraceTarget

ManagedFunction-ncO:

type: object

properties:

PerfMetricJob:

$ref: '#/components/schemas/PerfMetricJob-Multiple'

ThresholdMonitor:

$ref: '#/components/schemas/ThresholdMonitor-Multiple'

ManagedNFService:

$ref: '#/components/schemas/ManagedNFService-Multiple'

TraceJob:

$ref: '#/components/schemas/TraceJob-Multiple'

MnsRegistry:

type: object

properties:

attributes:

$ref: '#/components/schemas/MnsData-Multiple'

#-------- Definition of concrete IOCs --------------------------------------------

VsDataContainer-Single:

type: object

properties:

id:

type: string

attributes:

type: object

properties:

vsDataType:

type: string

vsDataFormatVersion:

type: string

vsData:

nullable: true

VsDataContainer:

$ref: '#/components/schemas/VsDataContainer-Multiple'

ManagedNFService-Single:

allOf:

- $ref: '#/components/schemas/Top'

- type: object

properties:

attributes:

type: object

properties:

userLabel:

type: string

nFServiceType:

$ref: '#/components/schemas/NFServiceType'

sAP:

$ref: '#/components/schemas/SAP'

operations:

type: array

items:

$ref: '#/components/schemas/Operation'

administrativeState:

$ref: 'comDefs.yaml#/components/schemas/AdministrativeState'

operationalState:

$ref: 'comDefs.yaml#/components/schemas/OperationalState'

usageState:

$ref: 'comDefs.yaml#/components/schemas/UsageState'

registrationState:

$ref: '#/components/schemas/RegistrationState'

ManagementNode-Single:

allOf:

- $ref: '#/components/schemas/Top'

- type: object

properties:

attributes:

type: object

properties:

userLabel:

type: string

managedElements:

$ref: 'comDefs.yaml#/components/schemas/DnList'

vendorName:

type: string

userDefinedState:

type: string

locationName:

type: string

swVersion:

type: string

MeContext-Single:

allOf:

- $ref: '#/components/schemas/Top'

- type: object

properties:

attributes:

type: object

properties:

dnPrefix:

type: string

PerfMetricJob-Single:

allOf:

- $ref: '#/components/schemas/Top'

- type: object

properties:

attributes:

type: object

properties:

administrativeState:

$ref: 'comDefs.yaml#/components/schemas/AdministrativeState'

operationalState:

$ref: 'comDefs.yaml#/components/schemas/OperationalState'

jobId:

type: string

performanceMetrics:

type: array

items:

type: string

granularityPeriod:

type: integer

minimum: 1

objectInstances:

$ref: 'comDefs.yaml#/components/schemas/DnList'

rootObjectInstances:

$ref: 'comDefs.yaml#/components/schemas/DnList'

reportingCtrl:

$ref: '#/components/schemas/ReportingCtrl'

ThresholdMonitor-Single:

allOf:

- $ref: '#/components/schemas/Top'

- type: object

properties:

attributes:

type: object

properties:

administrativeState:

$ref: 'comDefs.yaml#/components/schemas/AdministrativeState'

operationalState:

$ref: 'comDefs.yaml#/components/schemas/OperationalState'

performanceMetrics:

type: array

items:

type: string

thresholdInfoList:

type: array

items:

$ref: '#/components/schemas/ThresholdInfo'

monitorGranularityPeriod:

type: integer

minimum: 1

objectInstances:

$ref: 'comDefs.yaml#/components/schemas/DnList'

rootObjectInstances:

$ref: 'comDefs.yaml#/components/schemas/DnList'

NtfSubscriptionControl-Single:

allOf:

- $ref: '#/components/schemas/Top'

- type: object

properties:

attributes:

type: object

properties:

notificationRecipientAddress:

$ref: 'comDefs.yaml#/components/schemas/Uri'

notificationTypes:

type: array

items:

$ref: 'comDefs.yaml#/components/schemas/NotificationType'

scope:

$ref: '#/components/schemas/Scope'

notificationFilter:

type: string

HeartbeatControl:

$ref: '#/components/schemas/HeartbeatControl-Single'

HeartbeatControl-Single:

allOf:

- $ref: '#/components/schemas/Top'

- type: object

properties:

attributes:

type: object

properties:

heartbeatNtfPeriod:

type: integer

triggerHeartbeatNtf:

type: boolean

TraceJob-Single:

allOf:

- $ref: '#/components/schemas/Top'

- type: object

properties:

attributes:

$ref: '#/components/schemas/TraceJob-Attr'

AlarmList-Single:

allOf:

- $ref: '#/components/schemas/Top'

- type: object

properties:

attributes:

type: object

properties:

administrativeState:

$ref: 'comDefs.yaml#/components/schemas/AdministrativeState'

operationalState:

$ref: 'comDefs.yaml#/components/schemas/OperationalState'

numOfAlarmRecords:

type: integer

lastModification:

$ref: 'comDefs.yaml#/components/schemas/DateTime'

alarmRecords:

description: >-

This resource represents a map of alarm records.

The alarmIds are used as keys in the map.

type: object

additionalProperties:

$ref: 'faultMnS.yaml#/components/schemas/AlarmRecord'

MnsData-Single:

allOf:

- $ref: '#/components/schemas/Top'

- type: object

properties:

attributes:

type: object

properties:

mnsLabel:

type: string

mnsType:

type: string

mnsVersion:

type: string

componentTypeAAddress:

type: string

componentTypeBAddress:

type: string

#-------- Definition of YAML arrays for name-contained IOCs ----------------------

VsDataContainer-Multiple:

type: array

items:

$ref: '#/components/schemas/VsDataContainer-Single'

ManagedNFService-Multiple:

type: array

items:

$ref: '#/components/schemas/ManagedNFService-Single'

ManagementNode-Multiple:

type: array

items:

$ref: '#/components/schemas/ManagementNode-Single'

MeContext-Multiple:

type: array

items:

$ref: '#/components/schemas/MeContext-Single'

PerfMetricJob-Multiple:

type: array

items:

$ref: '#/components/schemas/PerfMetricJob-Single'

ThresholdMonitor-Multiple:

type: array

items:

$ref: '#/components/schemas/ThresholdMonitor-Single'

TraceJob-Multiple:

type: array

items:

$ref: '#/components/schemas/TraceJob-Single'

NtfSubscriptionControl-Multiple:

type: array

items:

$ref: '#/components/schemas/NtfSubscriptionControl-Single'

MnsData-Multiple:

type: array

items:

$ref: '#/components/schemas/MnsData-Single'

#-------- Definitions in TS 28.623 for TS 28.532 ---------------------------------

resources-genericNrm:

oneOf:

- $ref: '#/components/schemas/VsDataContainer-Single'

- $ref: '#/components/schemas/ManagementNode-Single'

- $ref: '#/components/schemas/MeContext-Single'

- $ref: '#/components/schemas/ManagedNFService-Single'

- $ref: '#/components/schemas/PerfMetricJob-Single'

- $ref: '#/components/schemas/ThresholdMonitor-Single'

- $ref: '#/components/schemas/TraceJob-Single'

- $ref: '#/components/schemas/NtfSubscriptionControl-Single'

- $ref: '#/components/schemas/HeartbeatControl-Single'

- $ref: '#/components/schemas/AlarmList-Single'

|  |
| --- |
| **End of changes** |