**3GPP TSG-SA5 Meeting #137e *S5-213255rev1***

**electronic meeting, online, 10 - 19 May 2021** Revision of S5-20xxxx

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v11.4* | | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | | |
|  | | | | | | | | | |
|  | **32.255** | **CR** | **0308** | **rev** | **1** | **Current version:** | **17.1.1** |  |
|  | | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | | |
|  | | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Remove the editor's note about the usage reporting | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Huawei | | | | | | | | | |
| ***Source to TSG:*** | S5 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | 5G\_URLLC | | | | |  | ***Date:*** | | | 2021-04-14 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) Rel-12 (Release 12)* *Rel-13 (Release 13) Rel-14 (Release 14) Rel-15 (Release 15) Rel-16 (Release 16)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | As per TS 23.501 and TS 23.502, for the URLLC charging, the redundant transmission at transport layer is the redundancy of PDU sessions.and redundant transmission on the N3/N9 interface is the redundancy of QoS flows.The corresponding description should be added for each redundant transmission type. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Clarify the usage reporting of the redundant transmission at transport layer and N3/N9 interface.  Remove the editor’s note. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Can not support the URLLC service charging. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.2.1.12 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |

|  |
| --- |
| **First change** |

#### 5.2.1.12 URLLC Charging

The CHF can be aware of redundant transmission type (i.e.dual connectivity, redundant transmission on N3/N9 and redundant transmission at transport layer) and provide the quota allocation based on the redundant transmission type:

* For dual connectivity based end to end redundant user plane paths, the granted quotas is allocated for each PDU session.
* For the redundant transmission on N3/N9 interfaces and at transport layer, the CHF grants the quota for the non-redundant transmission.

The SMF shall collect and report the usage for the redundant transmission as the following:

* For dual connectivity based end to end Redundant User Plane Paths, SMF shall collect and report the usage for each redundant PDU session.

Editor’s note: the definition of "non-redundant transmission" is ffs

Editor’s note: the usage reporting for the redundant transmission at transport layer and N3/N9 interface is ffs.

|  |
| --- |
| **End of change** |