**3GPP TSG SA WG5 Meeting #137e S5-213288**

**Online, , 10 May 2021- 19 May 2021**

**Source: Samsung**

**Title: S5-213288 pCR TS 28.312 IntentExpectation Datatype definition**

**Document for: Approval**

**Agenda Item: 6.5.2**

# 1 Decision/action requested

***The group is asked to discuss and approve the proposals.***

# 2 References

None

# 3 Rationale

This contribution provides the concrete IntentExpectation definition.

# 4 Detailed proposal

|  |
| --- |
| **1st modified section** |

#### 6.2.1.2.x serviceProvExpectation <<IOC>>

#### 6.2.1.2.x.1 Definition

This data type defines the expectation for a service deployment intent.

#### 6.2.1.2.x.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
|  |  |  |  |  |  |
| serviceProfile | M | T | T | T | T |
| serviceAccessibility | O | T | T | T | T |
| geoLocation | CM | T | T | T | T |

#### 6.2.1.2.x.3 Attribute constraints

|  |  |
| --- | --- |
| Name | Definition |
|  |  |
|  |  |

**Editor note: Expectation to be modelled as IOC or datatype to be revisited.**

#### 6.2.1.2.x.4 Notifications

TBD

|  |
| --- |
| **End of 1st modified section** |

|  |
| --- |
| **End of 2nd modified section** |

#### 6.2.1.3.z ServiceAva <<dataType>>

#### 6.2.1.3.z.1 Definition

This data type defines the time deration when the service will be available.

#### 6.2.1.3.z.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| startTime | M | T | T | T | T |
| endTime | M | T | T | T | T |

#### 6.2.1.3.z.3 Attribute constraints

None

#### 6.2.1.3.z.4 Notifications

TBD

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |

|  |  |
| --- | --- |
|  |  |
|  |  |
|  |  |

|  |
| --- |
| **End of 2nd modified section** |

|  |
| --- |
| **3rd modified section** |

#### 6.2.1.4 Attribute definition

| Attribute Name | Documentation and Allowed Values | Properties |
| --- | --- | --- |
| userLabel | A user-friendly (and user assignable) name of the intent.allowedValues: Not Applicable | type: Stringmultiplicity: 1isOrdered: FisUnique: FdefaultValue: NoneisNullable: False |
| intentExpectation | It indicates the expectations including requirements, goals and constraints given to a 3GPP system.The intentExpectation includes the intentAreas which describes a list of coverage areas for the intent to be applied.Editor’s Note: the detailed intentExpectation is for further discussion | type: FFSmultiplicity: \*isOrdered: FisUnique: FdefaultValue: NoneisNullable: False |
| intentFulfilStatus | It describes the status of the intent fulfilment result, which is configured by MnS producer and can be read by MnS consumer.allowedValues: "FULFILLED", “NOT\_FULFILLEDEditor’s Note: whether other allowed values should be supported is FFS, and the name for the attribute intentFulfilStatus is FFS. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
|  |  |  |
| serviceprofile | Defined in TS 28.541. | type: ServiceProfilemultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| serviceAccessibility | This describes the time window during which the service shall be available. | type: ServiceAvamultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
|  |  |  |
| startTime | This describes the beginning time of the service availability time window. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| endTime | This describes the ending time of the service availability time window. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
|  |  |  |
| geoLocation | This describes the geographical area at which the service should be deployed and made available. This will take a form of either single latitude & longitude or a TAI. This attribute can be used to select the appropriate edge network where the service need to be deployed. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
|  |  |  |
|  |  |  |

|  |
| --- |
| **End of 3rd modified section** |