**3GPP TSG-SA5 Meeting #137eS5-213383**

**e-meeting, 10 - 19 May 2021**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v11.4* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **28.541** | **CR** | **0503** | **rev** | **-** | **Current version:** | **17.2.0** |  |
|  | | | | | | | | |
| *For* [***HELP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | fix inheritance relation of network slice NRM | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Nokia, Nokia Shanghai Bell, HPE | | | | | | | | | |
| ***Source to TSG:*** | S5 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | TEI16 | | | | |  | ***Date:*** | | | 2021-04-29 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **A** |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) Rel-12 (Release 12) Rel-13 (Release 13) Rel-14 (Release 14) Rel-15 (Release 15) Rel-16 (Release 16)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | According to TS 28.620 and 28.622, SubNetwork represents a set of managed entities, and those managed entities subject to common administration. NetworkSlice is used to model network slice, which is a logical network that provides specific network capabilities and network characteristics, supporting various service properties for network slice customers. NetworkSliceSubnet is collection/group of resources to support network slice or other services. Therefore, neither NetworkSlice nor NetworkSliceSubnet inherits properties of SubNetwork. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Fix inheritance relationship of NetworkSlice and NetworkSliceSubnet | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Incorrect inheritance relationship will cause error implementation | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 6.2.2, J.4.3 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | Forge branch: 28.541\_Rel17\_0503\_fix\_inheritance\_relation\_of\_network\_slice\_NRM | | | | | | | | |

|  |
| --- |
| **Start of 1st modification** |

### 6.2.2 Inheritance




Figure 6.2.2-1: Network slice inheritance relationship

|  |
| --- |
| **End of modification** |

|  |
| --- |
| **Start of 2nd modification** |

## J.4.3 OpenAPI document "sliceNrm.yaml"

openapi: 3.0.1

info:

title: Slice NRM

version: 17.2.0

description: >-

OAS 3.0.1 specification of the Slice NRM

@ 2020, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: 3GPP TS 28.541 V17.2.0; 5G NRM, Slice NRM

url: http://www.3gpp.org/ftp/Specs/archive/28\_series/28.541/

paths: {}

components:

schemas:

#------------ Type definitions ---------------------------------------------------

Float:

type: number

format: float

MobilityLevel:

type: string

enum:

- STATIONARY

- NOMADIC

- RESTRICTED MOBILITY

- FULLY MOBILITY

SynAvailability:

type: string

enum:

- NOT SUPPORTED

- BETWEEN BS AND UE

- BETWEEN BS AND UE & UE AND UE

PositioningAvailability:

type: array

items:

type: string

enum:

- CIDE-CID

- OTDOA

- RF FINGERPRINTING

- AECID

- HYBRID POSITIONING

- NET-RTK

Predictionfrequency:

type: string

enum:

- PERSEC

- PERMIN

- PERHOUR

SharingLevel:

type: string

enum:

- SHARED

- NON-SHARED

NetworkSliceSharingIndicator:

type: string

enum:

- SHARED

- NON-SHARED

ServiceType:

type: string

enum:

- eMBB

- RLLC

- MIoT

- V2X

SliceSimultaneousUse:

type: string

enum:

- ZERO

- ONE

- TWO

- THREE

- FOUR

PerfReqEmbb:

type: object

properties:

expDataRateDL:

type: number

expDataRateUL:

type: number

areaTrafficCapDL:

type: number

areaTrafficCapUL:

type: number

userDensity:

type: number

activityFactor:

type: number

PerfReqEmbbList:

type: array

items:

$ref: '#/components/schemas/PerfReqEmbb'

PerfReqUrllc:

type: object

properties:

cSAvailabilityTarget:

type: number

cSReliabilityMeanTime:

type: string

expDataRate:

type: number

msgSizeByte:

type: string

transferIntervalTarget:

type: string

survivalTime:

type: string

PerfReqUrllcList:

type: array

items:

$ref: '#/components/schemas/PerfReqUrllc'

PerfReq:

oneOf:

- $ref: '#/components/schemas/PerfReqEmbbList'

- $ref: '#/components/schemas/PerfReqUrllcList'

Category:

type: string

enum:

- CHARACTER

- SCALABILITY

Tagging:

type: array

items:

type: string

enum:

- PERFORMANCE

- FUNCTION

- OPERATION

Exposure:

type: string

enum:

- API

- KPI

ServAttrCom:

type: object

properties:

category:

$ref: '#/components/schemas/Category'

tagging:

$ref: '#/components/schemas/Tagging'

exposure:

$ref: '#/components/schemas/Exposure'

Support:

type: string

enum:

- NOT SUPPORTED

- SUPPORTED

DelayTolerance:

type: object

properties:

servAttrCom:

$ref: '#/components/schemas/ServAttrCom'

support:

$ref: '#/components/schemas/Support'

DeterministicComm:

type: object

properties:

servAttrCom:

$ref: '#/components/schemas/ServAttrCom'

availability:

$ref: '#/components/schemas/Support'

periodicityList:

type: string

DLThptPerSlice:

type: object

properties:

servAttrCom:

$ref: '#/components/schemas/ServAttrCom'

guaThpt:

$ref: '#/components/schemas/Float'

maxThpt:

$ref: '#/components/schemas/Float'

DLThptPerUE:

type: object

properties:

servAttrCom:

$ref: '#/components/schemas/ServAttrCom'

guaThpt:

$ref: '#/components/schemas/Float'

maxThpt:

$ref: '#/components/schemas/Float'

ULThptPerSlice:

type: object

properties:

servAttrCom:

$ref: '#/components/schemas/ServAttrCom'

guaThpt:

$ref: '#/components/schemas/Float'

maxThpt:

$ref: '#/components/schemas/Float'

ULThptPerUE:

type: object

properties:

servAttrCom:

$ref: '#/components/schemas/ServAttrCom'

guaThpt:

$ref: '#/components/schemas/Float'

maxThpt:

$ref: '#/components/schemas/Float'

DLThptPerSliceSubnet:

type: object

properties:

guaThpt:

$ref: '#/components/schemas/Float'

maxThpt:

$ref: '#/components/schemas/Float'

DLThptPerUEPerSubnet:

type: object

properties:

guaThpt:

$ref: '#/components/schemas/Float'

maxThpt:

$ref: '#/components/schemas/Float'

ULThptPerSliceSubnet:

type: object

properties:

guaThpt:

$ref: '#/components/schemas/Float'

maxThpt:

$ref: '#/components/schemas/Float'

ULThptPerUEPerSubnet:

type: object

properties:

guaThpt:

$ref: '#/components/schemas/Float'

maxThpt:

$ref: '#/components/schemas/Float'

MaxPktSize:

type: object

properties:

servAttrCom:

$ref: '#/components/schemas/ServAttrCom'

maxsize:

type: integer

MaxNumberofPDUSessions:

type: object

properties:

servAttrCom:

$ref: '#/components/schemas/ServAttrCom'

nOofPDUSessions:

type: integer

KPIMonitoring:

type: object

properties:

servAttrCom:

$ref: '#/components/schemas/ServAttrCom'

kPIList:

type: string

NBIoT:

type: object

properties:

servAttrCom:

$ref: '#/components/schemas/ServAttrCom'

support:

$ref: '#/components/schemas/Support'

Synchronicity:

type: object

properties:

servAttrCom:

$ref: '#/components/schemas/ServAttrCom'

availability:

$ref: '#/components/schemas/SynAvailability'

accuracy:

$ref: '#/components/schemas/Float'

Positioning:

type: object

properties:

servAttrCom:

$ref: '#/components/schemas/ServAttrCom'

availability:

$ref: '#/components/schemas/PositioningAvailability'

predictionfrequency:

$ref: '#/components/schemas/Predictionfrequency'

accuracy:

$ref: '#/components/schemas/Float'

UserMgmtOpen:

type: object

properties:

servAttrCom:

$ref: '#/components/schemas/ServAttrCom'

support:

$ref: '#/components/schemas/Support'

V2XCommModels:

type: object

properties:

servAttrCom:

$ref: '#/components/schemas/ServAttrCom'

v2XMode:

$ref: '#/components/schemas/Support'

TermDensity:

type: object

properties:

servAttrCom:

$ref: '#/components/schemas/ServAttrCom'

density:

type: integer

NsInfo:

type: object

properties:

nsInstanceId:

type: string

nsName:

type: string

CNSliceSubnetProfile:

type: object

properties:

maxNumberofUEs:

type: integer

latency:

type: integer

dLThptPerSliceSubnet:

$ref: '#/components/schemas/DLThptPerSliceSubnet'

dLThptPerUEPerSubnet:

$ref: '#/components/schemas/DLThptPerUEPerSubnet'

uLThptPerSliceSubnet:

$ref: '#/components/schemas/ULThptPerSliceSubnet'

uLThptPerUEPerSubnet:

$ref: '#/components/schemas/ULThptPerUEPerSubnet'

maxNumberOfPDUSessions:

type: integer

maxPktSize:

type: integer

delayTolerance:

$ref: '#/components/schemas/DelayTolerance'

sliceSimultaneousUse:

$ref: '#/components/schemas/SliceSimultaneousUse'

RANSliceSubnetProfile:

type: object

properties:

coverageAreaTAList:

type: integer

MobilityLevel:

$ref: '#/components/schemas/MobilityLevel'

resourceSharingLevel:

$ref: '#/components/schemas/SharingLevel'

maxNumberofUEs:

type: integer

activityFactor:

type: integer

dLThptPerUEPerSubnet:

$ref: '#/components/schemas/ULThptPerUEPerSubnet'

uLThptPerUEPerSubnet:

$ref: '#/components/schemas/ULThptPerUEPerSubnet'

uESpeed:

type: integer

reliability:

type: string

serviceType:

$ref: '#/components/schemas/ServiceType'

maxPktSize:

type: integer

delayTolerance:

$ref: '#/components/schemas/DelayTolerance'

sliceSimultaneousUse:

$ref: '#/components/schemas/SliceSimultaneousUse'

TopSliceSubnetProfile:

type: object

properties:

coverageArea:

type: string

latency:

type: integer

maxNumberofUEs:

type: integer

dLThptPerSliceSubnet:

$ref: '#/components/schemas/DLThptPerSliceSubnet'

dLThptPerUEPerSubnet:

$ref: '#/components/schemas/DLThptPerUEPerSubnet'

uLThptPerSliceSubnet:

$ref: '#/components/schemas/ULThptPerSliceSubnet'

uLThptPerUEPerSubnet:

$ref: '#/components/schemas/ULThptPerUEPerSubnet'

maxPktSize:

type: integer

delayTolerance:

$ref: '#/components/schemas/DelayTolerance'

sliceSimultaneousUse:

$ref: '#/components/schemas/SliceSimultaneousUse'

ServiceProfile:

type: object

properties:

serviceProfileId:

type: string

plmnInfoList:

$ref: 'nrNrm.yaml#/components/schemas/PlmnInfoList'

maxNumberofUEs:

type: number

latency:

type: number

uEMobilityLevel:

$ref: '#/components/schemas/MobilityLevel'

sst:

$ref: 'nrNrm.yaml#/components/schemas/Sst'

networkSliceSharingIndicator:

$ref: '#/components/schemas/NetworkSliceSharingIndicator'

availability:

type: number

delayTolerance:

$ref: '#/components/schemas/DelayTolerance'

deterministicComm:

$ref: '#/components/schemas/DeterministicComm'

dLThptPerSlice:

$ref: '#/components/schemas/DLThptPerSlice'

dLThptPerUE:

$ref: '#/components/schemas/DLThptPerUE'

uLThptPerSlice:

$ref: '#/components/schemas/ULThptPerSlice'

uLThptPerUE:

$ref: '#/components/schemas/ULThptPerUE'

maxPktSize:

$ref: '#/components/schemas/MaxPktSize'

maxNumberofPDUSessions:

$ref: '#/components/schemas/MaxNumberofPDUSessions'

kPIMonitoring:

$ref: '#/components/schemas/KPIMonitoring'

nBIoT:

$ref: '#/components/schemas/NBIoT'

synchronicity:

$ref: '#/components/schemas/Synchronicity'

positioning:

$ref: '#/components/schemas/Positioning'

userMgmtOpen:

$ref: '#/components/schemas/UserMgmtOpen'

v2XModels:

$ref: '#/components/schemas/V2XCommModels'

coverageArea:

type: string

termDensity:

$ref: '#/components/schemas/TermDensity'

activityFactor:

$ref: '#/components/schemas/Float'

uESpeed:

type: integer

jitter:

type: integer

survivalTime:

type: string

reliability:

type: string

maxDLDataVolume:

type: string

maxULDataVolume:

type: string

sliceSimultaneousUse:

$ref: '#/components/schemas/SliceSimultaneousUse'

SliceProfile:

type: object

properties:

serviceProfileId:

type: string

plmnInfoList:

$ref: 'nrNrm.yaml#/components/schemas/PlmnInfoList'

perfReq:

$ref: '#/components/schemas/PerfReq'

cNSliceSubnetProfile:

$ref: '#/components/schemas/CNSliceSubnetProfile'

rANSliceSubnetProfile:

$ref: '#/components/schemas/RANSliceSubnetProfile'

topSliceSubnetProfile:

$ref: '#/components/schemas/TopSliceSubnetProfile'

IpAddress:

oneOf:

- $ref: 'genericNrm.yaml#/components/schemas/Ipv4Addr'

- $ref: 'genericNrm.yaml#/components/schemas/Ipv6Addr'

ServiceProfileList:

type: array

items:

$ref: '#/components/schemas/ServiceProfile'

SliceProfileList:

type: array

items:

$ref: '#/components/schemas/SliceProfile'

#------------ Definition of concrete IOCs ----------------------------------------

SubNetwork-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/SubNetwork-Attr'

- $ref: 'genericNrm.yaml#/components/schemas/SubNetwork-ncO'

- type: object

properties:

SubNetwork:

$ref: '#/components/schemas/SubNetwork-Multiple'

NetworkSlice:

$ref: '#/components/schemas/NetworkSlice-Multiple'

NetworkSliceSubnet:

$ref: '#/components/schemas/NetworkSliceSubnet-Multiple'

EP\_Transport:

$ref: '#/components/schemas/EP\_Transport-Multiple'

NetworkSlice-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

allOf:

- type: object

properties:

networkSliceSubnetRef:

$ref: 'genericNrm.yaml#/components/schemas/Dn'

operationalState:

$ref: 'genericNrm.yaml#/components/schemas/OperationalState'

administrativeState:

$ref: 'genericNrm.yaml#/components/schemas/AdministrativeState'

serviceProfileList:

$ref: '#/components/schemas/ServiceProfileList'

NetworkSliceSubnet-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

allOf:

- type: object

properties:

managedFunctionRefList:

$ref: 'genericNrm.yaml#/components/schemas/DnList'

networkSliceSubnetRefList:

$ref: 'genericNrm.yaml#/components/schemas/DnList'

operationalState:

$ref: 'genericNrm.yaml#/components/schemas/OperationalState'

administrativeState:

$ref: 'genericNrm.yaml#/components/schemas/AdministrativeState'

nsInfo:

$ref: '#/components/schemas/NsInfo'

sliceProfileList:

$ref: '#/components/schemas/SliceProfileList'

epTransportRefList:

$ref: 'genericNrm.yaml#/components/schemas/DnList'

EP\_Transport-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top-Attr'

- type: object

properties:

attributes:

type: object

properties:

ipAddress:

$ref: '#/components/schemas/IpAddress'

logicInterfaceId:

type: string

nextHopInfo:

type: string

qosProfile:

type: string

epApplicationRefs:

$ref: 'genericNrm.yaml#/components/schemas/DnList'

#-------- Definition of JSON arrays for name-contained IOCs ----------------------

SubNetwork-Multiple:

type: array

items:

$ref: '#/components/schemas/SubNetwork-Single'

NetworkSlice-Multiple:

type: array

items:

$ref: '#/components/schemas/NetworkSlice-Single'

NetworkSliceSubnet-Multiple:

type: array

items:

$ref: '#/components/schemas/NetworkSliceSubnet-Single'

EP\_Transport-Multiple:

type: array

items:

$ref: '#/components/schemas/EP\_Transport-Single'

#------------ Definitions in TS 28.541 for TS 28.532 -----------------------------

resources-sliceNrm:

oneOf:

- $ref: '#/components/schemas/SubNetwork-Single'

- $ref: '#/components/schemas/NetworkSlice-Single'

- $ref: '#/components/schemas/NetworkSliceSubnet-Single'

- $ref: '#/components/schemas/EP\_Transport-Single'

|  |
| --- |
| **End of modification** |