**3GPP TSG SA WG5 Meeting #139e S5-215136**

**Online, , 11 Oct 2021- 20 Oct 2021**

**Source: Samsung**

**Title: pCR 28.538 EASFunction definition**

**Document for: Approval**

**Agenda Item: 6.4.21**

# 1 Decision/action requested

***The group is asked to discuss and approve the proposals.***

# 2 References

None

# 3 Rationale

This contribution defined the EASFunction IOC.

# 4 Detailed proposal

|  |
| --- |
| **First modification** |

## 6.3 Class definition

6.3.1 EASFunction

6.3.1.1 Definition

This IOC represent the properties of a EAS in a 3GPP network. For more information about EAS, see 3GPP TS 23.558.

6.3.1.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| eASIdentifier | M | T | T | F | T |
| **Attribute related to role** |  |  |  |  |  |
| eASRequirementsRef | M | T | T | F | T |
| eASProfileRef | M | T | T | F | T |
|  |  |  |  |  |  |

#### 6.3.1.3 Attribute constraints

#### 6.3.1.4 Notifications

The common notifications defined in subclause Y.3 are valid for this IOC, without exceptions or additions.

6.3.2 EASRequirements

6.3.2.1 Definition

This represent the deployment requirements of an EAS which need to be considered during EASFunction instantiation.

6.3.2.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| requiredEASservingLocation | M | T | F | F | T |
|  |  |  |  |  |  |
|  |  |  |  |  |  |

#### 6.3.2.3 Attribute constraints

#### 6.3.2.4 Notifications

The common notifications defined in subclause Y.3 are valid for this IOC, without exceptions or additions.

6.3.3 ServingLocation <<datatype>>

6.3.3.1 Definition

This datatype represent the location which is to be served by the node.

6.3.3.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| geographicalLocation | CM | T | F | F | T |
| topologicalLocation | CM | T | F | F | T |
|  |  |  |  |  |  |

#### 6.3.3.3 Attribute constraints

|  |  |
| --- | --- |
| Name | Definition |
| geographicalLocation Support Qualifier | Condition: either geographicalLocation or topologicalLocation shall be present. |
| topologicalLocation Support Qualifier | Condition: either geographicalLocation or topologicalLocation shall be present. |

#### 6.3.3.4 Notifications

The common notifications defined in subclause Y.3 are valid for this IOC, without exceptions or additions.

6.3.4 EASProfile

6.3.1.1 Definition

This IOC represent the EAS profile, see 3GPP TS 23.558.

6.3.1.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| eASservingLocation | M | T | T | F | T |
| eASProvider | O | T | T | F | T |
| eASType | O | T | T | F | T |
| eASDescription | O | T | T | F | T |
|  |  |  |  |  |  |

#### 6.3.1.3 Attribute constraints

#### 6.3.1.4 Notifications

The common notifications defined in subclause Y.3 are valid for this IOC, without exceptions or additions.

6.3.5 GeoLoc <<datatype>>

6.3.5.1 Definition

This datatype represent the geographical location.

6.3.5.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| geoPoint | CM | T | T | F | T |
| civicAddress | CM | T | T | F | T |

#### 6.3.5.3 Attribute constraints

|  |  |
| --- | --- |
| Name | Definition |
| geoPoint Support Qualifier | Condition: either geoPoint or civicAddress shall be present. |
| civicAddress Support Qualifier | Condition: either geoPoint or civicAddress shall be present. |

#### 6.3.5.4 Notifications

The common notifications defined in subclause Y.3 are valid for this IOC, without exceptions or additions.

6.3.6 GeoP <<datatype>>

6.3.6.1 Definition

This datatype represent the geographical location.

6.3.6.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| lat | M | T | T | F | T |
| long | M | T | T | F | T |

#### 6.3.6.3 Attribute constraints

#### 6.3.6.4 Notifications

The common notifications defined in subclause Y.3 are valid for this IOC, without exceptions or additions.

6.3.7 TopoLoc <<datatype>>

6.3.7.1 Definition

This datatype represent the topological location.

6.3.7.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Support Qualifier | isReadable | isWritable | isInvariant | isNotifyable |
| cellID | O | T | T | F | T |
| tAI | O | T | T | F | T |
| pLMNID | O | T | T | F | T |

#### 6.3.7.3 Attribute constraints

#### 6.3.7.4 Notifications

The common notifications defined in subclause Y.3 are valid for this IOC, without exceptions or additions.

## 6.4 Attribute definition

6.4.1 Attribute Properties

| Attribute Name | Documentation and Allowed Values | Properties |
| --- | --- | --- |
| eASIdentifier | It identifies the EAS, see 3GPP TS 23.558. | type: String  multiplicity: 1  isOrdered: N/A  isUnique: True  defaultValue: None  isNullable: False |
| eASREquirementsRef | This is the DN of EASRequirements.  allowedValues: DN of the EASRequirements MOI. | type: String  multiplicity: 1  isOrdered: N/A  isUnique: True  defaultValue: None  isNullable: False |
| eASservingLocation | It defines the serving location for an EAS. | type: ServingLocation  multiplicity: 1..\*  isOrdered: N/A  isUnique: True  defaultValue: None  isNullable: False |
| eASProvider | It defines the EAS Provider Identifier, see 3GPP TS 23.558. | type: String  multiplicity: 1  isOrdered: N/A  isUnique: True  defaultValue: None  isNullable: False |
| eASType | It defines the EAS Type, see 3GPP TS 23.558. | type: String  multiplicity: 1  isOrdered: N/A  isUnique: True  defaultValue: None  isNullable: False |
| eASDescription | It defines the EAS description, see 3GPP TS 23.558. | type: Sting  multiplicity: 1  isOrdered: N/A  isUnique: True  defaultValue: None  isNullable: False |
| requiredEASservingLocation | It defines the location where the EAS service should be available. | type: ServingLocation  multiplicity: 1..\*  isOrdered: N/A  isUnique: True  defaultValue: None  isNullable: False |
|  |  |  |
| topologicalLocation | This refers to the Topological Service Area, see 3GPP TS 23.558. | type: TopoLoc  multiplicity: 1  isOrdered: N/A  isUnique: True  defaultValue: None  isNullable: False |
| geographicalLocation | This refers to the Geographical Service Area, see 3GPP TS 23.558. | type: GeoLoc  multiplicity: 1  isOrdered: N/A  isUnique: True  defaultValue: None  isNullable: False |
| eASProfileRef | This is the DN of EASProfile.  allowedValues: DN of the EASProfile MOI. | type: String  multiplicity: 1  isOrdered: N/A  isUnique: True  defaultValue: None  isNullable: False |
| geoPoint | This defines the location in terms of latitude and longitude. | type: geoP  multiplicity: 1  isOrdered: N/A  isUnique: True  defaultValue: None  isNullable: False |
| lat | This defines the single latitude coordinate. | type: Float  multiplicity: 1  isOrdered: N/A  isUnique: True  defaultValue: None  isNullable: False |
| long | This defines the single longtitude coordinate. | type: Float  multiplicity: 1  isOrdered: N/A  isUnique: True  defaultValue: None  isNullable: False |
| civicAddress | This defines the location in terms of a civic address | type: String  multiplicity: 1  isOrdered: N/A  isUnique: True  defaultValue: None  isNullable: False |
| cellID | The list of cell IDs defining the topological service area | type: String  multiplicity: 1..\*  isOrdered: N/A  isUnique: True  defaultValue: None  isNullable: False |
| tAI | The list of Tracking Area IDs defining the topological service area | type: String  multiplicity: 1..\*  isOrdered: N/A  isUnique: True  defaultValue: None  isNullable: False |
| pLMNID | The list of PLMN IDs defining the topological service area | type: String  multiplicity: 1..\*  isOrdered: N/A  isUnique: True  defaultValue: None  isNullable: False |
|  |  |  |

|  |
| --- |
| **End of First modification** |

|  |
| --- |
| **Second modification** |

# P.1 General

This annex contains the OpenAPI definition of the Edge NRM in YAML format.

The Information Service (IS) of the Edge NRM is defined in clause 6.

Mapping rules to produce the OpenAPI definition based on the IS are defined in TS 32.160 [10].

# P.2 Solution Set (SS) definitions

## P.2.1 OpenAPI document "edgeNrm.yml"

openapi: 3.0.1

info:

title: 3GPP Edge NRM

version: 17.1.0

description: >-

OAS 3.0.1 specification of the Edge NRM

© 2020, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: 3GPP TS 28.538; Edge NRM

url: http://www.3gpp.org/ftp/Specs/archive/28\_series/28.538/

paths: {}

components:

schemas:

#-------- Definition of types-----------------------------------------------------

GeoLoc:

type: object

properties:

geoPoint:

$ref: '#/components/schemas/GeoP'

civicAddress:

Type: String

GeoP:

type: object

properties:

lat:

type: float

long:

type: float

TopoLoc:

type: object

properties:

cellID:

Type: string

tAI:

Type: string

pLMNID:

Type: string

#-------- Definition of concrete IOCs --------------------------------------------

SubNetwork-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/SubNetwork-Attr'

- $ref: 'genericNrm.yaml#/components/schemas/SubNetwork-ncO'

- type: object

properties:

EASFunction:

$ref: '5GCNrm.yaml#/components/schemas/EASFunction-Multiple'

EASFunction-Single:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/ManagedFunction'

- type: object

properties:

attributes:

allOf:

- type: object

properties:

eASIdentifier:

type: string

EASProfile:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- type: object

properties:

eASservingLocation:

$ref: '#/components/schemas/ServingLocation'

eASProvider:

Type: string

eASType:

Type: string

eASDescription:

Type: string

EASRequirements:

allOf:

- $ref: 'genericNrm.yaml#/components/schemas/Top'

- type: object

properties:

attributes:

allOf:

- type: object

properties:

requiredEASservingLocation:

$ref: '#/components/schemas/ServingLocation'

ServingLocation:

type: object

geographicalLocation:

$ref: '#/components/schemas/GeoLoc'

topologicalLocation:

$ref: '#/components/schemas/TopoLoc'

#-------- Definition of JSON arrays for name-contained IOCs ----------------------

EASFunction-Multiple:

type: array

items:

$ref: '#/components/schemas/EASFunction-Single'

|  |
| --- |
| **End of second modification** |