**3GPP TSG-SA5 Meeting #139-e *S5-215324***

**e-meeting, 11 - 20 October 2021** Revision of S5-20xxxx

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **32.291** | **CR** | **0354** | **rev** | **1** | **Current version:** | **17.0.0** |  |
|  |
| *For* [***HELP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Addition of QoS Monitoring to Assist URLLC Service |
|  |  |
| ***Source to WG:*** | Huawei |
| ***Source to TSG:*** | S5 |
|  |  |
| ***Work item code:*** | 5G\_URLLC |  | ***Date:*** | 2021-10-15 |
|  |  |  |  |  |
| ***Category:*** | F |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | For the QoS Monitoring to Assist URLLC Service, the SMF may report the packet delay measurement per QoS Flow per UE to CHF. The coresponding parameters should be added. |
|  |  |
| ***Summary of change:*** | Add the related parameters for QoS Monitoring to Assist URLLC Service |
|  |  |
| ***Consequences if not approved:*** | Can not support the URLCC charging. |
|  |  |
| ***Clauses affected:*** | 2,6.1.6.1,6.1.6.2.2.8,6.1.8,7.2,A.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** | **X** |  |  O&M Specifications | TS 32.255 CR 0338 TS 32.298 CR 0881 |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

|  |
| --- |
| **First change** |

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TS 32.240: "Telecommunication management; Charging management; Charging architecture and principles".

[2] - [13] Void.

[14] 3GPP TS 32.254: "Telecommunication management; Charging management; Exposure function Northbound Application Program Interfaces (APIs) charging ".

[15] - [28] Void.

[29] 3GPP TS 32.274: "Telecommunication management; Charging management;Short Message Service (SMS) charging".

[30] 3GPP TS 32.255: "Telecommunication management; Charging management; 5G Data connectivity domain charging; stage 2".

[31] 3GPP TS 32.256: "Telecommunication management; Charging management; 5G connection and mobility domain charging; stage 2".

[32] 3GPP TS 32.260: "Telecommunication management; Charging management; IP Multimedia Subsystem (IMS) charging".

[33] - [49] Void.

[50] - [57] Void.

[58] 3GPP TS 32.290: "Telecommunication management; Charging management; 5G system; Services, operations and procedures of charging using Service Based Interface (SBI).

[59] - [69] Void.[70] 3GPP TS 28.201: "Charging management; Network slice performance and analytics charging in the 5G System (5GS); Stage 2".

[71] 3GPP TS 28.202: "Charging management; Network slice management charging in the 5G System (5GS); Stage 2".

[72] - [99] Void.

[100] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[101] 3GPP TR 21.900: "Technical Specification Group working methods".

[102] - [199] Void

[200] - [252] Void

[253] 3GPP TS 28.532: "Management and orchestration; Management services".

[254] 3GPP TS 28.541: "Management and orchestration; 5G Network Resource Model (NRM); Stage 2 and stage 3".

[255] 3GPP TS 32.300: "Telecommunication management; Configuration Management (CM); Name convention for Managed Objects".

[256] 3GPP TS 28.554: "Management and orchestration;5G end to end Key Performance Indicators (KPI)".

[257] 3GPP TS 28.623: "Telecommunication management; Generic Network Resource Model (NRM) Integration Reference Point (IRP); Solution Set (SS) definitions".

[258] - [298] Void

[299] 3GPP TS 29.500: "5G System; Technical Realization of Service Based Architecture; Stage 3".

[300] 3GPP TS 29.501: "5G System; Principles and Guidelines for Services Definition; Stage 3".

[301] 3GPP TS 29.594: "5G System; Spending Limit Control Service; Stage 3".

[302] 3GPP TS 29.512: "5G System; Session Management Policy Control Service; Stage 3".

[303] 3GPP TS 24.501: "Non-Access-Stratum (NAS) Protocol for 5G System (5GS); Stage 3".

[304] 3GPP TS 38.413: "NG-RAN; NG Application Protocol (NGAP)".

[305] 3GPP TS 29.510: "Network Function Repository Services; Stage 3".

[306] 3GPP TS 29.520: "5G System; Network Data Analytics Services;Stage 3".

[307] 3GPP TS 29.514: "5G System; Network Data Analytics Services;Stage 3".

[307] - [370] Void

[371] 3GPP TS 29.571: "5G System; Common Data Types for Service Based Interfaces; Stage 3".

[372] - [389] Void

[390] 3GPP TS 33.501: "Security architecture and procedures for 5G System".

[391] - [399] Void

[400] Void.

[401] IETF RFC 7540: "Hypertext Transfer Protocol Version 2 (HTTP/2) ".

[402] IETF RFC 8259: "The JavaScript Object Notation (JSON) Data Interchange Format ".

[403] IETF RFC 6749: "The OAuth 2.0 Authorization Framework".

[404] - [499] Void.

[500] OpenAPI: "OpenAPI 3.0.0 Specification", <https://github.com/OAI/OpenAPI-Specification/blob/master/versions/3.0.0.md>.

[501] - [599] Void.

|  |
| --- |
| **Next change** |

#### 6.1.6.1 General

This subclause specifies the application data model supported by the API.

The Nchf\_ConvergedCharging Service API allows the NF consumer to consume the converged charging service from the CHF as defined in 3GPP TS 32.290 [58].

Table 6.1.6.1-1 specifies the data types defined for the ConvergedCharging service based interface protocol.

Table 6.1.6.1-1: Nchf\_ ConvergedCharging specific Data Types

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Section defined | Description | Applicability |
| ChargingDataRequest | 6.1.6.2.1.16.1.6.2.2.1 | Describes the attributes of Charging Data Request to CHF for initial, update and termination of the charging session. |  |
| ChargingDataResponse | 6.1.6.2.1.26.1.6.2.2.2 | Describes the attributes of Charging Data Response from CHF on charging session initial, update and termination. |  |
| ChargingNotifyRequest | 6.1.6.2.1.3 | Describes Notifications about events that occurred in request message. |  |
| ChargingNotifyResponse | 6.1.6.2.1.16 | Describes the response of notification. |  |

Table 6.1.6.1-2 specifies data types re-used by the Nchf\_ConvergedCharging service based interface protocol from other specifications, including a reference to their respective specifications and when needed, a short description of their use within the Nchf\_ConvergedCharging service based interface.

Table 6.1.6.1-2: Nchf\_ConvergedCharging re-used Data Types

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Reference | Comments | Applicability |
| Supi | 3GPP TS 29.571 [371] | The identification of the user (i.e. IMSI, NAI, GLI, GCI).(NOTE 1) |  |
| Uint32 | 3GPP TS 29.571 [371] | Unsigned 32-bit integers |  |
| Uint64 | 3GPP TS 29.571 [371] | Unsigned 64-bit integers |  |
| PduSessionId | 3GPP TS 29.571 [371] | The identification of the PDU session. |  |
| PduSessionType | 3GPP TS 29.571 [371] | the type of a PDU session |  |
| Uri | 3GPP TS 29.571 [371] | String providing an URI |  |
| AccessType | 3GPP TS 29.571 [371] | The identification of the type of access network. |  |
| DateTime | 3GPP TS 29.571 [371] | The time. |  |
| ChargingId | 3GPP TS 29.571 [371] | Charging identifier allowing correlation of charging information |  |
| RatType | 3GPP TS 29.571 [371] | The identification of the RAT type. |  |
| RatingGroup | 3GPP TS 29.571 [371] | The identification of the rating group |  |
| Ipv4Addr | 3GPP TS 29.571 [371] | Ipv4 address.  |  |
| Ipv6Prefix | 3GPP TS 29.571 [371] | The Ipv6 prefix allocated for the user. |  |
| Ipv6Addr | 3GPP TS 29.571 [371] | Ipv6 Address. |  |
| Pei | 3GPP TS 29.571 [371] | The Identification of a Permanent Equipment. |  |
| TimeZone | 3GPP TS 29.571 [371] | Time zone information |  |
| NfInstanceId | 3GPP TS 29.571 [371] | String uniquely identifying a NF instance. |  |
| Gpsi | 3GPP TS 29.571 [371] | String identifying a Gpsi |  |
| DefaultQosInformation | 3GPP TS 29.571 [371] | Identifies the information of the default QoS. |  |
| SubscribedDefaultQos | 3GPP TS 29.571 [371] | subscribed default QoS. |  |
| AuthorizedDefaultQos | 3GPP TS 29.512 [302] | Authorized default QoS. |  |
| Ambr | 3GPP TS 29.571 [371] | Aggregate Maximum Bit rate  |  |
| QosData | 3GPP TS 29.512 [302] | Contains QoS parameters |  |
| UserLocation | 3GPP TS 29.571 [371] | User location information |  |
| PlmnId | 3GPP TS 29.571 [371] | PLMN id |  |
| Guami | 3GPP TS 29.571 [371] | Globally Unique AMF Identifier |  |
| DurationSec | 3GPP TS 29.571 [371] | Identifies a period of time in units of seconds. |  |
| Snssai | 3GPP TS 29.571 [371] | SNSSAI |  |
| ProblemDetails | 3GPP TS 29.571 [371] | additional details of the error |  |
| ServiceId | 3GPP TS 29.571 [371] | Identifier of service |  |
| SscMode | 3GPP TS 29.571 [371] | SSC Mode type |  |
| PresenceInfo | 3GPP TS 29.571 [371] | PRA information including PRAId, PRA element list and PRA status |  |
| Qfi | 3GPP TS 29.571 [371] | QoS flow identifier designated as "Qfi". |  |
| AmfId | 3GPP TS 29.571 [371] | AMF identifier |  |
| Dnn | 3GPP TS 29.571 [371] | Data Network Name |  |
| GroupId | 3GPP TS 29.571 [371] | Network internal Identifier for a group of IMSIs |  |
| ExternalGroupId | 3GPP TS 29.571 [371] | External Group Identifier for one or more subscriptions associated to a group of IMSIs  |  |
| Bytes | 3GPP TS 29.571 [371] | String with format "byte" |  |
| Tai | 3GPP TS 29.571 [371] | Tracking Area Identifier |  |
| Area | 3GPP TS 29.571 [371] | List of TACs or Operator specific codes |  |
| CoreNetworkType | 3GPP TS 29.571 [371] | 5GC or EPC |  |
| ServiceAreaRestriction | 3GPP TS 29.571 [371] | Service Area restriction |  |
| GlobalRanNodeId | 3GPP TS 29.571 [371] | Global RAN Node Id |  |
| QosCharacteristics | 3GPP TS 29.512 [302] | Map of QoS characteristics for non standard 5QIs and non-preconfigured 5QIs. |  |
| SupportedFeatures | 3GPP TS 29.571 [371] | See 3GPP TS 29.500 [4] clause 6.6 |  |
| NsiLoadLevelInfo | 3GPP TS 29.520 [306] | Represents the load level information for an S-NSSAI and the associated network slice instance |  |
| ServiceExperienceInfo | 3GPP TS 29.520 [306] | ServiceExperience |  |
| ApplicationChargingId | 3GPP TS 29.571 [371] | Application provided charging identifier allowing correlation of charging information. | AF\_Charging\_Identifier |
| SharingLevel | 3GPP TS 28.541 [254] | Ressources sharing level |  |
| MobilityLevel | 3GPP TS 28.541 [254] | UE mobility Level |  |
| SsT | 3GPP TS 28.541 [254] | Slice Service type (SST) |  |
| Support | 3GPP TS 28.541 [254] | Supported, Not Supported indicator |  |
| Float | 3GPP TS 29.571 [371] | Number with format "float"  |  |
| MaPduIndication | 3GPP TS 29.512 [302] | MA PDU session indication | ATSSS |
| AtsssCapability | 3GPP TS 29.571 [371] | ATSSS capabilities  | ATSSS |
| SteeringFunctionality | 3GPP TS 29.571 [371] | Steering functionalities for MA PDU session | ATSSS |
| SteeringMode | 3GPP TS 29.512 [302] | Steering mode for MA PDU session | ATSSS |
| OperationalState | 3GPP TS 28.623 [257] | Operational state |  |
| AdministrativeState | 3GPP TS 28.623 [257] | Administrative state |  |
| RanNasRelCause | 3GPP TS 29.512 [302] | Indicates the RAN or NAS release cause code information. | EnhancedDiagnostics |
| Ecgi | 3GPP TS 29.571 [371] | E-UTRA Cell Id |  |
| Ncgi | 3GPP TS 29.571 [371] | NR Cell Id |  |
| QosMonitoringReport | 3GPP TS 29.541 [xxx] | Indicates the service data flows QoS Monitoring. | QoSMonitoring |
| NOTE 1: A SUPI containing GLI or GCI is used to support 5G-RG and FN-RG in scenarios of wireline network. |

|  |
| --- |
| **Next change** |

###### 6.1.6.2.2.8 Type PDUSessionInformation

Table 6.1.6.2.2.8-1: Definition of type PDUSessionInformation

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| networkSlicingInfo | NetworkSlicingInfo  | OM | 0..1 | information of network slice serving the PDU session |  |
| pduSessionID | PduSessionId | M | 1 |  |  |
| pduType | PduSessionType | OM | 0..1 | type of the PDU session |  |
| sscMode | SscMode | OC | 0..1 | information of SSC Mode type. |  |
| hPlmnId | PlmnId | OC | 0..1 | PLMN identifier of the home network |  |
| servingNetworkFunctionID | ServingNetworkFunctionID | OC | 0..1 | This field holds serving Network Function identifier. |  |
| servingCNPlmnId | PlmnId | OC | 0..1 | Serving Core Network Operator PLMN ID selected by the UE in shared networks. |  |
| ratType | RatType | OC | 0..1 | the RAT Type of the PDU session |  |
| mAPDUNon3GPPRATType | RatType | OC | 0..1 | the RAT Type of non-3GPP access for the MA PDU session | ATSSS |
| dnnId | Dnn | M | 1 | a Data Network Name |  |
| dnnSelectionMode | DnnSelectionMode | OC | 0..1 | This field indicates how the DNN was selected. |  |
| chargingCharacteristics | string | OC | 0..1 | the Charging Characteristics for this PDU session.It carries the value in hexadecimal representationPattern: '^[0-9a-fA-F]{1,4}$' |  |
| chargingCharacteristicsSelectionMode | ChargingCharacteristicsSelectionMode | OC | 0..1 | information about how the "Charging Characteristics" was selected.  |  |
| startTime | DateTime | OC | 0..1 | the UTC time which represents the start of a PDU session at the SMF |  |
| stopTime | DateTime | OC | 0..1 | the UTC time which represents the stop of a PDU session at the SMF |  |
| 3gppPSDataOffStatus | 3GPPPSDataOffStatus | OC | 0..1 | This field holds the 3GPP Data off Status when UE’s 3GPP Data Off status is Activated or Deactivated. |  |
| sessionStopIndicator | boolean | OC | 0..1 | This field indicates to the CHF that the PDU session has been terminated. |  |
| pduAddress | PDUAddress | OC | 0..1 | Group of user ip address/prefix |  |
| diagnostics | Diagnostics | OC | 0..1 | provides a detailed cause value from SMF. |  |
| enhancedDiagnostics | EnhancedDiagnostics5G | OC | 0..N | provides a more detailed cause value from SMF. | EnhancedDiagnostics |
| authorizedQoSInformation | AuthorizedDefaultQos | OC | 0..1 | This field holds the authorized QoS applied to PDU session. |  |
| subscribedQoSInformation | SubscribedDefaultQos | OC | 0..1 | This field holds the subscribed Default QoS  |  |
| authorizedSessionAMBR | Ambr | OC | 0..1 | This field holds the authorized session-AMBR. |  |
| subscribedSessionAMBR | Ambr | OC | 0..1 | This field holds the subscribed session-AMBR. |  |
| mAPDUSessionInformation | MAPDUSessionInformation | OC | 0..1 | This field holds the MA PDU session information. | ATSSS |
| redundantTransmissionType | RedundantTransmissionType | OC | 0..1 | Indicates the redundant transmission type.If this field isn’t present, it should be seen as a non-redundant transmission. | URLLC |
| qosMonitoringInformation | array(QosMonitoringReport) | OC | 0..1 | This field holds QoS Monitoring reporting information.It may be present when the URLLC is supported.  | QoSMonitoring |
| pDUSessionPairID | Uint32 | OC | 0..1 | This field identifies the two redundant PDU Sessions that belong together for dual connectivity based end to end redundant user plane paths type. | URLLC |

|  |
| --- |
| **Next change** |

### 6.1.8 Feature negotiation

The optional features in table 6.1.8-1 are defined for the Nchf\_ConvergedCharging API. They shall be negotiated using the extensibility mechanism defined in subclause 6.6 of 3GPP TS 29.500 [299].

Table 6.1.8-1: Supported Features

|  |  |  |
| --- | --- | --- |
| Feature number | Feature Name | Description |
| 1 | CHFCQM | CHF-controlled quota management i.e. support for temporary offline |
| 2 | AF\_Charging\_Identifier | Indicates the support of long character strings as charging identifiers. |
| 3 | 5GIEPC\_CH | 5GS interworking with EPC |
| 4 | ATSSS | This feature indicates support of Access Traffic Steering, Switching, Splitting (ATSSS). |
| 5 | ETSUN | This feature indicates support of Enhancing Topology of SMF and UPF in 5G Networks (ETSUN). |
| 6 | EnhancedDiagnostics | Support the enhanced diagnostics |
| 7 | AMF\_subs\_PRA | PRA(s) subscription by CHF in AMF |
| 8 | FilterRuleList | Support of multiple filter rules in the final unit indication |
| 9 | TEI17\_NIESGU | This feature indicates support of GERAN/UTRAN access |
| 10 | IMS | This feature indicates support of IMS. |
| 11 | QoSMonitoring | This feature indicates support of QoS Monitoring |

|  |
| --- |
| **Next change** |

## 7.2 Bindings for 5G data connectivity

Table 7.2-1: Bindings of 5G data connectivity CDR field, Information Element and Resource Attribute

| Information Element | CDR Field | Resource Attribute |
| --- | --- | --- |
|  |  | **ChargingDataRequest** |
| Supported Features | - | **/**supportedFeatures |
| Multiple Unit Usage |  List of Multiple Unit Usage | /multipleUnitUsage |
| UPF ID | UPF ID | /multipleUnitUsage/uPFID |
| multi-homed PDU address | Multi-homed PDU address | /multipleUnitUsage/multihomedPDUAddress |
| Used Unit Container | Used Unit Container  | /multipleUnitUsage/usedUnitContainer |
| PDU Container Information | PDU Container Information | /multipleUnitUsage/usedUnitContainer/pDUContainerInformation |
| Time of First Usage | Time of First Usage | /multipleUnitUsage/usedUnitContainer/pDUContainerInformation/timeofFirstUsage |
| Time of Last Usage | Time of Last Usage | /multipleUnitUsage/usedUnitContainer/pDUContainerInformation/timeofLastUsage |
| QoS Information | QoS Information | /multipleUnitUsage/usedUnitContainer/pDUContainerInformation/qoSInformation |
| QoS Characteristics | QoS Characteristics | /multipleUnitUsage/usedUnitContainer/pDUContainerInformation/qoSCharacteristics |
| AF Charging Identifier | AF Charging Identifier | /multipleUnitUsage/usedUnitContainer/pDUContainerInformation/afChargingIdentifier |
| AF Charging Id String | AF Charging Id String | /multipleUnitUsage/usedUnitContainer/pDUContainerInformation/afChargingIdString |
| User Location Information | User Location Information | /multipleUnitUsage/usedUnitContainer/pDUContainerInformation/userLocationInformation |
| UE Time Zone | UE Time Zone | /multipleUnitUsage/usedUnitContainer/pDUContainerInformation/uetimeZone |
| RAT Type | RAT Type | /multipleUnitUsage/usedUnitContainer/pDUContainerInformation/rATType |
| Serving Network Function ID | Serving Network Function ID | /multipleUnitUsage/usedUnitContainer/pDUContainerInformation/servingNodeID |
| Presence Reporting Area Information | Presence Reporting AreaInformation | /multipleUnitUsage/usedUnitContainer/pDUContainerInformation/ presenceReportingAreaInformation |
| 3GPP PS Data Off Status | 3GPP PS Data Off Status | /multipleUnitUsage/usedUnitContainer/pDUContainerInformation/3gppPSDataOffStatus |
| MA PDU Steering functionality | MA PDU Steering functionality | /multipleUnitUsage/usedUnitContainer/pDUContainerInformation/mAPDUSteeringFunctionality |
| MA PDU Steering mode | MA PDU Steering mode | /multipleUnitUsage/usedUnitContainer/pDUContainerInformation/mAPDUSteeringMode |
| Sponsor Identity | Sponsor Identity | /multipleUnitUsage/usedUnitContainer/pDUContainerInformation/sponsorIdentity |
| Application Service ProviderIdentity | Application Service ProviderIdentity | /multipleUnitUsage/usedUnitContainer/pDUContainerInformation/applicationserviceProviderIdentity |
| Charging Rule Base Name | Charging Rule Base Name | /multipleUnitUsage/usedUnitContainer/pDUContainerInformation/chargingRuleBaseName |
| PDU Session Charging Information | PDU Session Charging Information | /pDUSessionChargingInformation  |
| Charging Id | Charging Id | /pDUSessionChargingInformation/chargingId |
| Home Provided ChargingId | Home Provided ChargingId | /pDUSessionChargingInformation/ homeProvidedChargingId |
| User Information | User Information | /pDUSessionChargingInformation/ userInformation |
| User Identifier | User Identifier | /pDUSessionChargingInformation/userInformation/servedGPSI |
| User Equipment Info | User Equipment Info | /pDUSessionChargingInformation/userInformation/ servedPEI |
| Unauthenticated Flag | Unauthenticated Flag | /pDUSessionChargingInformation/userInformation/ unauthenticatedFlag |
| Roamer In Out | Roamer In Out | /pDUSessionChargingInformation/userInformation/ roamerInOut |
| User Location Info | User Location Info | /pDUSessionChargingInformation/ userLocationinfo |
| MA PDU Non 3GPP User Location info | MA PDU Non 3GPP User Location info  | /pDUSessionChargingInformation/mAPDUNon3GPPUserLocationInfo |
| UE Time Zone | UE Time Zone | /pDUSessionChargingInformation/uEtimeZone |
| Presence Reporting AreaInformation | Presence Reporting AreaInformation | /pDUSessionChargingInformation/ presenceReportingAreaInformation |
| PDU Session Information | PDU Session Information | /pDUSessionChargingInformation/pduSessionInformation |
| PDU Session ID | PDU Session ID | /pDUSessionChargingInformation/pduSessionInformation/pduSessionID |
| Network Slice InstanceIdentifier | Network Slice Instance Identifier | /pDUSessionChargingInformation/pduSessionInformation/networkSlicingInfo |
| PDU Type | PDU Type | /pDUSessionChargingInformation /pduSessionInformation/pduType |
| PDU Address | PDU Address | /pDUSessionChargingInformation /pduSessionInformation/pduAddress |
| PDU IPv4 Address | PDU IPv4 Address | /pDUSessionChargingInformation/pduSessionInformation/pduAddress/pduIPv4Address |
| PDU IPv6 Address withprefix | PDU IPv6 Address with prefix | /pDUSessionChargingInformation/pduSessionInformation/pduAddress/pduIPv6Addresswithprefix |
| PDU Address prefix length | PDU Address prefix length | /pDUSessionChargingInformation /pduSessionInformation/pduAddress/pduAddressprefixlength |
| IPv4 Dynamic AddressFlag | IPv4 Dynamic Address Flag | /pDUSessionChargingInformation /pduSessionInformation/pduAddress/ iPv4dynamicAddressFlag |
| IPv6 Dynamic Address Flag | IPv6 Dynamic Prefix Flag | pDUSessionChargingInformation /pduSessionInformation/pduAddress/ iPv6dynamicPrefixFlag |
| Additional PDU IPv6Prefixes  | Additional PDU IPv6 Prefixes  | pDUSessionChargingInformation /pduSessionInformation/pduAddress/ addIpv6AddrPrefixes |
| SSC Mode | SSC Mode | /pDUSessionChargingInformation /pduSessionInformation/sscMode |
| MA PDU session information | MA PDU session information | /pDUSessionChargingInformation /pduSessionInformation/mAPDUSessionInformation |
| MA PDU session indicator | MA PDU session indicator | /pDUSessionChargingInformation /pduSessionInformation/mAPDUSessionInformation/mAPDUSessionIndicator |
| ATSSS capability | ATSSS capability | /pDUSessionChargingInformation /pduSessionInformation/mAPDUSessionInformation/aTSSSCapability |
| SUPI PLMN ID | SUPI PLMN ID | /pDUSessionChargingInformation /pduSessionInformation/hPlmnId |
| Serving Network Function ID | Serving Network Function ID | /pDUSessionChargingInformation /pduSessionInformation/ servingNetworkFunctionID |
| Serving CN PLMN ID | Serving CN PLMN ID | /pDUSessionChargingInformation/pduSessionInformation/servingCNPlmnId |
| RAT Type | RAT Type | /pDUSessionChargingInformation /pduSessionInformation/ratType |
| MA PDU Non 3GPP RAT Type | MA PDU Non 3GPP RAT Type | /pDUSessionChargingInformation /pduSessionInformation/mAPDUNon3GPPRATType |
| Data Network Name Identifier | Data Network Name Identifier | /pDUSessionChargingInformation /pduSessionInformation/dnnid |
| DNN Selection Mode | DNN Selection Mode | /pDUSessionChargingInformation /pduSessionInformation/dNNselectionMode |
| Authorized QoS information | Authorized Qos Information | /pDUSessionChargingInformation /pduSessionInformation/authorized qoSInformation |
| Subscribed QoS Information | Subscribed QoS Information | /pDUSessionChargingInformation /pduSessionInformation/subscribedQoSInformation |
| Authorized Session-AMBR | Authorized Session-AMBR | /pDUSessionChargingInformation /pduSessionInformation/authorizedSessionAMBR |
| Subscribed Session-AMBR | Subscribed Session-AMBR | /pDUSessionChargingInformation /pduSessionInformation/subscribedSessionAMBR |
| Charging Characteristics | Charging Characteristics | /pDUSessionChargingInformation /pduSessionInformation/ chargingCharacteristics |
| Charging CharacteristicsSelection Mode | Charging Characteristics Selection Mode | /pDUSessionChargingInformation /pduSessionInformation/chargingCharacteristicsSelectionMode |
| PDU session start Time | PDU session start Time | /pDUSessionChargingInformation /pduSessionInformation/startTime |
| PDU session stop Time | PDU session stop Time | /pDUSessionChargingInformation /pduSessionInformation/stopTime |
| Diagnostics | Diagnostics | /pDUSessionChargingInformation /pduSessionInformation/diagnostics |
| Enhanced Diagnostics | Enhanced Diagnostics | /pDUSessionChargingInformation /pduSessionInformation/enhancedDiagnostics |
| 3GPP PS Data Off Status | 3GPP PS Data Off Status | /pDUSessionChargingInformation /pduSessionInformation/3gppPSDataOffStatus |
| Session Stop Indicator | Session Stop Indicator | /pDUSessionChargingInformation /pduSessionInformation/sessionStopIndicator  |
| Redundant Transmission Type | Redundant Transmission Type | /pDUSessionChargingInformation /pduSessionInformation/redundantTransmissionType |
| PDU Session Pair ID | PDU Session Pair ID | /pDUSessionChargingInformation /pduSessionInformation/pDUSessionPairID |
| Qos Monitoring Information | Qos Monitoring Information | /pDUSessionChargingInformation /pduSessionInformation/qosMonitoringInformation |
| Unit Count Inactivity Timer | - | /pDUSessionChargingInformation/unitCountInactivityTimer |
| RAN Secondary RAT Usage Report | RAN Secondary RAT Usage Report | /pDUSessionChargingInformation/rANSecondaryRATUsageReport |
| NG RAN Secondary RAT Type | NG RAN Secondary RAT Type | /pDUSessionChargingInformation/rANSecondaryRATUsageReport/rANSecondaryRATType |
| Qos Flows Usage Reports | Qos Flows Usage Reports | /pDUSessionChargingInformation/rANSecondaryRATUsageReport/qosFlowsUsageReports |
| Roaming QBC information | Roaming QBC information | /roamingQBCInformation |
| Multiple QFI container | Multiple QFI container | /roamingQBCInformation/multipleQFIcontainer |
| Triggers | Triggers | /roamingQBCInformation/multipleQFIcontainer/triggers |
| Trigger Timestamp | Trigger Timestamp | /roamingQBCInformation/multipleQFIcontainer/triggerTimestamp |
| Time | Time | /roamingQBCInformation/multipleQFIcontainer/time |
| Total Volume | Total Volume | /roamingQBCInformation/multipleQFIcontainer/totalVolume |
| Uplink Volume | Uplink Volume | /roamingQBCInformation/multipleQFIcontainer/uplinkVolume |
| Downlink Volume | Downlink Volume | /roamingQBCInformation/multipleQFIcontainer/downlinkVolume |
| Local Sequence Number | Local Sequence Number | /roamingQBCInformation/multipleQFIcontainer/localSequenceNumber |
| QFI Container information | QFI Container information | /roamingQBCInformation/multipleQFIcontainer/qFIContainerInformation |
| QoS Flow Id | QoS Flow Id | /roamingQBCInformation/multipleQFIcontainer/ qFIContainerInformation/qFI |
| Time of First Usage | Time of First Usage | /roamingQBCInformation/multipleQFIcontainer/qFIContainerInformation/ timeofFirstUsage |
| Time of Last Usage | Time of Last Usage | /roamingQBCInformation/multipleQFIcontainer/qFIContainerInformation/timeofLastUsage |
| QoS Information | QoS Information | /roamingQBCInformation/multipleQFIcontainer/qFIContainerInformation/qoSInformation |
| QoS Characteristics | QoS Characteristics | /roamingQBCInformation/multipleQFIcontainer/ qFIContainerInformation/qoSCharacteristics |
| User Location Information | User Location Information | /roamingQBCInformation/multipleQFIcontainer/qFIContainerInformation/ userLocationInformation |
| UE Time Zone | UE Time Zone | /roamingQBCInformation/multipleQFIcontainer/qFIContainerInformation/uetimeZone |
| Presence Reporting Area Information | Presence Reporting Area Information | /roamingQBCInformation/multipleQFIcontainer/qFIContainerInformation/presenceReportingAreaInformation |
| RAT Type | RAT Type | /roamingQBCInformation/multipleQFIcontainer/qFIContainerInformation/rATType |
| Report Time | Report Time | /roamingQBCInformation/multipleQFIcontainer/ qFIContainerInformation/reportTime |
| Serving Network Function ID  | Serving Network Function ID  | /roamingQBCInformation/multipleQFIcontainer/qFIContainerInformation/ servingNetworkFunctionID |
| 3GPP PS Data Off Status | 3GPP PS Data Off Status | /roamingQBCInformation/multipleQFIcontainer/qFIContainerInformation/3gppPSDataOffStatus |
| EPS bearer Charging Id | EPS bearer Charging Id | /roamingQBCInformation/multipleQFIcontainer/qFIContainerInformation/3gppChargingId |
| Diagnostics | Diagnostics | /roamingQBCInformation/multipleQFIcontainer/qFIContainerInformation/diagnostics |
| Enhanced Diagnostics | Enhanced Diagnostics | /roamingQBCInformation/multipleQFIcontainer/qFIContainerInformation/enhancedDiagnostics |
| UPF ID | UPF ID | /roamingQBCInformation/uPFID |
| Roaming Charging Profile | Roaming Charging Profile | /roamingQBCInformation/roamingChargingProfile |
| Trigger  | Trigger  | /roamingQBCInformationroamingChargingProfile/trigger |
| Partial record method | Partial record method | /roamingQBCInformation/roamingChargingProfile/partialRecordMethod |
|  |  | **ChargingDataResponse** |
| Supported Features | - | **/**supportedFeatures |
| Multiple Unit information | - | /multipleUnitInformation |
| UPF ID | - | /multipleUnitInformation/uPFID |
| PDU Session Charging Information | - | /pDUSessionChargingInformation  |
| Presence Reporting AreaInformation | - | /pDUSessionChargingInformation/ presenceReportingAreaInformation |
| Unit Count Inactivity Timer | - | /pDUSessionChargingInformation/unitCountInactivityTimer |
| Roaming QBC information | - | /roamingQBCInformation |
| Roaming Charging Profile | - | /roamingQBCInformation/roamingChargingProfile |

|  |
| --- |
| **Next change** |

## A.2 Nchf\_ConvergedCharging API

openapi: 3.0.0

info:

 title: Nchf\_ConvergedCharging

 version: 3.1.0-alpha.1

 description: |

 ConvergedCharging Service © 2021, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

externalDocs:

 description: >

 3GPP TS 32.291 V17.0.0: Telecommunication management; Charging management;

 5G system, charging service; Stage 3.

 url: 'http://www.3gpp.org/ftp/Specs/archive/32\_series/32.291/'

servers:

 - url: '{apiRoot}/nchf-convergedcharging/v3'

 variables:

 apiRoot:

 default: https://example.com

 description: apiRoot as defined in subclause 4.4 of 3GPP TS 29.501.

security:

 - {}

 - oAuth2ClientCredentials:

 - nchf-convergedcharging

paths:

 /chargingdata:

 post:

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/ChargingDataRequest'

 responses:

 '201':

 description: Created

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/ChargingDataResponse'

 '400':

 description: Bad request

 content:

 application/problem+json:

 schema:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

 '403':

 description: Forbidden

 content:

 application/problem+json:

 schema:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

 '404':

 description: Not Found

 content:

 application/problem+json:

 schema:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '410':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/410'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 callbacks:

 chargingNotification:

 '{$request.body#/notifyUri}':

 post:

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/ChargingNotifyRequest'

 responses:

 '204':

 description: 'No Content, Notification was succesfull'

 '400':

 description: Bad request

 content:

 application/problem+json:

 schema:

 $ref: >-

 TS29571\_CommonData.yaml#/components/schemas/ProblemDetails

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 '/chargingdata/{ChargingDataRef}/update':

 post:

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/ChargingDataRequest'

 parameters:

 - name: ChargingDataRef

 in: path

 description: a unique identifier for a charging data resource in a PLMN

 required: true

 schema:

 type: string

 responses:

 '200':

 description: OK. Updated Charging Data resource is returned

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/ChargingDataResponse'

 '400':

 description: Bad request

 content:

 application/problem+json:

 schema:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

 '403':

 description: Forbidden

 content:

 application/problem+json:

 schema:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

 '404':

 description: Not Found

 content:

 application/problem+json:

 schema:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '410':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/410'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 '/chargingdata/{ChargingDataRef}/release':

 post:

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/ChargingDataRequest'

 parameters:

 - name: ChargingDataRef

 in: path

 description: a unique identifier for a charging data resource in a PLMN

 required: true

 schema:

 type: string

 responses:

 '204':

 description: No Content.

 '404':

 description: Not Found

 content:

 application/problem+json:

 schema:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '410':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/410'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

components:

 securitySchemes:

 oAuth2ClientCredentials:

 type: oauth2

 flows:

 clientCredentials:

 tokenUrl: '{nrfApiRoot}/oauth2/token'

 scopes:

 nchf-convergedcharging: Access to the Nchf\_ConvergedCharging API

 schemas:

 ChargingDataRequest:

 type: object

 properties:

 subscriberIdentifier:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 tenantIdentifier:

 type: string

 chargingId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ChargingId'

 mnSConsumerIdentifier:

 type: string

 nfConsumerIdentification:

 $ref: '#/components/schemas/NFIdentification'

 invocationTimeStamp:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 invocationSequenceNumber:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 retransmissionIndicator:

 type: boolean

 oneTimeEvent:

 type: boolean

 oneTimeEventType:

 $ref: '#/components/schemas/oneTimeEventType'

 notifyUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 supportedFeatures:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 serviceSpecificationInfo:

 type: string

 multipleUnitUsage:

 type: array

 items:

 $ref: '#/components/schemas/MultipleUnitUsage'

 minItems: 0

 triggers:

 type: array

 items:

 $ref: '#/components/schemas/Trigger'

 minItems: 0

 pDUSessionChargingInformation:

 $ref: '#/components/schemas/PDUSessionChargingInformation'

 roamingQBCInformation:

 $ref: '#/components/schemas/RoamingQBCInformation'

 sMSChargingInformation:

 $ref: '#/components/schemas/SMSChargingInformation'

 nEFChargingInformation:

 $ref: '#/components/schemas/NEFChargingInformation'

 registrationChargingInformation:

 $ref: '#/components/schemas/RegistrationChargingInformation'

 n2ConnectionChargingInformation:

 $ref: '#/components/schemas/N2ConnectionChargingInformation'

 locationReportingChargingInformation:

 $ref: '#/components/schemas/LocationReportingChargingInformation'

 nSPAChargingInformation:

 $ref: '#/components/schemas/NSPAChargingInformation'

 nSMChargingInformation:

 $ref: '#/components/schemas/NSMChargingInformation'

 required:

 - nfConsumerIdentification

 - invocationTimeStamp

 - invocationSequenceNumber

 ChargingDataResponse:

 type: object

 properties:

 invocationTimeStamp:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 invocationSequenceNumber:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 invocationResult:

 $ref: '#/components/schemas/InvocationResult'

 sessionFailover:

 $ref: '#/components/schemas/SessionFailover'

 supportedFeatures:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 multipleUnitInformation:

 type: array

 items:

 $ref: '#/components/schemas/MultipleUnitInformation'

 minItems: 0

 triggers:

 type: array

 items:

 $ref: '#/components/schemas/Trigger'

 minItems: 0

 pDUSessionChargingInformation:

 $ref: '#/components/schemas/PDUSessionChargingInformation'

 roamingQBCInformation:

 $ref: '#/components/schemas/RoamingQBCInformation'

 locationReportingChargingInformation:

 $ref: '#/components/schemas/LocationReportingChargingInformation'

 required:

 - invocationTimeStamp

 - invocationSequenceNumber

 ChargingNotifyRequest:

 type: object

 properties:

 notificationType:

 $ref: '#/components/schemas/NotificationType'

 reauthorizationDetails:

 type: array

 items:

 $ref: '#/components/schemas/ReauthorizationDetails'

 minItems: 0

 required:

 - notificationType

 ChargingNotifyResponse:

 type: object

 properties:

 invocationResult:

 $ref: '#/components/schemas/InvocationResult'

 NFIdentification:

 type: object

 properties:

 nFName:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 nFIPv4Address:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 nFIPv6Address:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

 nFPLMNID:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

 nodeFunctionality:

 $ref: '#/components/schemas/NodeFunctionality'

 nFFqdn:

 type: string

 required:

 - nodeFunctionality

 MultipleUnitUsage:

 type: object

 properties:

 ratingGroup:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatingGroup'

 requestedUnit:

 $ref: '#/components/schemas/RequestedUnit'

 usedUnitContainer:

 type: array

 items:

 $ref: '#/components/schemas/UsedUnitContainer'

 minItems: 0

 uPFID:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 multihomedPDUAddress:

 $ref: '#/components/schemas/PDUAddress'

 required:

 - ratingGroup

 InvocationResult:

 type: object

 properties:

 error:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

 failureHandling:

 $ref: '#/components/schemas/FailureHandling'

 Trigger:

 type: object

 properties:

 triggerType:

 $ref: '#/components/schemas/TriggerType'

 triggerCategory:

 $ref: '#/components/schemas/TriggerCategory'

 timeLimit:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 volumeLimit:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 volumeLimit64:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 eventLimit:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 maxNumberOfccc:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 tariffTimeChange:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 required:

 - triggerType

 - triggerCategory

 MultipleUnitInformation:

 type: object

 properties:

 resultCode:

 $ref: '#/components/schemas/ResultCode'

 ratingGroup:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatingGroup'

 grantedUnit:

 $ref: '#/components/schemas/GrantedUnit'

 triggers:

 type: array

 items:

 $ref: '#/components/schemas/Trigger'

 minItems: 0

 validityTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 quotaHoldingTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 finalUnitIndication:

 $ref: '#/components/schemas/FinalUnitIndication'

 timeQuotaThreshold:

 type: integer

 volumeQuotaThreshold:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 unitQuotaThreshold:

 type: integer

 uPFID:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 required:

 - ratingGroup

 RequestedUnit:

 type: object

 properties:

 time:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 totalVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 uplinkVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 downlinkVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 serviceSpecificUnits:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 UsedUnitContainer:

 type: object

 properties:

 serviceId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ServiceId'

 quotaManagementIndicator:

 $ref: '#/components/schemas/QuotaManagementIndicator'

 triggers:

 type: array

 items:

 $ref: '#/components/schemas/Trigger'

 minItems: 0

 triggerTimestamp:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 time:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 totalVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 uplinkVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 downlinkVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 serviceSpecificUnits:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 eventTimeStamps:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 minItems: 0

 localSequenceNumber:

 type: integer

 pDUContainerInformation:

 $ref: '#/components/schemas/PDUContainerInformation'

 nSPAContainerInformation:

 $ref: '#/components/schemas/NSPAContainerInformation'

 required:

 - localSequenceNumber

 GrantedUnit:

 type: object

 properties:

 tariffTimeChange:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 time:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 totalVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 uplinkVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 downlinkVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 serviceSpecificUnits:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 FinalUnitIndication:

 type: object

 properties:

 finalUnitAction:

 $ref: '#/components/schemas/FinalUnitAction'

 restrictionFilterRule:

 $ref: '#/components/schemas/IPFilterRule'

 restrictionFilterRuleList:

 type: array

 items:

 $ref: '#/components/schemas/IPFilterRule'

 minItems: 1

 filterId:

 type: string

 filterIdList:

 type: array

 items:

 type: string

 minItems: 1

 redirectServer:

 $ref: '#/components/schemas/RedirectServer'

 required:

 - finalUnitAction

 RedirectServer:

 type: object

 properties:

 redirectAddressType:

 $ref: '#/components/schemas/RedirectAddressType'

 redirectServerAddress:

 type: string

 required:

 - redirectAddressType

 - redirectServerAddress

 ReauthorizationDetails:

 type: object

 properties:

 serviceId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ServiceId'

 ratingGroup:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatingGroup'

 quotaManagementIndicator:

 $ref: '#/components/schemas/QuotaManagementIndicator'

 PDUSessionChargingInformation:

 type: object

 properties:

 chargingId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ChargingId'

 homeProvidedChargingId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ChargingId'

 userInformation:

 $ref: '#/components/schemas/UserInformation'

 userLocationinfo:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 mAPDUNon3GPPUserLocationInfo:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 presenceReportingAreaInformation:

 type: object

 additionalProperties:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

 minProperties: 0

 uetimeZone:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

 pduSessionInformation:

 $ref: '#/components/schemas/PDUSessionInformation'

 unitCountInactivityTimer:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'
 rANSecondaryRATUsageReport:

 $ref: '#/components/schemas/RANSecondaryRATUsageReport'

 UserInformation:

 type: object

 properties:

 servedGPSI:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 servedPEI:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Pei'

 unauthenticatedFlag:

 type: boolean

 roamerInOut:

 $ref: '#/components/schemas/RoamerInOut'

 PDUSessionInformation:

 type: object

 properties:

 networkSlicingInfo:

 $ref: '#/components/schemas/NetworkSlicingInfo'

 pduSessionID:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PduSessionId'

 pduType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PduSessionType'

 sscMode:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SscMode'

 hPlmnId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

 servingNetworkFunctionID:

 $ref: '#/components/schemas/ServingNetworkFunctionID'

 ratType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 mAPDUNon3GPPRATType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 dnnId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 dnnSelectionMode:

 $ref: '#/components/schemas/dnnSelectionMode'

 chargingCharacteristics:

 type: string

 pattern: '^[0-9a-fA-F]{1,4}$'

 chargingCharacteristicsSelectionMode:

 $ref: '#/components/schemas/ChargingCharacteristicsSelectionMode'

 startTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 stopTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 3gppPSDataOffStatus:

 $ref: '#/components/schemas/3GPPPSDataOffStatus'

 sessionStopIndicator:

 type: boolean

 pduAddress:

 $ref: '#/components/schemas/PDUAddress'

 diagnostics:

 $ref: '#/components/schemas/Diagnostics'

 authorizedQoSInformation:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/AuthorizedDefaultQos'

 subscribedQoSInformation:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SubscribedDefaultQos'

 authorizedSessionAMBR:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ambr'

 subscribedSessionAMBR:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ambr'

 servingCNPlmnId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

 mAPDUSessionInformation:

 $ref: '#/components/schemas/MAPDUSessionInformation'

 enhancedDiagnostics:

 $ref: '#/components/schemas/EnhancedDiagnostics5G'

 redundantTransmissionType:

 $ref: '#/components/schemas/RedundantTransmissionType'

 pDUSessionPairID:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 qosMonReports:

 type: array

 items:

 $ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/QosMonitoringReport'

 minItems: 1

 required:

 - pduSessionID

 - dnnId

 PDUContainerInformation:

 type: object

 properties:

 timeofFirstUsage:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 timeofLastUsage:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 qoSInformation:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/QosData'

 qoSCharacteristics:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/QosCharacteristics'

 afChargingIdentifier:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ChargingId'

 afChargingIdString:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationChargingId'

 userLocationInformation:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 uetimeZone:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

 rATType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 servingNodeID:

 type: array

 items:

 $ref: '#/components/schemas/ServingNetworkFunctionID'

 minItems: 0

 presenceReportingAreaInformation:

 type: object

 additionalProperties:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

 minProperties: 0

 3gppPSDataOffStatus:

 $ref: '#/components/schemas/3GPPPSDataOffStatus'

 sponsorIdentity:

 type: string

 applicationserviceProviderIdentity:

 type: string

 chargingRuleBaseName:

 type: string

 mAPDUSteeringFunctionality:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/SteeringFunctionality'

 mAPDUSteeringMode:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/SteeringMode'

 NSPAContainerInformation:

 type: object

 properties:

 latency:

 type: integer

 throughput:

 $ref: '#/components/schemas/Throughput'

 maximumPacketLossRate:

 type: string

 serviceExperienceStatisticsData:

 $ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/ServiceExperienceInfo'

 theNumberOfPDUSessions:

 type: integer

 theNumberOfRegisteredSubscribers:

 type: integer

 loadLevel:

 $ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/NsiLoadLevelInfo'

 NSPAChargingInformation:

 type: object

 properties:

 singleNSSAI:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 required:

 - singleNSSAI

 NetworkSlicingInfo:

 type: object

 properties:

 sNSSAI:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 required:

 - sNSSAI

 PDUAddress:

 type: object

 properties:

 pduIPv4Address:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 pduIPv6AddresswithPrefix:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

 pduAddressprefixlength:

 type: integer

 iPv4dynamicAddressFlag:

 type: boolean

 iPv6dynamicPrefixFlag:

 type: boolean

 addIpv6AddrPrefixes:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Prefix'

 ServingNetworkFunctionID:

 type: object

 properties:

 servingNetworkFunctionInformation:

 $ref: '#/components/schemas/NFIdentification'

 aMFId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/AmfId'

 required:

 - servingNetworkFunctionInformation

 RoamingQBCInformation:

 type: object

 properties:

 multipleQFIcontainer:

 type: array

 items:

 $ref: '#/components/schemas/MultipleQFIcontainer'

 minItems: 0

 uPFID:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 roamingChargingProfile:

 $ref: '#/components/schemas/RoamingChargingProfile'

 MultipleQFIcontainer:

 type: object

 properties:

 triggers:

 type: array

 items:

 $ref: '#/components/schemas/Trigger'

 minItems: 0

 triggerTimestamp:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 time:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 totalVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 uplinkVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 downlinkVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 localSequenceNumber:

 type: integer

 qFIContainerInformation:

 $ref: '#/components/schemas/QFIContainerInformation'

 required:

 - localSequenceNumber

 QFIContainerInformation:

 type: object

 properties:

 qFI:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Qfi'

 reportTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 timeofFirstUsage:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 timeofLastUsage:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 qoSInformation:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/QosData'

 qoSCharacteristics:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/QosCharacteristics'

 userLocationInformation:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 uetimeZone:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

 presenceReportingAreaInformation:

 type: object

 additionalProperties:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

 minProperties: 0

 rATType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 servingNetworkFunctionID:

 type: array

 items:

 $ref: '#/components/schemas/ServingNetworkFunctionID'

 minItems: 0

 3gppPSDataOffStatus:

 $ref: '#/components/schemas/3GPPPSDataOffStatus'

 3gppChargingId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ChargingId'

 diagnostics:

 $ref: '#/components/schemas/Diagnostics'

 enhancedDiagnostics:

 type: array

 items:

 type: string

 required:

 - reportTime

 RoamingChargingProfile:

 type: object

 properties:

 triggers:

 type: array

 items:

 $ref: '#/components/schemas/Trigger'

 minItems: 0

 partialRecordMethod:

 $ref: '#/components/schemas/PartialRecordMethod'

 SMSChargingInformation:

 type: object

 properties:

 originatorInfo:

 $ref: '#/components/schemas/OriginatorInfo'

 recipientInfo:

 type: array

 items:

 $ref: '#/components/schemas/RecipientInfo'

 minItems: 0

 userEquipmentInfo:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Pei'

 roamerInOut:

 $ref: '#/components/schemas/RoamerInOut'

 userLocationinfo:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 uetimeZone:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

 rATType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 sMSCAddress:

 type: string

 sMDataCodingScheme:

 type: integer

 sMMessageType:

 $ref: '#/components/schemas/SMMessageType'

 sMReplyPathRequested:

 $ref: '#/components/schemas/ReplyPathRequested'

 sMUserDataHeader:

 type: string

 sMStatus:

 type: string

 pattern: '^[0-7]?[0-9a-fA-F]$'

 sMDischargeTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 numberofMessagesSent:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 sMServiceType:

 $ref: '#/components/schemas/SMServiceType'

 sMSequenceNumber:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 sMSresult:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 submissionTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 sMPriority:

 $ref: '#/components/schemas/SMPriority'

 messageReference:

 type: string

 messageSize:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 messageClass:

 $ref: '#/components/schemas/MessageClass'

 deliveryReportRequested:

 $ref: '#/components/schemas/DeliveryReportRequested'

 OriginatorInfo:

 type: object

 properties:

 originatorSUPI:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 originatorGPSI:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 originatorOtherAddress:

 $ref: '#/components/schemas/SMAddressInfo'

 originatorReceivedAddress:

 $ref: '#/components/schemas/SMAddressInfo'

 originatorSCCPAddress:

 type: string

 sMOriginatorInterface:

 $ref: '#/components/schemas/SMInterface'

 sMOriginatorProtocolId:

 type: string

 RecipientInfo:

 type: object

 properties:

 recipientSUPI:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 recipientGPSI:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 recipientOtherAddress:

 $ref: '#/components/schemas/SMAddressInfo'

 recipientReceivedAddress:

 $ref: '#/components/schemas/SMAddressInfo'

 recipientSCCPAddress:

 type: string

 sMDestinationInterface:

 $ref: '#/components/schemas/SMInterface'

 sMrecipientProtocolId:

 type: string

 SMAddressInfo:

 type: object

 properties:

 sMaddressType:

 $ref: '#/components/schemas/SMAddressType'

 sMaddressData:

 type: string

 sMaddressDomain:

 $ref: '#/components/schemas/SMAddressDomain'

 RecipientAddress:

 type: object

 properties:

 recipientAddressInfo:

 $ref: '#/components/schemas/SMAddressInfo'

 sMaddresseeType:

 $ref: '#/components/schemas/SMAddresseeType'

 MessageClass:

 type: object

 properties:

 classIdentifier:

 $ref: '#/components/schemas/ClassIdentifier'

 tokenText:

 type: string

 SMAddressDomain:

 type: object

 properties:

 domainName:

 type: string

 3GPPIMSIMCCMNC:

 type: string

 SMInterface:

 type: object

 properties:

 interfaceId:

 type: string

 interfaceText:

 type: string

 interfacePort:

 type: string

 interfaceType:

 $ref: '#/components/schemas/InterfaceType'

 RANSecondaryRATUsageReport:

 type: object

 properties:

 rANSecondaryRATType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 qosFlowsUsageReports:

 type: array

 items:

 $ref: '#/components/schemas/QosFlowsUsageReport'

 Diagnostics:

 type: integer

 IPFilterRule:

 type: string

 QosFlowsUsageReport:

 type: object

 properties:

 qFI:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Qfi'

 startTimestamp:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 endTimestamp:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 uplinkVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 downlinkVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 NEFChargingInformation:

 type: object

 properties:

 externalIndividualIdentifier:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 externalGroupIdentifier:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ExternalGroupId'

 groupIdentifier:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

 aPIDirection:

 $ref: '#/components/schemas/APIDirection'

 aPITargetNetworkFunction:

 $ref: '#/components/schemas/NFIdentification'

 aPIResultCode:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 aPIName:

 type: string

 aPIReference:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 aPIContent:

 type: string

 required:

 - aPIName

 RegistrationChargingInformation:

 type: object

 properties:

 registrationMessagetype:

 $ref: '#/components/schemas/RegistrationMessageType'

 userInformation:

 $ref: '#/components/schemas/UserInformation'

 userLocationinfo:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 pSCellInformation:

 $ref: '#/components/schemas/PSCellInformation'

 uetimeZone:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

 rATType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 5GMMCapability:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Bytes'

 mICOModeIndication:

 $ref: '#/components/schemas/MICOModeIndication'

 smsIndication:

 $ref: '#/components/schemas/SmsIndication'

 taiList:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Tai'

 minItems: 0

 serviceAreaRestriction:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ServiceAreaRestriction'

 minItems: 0

 requestedNSSAI:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 minItems: 0

 allowedNSSAI:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 minItems: 0

 rejectedNSSAI:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 minItems: 0

 nSSAIMapList:

 type: array

 items:

 $ref: '#/components/schemas/NSSAIMap'

 minItems: 0

 amfUeNgapId:

 type: integer

 ranUeNgapId:

 type: integer

 ranNodeId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/GlobalRanNodeId'

 required:

 - registrationMessagetype

 PSCellInformation:

 type: object

 properties:

 nrcgi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ncgi'

 ecgi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ecgi'

 NSSAIMap:

 type: object

 properties:

 servingSnssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 homeSnssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 required:

 - servingSnssai

 - homeSnssai

 N2ConnectionChargingInformation:

 type: object

 properties:

 n2ConnectionMessageType:

 $ref: '#/components/schemas/N2ConnectionMessageType'

 userInformation:

 $ref: '#/components/schemas/UserInformation'

 userLocationinfo:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 pSCellInformation:

 $ref: '#/components/schemas/PSCellInformation'

 uetimeZone:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

 rATType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 amfUeNgapId:

 type: integer

 ranUeNgapId:

 type: integer

 ranNodeId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/GlobalRanNodeId'

 restrictedRatList:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 minItems: 0

 forbiddenAreaList:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Area'

 minItems: 0

 serviceAreaRestriction:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ServiceAreaRestriction'

 minItems: 0

 restrictedCnList:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/CoreNetworkType'

 minItems: 0

 allowedNSSAI:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 minItems: 0

 rrcEstCause:

 type: string

 pattern: '^[0-9a-fA-F]+$'

 required:

 - n2ConnectionMessageType

 LocationReportingChargingInformation:

 type: object

 properties:

 locationReportingMessageType:

 $ref: '#/components/schemas/LocationReportingMessageType'

 userInformation:

 $ref: '#/components/schemas/UserInformation'

 userLocationinfo:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 pSCellInformation:

 $ref: '#/components/schemas/PSCellInformation'

 uetimeZone:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

 rATType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 presenceReportingAreaInformation:

 type: object

 additionalProperties:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

 minProperties: 0

 required:

 - locationReportingMessageType

 N2ConnectionMessageType:

 type: integer

 LocationReportingMessageType:

 type: integer

 NSMChargingInformation:

 type: object

 properties:

 managementOperation:

 $ref: '#/components/schemas/ManagementOperation'

 idNetworkSliceInstance:

 type: string

 listOfserviceProfileChargingInformation:

 type: array

 items:

 $ref: '#/components/schemas/ServiceProfileChargingInformation'

 minItems: 0

 managementOperationStatus:

 $ref: '#/components/schemas/ManagementOperationStatus'

# To be introduced once the reference to 'generic.yaml is resolved

# managementOperationalState:

# $ref: 'genericNrm.yaml#/components/schemas/OperationalState'

# managementAdministrativeState:

# $ref: 'genericNrm.yaml#/components/schemas/AdministrativeState'

 required:

 - managementOperation

 ServiceProfileChargingInformation:

 type: object

 properties:

 serviceProfileIdentifier:

 type: string

 sNSSAIList:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 minItems: 0

# To be introduced once the reference to 'nrNrm.yaml is resolved

# sST:

# $ref: 'nrNrm.yaml#/components/schemas/Sst'

 latency:

 type: integer

 availability:

 type: number

# To be introduced once the reference to sliceNrm.yaml is resolved

# resourceSharingLevel:

# $ref: 'sliceNrm.yaml#/components/schemas/SharingLevel'

 jitter:

 type: integer

 reliability:

 type: string

 maxNumberofUEs:

 type: integer

 coverageArea:

 type: string

# To be introduced once the reference to sliceNrm.yaml is resolved

# uEMobilityLevel:

# $ref: 'sliceNrm.yaml#/components/schemas/MobilityLevel'

# delayToleranceIndicator:

# $ref: 'sliceNrm.yaml#/components/schemas/Support'

 dLThptPerSlice:

 $ref: '#/components/schemas/Throughput'

 dLThptPerUE:

 $ref: '#/components/schemas/Throughput'

 uLThptPerSlice:

 $ref: '#/components/schemas/Throughput'

 uLThptPerUE:

 $ref: '#/components/schemas/Throughput'

 maxNumberofPDUsessions:

 type: integer

 kPIMonitoringList:

 type: string

 supportedAccessTechnology:

 type: integer

# To be introduced once the reference to sliceNrm.yaml is resolved

# v2XCommunicationModeIndicator:

# $ref: 'sliceNrm.yaml#/components/schemas/Support'

 addServiceProfileInfo:

 type: string

 Throughput:

 type: object

 properties:

 guaranteedThpt:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 maximumThpt:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 MAPDUSessionInformation:

 type: object

 properties:

 mAPDUSessionIndicator:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/MaPduIndication'

 aTSSSCapability:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/AtsssCapability'

 EnhancedDiagnostics5G:

 $ref: '#/components/schemas/RanNasCauseList'

 RanNasCauseList:

 type: array

 items:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/RanNasRelCause'

 NotificationType:

 anyOf:

 - type: string

 enum:

 - REAUTHORIZATION

 - ABORT\_CHARGING

 - type: string

 NodeFunctionality:

 anyOf:

 - type: string

 enum:

 - AMF

 - SMF

 - SMS

 - PGW\_C\_SMF

 - NEFF # Included for backwards compatibility, shall not be used

 - SGW

 - I\_SMF

 - ePDG

 - CEF

 - NEF

 - MnS\_Producer

 - SGSN

 - type: string

 ChargingCharacteristicsSelectionMode:

 anyOf:

 - type: string

 enum:

 - HOME\_DEFAULT

 - ROAMING\_DEFAULT

 - VISITING\_DEFAULT

 - type: string

 TriggerType:

 anyOf:

 - type: string

 enum:

 - QUOTA\_THRESHOLD

 - QHT

 - FINAL

 - QUOTA\_EXHAUSTED

 - VALIDITY\_TIME

 - OTHER\_QUOTA\_TYPE

 - FORCED\_REAUTHORISATION

 - UNUSED\_QUOTA\_TIMER # Included for backwards compatibility, shall not be used

 - UNIT\_COUNT\_INACTIVITY\_TIMER

 - ABNORMAL\_RELEASE

 - QOS\_CHANGE

 - VOLUME\_LIMIT

 - TIME\_LIMIT

 - EVENT\_LIMIT

 - PLMN\_CHANGE

 - USER\_LOCATION\_CHANGE

 - RAT\_CHANGE

 - SESSION\_AMBR\_CHANGE

 - UE\_TIMEZONE\_CHANGE

 - TARIFF\_TIME\_CHANGE

 - MAX\_NUMBER\_OF\_CHANGES\_IN\_CHARGING\_CONDITIONS

 - MANAGEMENT\_INTERVENTION

 - CHANGE\_OF\_UE\_PRESENCE\_IN\_PRESENCE\_REPORTING\_AREA

 - CHANGE\_OF\_3GPP\_PS\_DATA\_OFF\_STATUS

 - SERVING\_NODE\_CHANGE

 - REMOVAL\_OF\_UPF

 - ADDITION\_OF\_UPF

 - INSERTION\_OF\_ISMF

 - REMOVAL\_OF\_ISMF

 - CHANGE\_OF\_ISMF

 - START\_OF\_SERVICE\_DATA\_FLOW

 - ECGI\_CHANGE

 - TAI\_CHANGE

 - HANDOVER\_CANCEL

 - HANDOVER\_START

 - HANDOVER\_COMPLETE

 - GFBR\_GUARANTEED\_STATUS\_CHANGE

 - ADDITION\_OF\_ACCESS

 - REMOVAL\_OF\_ACCESS

 - START\_OF\_SDF\_ADDITIONAL\_ACCESS

 - REDUNDANT\_TRANSMISSION\_CHANGE

 - CGI\_SAI\_CHANGE

 - RAI\_CHANGE

 - type: string

 FinalUnitAction:

 anyOf:

 - type: string

 enum:

 - TERMINATE

 - REDIRECT

 - RESTRICT\_ACCESS

 - type: string

 RedirectAddressType:

 anyOf:

 - type: string

 enum:

 - IPV4

 - IPV6

 - URL

 - type: string

 TriggerCategory:

 anyOf:

 - type: string

 enum:

 - IMMEDIATE\_REPORT

 - DEFERRED\_REPORT

 - type: string

 QuotaManagementIndicator:

 anyOf:

 - type: string

 enum:

 - ONLINE\_CHARGING

 - OFFLINE\_CHARGING

 - QUOTA\_MANAGEMENT\_SUSPENDED

 - type: string

 FailureHandling:

 anyOf:

 - type: string

 enum:

 - TERMINATE

 - CONTINUE

 - RETRY\_AND\_TERMINATE

 - type: string

 SessionFailover:

 anyOf:

 - type: string

 enum:

 - FAILOVER\_NOT\_SUPPORTED

 - FAILOVER\_SUPPORTED

 - type: string

 3GPPPSDataOffStatus:

 anyOf:

 - type: string

 enum:

 - ACTIVE

 - INACTIVE

 - type: string

 ResultCode:

 anyOf:

 - type: string

 enum:

 - SUCCESS

 - END\_USER\_SERVICE\_DENIED

 - QUOTA\_MANAGEMENT\_NOT\_APPLICABLE

 - QUOTA\_LIMIT\_REACHED

 - END\_USER\_SERVICE\_REJECTED

 - USER\_UNKNOWN

 - RATING\_FAILED

 - QUOTA\_MANAGEMENT

 - type: string

 PartialRecordMethod:

 anyOf:

 - type: string

 enum:

 - DEFAULT

 - INDIVIDUAL

 - type: string

 RoamerInOut:

 anyOf:

 - type: string

 enum:

 - IN\_BOUND

 - OUT\_BOUND

 - type: string

 SMMessageType:

 anyOf:

 - type: string

 enum:

 - SUBMISSION

 - DELIVERY\_REPORT

 - SM\_SERVICE\_REQUEST

 - DELIVERY

 - type: string

 SMPriority:

 anyOf:

 - type: string

 enum:

 - LOW

 - NORMAL

 - HIGH

 - type: string

 DeliveryReportRequested:

 anyOf:

 - type: string

 enum:

 - YES

 - NO

 - type: string

 InterfaceType:

 anyOf:

 - type: string

 enum:

 - UNKNOWN

 - MOBILE\_ORIGINATING

 - MOBILE\_TERMINATING

 - APPLICATION\_ORIGINATING

 - APPLICATION\_TERMINATING

 - type: string

 ClassIdentifier:

 anyOf:

 - type: string

 enum:

 - PERSONAL

 - ADVERTISEMENT

 - INFORMATIONAL

 - AUTO

 - type: string

 SMAddressType:

 anyOf:

 - type: string

 enum:

 - EMAIL\_ADDRESS

 - MSISDN

 - IPV4\_ADDRESS

 - IPV6\_ADDRESS

 - NUMERIC\_SHORTCODE

 - ALPHANUMERIC\_SHORTCODE

 - OTHER

 - IMSI

 - type: string

 SMAddresseeType:

 anyOf:

 - type: string

 enum:

 - TO

 - CC

 - BCC

 - type: string

 SMServiceType:

 anyOf:

 - type: string

 enum:

 - VAS4SMS\_SHORT\_MESSAGE\_CONTENT\_PROCESSING

 - VAS4SMS\_SHORT\_MESSAGE\_FORWARDING

 - VAS4SMS\_SHORT\_MESSAGE\_FORWARDING\_MULTIPLE\_SUBSCRIPTIONS

 - VAS4SMS\_SHORT\_MESSAGE\_FILTERING

 - VAS4SMS\_SHORT\_MESSAGE\_RECEIPT

 - VAS4SMS\_SHORT\_MESSAGE\_NETWORK\_STORAGE

 - VAS4SMS\_SHORT\_MESSAGE\_TO\_MULTIPLE\_DESTINATIONS

 - VAS4SMS\_SHORT\_MESSAGE\_VIRTUAL\_PRIVATE\_NETWORK(VPN)

 - VAS4SMS\_SHORT\_MESSAGE\_AUTO\_REPLY

 - VAS4SMS\_SHORT\_MESSAGE\_PERSONAL\_SIGNATURE

 - VAS4SMS\_SHORT\_MESSAGE\_DEFERRED\_DELIVERY

 - type: string

 ReplyPathRequested:

 anyOf:

 - type: string

 enum:

 - NO\_REPLY\_PATH\_SET

 - REPLY\_PATH\_SET

 - type: string

 oneTimeEventType:

 anyOf:

 - type: string

 enum:

 - IEC

 - PEC

 - type: string

 dnnSelectionMode:

 anyOf:

 - type: string

 enum:

 - VERIFIED

 - UE\_DNN\_NOT\_VERIFIED

 - NW\_DNN\_NOT\_VERIFIED

 - type: string

 APIDirection:

 anyOf:

 - type: string

 enum:

 - INVOCATION

 - NOTIFICATION

 - type: string

 RegistrationMessageType:

 anyOf:

 - type: string

 enum:

 - INITIAL

 - MOBILITY

 - PERIODIC

 - EMERGENCY

 - DEREGISTRATION

 - type: string

 MICOModeIndication:

 anyOf:

 - type: string

 enum:

 - MICO\_MODE

 - NO\_MICO\_MODE

 - type: string

 SmsIndication:

 anyOf:

 - type: string

 enum:

 - SMS\_SUPPORTED

 - SMS\_NOT\_SUPPORTED

 - type: string

 ManagementOperation:

 anyOf:

 - type: string

 enum:

 - CreateMOI

 - ModifyMOIAttributes

 - DeleteMOI

 - type: string

 ManagementOperationStatus:

 anyOf:

 - type: string

 enum:

 - OPERATION\_SUCCEEDED

 - OPERATION\_FAILED

 - type: string

 RedundantTransmissionType:

 anyOf:

 - type: string

 enum:

 - NON\_TRANSMISSION

 - END\_TO\_END\_USER\_PLANE\_PATHS

 - N3/N9

 - TRANSPORT\_LAYER

 - type: string

|  |
| --- |
| **End of change** |