**3GPP TSG-SA5 Meeting #139-e *S5-215368***

**Online, , 11th Oct 2021 - 20th Oct 2021**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **28.623** | **CR** | **0139** | **rev** | **-** | **Current version:** | **16.9.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Correction of YANG Solution set | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Ericsson Hungary Ltd | | | | | | | | | |
| ***Source to TSG:*** | S5 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | adNRM | | | | |  | ***Date:*** | | | 2021-10-01 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-16 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | The YANG mapping of some earlier agreed Stage 2 elements is not complete. It is fixed here. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Only YANG is updated to match stage 2. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Faulty/Missing parts in the YANG solution set. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | Forge link: <https://forge.3gpp.org/rep/sa5/MnS/tree/S5-215368_Rel-16_CR_28.623_Correction_of_YANG_Solution_set> | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

***First change***

## D.2.10 module \_3gpp-common-trace.yang

<CODE BEGINS>

module \_3gpp-common-trace {

yang-version 1.1;

namespace "urn:3gpp:sa5:\_3gpp-common-trace";

prefix "trace3gpp";

import \_3gpp-common-top { prefix top3gpp; }

import \_3gpp-common-yang-types {prefix types3gpp; }

import ietf-inet-types { prefix inet; }

organization "3GPP SA5";

contact "https://www.3gpp.org/DynaReport/TSG-WG--S5--officials.htm?Itemid=464";

description "Trace handling";

reference "3GPP TS 28.623

Generic Network Resource Model (NRM)

Integration Reference Point (IRP);

Solution Set (SS) definitions

3GPP TS 28.622

Generic Network Resource Model (NRM)

Integration Reference Point (IRP);

Information Service (IS)";

revision 2021-10-18 { reference "CR-0139"; }

revision 2021-07-22 { reference "CR-0137"; }

revision 2021-01-25 { reference "CR-0122"; }

revision 2020-11-16 { reference "CR-0117"; }

revision 2020-08-06 { reference "CR-0102"; }

grouping TraceJobGrp {

leaf tjJobType {

type enumeration {

enum IMMEDIATE\_MDT\_ONLY;

enum LOGGED\_MDT\_ONLY;

enum TRACE\_ONLY;

enum IMMEDIATE\_MDT\_AND\_TRACE;

enum RLF\_REPORT\_ONLY;

enum RCEF\_REPORT\_ONLY;

enum LOGGED\_MBSFN\_MDT;

}

default TRACE\_ONLY;

description "Specifies the MDT mode and it specifies also whether the

TraceJob represents only MDT, Logged MBSFN MDT, Trace or a combined

Trace and MDT job. The attribute is applicable for Trace, MDT, RCEF and

RLF reporting.";

reference "Clause 5.9a of 3GPP TS 32.422 for additional details on the

allowed values.";

}

list tjListOfInterfaces {

key idx;

must 'count(MSCServerInterfaces)+count(MGWInterfaces)+count(RNCInterfaces)'

+'+count(SGSNInterfaces)+count(GGSNInterfaces)+count(S-CSCFInterfaces)'

+'+count(P-CSCFInterfaces)+count(I-CSCFInterfaces)+count(MRFCInterfaces)'

+'+count(MGCFInterfaces)+count(IBCFInterfaces)+count(E-CSCFInterfaces)'

+'+count(BGCFInterfaces)+count(ASInterfaces)+count(HSSInterfaces)'

+'+count(EIRInterfaces)+count(BM-SCInterfaces)+count(MMEInterfaces)'

+'+count(SGWInterfaces)+count(PDN\_GWInterfaces)+count(eNBInterfaces)'

+'+count(en-gNBInterfaces)+count(AMFInterfaces)+count(AUSFInterfaces)'

+'+count(NEFInterfaces)+count(NRFInterfaces)+count(NSSFInterfaces)'

+'+count(PCFInterfaces)+count(SMFInterfaces)+count(SMSFInterfaces)'

+'+count(UDMInterfaces)+count(UPFInterfaces)+count(ng-eNBInterfaces)'

+'+count(gNB-CU-CPInterfaces)+count(gNB-CU-UPInterfaces)'

+'+count(gNB-DUInterfaces)';

description "Specifies the interfaces that need to be traced in the given

ManagedEntityFunction.The attribute is applicable only for Trace. In

case this attribute is not used, it carries a null semantic.";

reference "Clause 5.5 of 3GPP TS 32.422 for additional details on the

allowed values.";

leaf idx { type uint32 ; }

leaf-list MSCServerInterfaces {

type enumeration {

enum A ;

enum Iu-CS ;

enum Mc ;

enum MAP-G ;

enum MAP-B ;

enum MAP-E ;

enum MAP-F ;

enum MAP-D ;

enum MAP-C ;

enum CAP ;

}

}

leaf-list MGWInterfaces {

type enumeration {

enum Mc ;

enum Nb-UP ;

enum Iu-UP ;

}

}

leaf-list RNCInterfaces {

type enumeration {

enum Iu-CS ;

enum Iu-PS ;

enum Iur ;

enum Iub ;

enum Uu ;

}

}

leaf-list SGSNInterfaces {

type enumeration {

enum Gb ;

enum Iu-PS ;

enum Gn ;

enum MAP-Gr ;

enum MAP-Gd ;

enum MAP-Gf ;

enum Ge ;

enum Gs ;

enum S6d ;

enum S4 ;

enum S3 ;

enum S13 ;

}

}

leaf-list GGSNInterfaces {

type enumeration {

enum Gn ;

enum Gi ;

enum Gmb ;

}

}

leaf-list S-CSCFInterfaces {

type enumeration {

enum Mw ;

enum Mg ;

enum Mr ;

enum Mi ;

}

}

leaf-list P-CSCFInterfaces {

type enumeration {

enum Gm ;

enum Mw ;

}

}

leaf-list I-CSCFInterfaces {

type enumeration {

enum Cx ;

enum Dx ;

enum Mg ;

enum Mw ;

}

}

leaf-list MRFCInterfaces {

type enumeration {

enum Mp ;

enum Mr ;

}

}

leaf-list MGCFInterfaces {

type enumeration {

enum Mg ;

enum Mj ;

enum Mn ;

}

}

leaf-list IBCFInterfaces {

type enumeration {

enum Ix ;

enum Mx ;

}

}

leaf-list E-CSCFInterfaces {

type enumeration {

enum Mw ;

enum Ml ;

enum Mm ;

enum Mi-Mg ;

}

}

leaf-list BGCFInterfaces {

type enumeration {

enum Mi ;

enum Mj ;

enum Mk ;

}

}

leaf-list ASInterfaces {

type enumeration {

enum Dh ;

enum Sh ;

enum ISC ;

enum Ut ;

}

}

leaf-list HSSInterfaces {

type enumeration {

enum MAP-C ;

enum MAP-D ;

enum Gc ;

enum Gr ;

enum Cx ;

enum S6d ;

enum S6a ;

enum Sh ;

}

}

leaf-list EIRInterfaces {

type enumeration {

enum MAP-F ;

enum S13 ;

enum MAP-Gf ;

}

}

leaf-list BM-SCInterfaces {

type enumeration {

enum Gmb ;

}

}

leaf-list MMEInterfaces {

type enumeration {

enum S1-MME ;

enum S3 ;

enum S6a ;

enum S10 ;

enum S11 ;

enum S13 ;

}

}

leaf-list SGWInterfaces {

type enumeration {

enum S4 ;

enum S5 ;

enum S8 ;

enum S11 ;

enum Gxc ;

}

}

leaf-list PDN\_GWInterfaces {

type enumeration {

enum S2a ;

enum S2b ;

enum S2c ;

enum S5 ;

enum S6b ;

enum Gx ;

enum S8 ;

enum SGi ;

}

}

leaf-list eNBInterfaces {

type enumeration {

enum S1-MME ;

enum X2 ;

}

}

leaf-list en-gNBInterfaces {

type enumeration {

enum S1-MME ;

enum X2 ;

enum Uu ;

enum F1-C ;

enum E1 ;

}

}

leaf-list AMFInterfaces {

type enumeration {

enum N1 ;

enum N2 ;

enum N8 ;

enum N11 ;

enum N12 ;

enum N14 ;

enum N15 ;

enum N20 ;

enum N22 ;

enum N26 ;

}

}

leaf-list AUSFInterfaces {

type enumeration {

enum N12 ;

enum N13 ;

}

}

leaf-list NEFInterfaces {

type enumeration {

enum N29 ;

enum N30 ;

enum N33 ;

}

}

leaf-list NRFInterfaces {

type enumeration {

enum N27 ;

}

}

leaf-list NSSFInterfaces {

type enumeration {

enum N22 ;

enum N31 ;

}

}

leaf-list PCFInterfaces {

type enumeration {

enum N5 ;

enum N7 ;

enum N15 ;

}

}

leaf-list SMFInterfaces {

type enumeration {

enum N4 ;

enum N7 ;

enum N10 ;

enum N11 ;

enum S5-C ;

}

}

leaf-list SMSFInterfaces {

type enumeration {

enum N20 ;

enum N21 ;

}

}

leaf-list UDMInterfaces {

type enumeration {

enum N8 ;

enum N10 ;

enum N13 ;

enum N21 ;

}

}

leaf-list UPFInterfaces {

type enumeration {

enum N4 ;

}

}

leaf-list ng-eNBInterfaces {

type enumeration {

enum NG-C ;

enum Xn-C ;

enum Uu ;

}

}

leaf-list gNB-CU-CPInterfaces {

type enumeration {

enum NG-C ;

enum Xn-C ;

enum Uu ;

enum F1-C ;

enum E1 ;

enum X2-C ;

}

}

leaf-list gNB-CU-UPInterfaces {

type enumeration {

enum E1 ;

}

}

leaf-list gNB-DUInterfaces {

type enumeration {

enum F1-C ;

}

}

}

leaf-list tjListOfNeTypes {

type enumeration {

enum MSC\_SERVER;

enum SGSN;

enum MGW;

enum GGSN;

enum RNC;

enum BM\_SC;

enum MME;

enum SGW;

enum PGW;

enum ENB;

enum EN\_GNB;

enum GNB\_CU\_CP;

enum GNB\_CU\_UP;

enum GNB\_DU;

}

description "Specifies in which type of ManagedFunction the trace should

be activated. The attribute is applicable only for Trace with

Signalling Based Trace activation. In case this attribute is not used,

it carries a null semantic";

reference "Clause 5.4 of 3GPP TS 32.422 for additional details on the

allowed values";

}

leaf tjPLMNTarget {

type string;

mandatory true;

description "Specifies which PLMN that the subscriber of the session to

be recorded uses as selected PLMN. PLMN Target might differ from the

PLMN specified in the Trace Reference";

reference "Clause 5.9b of 3GPP TS 32.422";

}

leaf tjStreamingTraceConsumerURI {

when './tjTraceReportingFormat = "STREAMING"';

type inet:uri;

mandatory true;

description "URI of the Streaming Trace data reporting MnS consumer

(a.k.a. streaming target).

This attribute shall be present if file based trace data reporting is

supported and tjTraceReportingFormat set to 'file based' or when

tjJobType is set to Logged MDT or Logged MBSFN MDT.";

reference "Clause 5.9 of 3GPP TS 32.422";

}

leaf tjTraceCollectionEntityAddress {

when './tjTraceReportingFormat = "FILE\_BASED" or '

+'./tjJobType = "LOGGED\_MDT\_ONLY" or ./tjJobType = "LOGGED\_MBSFN\_MDT"';

type union {

type inet:uri;

type inet:ip-address;

}

mandatory true;

description "Specifies the address of the Trace Collection Entity when

the attribute tjTraceReportingFormat is configured for the file-based

reporting. The attribute is applicable for both Trace and MDT.";

reference "Clause 5.9 of 3GPP TS 32.422";

}

leaf tjTraceDepth {

when './tjJobType = "TRACE\_ONLY"'

+ ' or ./tjJobType = "IMMEDIATE\_MDT\_AND\_TRACE"';

type enumeration {

enum MINIMUM;

enum MEDIUM;

enum MAXIMUM;

enum VENDORMINIMUM;

enum VENDORMEDIUM;

enum VENDORMAXIMUM;

}

default MAXIMUM;

description "Specifies how detailed information should be recorded in the

Network Element. The Trace Depth is a paremeter for Trace Session level,

i.e., the Trace Depth is the same for all of the NEs to be traced in

the same Trace Session.

The attribute is applicable only for Trace, otherwise it carries a null

semantic.";

reference "Clause 5.3 of 3GPP TS 32.422";

}

leaf tjTraceReference {

type uint64;

mandatory true;

description "A globally unique identifier, which uniquely identifies the

Trace Session that is created by the TraceJob.

In case of shared network, it is the MCC and MNC of the Participating

Operator that request the trace session that shall be provided.

The attribute is applicable for both Trace and MDT.";

}

leaf tjTraceRecordSessionReference {

type string;

mandatory true;

description "An identifier, which identifies the Trace Recording Session.

The attribute is applicable for both Trace and MDT.

See the clause 5.7 of 3GPP TS 32.422 for additional details on the

allowed values.";

}

leaf tjTraceReportingFormat {

type enumeration {

enum FILE\_BASED;

enum STREAMING;

}

default FILE\_BASED;

description "Specifies the trace reporting format - streaming trace

reporting or file-based trace reporting";

reference "3GPP TS 32.422 clause 5.11";

}

list tjTraceTarget {

key "targetIdType targetIdValue";

max-elements 1;

leaf targetIdType {

type enumeration {

enum IMSI;

enum IMEI;

enum IMEISV;

enum PUBLIC\_ID;

enum UTRAN\_CELL;

enum E\_UTRAN\_CELL;

enum NG\_RAN\_CELL;

enum ENB;

enum RNC;

enum GNB;

enum SUPI;

}

}

leaf targetIdValue {

type string;

}

description "Specifies the target object of the Trace and MDT. The

attribute is applicable for both Trace and MDT. This attribute

includes the ID type of the target as an enumeration and the ID value.

The tjTraceTarget shall be public ID in case of a Management Based

Activation is done to an ScscfFunction. The tjTraceTarget shall be

cell only in case of the UTRAN cell traffic trace function.

The tjTraceTarget shall be E-UtranCell only in case of E-UTRAN cell

traffic trace function.The tjTraceTarget shall be either IMSI or

IMEI(SV) if the Trace Session is activated to any of the following

ManagedEntity(ies):

- HssFunction

- MscServerFunction

- SgsnFunction

- GgsnFunction

- BmscFunction

- RncFunction

- MmeFunction

The tjTraceTarget shall be IMSI if the Trace Session is activated to a

ManagedEntity playing a role of ServinGWFunction.

In case of signaling based Trace/MDT, the tjTraceTarget attribute shall

be able to carry (IMSI or IMEI(SV)or SUPI), the tjMDTAreaScope attribute

shall be able to carry a list of (cell or E-UtranCell or NRCellDU or

TA/LA/RA).

In case of management based Immediate MDT, the tjTraceTarget attribute

shall be null value, the tjMDTAreaScope attribute shall carry a list of

(Utrancell or E-UtranCell or NRCellDU).

In case of management based Logged MDT, the tjTraceTarget attribute

shall carry an eBs or a RNC or gNBs. The Logged MDT should be initiated

on the specified eNB or RNC or gNB in tjTraceTarget. The tjMDTAreaScope

attribute shall carry a list of (Utrancell or E-UtranCell or NRCellDU or

TA/LA/RA).

In case of RLF reporting, or RCEF reporting, the tjTraceTarget

attribute shall be null value, the tjMDTAreaScope attribute shall carry

one or list of eNBs/gNBs";

reference "3GPP TS 32.422";

}

leaf tjTriggeringEvent {

when './tjJobType = "TRACE" or ./tjJobType = "IMMEDIATE\_MDT\_AND\_TRACE"';

type string ;

mandatory true;

description "Specifies the triggering event parameter of the trace session.

The attribute is applicable only for Trace. In case this attribute is

not used, it carries a null semantic.";

reference "Clause 5.1 of 3GPP TS 32.422";

}

leaf tjMDTAnonymizationOfData {

when ./tjMDTAreaScope ;

type enumeration {

enum NO\_IDENTITY;

enum TAC\_OF\_IMEI;

}

default NO\_IDENTITY;

description "Specifies level of MDT anonymization.";

reference "3GPP TS 32.422 clause 5.10.12.";

}

list tjMDTAreaConfigurationForNeighCell {

when './tjJobType = "LOGGED\_MDT\_ONLY"';

key "idx";

min-elements 1;

leaf idx { type uint32 ; }

description "It specifies the area for which UE is requested to perform

measurement logging for neighbour cells which have list of frequencies.

If it is not configured, the UE shall perform measurement logging for

all the neighbour cells.

Applicable only to NR Logged MDT.";

reference "3GPP TS 32.422 clause 5.10.26.";

leaf frequency {

type string;

}

leaf cell {

type string;

}

}

leaf-list tjMDTAreaScope {

type string;

description "specifies MDT area scope when activates an MDT job.

For RLF and RCEF reporting it specifies the eNB or list of eNBs where the

RLF or RCEF reports should be collected.

List of cells/TA/LA/RA for signaling based MDT or management based Logged

MDT.

List of cells for management based Immediate MDT.

Cell, TA, LA, RA are mutually exclusive.

One or list of eNBs for RLF and RCEFreporting";

reference "Clause 5.10.2 of 3GPP TS 32.422";

}

leaf tjMDTCollectionPeriodRrmLte {

when './tjJobType = "IMMEDIATE\_MDT\_ONLY"'

+ ' or ./tjJobType = "IMMEDIATE\_MDT\_AND\_TRACE"';

type uint32 {

range "250|500|1000|2000|3000|4000|6000|8000|12000|16000|20000|"

+"24000|28000|32000|64000";

}

units milliseconds;

description "Specifies the collection period for collecting RRM configured

measurement samples for M2, M3 in LTE. The attribute is applicable only

for Immediate MDT. In case this attribute is not used, it carries a

null semantic.";

reference "Clause 5.10.20 of 3GPP TS 32.422";

}

leaf tjMDTCollectionPeriodM6Lte {

when './tjJobType = "IMMEDIATE\_MDT\_ONLY"'

+ ' or ./tjJobType = "IMMEDIATE\_MDT\_AND\_TRACE"';

type uint32 {

range "1024|2048|5120|10240";

}

units milliseconds;

description "Specifies the collection period for the Packet Delay

measurement (M6) for MDT taken by the eNB. The attribute is applicable

only for Immediate MDT. In case this attribute is not used,

it carries a null semantic.";

reference "Clause 5.10.32 of TS 32.422 ";

}

leaf tjMDTCollectionPeriodM7Lte {

when './tjJobType = "IMMEDIATE\_MDT\_ONLY"'

+ ' or ./tjJobType = "IMMEDIATE\_MDT\_AND\_TRACE"';

type uint16 {

range 1..60 ;

}

description "It specifies the collection period for the Data Volume (M6)

and Throughput measurements (M7) for UMTS MDT taken by RNC. The

attribute is applicable only for Immediate MDT. In case this attribute

is not used, it carries a null semantic.";

reference "Clause 5.10.22 of TS 32.422 .";

}

leaf tjMDTCollectionPeriodRrmUmts {

when './tjJobType = "IMMEDIATE\_MDT\_ONLY"'

+ ' or ./tjJobType = "IMMEDIATE\_MDT\_AND\_TRACE"';

type uint32 {

range "1024|1280|2048|2560|5120|"

+"10240|60000";

}

units milliseconds;

description "Specifies the collection period for collecting RRM configured

measurement samples for M3, M4, M5 in UMTS. The attribute is applicable

only for Immediate MDT. In case this attribute is not used, it carries

a null semantic";

reference "Clause 5.10.21 of 3GPP TS 32.422";

}

leaf tjMDTCollectionPeriodRrmNR {

when './tjJobType = "IMMEDIATE\_MDT\_ONLY"'

+ ' or ./tjJobType = "IMMEDIATE\_MDT\_AND\_TRACE"';

type uint32 {

range "1024|2048|5120|10240|60000";

}

units milliseconds;

description "Specifies the collection period for collecting RRM

configured measurement samples for M4, M5 in NR. The attribute is

applicable only for Immediate MDT. In case this attribute is not

used, it carries a null semantic.";

reference "Clause 5.10.30 of 3GPP TS 32.422";

}

leaf tjMDTCollectionPeriodM6NR {

when './tjJobType = "IMMEDIATE\_MDT\_ONLY"'

+ ' or ./tjJobType = "IMMEDIATE\_MDT\_AND\_TRACE"';

type enumeration {

enum 120ms;

enum 240ms;

enum 480ms;

enum 640ms;

enum 1024ms;

enum 2048ms;

enum 5120ms;

enum 10240ms;

enum 20480ms;

enum 40960ms;

enum 1min;

enum 6min;

enum 12min;

enum 30min;

}

description "It specifies the collection period for the Packet Delay

measurement (M6) for NR MDT taken by the gNB. The attribute is

applicable only for Immediate MDT. In case this attribute is not used,

it carries a null semantic.";

reference "clause 5.10.34 of TS 32.422";

}

leaf tjMDTCollectionPeriodM7NR {

when './tjJobType = "IMMEDIATE\_MDT\_ONLY"'

+ ' or ./tjJobType = "IMMEDIATE\_MDT\_AND\_TRACE"';

type uint32 {

range "1..60";

}

description "It specifies the collection period for the Packet Loss Rate

measurement (M7) for NR MDT taken by the gNB. The attribute is

applicable only for Immediate MDT. In case this attribute is not used,

it carries a null semantic.";

reference "clause 5.10.35 of TS 32.422";

}

leaf tjMDTEventListForTriggeredMeasurement {

when './tjJobType = "LOGGED\_MDT\_ONLY"';

type enumeration {

enum OUT\_OF\_COVERAGE ;

enum A2\_EVENT ;

}

mandatory true;

description "Specifies event types for event triggered measurement in the

case of logged NR MDT. Each trace session may configure at most one

event. The UE shall perform logging of measurements only upon certain

condition being fulfilled:

- Out of coverage.

- A2 event.";

reference "Clause 5.10.28 of 3GPP TS 32.422";

}

leaf tjMDTEventThreshold {

type int64;

description "Specifies the threshold which should trigger the reporting

in case A2 event reporting in LTE or 1F/1l event in UMTS. The attribute

is applicable only for Immediate MDT and when reportingTrigger is

configured for A2 event in LTE or 1F event or 1l event in UMTS. In

case this attribute is not used, it carries a null semantic.";

reference "Clauses 5.10.7 and 5.10.7a of 3GPP TS 32.422";

}

leaf tjMDTListOfMeasurements {

when './tjJobType = "IMMEDIATE\_MDT"';

type int64;

mandatory true;

description "It specifies the UE measurements that shall be collected in

an Immediate MDT job. The attribute is applicable only for Immediate MDT.

In case this attribute is not used, it carries a null semantic.";

reference "3GPP TS 32.422 clause 5.10.3";

}

leaf tjMDTLoggingDuration {

when './tjJobType = "LOGGED\_MDT\_ONLY" or ./tjJobType = "LOGGED\_MBSFN\_MDT"';

type uint32 {

range "600|1200|2400|3600|5400|7200";

}

units seconds;

mandatory true;

description "Specifies how long the MDT configuration is valid at the

UE in case of Logged MDT. The attribute is applicable only for

Logged MDT and Logged MBSFN MDT. In case this attribute is not used, it

carries a null semantic.";

reference "5.10.9 of 3GPP TS 32.422";

}

leaf tjMDTLoggingInterval {

when './tjJobType = "LOGGED\_MDT\_ONLY" or ./tjJobType = "LOGGED\_MBSFN\_MDT"';

type uint32 {

range "1280|2560|5120|10240|20480|"

+"30720|40960|61440";

}

units milliseconds;

mandatory true;

description "Specifies the periodicty for Logged MDT. The attribute is

applicable only for Logged MDT and Logged MBSFN MDT. In case this

attribute is not used, it carries a null semantic";

reference "5.10.8 of 3GPP TS 32.422";

}

leaf tjMDTLoggingEventThreshold {

when './tjJobType = "LOGGED\_MDT\_ONLY" or ./tjJobType = "LOGGED\_MBSFN\_MDT"';

type uint32 {

range "0..127";

}

description "It specifies the threshold which should trigger

the reporting in case of event based reporting of logged NR MDT.

The attribute is applicable only for Logged MDT and when tjMDTReportType

is configured for event triggered reporting and when

tjMDTEventListForTriggeredMeasurement is configured for L1 event.

In case this attribute is not used, it carries a null semantic.";

reference "clause 5.10.36 of TS 32.422";

}

leaf tjMDTLoggedHysteresis {

when './tjJobType = "LOGGED\_MDT\_ONLY" or ./tjJobType = "LOGGED\_MBSFN\_MDT"';

type uint32 {

range "0..30";

}

description "It specifies the hysteresis used within the entry and leave

condition of the L1 event based reporting of logged NR MDT.

The attribute is applicable only for Logged MDT, when tjMDTReportType

is configured for event triggered reporting and when

tjMDTEventListForTriggeredMeasurement is configured for L1 event.

In case this attribute is not used, it carries a null semantic.";

reference "clause 5.10.37 of TS 32.422";

}

leaf tjMDTLoggedTimeToTrigger {

when './tjJobType = "LOGGED\_MDT\_ONLY" or ./tjJobType = "LOGGED\_MBSFN\_MDT"';

type int32 ;

description "It specifies the threshold which should trigger

the reporting in case of event based reporting of logged NR MDT.

The attribute is applicable only for Logged MDT, when tjMDTReportType

is configured for event triggered reporting and when

tjMDTEventListForTriggeredMeasurement is configured for L1 event.

In case this attribute is not used, it carries a null semantic.";

reference "clauses 5.10.38 of TS 32.422";

}

leaf-list tjMDTMBSFNAreaList {

when './tjJobType = "LOGGED\_MBSFN\_MDT"';

type string;

min-elements 1;

max-elements 8;

description "The MBSFN Area consists of a MBSFN Area ID and Carrier

Frequency (EARFCN). The target MBSFN area List can have up to 8 entries.

This parameter is applicable only if the job type is Logged MBSFN MDT.";

reference "5.10.25 of 3GPP TS 32.422";

}

leaf tjMDTMeasurementPeriodLTE {

when './tjJobType = "IMMEDIATE\_MDT\_ONLY"'

+ ' or ./tjJobType = "IMMEDIATE\_MDT\_AND\_TRACE"';

type uint32 {

range "1024|1280|2048|2560|5120|"

+"10240|60000";

}

units milliseconds;

mandatory true;

description "It specifies the measurement period for the Data Volume and

Scheduled IP throughput measurements for MDT taken by the eNB.

The attribute is applicable only for Immediate MDT. In case this

attribute is not used, it carries a null semantic.";

reference "Clause 5.10.23 of 3GPP TS 32.422";

}

leaf tjMDTMeasurementPeriodUMTS {

when './tjJobType = "IMMEDIATE\_MDT\_ONLY"'

+ 'or ./tjJobType = "IMMEDIATE\_MDT\_AND\_TRACE"';

type uint32 {

range "250|500|1000|2000|3000|4000|6000|8000|12000|16000|20000|"

+"24000|28000|32000|64000";

}

units milliseconds;

mandatory true;

description "It specifies the measurement period for the Data Volume and

Throughput measurements for MDT taken by RNC.

The attribute is applicable only for Immediate MDT. In case this

attribute is not used, it carries a null semantic.";

reference "Clause 5.10.22 of 3GPP TS 32.422";

}

leaf tjMDTMeasurementQuantity {

when './tjJobType = "IMMEDIATE\_MDT\_ONLY"'

+ ' or ./tjJobType = "IMMEDIATE\_MDT\_AND\_TRACE"';

type uint64 ;

mandatory true;

description "It specifies the measurements that are collected in an MDT

job for a UMTS MDT configured for event triggered reporting.";

reference "Clause 5.10.15 of 3GPP TS 32.422";

}

leaf tjMDTM4ThresholdUmts {

when './tjJobType = "IMMEDIATE\_MDT\_ONLY"'

+ ' or ./tjJobType = "IMMEDIATE\_MDT\_AND\_TRACE"';

type uint16 {

range 0..31 ;

}

description "It specifies the threshold which should trigger

the reporting in case of event-triggered periodic reporting for M4

(UE power headroom measurement) in UMTS. In case this attribute is

not used, it carries a null semantic.";

reference "3GPP TS 32.422 clause 5.10.A";

}

list tjMDTPLMList {

when './tjJobType = "LOGGED\_MDT\_ONLY"';

key "mcc mnc";

uses types3gpp:PLMNId;

min-elements 1;

max-elements 16;

description "It indicates the PLMNs where measurement collection, status

indication and log reporting is allowed.";

reference "Clause 5.10.24 of 3GPP TS 32.422";

}

leaf tjMDTPositioningMethod {

when './tjJobType = "IMMEDIATE\_MDT\_ONLY"'

+ ' or ./tjJobType = "IMMEDIATE\_MDT\_AND\_TRACE"';

type enumeration {

enum GNSS;

enum E\_CELL\_ID;

}

mandatory true;

description "It specifies what positioning method should be used in the

MDT job.";

reference "Clause 5.10.19 of 3GPP TS 32.422";

}

leaf tjMDTReportAmount {

when './tjJobType = "IMMEDIATE\_MDT\_ONLY"'

+ ' and ./tjMDTReportingTrigger = "PERIODICAL"';

type union {

type uint32 {

range "1|4|8|16|32|64" ;

}

type enumeration {

enum INFINITY;

}

}

mandatory true;

description "It specifies the number of measurement reports that shall be

taken for periodic reporting while the UE is in connected.

The attribute is applicable only for Immediate MDT and when

tjMDTReportingTrigger is configured for periodical measurements. In

case this attribute is not used, it carries a null semantic.";

reference "Clause 5.10.6 of 3GPP TS 32.422";

}

leaf tjMDTReportingTrigger {

when './tjJobType = "IMMEDIATE\_MDT\_ONLY"';

type enumeration {

enum PERIODICAL;

enum A2\_FOR\_LTE;

enum 1F\_FOR\_UMTS;

enum 1I\_FOR\_UMTS\_MCPS\_TDD;

enum A2\_TRIGGERED\_PERIODIC\_FOR\_LTE;

enum ALL\_CONFIGURED\_RRM\_FOR\_LTE;

enum ALL\_CONFIGURED\_RRM\_FOR\_UMTS;

}

description "It specifies whether periodic or event based measurements

should be collected.

The attribute is applicable only for Immediate MDT and when the

tjMDTListOfMeasurements is configured for M1 (for both UMTS and LTE)

or M2 (only for UMTS). In case this attribute is not used, it carries

a null semantic.";

reference "Clause 5.10.4 of 3GPP TS 32.422";

}

leaf tjMDTReportInterval {

when './tjJobType = "IMMEDIATE\_MDT\_ONLY"'

+ ' and ./tjMDTReportingTrigger = "PERIODICAL"';

type uint32 {

range "120|240|250|480|500|640|1000|1024|2000|2048|3000|4000|"

+"5120|6000|8000|10240|12000|16000|20000|"

+"24000|28000|32000|60000|64000|"

+"360000|720000|1800000|3600000";

}

units milliseconds;

mandatory true;

description "It specifies the interval between the periodical measurements

that shall be taken when the UE is in connected mode.

The attribute is applicable only for Immediate MDT and when

tjMDTReportingTrigger is configured for periodical measurements. In case

this attribute is not used, it carries a null semantic.";

reference "5.10.5 of 3GPP TS 32.422";

}

leaf tjMDTReportType {

when './tjJobType = "LOGGED\_MDT\_ONLY"';

type enumeration {

enum PERIODICAL;

enum EVENT\_TRIGGERED;

}

mandatory true;

description "It specifies report type for logged NR MDT";

reference "Clause 5.10.27 of 3GPP TS 32.422";

}

leaf tjMDTSensorInformation {

type bits {

bit BAROMETRIC\_PRESSURE;

bit UE\_SPEED;

bit UE\_ORIENTATION;

}

default "";

description "It specifies which sensor information shall be included in

logged NR MDT and immediate NR MDT measurement if they are available.

The following sensor measurement can be included or excluded for

the UE.";

reference "Clause 5.10.29 of 3GPP TS 32.422";

}

leaf tjMDTTraceCollectionEntityID {

when './tjJobType = "LOGGED\_MDT\_ONLY" or ./tjJobType = "LOGGED\_MBSFN\_MDT"';

type uint8;

mandatory true;

description "It specifies the TCE Id which is sent to the UE in

Logged MDT.";

reference "Clause 5.10.11 of 3GPP TS 32.422";

}

}

grouping TraceSubtree {

description "Contains classes that manage Tracing.

Should be used in all classes (or classes inheriting from)

- SubNnetwork

- ManagedElement

- ManagedFunction

If a YANG module wants to augment these classes/list/groupings they must

augment all user classes!";

list TraceJob {

description "Represents the Trace Control and Configuration parameters of a

particular Trace Job (see TS 32.421 and TS 32.422 for details).

It can be name-contained by SubNetwork, ManagedElement, ManagedFunction

or NetworkSliceSubnet.

To activate Trace Jobs, a MnS consumer has to create TraceJob object

instances on the MnS producer. A MnS consumer can activate a Trace Job

for another MnS consumer since it is not required the value of

tjTraceCollectionEntityAddress or tjStreamingTraceConsumerUri to be his

own.

When a MnS consumer wishes to deactivate a Trace Job, the MnS consumer

shall delete the corresponding TraceJob instance.

For details of management Trace Job activation/deactivation see clause

4.1.1.1.2 of TS 32.422.

The attribute tjJobType specifies the kind of data to collect. Dependent

on the selected type various parameters shall be available. The

attributes tjJobType, tjTraceReference, tjTraceRecordSessionReference,

tjTraceCollectionEntityAddress and tjTraceReportingFormat are mandatory

for all job types. If streaming reporting is selected for

tjTraceReportingFormat, tjStreamingTraceConsumerURI shall be present

additionally. The attribute tjPLMNTarget shall be present if trace

activation method is management based.

For the different job types the attributes are differentiated as follows:

- In case of TRACE\_ONLY additionally the following attributes shall be

available: tjListOfNeTypes, tjTraceDepth, tjTraceTarget and

tjTriggeringEvent.

For this case the optional attribute tjListOfInterfaces allows to

specify the interfaces to be recorded.

- In case of IMMEDIATE\_MDT\_ONLY additionally the following attributes

shall be available:

- tjTraceTarget

- tjMDTAnonymizationOfData,

- tjMDTListOfMeasurements,

- tjMDTCollectionPeriodRrmUmts (conditional for M3, M4 and M5 in UMTS),

- tjMDTMeasurementPeriodUMTS (conditional for M6 and M7 in UMTS),

- tjMDTCollectionPeriodRrmLte (conditional for M2 and M3 in LTE),

- tjMDTMeasurementPeriodLTE (conditional for M4 and M5 in LTE),

- tjMDTCollectionPeriodM6Lte (conditional for M6 in LTE),

- tjMDTCollectionPeriodM7Lte (conditional for M7 in LTE),

- tjMDTCollectionPeriodRrmNR (conditional for M4 and M5 in NR),

- tjMDTCollectionPeriodM6NR (conditional for M6 in NR),

- tjMDTCollectionPeriodM7NR (conditional for M7 in NR),

- tjMDTReportInterval (conditional for M1 in LTE or NR and M1/M2 in

UMTS),

- tjMDTReportAmount (conditional for M1 in LTE or NR and M1/M2 in

UMTS),

- tjMDTReportingTrigger (conditional for M1 in LTE or NR and M1/M2 in

UMTS),

- tjMDTEventThreshold (conditional for A2 event reporting or A2 event

triggered periodic reporting),

- tjMDTMeasurementQuantity (conditional for 1F event reporting).

For this case the optional attribute tjMDTAreaScope allows to specify

the area in terms of cells or Tracking Area/Routing Area/Location area

where the MDT data collection shall take place and the optional

attributes tjMDTPositioningMethod, tjMDTSensorInformation allow to

specify the positioning methods to use or the sensor information to

include.

- In case of IMMEDIATE\_MDT\_AND\_TRACE both additional attributes of

TRACE\_ONLY and IMMEDIATE\_MDT\_ONLY shall apply.

- In case of LOGGED\_MDT\_ONLY additionally the following attributes

shall be available: tjTraceTarget, tjMDTAnonymizationOfData,

tjMDTTraceCollectionEntityID, tjMDTLoggingInterval,

tjMDTLoggingDuration, tjMDTReportType,

tjMDTEventListForTriggeredMeasurements.

For this case the optional attribute tjMDTAreaScope allows to specify

the area in terms of cells or Tracking Area/Routing Area/Location area

where the MDT data collection shall take place, the optional attribute

tjMDTPLMNList allows to specify the PLMNs where measurement collection,

status indication and log reporting is allowed, the optional attribute

tjMDTAreaConfigurationForNeighCell allows to specify the area for

which UE is requested to perform measurements logging for neighbour

cells which have list of frequencies and the optional attribute

tjMDTSensorInformation allows to specify the sensor information to

include.

- In case of RLF\_REPORT\_ONLY and RCEF\_REPORT\_ONLY additionally the

attribute tjTraceTarget shall be available, the optional attribute

tjMDTAreaScope allows to specify the eNB or list of eNBs or gNB or

list of gNBs where the reports should be collected.

- In case of LOGGED\_MBSFN\_MDT additionally the following attributes

shall be available: tjMDTAnonymizationOfData, tjMDTLoggingInterval,

tjMDTLoggingDuration, tjMDTMBSFNAreaList.

Creation and deletion of TraceJob instances by MnS consumers is optional;

when not supported, the TraceJob instances may be created and deleted by

the system or be pre-installed.";

key id;

uses top3gpp:Top\_Grp ;

container attributes {

uses TraceJobGrp ;

}

}

}

}

<CODE ENDS>

***Next change***

***End of changes***