**3GPP TSG-SA5 Meeting #139-eS5-215533**

**e-meeting, 11 - 20 October 2021**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **28.623** | **CR** | **xxxx** | **rev** | **-** | **Current version:** | **16.9.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **x** | Core Network | **x** |

|  |
| --- |
|  |
| ***Title:***  |  Add support for MnS Discovery |
|  |  |
| ***Source to WG:*** | S5 |
| ***Source to TSG:*** | Huawei |
|  |  |
| ***Work item code:*** | 5GDMS |  | ***Date:*** | 2021-10-19 |
|  |  |  |  |  |
| ***Category:*** | B |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | Add solution sets for discovery of management services. |
|  |  |
| ***Summary of change:*** | OpenAPI and YANG solution sets are added. |
|  |  |
| ***Consequences if not approved:*** | NRM does not support discovery of management services. |
|  |  |
| ***Clauses affected:*** | C.4.3, D.2.X |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ... |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

|  |
| --- |
| **1st change** |

## C.4.3 OpenAPI document "genericNrm.yaml"

openapi: 3.0.1

info:

 title: Generic NRM

 version: 16.8.0

 description: >-

 OAS 3.0.1 definition of the Generic NRM

 © 2021, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

externalDocs:

 description: 3GPP TS 28.623; Generic NRM

 url: http://www.3gpp.org/ftp/Specs/archive/28\_series/28.623/

paths: {}

components:

 schemas:

#-------- Definition of types-----------------------------------------------------

 RegistrationState:

 type: string

 enum:

 - REGISTERED

 - DEREGISTERED

 VnfParameter:

 type: object

 properties:

 vnfInstanceId:

 type: string

 vnfdId:

 type: string

 flavourId:

 type: string

 autoScalable:

 type: boolean

 PeeParameter:

 type: object

 properties:

 siteIdentification:

 type: string

 siteDescription:

 type: string

 siteLatitude:

 $ref: 'comDefs.yaml#/components/schemas/Latitude'

 siteLongitude:

 $ref: 'comDefs.yaml#/components/schemas/Longitude'

 equipmentType:

 type: string

 environmentType:

 type: string

 powerInterface:

 type: string

 ThresholdInfo:

 type: object

 properties:

 thresholdDirection:

 type: string

 enum:

 - UP

 - DOWN

 - UP\_AND\_DOWN

 thresholdValue:

 oneOf:

 - type: integer

 - $ref: 'comDefs.yaml#/components/schemas/Float'

 hysteresis:

 oneOf:

 - type: integer

 minimum: 0

 - type: number

 format: float

 minimum: 0

 Operation:

 type: object

 properties:

 name:

 type: string

 allowedNFTypes:

 $ref: '#/components/schemas/NFType'

 operationSemantics:

 $ref: '#/components/schemas/OperationSemantics'

 NFType:

 type: string

 description: ' NF name defined in TS 23.501'

 enum:

 - NRF

 - UDM

 - AMF

 - SMF

 - AUSF

 - NEF

 - PCF

 - SMSF

 - NSSF

 - UDR

 - LMF

 - GMLC

 - 5G\_EIR

 - SEPP

 - UPF

 - N3IWF

 - AF

 - UDSF

 - DN

 OperationSemantics:

 type: string

 enum:

 - REQUEST\_RESPONSE

 - SUBSCRIBE\_NOTIFY

 SAP:

 type: object

 properties:

 host:

 $ref: 'comDefs.yaml#/components/schemas/HostAddr'

 port:

 type: integer

 NFServiceType:

 type: string

 enum:

 - Namf\_Communication

 - Namf\_EventExposure

 - Namf\_MT

 - Namf\_Location

 - Nsmf\_PDUSession

 - Nsmf\_EventExposure

 - Others

 TransportProtocol:

 anyOf:

 - type: string

 enum:

 - TCP

 - type: string

 SupportedPerfMetricGroup:

 type: object

 properties:

 performanceMetrics:

 type: array

 items:

 type: string

 granularityPeriods:

 type: array

 items:

 type: integer

 minimum: 1

 reportingMethods:

 type: array

 items:

 type: string

 enum:

 - FILE\_BASED\_LOC\_SET\_BY\_PRODUCER

 - FILE\_BASED\_LOC\_SET\_BY\_CONSUMER

 - STREAM\_BASED

 monitorGranularityPeriods:

 type: array

 items:

 type: integer

 minimum: 1

 ReportingCtrl:

 oneOf:

 - type: object

 properties:

 fileReportingPeriod:

 type: integer

 - type: object

 properties:

 fileReportingPeriod:

 type: integer

 fileLocation:

 $ref: 'comDefs.yaml#/components/schemas/Uri'

 - type: object

 properties:

 streamTarget:

 $ref: 'comDefs.yaml#/components/schemas/Uri'

 Scope:

 type: object

 properties:

 scopeType:

 type: string

 enum:

 - BASE\_ONLY

 - BASE\_ALL

 - BASE\_NTH\_LEVEL

 - BASE\_SUBTREE

 scopeLevel:

 type: integer

 AreaScope:

 oneOf:

 - type: array

 items:

 $ref: '#/components/schemas/EutraCellId'

 - type: array

 items:

 $ref: '#/components/schemas/NrCellId'

 - type: array

 items:

 $ref: '#/components/schemas/Tac'

 - type: array

 items:

 $ref: '#/components/schemas/Tai'

 Tai:

 type: object

 properties:

 mcc:

 $ref: 'comDefs.yaml#/components/schemas/Mcc'

 mnc:

 $ref: 'comDefs.yaml#/components/schemas/Mnc'

 tac:

 $ref: '#/components/schemas/Tac'

 AreaConfig:

 type: object

 properties:

 freqInfo:

 $ref: '#/components/schemas/FreqInfo'

 pciList:

 type: array

 items:

 type: integer

 FreqInfo:

 description: specifies the carrier frequency and bands used in a cell.

 type: object

 properties:

 arfcn:

 type: integer

 freqBands:

 type: array

 items:

 type: integer

 MbsfnArea:

 type: object

 properties:

 mbsfnAreaId:

 type: integer

 minimum: 1

 earfcn:

 type: integer

 minimum: 1

 Tac:

 type: string

 pattern: '(^[A-Fa-f0-9]{4}$)|(^[A-Fa-f0-9]{6}$)'

 EutraCellId:

 type: string

 pattern: '^[A-Fa-f0-9]{7}$'

 NrCellId:

 type: string

 pattern: '^[A-Fa-f0-9]{9}$'

 IpAddr:

 oneOf:

 - $ref: 'comDefs.yaml#/components/schemas/Ipv4Addr'

 - $ref: 'comDefs.yaml#/components/schemas/Ipv6Addr'

#-------- Definition of types used in Trace control NRM fragment------------------

 tjJobType-Type:

 type: string

 description: Specifies whether the TraceJob represents only MDT, Logged MBSFN MDT, Trace or a combined Trace and MDT job. Applicable for Trace, MDT, RCEF and RLF reporting. See 3GPP TS 32.422 clause 5.9a for additional details.

 enum:

 - IMMEDIATE\_MDT\_ONLY

 - LOGGED\_MDT\_ONLY

 - TRACE\_ONLY

 - IMMEDIATE\_MDT AND TRACE

 - RLF\_REPORT\_ONLY

 - RCEF\_REPORT\_ONLY

 - LOGGED\_MBSFN\_MDT

 tjListOfInterfaces-Type:

 description: The interfaces to be recorded in the Network Element. See 3GPP TS 32.422 clause 5.5 for additional details.

 type: object

 properties:

 MSCServerInterfaces:

 type: array

 items:

 type: string

 enum:

 - A

 - Iu-CS

 - Mc

 - MAP-G

 - MAP-B

 - MAP-E

 - MAP-F

 - MAP-D

 - MAP-C

 - CAP

 MGWInterfaces:

 type: array

 items:

 type: string

 enum:

 - Mc

 - Nb-UP

 - Iu-UP

 RNCInterfaces:

 type: array

 items:

 type: string

 enum:

 - Iu-CS

 - Iu-PS

 - Iur

 - Iub

 - Uu

 SGSNInterfaces:

 type: array

 items:

 type: string

 enum:

 - Gb

 - Iu-PS

 - Gn

 - MAP-Gr

 - MAP-Gd

 - MAP-Gf

 - Ge

 - Gs

 - S6d

 - S4

 - S3

 - S13

 GGSNInterfaces:

 type: array

 items:

 type: string

 enum:

 - Gn

 - Gi

 - Gmb

 S-CSCFInterfaces:

 type: array

 items:

 type: string

 enum:

 - Mw

 - Mg

 - Mr

 - Mi

 P-CSCFInterfaces:

 type: array

 items:

 type: string

 enum:

 - Gm

 - Mw

 I-CSCFInterfaces:

 type: array

 items:

 type: string

 enum:

 - Cx

 - Dx

 - Mg

 - Mw

 MRFCInterfaces:

 type: array

 items:

 type: string

 enum:

 - Mp

 - Mr

 MGCFInterfaces:

 type: array

 items:

 type: string

 enum:

 - Mg

 - Mj

 - Mn

 IBCFInterfaces:

 type: array

 items:

 type: string

 enum:

 - Ix

 - Mx

 E-CSCFInterfaces:

 type: array

 items:

 type: string

 enum:

 - Mw

 - Ml

 - Mm

 - Mi/Mg

 BGCFInterfaces:

 type: array

 items:

 type: string

 enum:

 - Mi

 - Mj

 - Mk

 ASInterfaces:

 type: array

 items:

 type: string

 enum:

 - Dh

 - Sh

 - ISC

 - Ut

 HSSInterfaces:

 type: array

 items:

 type: string

 enum:

 - MAP-C

 - MAP-D

 - Gc

 - Gr

 - Cx

 - S6d

 - S6a

 - Sh

 EIRInterfaces:

 type: array

 items:

 type: string

 enum:

 - MAP-F

 - S13

 - MAP-Gf

 BM-SCInterfaces:

 type: array

 items:

 type: string

 enum:

 - Gmb

 MMEInterfaces:

 type: array

 items:

 type: string

 enum:

 - S1-MME

 - S3

 - S6a

 - S10

 - S11

 - S13

 SGWInterfaces:

 type: array

 items:

 type: string

 enum:

 - S4

 - S5

 - S8

 - S11

 - Gxc

 PDN\_GWInterfaces:

 type: array

 items:

 type: string

 enum:

 - S2a

 - S2b

 - S2c

 - S5

 - S6b

 - Gx

 - S8

 - SGi

 eNBInterfaces:

 type: array

 items:

 type: string

 enum:

 - S1-MME

 - X2

 en-gNBInterfaces:

 type: array

 items:

 type: string

 enum:

 - S1-MME

 - X2

 - Uu

 - F1-C

 - E1

 AMFInterfaces:

 type: array

 items:

 type: string

 enum:

 - N1

 - N2

 - N8

 - N11

 - N12

 - N14

 - N15

 - N20

 - N22

 - N26

 AUSFInterfaces:

 type: array

 items:

 type: string

 enum:

 - N12

 - N13

 NEFInterfaces:

 type: array

 items:

 type: string

 enum:

 - N29

 - N30

 - N33

 NRFInterfaces:

 type: array

 items:

 type: string

 enum:

 - N27

 NSSFInterfaces:

 type: array

 items:

 type: string

 enum:

 - N22

 - N31

 PCFInterfaces:

 type: array

 items:

 type: string

 enum:

 - N5

 - N7

 - N15

 SMFInterfaces:

 type: array

 items:

 type: string

 enum:

 - N4

 - N7

 - N10

 - N11

 - S5-C

 SMSFInterfaces:

 type: array

 items:

 type: string

 enum:

 - N20

 - N21

 UDMInterfaces:

 type: array

 items:

 type: string

 enum:

 - N8

 - N10

 - N13

 - N21

 UPFInterfaces:

 type: array

 items:

 type: string

 enum:

 - N4

 ng-eNBInterfaces:

 type: array

 items:

 type: string

 enum:

 - NG-C

 - Xn-C

 - Uu

 gNB-CU-CPInterfaces:

 type: array

 items:

 type: string

 enum:

 - NG-C

 - Xn-C

 - Uu

 - F1-C

 - E1

 - X2-C

 gNB-CU-UPInterfaces:

 type: array

 items:

 type: string

 enum:

 - E1

 gNB-DUInterfaces:

 type: array

 items:

 type: string

 enum:

 - F1-C

 tjListOfNeTypes-Type:

 description: The Network Element types where Trace Session activation is needed. See 3GPP TS 32.422 clause 5.4 for additional details.

 type: array

 items:

 type: string

 enum:

 - MSC\_SERVER

 - SGSN

 - MGW

 - GGSN

 - RNC

 - BM\_SC

 - MME

 - SGW

 - PGW

 - ENB

 - EN\_GNB

 - GNB\_CU\_CP

 - GNB\_CU\_UP

 - GNB\_DU

 - AMF

 - PCF

 - SMF

 - UPF

 - AUSF

 - SMSF

 tjPLMNTarget-Type:

 type: object

 description: The PLMN for which sessions shall be selected in the Trace Session in case of management based activation when several PLMNs are supported in the RAN (this means that shared cells and not shared cells are allowed for the specified PLMN. Note that the PLMN Target might differ from the PLMN specified in the Trace Reference, as that specifies the PLMN that is containing the management system requesting the Trace Session from the NE. See 3GPP TS 32.422 clause 5.9b for additional details.

 properties:

 mcc:

 $ref: 'comDefs.yaml#/components/schemas/Mcc'

 mnc:

 $ref: 'comDefs.yaml#/components/schemas/Mnc'

 required:

 - mcc

 - mnc

 tjTraceDepth-Type:

 description: Specifies how detailed information should be recorded in the Network Element. The Trace Depth is a paremeter for Trace Session level, i.e., the Trace Depth is the same for all of the NEs to be traced in the same Trace Session. See 3GPP TS 32.422 clause 5.3 for additional details.

 type: string

 enum:

 - MINIMUM

 - MEDIUM

 - MAXIMUM

 - VENDORMINIMUM

 - VENDORMEDIUM

 - VENDORMAXIMUM

 tjTraceReference-Type:

 type: object

 description: The Trace Reference parameter shall be globally unique, therefore the Trace Reference shall compose as follows - MCC+MNC+Trace ID, where the MCC and MNC are coming with the Trace activation request from the management system to identify one PLMN containing the management system, and Trace ID is a 3 byte Octet String. See 3GPP TS 32.422 clause 5.6 for additional details.

 properties:

 mcc:

 $ref: 'comDefs.yaml#/components/schemas/Mcc'

 mnc:

 $ref: 'comDefs.yaml#/components/schemas/Mnc'

 traceId:

 type: string

 required:

 - mcc

 - mnc

 - traceId

 tjTraceReportingFormat-Type:

 type: string

 description: Specifies whether file-based or streaming reporting shall be used for this Trace Session. See 3GPP TS 32.422 clause 5.11 for additional details.

 enum:

 - FILE-BASED

 - STREAMING

 tjTraceTarget-Type:

 type: object

 description: Trace target conveying both the type and value of the target ID. For additional details see 3GPP TS 32.422

 properties:

 TargetIdType:

 type: string

 enum:

 - IMSI

 - IMEI

 - IMEISV

 - PUBLIC\_ID

 - UTRAN\_CELL

 - E-UTRAN\_CELL

 - NG-RAN\_CELL

 - eNB

 - RNC

 - gNB

 - SUPI

 TargetIdValue:

 type: string

 required:

 - TargetIdType

 - TargetIdValue

 tjTriggeringEvent-Type:

 type: object

 description: Specifies when to start a Trace Recording Session and which message shall be recorded first, when to stop a Trace Recording Session and which message shall be recorded last respectively. See 3GPP TS 32.422 clause 5.1 for additional detials.

 properties:

 NetworkElement:

 type: string

 enum:

 - MSC\_SERVER

 - SGSN

 - MGW

 - GGSN

 - BM\_SC

 - MME

 - SGW

 - PGW

 - AMF

 - SMF

 - PCF

 - UPF

 - AUSF

 - NEF

 - NRF

 - NSSF

 - SMSF

 - UDM

 EventBitmap:

 type: integer

 required:

 - NetworkElement

 - EventBitmap

 tjMDTAnonymizationOfData-Type:

 description: Specifies level of MDT anonymization. For additional details see 3GPP TS 32.422 clause 5.10.12.

 type: string

 enum:

 - NO\_IDENTITY

 - TAC\_OF\_IMEI

 tjMDTCollectionPeriodRrmLte-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.20.

 type: string

 enum:

 - 100ms

 - 1000ms

 - 1024ms

 - 1280ms

 - 2048ms

 - 2560ms

 - 5120ms

 - 10000ms

 - 10240ms

 - 60000ms

 tjMDTCollectionPeriodM6Lte-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.32.

 type: string

 enum:

 - 1024ms

 - 2048ms

 - 5120ms

 - 10240ms

 tjMDTCollectionPeriodM7Lte-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.33.

 type: integer

 minimum: 1

 maximum: 60

 tjMDTCollectionPeriodRrmUmts-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.21.

 type: string

 enum:

 - 100ms

 - 250ms

 - 500ms

 - 1000ms

 - 2000ms

 - 3000ms

 - 4000ms

 - 6000ms

 tjMDTCollectionPeriodRrmNR-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.30.

 type: string

 enum:

 - 1024ms

 - 2048ms

 - 5120ms

 - 10240ms

 - 60000ms

 tjMDTCollectionPeriodM6NR-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.34.

 type: string

 enum:

 - 120ms

 - 240ms

 - 480ms

 - 640ms

 - 1024ms

 - 2048ms

 - 5120ms

 - 10240ms

 - 20480ms

 - 40960ms

 - 1min

 - 6min

 - 12min

 - 30min

 tjMDTCollectionPeriodM7NR-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.35.

 type: integer

 minimum: 1

 maximum: 60

 tjMDTEventListForTriggeredMeasurement-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.28.

 type: string

 enum:

 - OUT\_OF\_COVERAGE

 - A2\_EVENT

 tjMDTEventThreshold-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.7, 5.10.7a, 5.10.13 and 5.10.14.

 type: object

 properties:

 EventThresholdRSRP:

 oneOf:

 - type: integer

 minimum: 0

 maximum: 97

 - type: integer

 minimum: 0

 maximum: 127

 EventThresholdRSRQ:

 oneOf:

 - type: integer

 minimum: 0

 maximum: 34

 - type: integer

 minimum: 0

 maximum: 127

 EventThreshold1F:

 type: object

 properties:

 CPICH\_RSCP:

 type: integer

 minimum: -120

 maximum: 25

 CPICH\_EcNo:

 type: integer

 minimum: -24

 maximum: 0

 PathLoss:

 type: integer

 minimum: 30

 maximum: 165

 EventThreshold1I:

 type: integer

 minimum: -120

 maximum: 25

 tjMDTListOfMeasurements-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.3 for details.

 type: object

 properties:

 UMTS:

 type: array

 items:

 type: string

 enum:

 - M1

 - M2

 - M3

 - M4

 - M5

 - M6\_DL

 - M6\_UL

 - M7\_DL

 - M7\_UL

 LTE:

 type: array

 items:

 type: string

 enum:

 - M1

 - M2

 - M3

 - M4

 - M5

 - M1\_EVENT\_TRIGGERED

 - M6

 - M7

 - M8

 - M9

 NR:

 type: array

 items:

 type: string

 enum:

 - M1

 - M2

 - M3

 - M4

 - M5

 - M6

 - M7

 - M1\_EVENT\_TRIGGERED

 - M8

 - M9

 tjMDTLoggingDuration-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.9.

 type: string

 enum:

 - 600s

 - 1200s

 - 2400s

 - 3600s

 - 5400s

 - 7200s

 tjMDTLoggingInterval-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.8.

 type: object

 properties:

 UMTS:

 type: array

 items:

 type: string

 enum:

 - 1.28s

 - 2.56s

 - 5.12s

 - 10.24s

 - 20.48s

 - 30.72s

 - 40.96s

 - 61.44s

 LTE:

 type: array

 items:

 type: string

 enum:

 - 1.28s

 - 2.56s

 - 5.12s

 - 10.24s

 - 20.48s

 - 30.72s

 - 40.96s

 - 61.44s

 NR:

 type: array

 items:

 type: string

 enum:

 - 0.32s

 - 0.64s

 - 1.28s

 - 2.56s

 - 5.12s

 - 10.24s

 - 20.48s

 - 30.72s

 - 40.96s

 - 61.44s

 - INFINITY

 tjMDTLoggingEventThreshold-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.X.

 type: object

 properties:

 RSRP:

 type: integer

 minimum: 0

 maximum: 127

 RSRQ:

 type: integer

 minimum: 0

 maximum: 127

 tjMDTLoggingHysteresis-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.Y.

 type: integer

 minimum: 0

 maximum: 30

 tjMDTLoggingTimeToTrigger-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.Z.

 type: string

 enum:

 - 0ms

 - 40ms

 - 64ms

 - 80ms

 - 100ms

 - 128ms

 - 160ms

 - 256ms

 - 320ms

 - 480ms

 - 512ms

 - 640ms

 - 1024ms

 - 1280ms

 - 2560ms

 - 5120ms

 tjMDTMeasurementPeriodLTE-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.23.

 type: string

 enum:

 - 1024ms

 - 2048ms

 - 5120ms

 - 10240ms

 - 1min

 tjMDTMeasurementPeriodUMTS-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.22.

 type: string

 enum:

 - 1000ms

 - 2000ms

 - 3000ms

 - 4000ms

 - 6000ms

 - 8000ms

 - 12000ms

 - 16000ms

 - 20000ms

 - 24000ms

 - 28000ms

 - 32000ms

 - 64000ms

 tjMDTMeasurementQuantity-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.15.

 type: string

 enum:

 - CPICH\_EcNo

 - CPICH\_RSCP

 - PathLoss

 tjMDTM4ThresholdUmts-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.A.

 type: integer

 minimum: 0

 maximum: 31

 tjMDTPLMNList-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.24.

 type: array

 items:

 type: object

 properties:

 mcc:

 $ref: 'comDefs.yaml#/components/schemas/Mcc'

 mnc:

 $ref: 'comDefs.yaml#/components/schemas/Mnc'

 required:

 - mcc

 - mnc

 maxItems: 16

 tjMDTPositioningMethod-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.19.

 type: string

 enum:

 - GNSS

 - E-CELL\_ID

 tjMDTReportAmount-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.6.

 type: string

 enum:

 - 1

 - 2

 - 4

 - 8

 - 16

 - 32

 - 64

 - INFINITY

 tjMDTReportingTrigger-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.4.

 type: array

 items:

 type: string

 enum:

 - PERIODICAL

 - A2\_FOR\_LTE\_NR

 - 1F\_FOR\_UMTS

 - 1I\_FOR\_UMTS\_MCPS\_TDD

 - A2\_TRIGGERED\_PERIODIC\_FOR\_LTE\_NR

 - ALL\_CONFIGURED\_RRM\_FOR\_LTE\_NR

 - ALL\_CONFIGURED\_RRM\_FOR\_UMTS

 tjMDTReportInterval-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.5.

 type: object

 properties:

 UMTS:

 type: array

 items:

 type: string

 enum:

 - 250ms

 - 500ms

 - 1000ms

 - 2000ms

 - 3000ms

 - 4000ms

 - 6000ms

 - 8000ms

 - 12000ms

 - 16000ms

 - 20000ms

 - 24000ms

 - 28000ms

 - 32000ms

 - 64000ms

 LTE:

 type: array

 items:

 type: string

 enum:

 - 120ms

 - 240ms

 - 480ms

 - 640ms

 - 1024ms

 - 2048ms

 - 5120ms

 - 10240ms

 - 60000ms

 - 360000ms

 - 720000ms

 - 1800000ms

 - 3600000ms

 NR:

 type: array

 items:

 type: string

 enum:

 - 120ms

 - 240ms

 - 480ms

 - 640ms

 - 1024ms

 - 2048ms

 - 5120ms

 - 10240ms

 - 60000ms

 - 360000ms

 - 720000ms

 - 1800000ms

 tjMDTReportType-Type:

 description: Report type for logged NR MDT. See details in 3GPP TS 32.422 clause 5.10.27.

 type: string

 enum:

 - PERIODICAL

 - EVENT\_TRIGGERED

 tjMDTSensorInformation-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.29.

 type: array

 items:

 type: string

 enum:

 - BAROMETRIC\_PRESSURE

 - UE\_SPEED

 - UE\_ORIENTATION

 tjMDTTraceCollectionEntityID-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.11. Only TCE Id value may be sent over the air to the UE being configured for Logged MDT.

 type: integer

#-------- end of Definition of types used in Trace control NRM fragment ----------

#-------- Definition of abstract IOC Top -----------------------------------------

 Top-Attr:

 # This definition will be deprecated, when all occurances of Top-Attr

 # are replaced by Top.

 type: object

 properties:

 id:

 type: string

 nullable: true

 objectClass:

 type: string

 objectInstance:

 $ref: 'comDefs.yaml#/components/schemas/Dn'

 VsDataContainer:

 $ref: '#/components/schemas/VsDataContainer-Multiple'

 required:

 - id

 Top:

 type: object

 properties:

 id:

 type: string

 nullable: true

 objectClass:

 type: string

 objectInstance:

 $ref: 'comDefs.yaml#/components/schemas/Dn'

 VsDataContainer:

 $ref: '#/components/schemas/VsDataContainer-Multiple'

 required:

 - id

#-------- Definition of IOCs with new name-containments defined in other TS ------

 SubNetwork-Attr:

 type: object

 properties:

 dnPrefix:

 type: string

 userLabel:

 type: string

 userDefinedNetworkType:

 type: string

 setOfMcc:

 type: array

 items:

 $ref: 'comDefs.yaml#/components/schemas/Mcc'

 priorityLabel:

 type: integer

 supportedPerfMetricGroups:

 type: array

 items:

 $ref: '#/components/schemas/SupportedPerfMetricGroup'

 ManagedElement-Attr:

 type: object

 properties:

 dnPrefix:

 type: string

 managedElementTypeList:

 type: array

 items:

 type: string

 userLabel:

 type: string

 locationName:

 type: string

 managedBy:

 $ref: 'comDefs.yaml#/components/schemas/DnList'

 vendorName:

 type: string

 userDefinedState:

 type: string

 swVersion:

 type: string

 priorityLabel:

 type: integer

 supportedPerfMetricGroups:

 type: array

 items:

 $ref: '#/components/schemas/SupportedPerfMetricGroup'

 SubNetwork-ncO:

 type: object

 properties:

 ManagementNode:

 $ref: '#/components/schemas/ManagementNode-Multiple'

 MnsAgent:

 $ref: '#/components/schemas/MnsAgent-Multiple'

 MeContext:

 $ref: '#/components/schemas/MeContext-Multiple'

 PerfMetricJob:

 $ref: '#/components/schemas/PerfMetricJob-Multiple'

 ThresholdMonitor:

 $ref: '#/components/schemas/ThresholdMonitor-Multiple'

 NtfSubscriptionControl:

 $ref: '#/components/schemas/NtfSubscriptionControl-Multiple'

 TraceJob:

 $ref: '#/components/schemas/TraceJob-Multiple'

 AlarmList:

 $ref: '#/components/schemas/AlarmList-Single'

 MnsRegistry:

 $ref: '#/components/schemas/MnsRegistry-Single'

 ManagedElement-ncO:

 type: object

 properties:

 MnsAgent:

 $ref: '#/components/schemas/MnsAgent-Multiple'

 PerfMetricJob:

 $ref: '#/components/schemas/PerfMetricJob-Multiple'

 ThresholdMonitor:

 $ref: '#/components/schemas/ThresholdMonitor-Multiple'

 NtfSubscriptionControl:

 $ref: '#/components/schemas/NtfSubscriptionControl-Multiple'

 TraceJob:

 $ref: '#/components/schemas/TraceJob-Multiple'

 AlarmList:

 $ref: '#/components/schemas/AlarmList-Single'

#-------- Definition of abstract IOCs --------------------------------------------

 ManagedFunction-Attr:

 type: object

 properties:

 userLabel:

 type: string

 vnfParametersList:

 type: array

 items:

 $ref: '#/components/schemas/VnfParameter'

 peeParametersList:

 type: array

 items:

 $ref: '#/components/schemas/PeeParameter'

 priorityLabel:

 type: integer

 supportedPerfMetricGroups:

 type: array

 items:

 $ref: '#/components/schemas/SupportedPerfMetricGroup'

 EP\_RP-Attr:

 type: object

 properties:

 userLabel:

 type: string

 farEndEntity:

 type: string

 supportedPerfMetricGroups:

 type: array

 items:

 $ref: '#/components/schemas/SupportedPerfMetricGroup'

 TraceJob-Attr:

 type: object

 description: abstract class used as a container of all TraceJob attributes

 properties:

 tjJobType:

 $ref: '#/components/schemas/tjJobType-Type'

 tjListOfInterfaces:

 $ref: '#/components/schemas/tjListOfInterfaces-Type'

 tjListOfNeTypes:

 $ref: '#/components/schemas/tjListOfNeTypes-Type'

 tjPLMNTarget:

 $ref: '#/components/schemas/tjPLMNTarget-Type'

 tjStreamingTraceConsumerURI:

 $ref: 'comDefs.yaml#/components/schemas/Uri'

 tjTraceCollectionEntityAddress:

 $ref: '#/components/schemas/IpAddr'

 tjTraceDepth:

 $ref: '#/components/schemas/tjTraceDepth-Type'

 tjTraceReference:

 $ref: '#/components/schemas/tjTraceReference-Type'

 tjTraceRecordSessionReference:

 type: string

 tjTraceReportingFormat:

 $ref: '#/components/schemas/tjTraceReportingFormat-Type'

 tjTraceTarget:

 $ref: '#/components/schemas/tjTraceTarget-Type'

 tjTriggeringEvent:

 $ref: '#/components/schemas/tjTriggeringEvent-Type'

 tjMDTAnonymizationOfData:

 $ref: '#/components/schemas/tjMDTAnonymizationOfData-Type'

 tjMDTAreaConfigurationForNeighCell:

 $ref: '#/components/schemas/AreaConfig'

 tjMDTAreaScope:

 type: array

 items:

 $ref: '#/components/schemas/AreaScope'

 tjMDTCollectionPeriodRrmLte:

 $ref: '#/components/schemas/tjMDTCollectionPeriodRrmLte-Type'

 tjMDTCollectionPeriodM6Lte:

 $ref: '#/components/schemas/tjMDTCollectionPeriodM6Lte-Type'

 tjMDTCollectionPeriodM7Lte:

 $ref: '#/components/schemas/tjMDTCollectionPeriodM7Lte-Type'

 tjMDTCollectionPeriodRrmUmts:

 $ref: '#/components/schemas/tjMDTCollectionPeriodRrmUmts-Type'

 tjMDTCollectionPeriodRrmNR:

 $ref: '#/components/schemas/tjMDTCollectionPeriodRrmNR-Type'

 tjMDTCollectionPeriodM6NR:

 $ref: '#/components/schemas/tjMDTCollectionPeriodM6NR-Type'

 tjMDTCollectionPeriodM7NR:

 $ref: '#/components/schemas/tjMDTCollectionPeriodM7NR-Type'

 tjMDTEventListForTriggeredMeasurement:

 $ref: '#/components/schemas/tjMDTEventListForTriggeredMeasurement-Type'

 tjMDTEventThreshold:

 $ref: '#/components/schemas/tjMDTEventThreshold-Type'

 tjMDTListOfMeasurements:

 $ref: '#/components/schemas/tjMDTListOfMeasurements-Type'

 tjMDTLoggingDuration:

 $ref: '#/components/schemas/tjMDTLoggingDuration-Type'

 tjMDTLoggingInterval:

 $ref: '#/components/schemas/tjMDTLoggingInterval-Type'

 tjMDTLoggingEventThreshold:

 $ref: '#/components/schemas/tjMDTLoggingEventThreshold-Type'

 tjMDTLoggingHysteresis:

 $ref: '#/components/schemas/tjMDTLoggingHysteresis-Type'

 tjMDTLoggingTimeToTrigger:

 $ref: '#/components/schemas/tjMDTLoggingTimeToTrigger-Type'

 tjMDTMBSFNAreaList:

 type: array

 items:

 $ref: '#/components/schemas/MbsfnArea'

 tjMDTMeasurementPeriodLTE:

 $ref: '#/components/schemas/tjMDTMeasurementPeriodLTE-Type'

 tjMDTMeasurementPeriodUMTS:

 $ref: '#/components/schemas/tjMDTMeasurementPeriodUMTS-Type'

 tjMDTMeasurementQuantity:

 $ref: '#/components/schemas/tjMDTMeasurementQuantity-Type'

 tjMDTM4ThresholdUmts:

 $ref: '#/components/schemas/tjMDTM4ThresholdUmts-Type'

 tjMDTPLMNList:

 $ref: '#/components/schemas/tjMDTPLMNList-Type'

 tjMDTPositioningMethod:

 $ref: '#/components/schemas/tjMDTPositioningMethod-Type'

 tjMDTReportAmount:

 $ref: '#/components/schemas/tjMDTReportAmount-Type'

 tjMDTReportingTrigger:

 $ref: '#/components/schemas/tjMDTReportingTrigger-Type'

 tjMDTReportInterval:

 $ref: '#/components/schemas/tjMDTReportInterval-Type'

 tjMDTReportType:

 $ref: '#/components/schemas/tjMDTReportType-Type'

 tjMDTSensorInformation:

 $ref: '#/components/schemas/tjMDTSensorInformation-Type'

 tjMDTTraceCollectionEntityID:

 $ref: '#/components/schemas/tjMDTTraceCollectionEntityID-Type'

 ManagedFunction-ncO:

 type: object

 properties:

 PerfMetricJob:

 $ref: '#/components/schemas/PerfMetricJob-Multiple'

 ThresholdMonitor:

 $ref: '#/components/schemas/ThresholdMonitor-Multiple'

 ManagedNFService:

 $ref: '#/components/schemas/ManagedNFService-Multiple'

 TraceJob:

 $ref: '#/components/schemas/TraceJob-Multiple'

 MnsRegistry-Single:

 type: object

 properties:

 MnsInfo:

 $ref: '#/components/schemas/MnsInfo-Multiple'

#-------- Definition of concrete IOCs --------------------------------------------

 VsDataContainer-Single:

 type: object

 properties:

 id:

 type: string

 attributes:

 type: object

 properties:

 vsDataType:

 type: string

 vsDataFormatVersion:

 type: string

 vsData:

 nullable: true

 VsDataContainer:

 $ref: '#/components/schemas/VsDataContainer-Multiple'

 ManagedNFService-Single:

 allOf:

 - $ref: '#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 type: object

 properties:

 userLabel:

 type: string

 nFServiceType:

 $ref: '#/components/schemas/NFServiceType'

 sAP:

 $ref: '#/components/schemas/SAP'

 operations:

 type: array

 items:

 $ref: '#/components/schemas/Operation'

 administrativeState:

 $ref: 'comDefs.yaml#/components/schemas/AdministrativeState'

 operationalState:

 $ref: 'comDefs.yaml#/components/schemas/OperationalState'

 usageState:

 $ref: 'comDefs.yaml#/components/schemas/UsageState'

 registrationState:

 $ref: '#/components/schemas/RegistrationState'

 ManagementNode-Single:

 allOf:

 - $ref: '#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 type: object

 properties:

 userLabel:

 type: string

 managedElements:

 $ref: 'comDefs.yaml#/components/schemas/DnList'

 vendorName:

 type: string

 userDefinedState:

 type: string

 locationName:

 type: string

 swVersion:

 type: string

 MnsAgent:

 $ref: '#/components/schemas/MnsAgent-Multiple'

 MnsAgent-Single:

 allOf:

 - $ref: '#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 type: object

 properties:

 systemDN:

 $ref: 'comDefs.yaml#/components/schemas/Dn'

 MeContext-Single:

 allOf:

 - $ref: '#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 type: object

 properties:

 dnPrefix:

 type: string

 PerfMetricJob-Single:

 allOf:

 - $ref: '#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 type: object

 properties:

 administrativeState:

 $ref: 'comDefs.yaml#/components/schemas/AdministrativeState'

 operationalState:

 $ref: 'comDefs.yaml#/components/schemas/OperationalState'

 jobId:

 type: string

 performanceMetrics:

 type: array

 items:

 type: string

 granularityPeriod:

 type: integer

 minimum: 1

 objectInstances:

 $ref: 'comDefs.yaml#/components/schemas/DnList'

 rootObjectInstances:

 $ref: 'comDefs.yaml#/components/schemas/DnList'

 reportingCtrl:

 $ref: '#/components/schemas/ReportingCtrl'

 ThresholdMonitor-Single:

 allOf:

 - $ref: '#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 type: object

 properties:

 administrativeState:

 $ref: 'comDefs.yaml#/components/schemas/AdministrativeState'

 operationalState:

 $ref: 'comDefs.yaml#/components/schemas/OperationalState'

 performanceMetrics:

 type: array

 items:

 type: string

 thresholdInfoList:

 type: array

 items:

 $ref: '#/components/schemas/ThresholdInfo'

 monitorGranularityPeriod:

 type: integer

 minimum: 1

 objectInstances:

 $ref: 'comDefs.yaml#/components/schemas/DnList'

 rootObjectInstances:

 $ref: 'comDefs.yaml#/components/schemas/DnList'

 NtfSubscriptionControl-Single:

 allOf:

 - $ref: '#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 type: object

 properties:

 notificationRecipientAddress:

 $ref: 'comDefs.yaml#/components/schemas/Uri'

 notificationTypes:

 type: array

 items:

 $ref: 'comDefs.yaml#/components/schemas/NotificationType'

 scope:

 $ref: '#/components/schemas/Scope'

 notificationFilter:

 $ref: 'comDefs.yaml#/components/schemas/Filter' HeartbeatControl:

 $ref: '#/components/schemas/HeartbeatControl-Single'

 HeartbeatControl-Single:

 allOf:

 - $ref: '#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 type: object

 properties:

 heartbeatNtfPeriod:

 type: integer

 minimum: 0

 triggerHeartbeatNtf:

 type: boolean

 TraceJob-Single:

 allOf:

 - $ref: '#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 $ref: '#/components/schemas/TraceJob-Attr'

 AlarmList-Single:

 allOf:

 - $ref: '#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 type: object

 properties:

 administrativeState:

 $ref: 'comDefs.yaml#/components/schemas/AdministrativeState'

 operationalState:

 $ref: 'comDefs.yaml#/components/schemas/OperationalState'

 numOfAlarmRecords:

 type: integer

 lastModification:

 $ref: 'comDefs.yaml#/components/schemas/DateTime'

 alarmRecords:

 description: >-

 This resource represents a map of alarm records.

 The alarmIds are used as keys in the map.

 type: object

 additionalProperties:

 $ref: 'faultMnS.yaml#/components/schemas/AlarmRecord'

 MnsInfo-Single:

 type: object

 properties:

 mnsLabel:

 type: string

 mnsType:

 type: string

 enum:

 - ProvMnS

 - FaultSupervisionMnS

 - StreamingDataReportingMnS

 - FileDataReportingMnS

 mnsVersion:

 type: string

 mnsAddress:

 description: Resource URI as defined in the relevant Technical Specification

 $ref: 'comDefs.yaml#/components/schemas/Uri'

#-------- Definition of YAML arrays for name-contained IOCs ----------------------

 VsDataContainer-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/VsDataContainer-Single'

 ManagedNFService-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/ManagedNFService-Single'

 ManagementNode-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/ManagementNode-Single'

 MnsAgent-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/MnsAgent-Single'

 MeContext-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/MeContext-Single'

 PerfMetricJob-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/PerfMetricJob-Single'

 ThresholdMonitor-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/ThresholdMonitor-Single'

 TraceJob-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/TraceJob-Single'

 NtfSubscriptionControl-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/NtfSubscriptionControl-Single'

 MnsInfo-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/MnsInfo-Single'

#-------- Definitions in TS 28.623 for TS 28.532 ---------------------------------

 resources-genericNrm:

 oneOf:

 - $ref: '#/components/schemas/VsDataContainer-Single'

 - $ref: '#/components/schemas/ManagementNode-Single'

 - $ref: '#/components/schemas/MnsAgent-Single'

 - $ref: '#/components/schemas/MeContext-Single'

 - $ref: '#/components/schemas/ManagedNFService-Single'

 - $ref: '#/components/schemas/PerfMetricJob-Single'

 - $ref: '#/components/schemas/ThresholdMonitor-Single'

 - $ref: '#/components/schemas/TraceJob-Single'

 - $ref: '#/components/schemas/NtfSubscriptionControl-Single'

 - $ref: '#/components/schemas/HeartbeatControl-Single'

 - $ref: '#/components/schemas/AlarmList-Single'

 - $ref: '#/components/schemas/MnsRegistry-Single'

 - $ref: '#/components/schemas/MnsInfo-Single'

|  |
| --- |
| **2nd change** |

## D.2.X module \_3gpp-common-mnsregistry.yang

<CODE BEGINS>

module \_3gpp-common-mnsregistry {

 yang-version 1.1;

 namespace "urn:3gpp:sa5:\_3gpp-common-mnsregistry";

 prefix "mnsregist3gpp";

 import \_3gpp-common-subnetwork { prefix subnet3gpp; }

 import \_3gpp-common-top { prefix top3gpp; }

 organization "3GPP SA5";

 contact "https://www.3gpp.org/DynaReport/TSG-WG--S5--officials.htm?Itemid=464";

 description "Defines the YANG mapping of the MNSRegistry Information Object

 Class (IOC) that is part of the Generic Network Resource Model (NRM).";

 reference "3GPP TS 28.623 Generic Network Resource Model (NRM)";

 revision 2021-10-18 { reference "S5-215263"; }

 revision 2021-08-29 { reference "Initial revision, S5-214388"; }

 grouping MNSInfoGrp {

 description "Represents the MNSInfo IOC.";

 reference "3GPP TS 28.622";

 leaf mnsLabel {

 description "Human-readable name of management service.";

 mandatory true;

 type string;

 }

 leaf mnsType {

 description "Type of management service.";

 type enumeration {

 enum ProvMnS;

 enum FaultSupervisionMnS;

 enum StreamingDataReportingMnS;

 enum FileDataReportingMnS;

 }

 }

 leaf mnsVersion {

 description "Version of management service.";

 type string;

 }

 leaf mnsAddress {

 description "Addressing information for Management Service operations.";

 mandatory true;

 type string;

 }

 }

 grouping MNSInfo {

 description "Represents the MNSInfo IOC.";

 reference "3GPP TS 28.622";

 uses top3gpp:Top\_Grp;

 container attributes {

 uses MNSInfoGrp;

 }

 }

 grouping MNSRegistryGrp {

 description "Represents the MNSRegistry IOC.";

 reference "3GPP TS 28.622";

 uses top3gpp:Top\_Grp;

 }

 grouping MNSRegistry {

 list mnsRegistry {

 description "Represents the MNSRegistry IOC.";

 reference "3GPP TS 28.622";

 uses top3gpp:Top\_Grp;

 key "mnsType mnsVersion mnsAddress";

 container attributes {

 uses MNSInfoGrp;

 }

 }

 }

 augment "/subnet3gpp:SubNetwork" {

 uses MNSRegistryGrp;

 }

}

<CODE ENDS>

|  |
| --- |
| **End of changes** |