|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **3GPP TSG-SA5 Meeting #143-e *S5-223440rev2***  **e-meeting, 9 - 17 May 2022**   |  |  |  |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | --- | --- | --- | | *CR-Form-v12.1* | | | | | | | | | | **CHANGE REQUEST** | | | | | | | | | |  | | | | | | | | | |  | **32.291** | **CR** | **0404** | **rev** | **1** | **Current version:** |  |  | |  | | | | | | | | | | *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | | |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | | | UICC apps | | | |  | ME |  | Radio Access Network | | | | |  | Core Network | **x** |
|  | | | | | | | | | | | | | | | | | |
| ***Title:*** | Introduce Data Type for 5G ProSe | | | | | | | | | | | | | | | | |
|  |  | | | | | | | | | | | | | | | | |
| ***Source to WG:*** |  | | | | | | | | | | | | | | | | |
| ***Source to TSG:*** | SA5 | | | | | | | | | | | | | | | | |
|  |  | | | | | | | | | | | | | | | | |
| ***Work item code:*** | 5G\_ProSe | | | | | | | | |  | ***Date:*** | | |  | | | |
|  |  | | | | |  | | | | |  | | |  | | | |
| ***Category:*** | **B** |  | | | | | | | | | ***Release:*** | | |  | | | |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | | | | |
|  |  | | | | | | | | | | | | | | | | |
| ***Reason for change:*** | | The corresponding Data type of 5G ProSe needs to be introduced | | | | | | | | | | | | | | | |
|  | |  | | | | | | | | | | | | | | | |
| ***Summary of change:*** | | Introduce specific Data Type for 5G ProSe. | | | | | | | | | | | | | | | |
|  | |  | | | | | | | | | | | | | | | |
| ***Consequences if not approved:*** | | No converged charging of 5G ProSe. | | | | | | | | | | | | | | | |
|  | |  | | | | | | | | | | | | | | | |
| ***Clauses affected:*** | | 2, 6.1.6.2.x (new), 6.1.6.3.4, 6.1.6.3.a-e (new), 6.1.8 | | | | | | | | | | | | | | | |
|  | |  | | | | | | | | | | | | | | | |
|  | | **Y** | | **N** |  | | | | | | |  | | | | | |
| ***Other specs*** | |  | | **X** | Other core specifications | | | | | | | TS/TR ... CR ... | | | | | |
| ***affected:*** | |  | | **X** | Test specifications | | | | | | | TS/TR ... CR ... | | | | | |
| ***(show related CRs)*** | |  | | **X** | O&M Specifications | | | | | | | TS/TR ... CR ... | | | | | |
|  | |  | | | | | | | | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | | | | | | | | |
|  | |  | | | | | | | | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | | | | | | | | |

|  |
| --- |
| **1st modified section** |

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TS 32.240: "Telecommunication management; Charging management; Charging architecture and principles".

[2] - [13] Void.

[14] 3GPP TS 32.254: "Telecommunication management; Charging management; Exposure function Northbound Application Program Interfaces (APIs) charging ".

[15] - [28] Void.

[29] 3GPP TS 32.274: "Telecommunication management; Charging management;Short Message Service (SMS) charging".

[30] 3GPP TS 32.255: "Telecommunication management; Charging management; 5G Data connectivity domain charging; stage 2".

[31] 3GPP TS 32.256: "Telecommunication management; Charging management; 5G connection and mobility domain charging; stage 2".

[32] 3GPP TS 32.260: "Telecommunication management; Charging management; IP Multimedia Subsystem (IMS) charging".

[33] 3GPP TS 32.275: "Telecommunication management; Charging management; MultiMedia Telephony (MMTel) charging".

[34] 3GPP TS 32.281: " Telecommunication management; Charging management; Announcement

[35] 3GPP TS 32.277: "Telecommunication management; Charging management; Proximity-based Services (ProSe) charging".

[36] - [49] Void.

[50] - [57] Void.

[58] 3GPP TS 32.290: "Telecommunication management; Charging management; 5G system; Services, operations and procedures of charging using Service Based Interface (SBI).

[59] - [69] Void.[70] 3GPP TS 28.201: "Charging management; Network slice performance and analytics charging in the 5G System (5GS); Stage 2".

[71] 3GPP TS 28.202: "Charging management; Network slice management charging in the 5G System (5GS); Stage 2".

[72] - [99] Void.

[100] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[101] 3GPP TR 21.900: "Technical Specification Group working methods".

[102] 3GPP TS 24.605: "Conference (CONF) using IP Multimedia (IM) Core Network (CN) subsystem; Protocol specification".

[103] - [199] Void

[200] - [252] Void

[253] 3GPP TS 28.532: "Management and orchestration; Management services".

[254] 3GPP TS 28.541: "Management and orchestration; 5G Network Resource Model (NRM); Stage 2 and stage 3".

[255] 3GPP TS 32.300: "Telecommunication management; Configuration Management (CM); Name convention for Managed Objects".

[256] 3GPP TS 28.554: "Management and orchestration;5G end to end Key Performance Indicators (KPI)".

[257] 3GPP TS 28.623: "Telecommunication management; Generic Network Resource Model (NRM) Integration Reference Point (IRP); Solution Set (SS) definitions".

[258] 3GPP TS 24.229: "IP Multimedia Call Control Protocol based on SIP and SDP; Stage 3".

[259] 3GPP TS 29.078: "Customised Applications for Mobile network Enhanced Logic (CAMEL); CAMEL Application Part (CAP) specification".".

[260] 3GPP TS 29.228: "IP Multimedia (IM) Subsystem Cx and Dx interface; signalling flows and message contents".

[261] 3GPP TS 29.002: "Mobile Application Part (MAP) specification".

[262] - [298] Void

[299] 3GPP TS 29.500: "5G System; Technical Realization of Service Based Architecture; Stage 3".

[300] 3GPP TS 29.501: "5G System; Principles and Guidelines for Services Definition; Stage 3".

[301] 3GPP TS 29.594: "5G System; Spending Limit Control Service; Stage 3".

[302] 3GPP TS 29.512: "5G System; Session Management Policy Control Service; Stage 3".

[303] 3GPP TS 24.501: "Non-Access-Stratum (NAS) Protocol for 5G System (5GS); Stage 3".

[304] 3GPP TS 38.413: "NG-RAN; NG Application Protocol (NGAP)".

[305] 3GPP TS 29.510: "Network Function Repository Services; Stage 3".

[306] 3GPP TS 29.520: "5G System; Network Data Analytics Services;Stage 3".

[307] - [370] Void

[371] 3GPP TS 29.571: "5G System; Common Data Types for Service Based Interfaces; Stage 3".

[372] - [389] Void

[390] 3GPP TS 33.501: "Security architecture and procedures for 5G System".

[391] - [399] Void

[400] Void.

[401] IETF RFC 7540: "Hypertext Transfer Protocol Version 2 (HTTP/2) ".

[402] IETF RFC 8259: "The JavaScript Object Notation (JSON) Data Interchange Format ".

[403] IETF RFC 6749: "The OAuth 2.0 Authorization Framework".

[404] IETF RFC 3986: "Uniform Resource Identifiers (URI): Generic Syntax".

[405] IETF RFC 7315: "Private Extensions to the Session Initiation Protocol (SIP) for the 3rd Generation Partnership Projects (3GPP)".

[406] IETF RFC 3261: "SIP: Session Initiation Protocol".

[407] IETF RFC 8866: "SDP: Session Description Protocol".

[408] IETF RFC 5646: "Tags for Identifying Languages".

[409] - [499] Void.

[500] OpenAPI: "OpenAPI 3.0.0 Specification", <https://github.com/OAI/OpenAPI-Specification/blob/master/versions/3.0.0.md>.

[501] - [599] Void.

|  |
| --- |
| **Next change** |

##### 6.1.6.2.x 5G ProSe Specified Data Type

###### 6.1.6.2.x.1 Type ChargingDataRequest

This clause is additional attributes of the type ChargingDataRequest defined in clause 6.x.2.2 for 5G ProSe charging described in 3GPP TS 32.277[35].

Table 6.1.6.2.x.1-1: 5G ProSe Specified attribute of type ChargingDataRequest

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| proseCharging Information | ProSeChargingInformation | OM | 0..1 | This field holds the 5G ProSe specific information. |  |

###### 6.1.6.2.x.2 Type ChargingDataResponse

This clause is additional attributes of the type ChargingDataResponse defined in clause 6.x.2.2 for 5G ProSe charging described in 3GPP TS 32.277[35].

Table 6.1.6.2.x.2-1: 5G ProSe Specified attribute of type ChargingDataResponse

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
|  |  |  |  |  |  |

###### 6.1.6.2.x.3 Type UsedUnitContainer

Table 6.1.6.2.2.5-1: 5G ProSe Specified portion of type UsedUnitContainer

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| pC5Container Information | PC5Container Information | OC | 0..1 | This field holds the PC5 container information |  |

###### 6.1.6.2.x.4 Type PC5ContainerInformation

This clause is additional portion of the type PC5ContainerInformation defined in clause 6.x.2.2 for 5G ProSe charging described in 3GPP TS 32.277[35].

Table 6.1.6.2.x.4-1: 5G ProSe Specified portion of type PC5ContainerInformation

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| coverageInfoList | array (CoverageInfo) | OC | 0..N | This IE provides information on the coverage information. |  |
| radioParameter SetInfoList | array (RadioParameter SetInfo) | OC | 0..N | This IE provides information on a radio parameter set configured in the UE for direct communication use |  |
| transmitterInfoList | array (TransmitterInfo) | OC | 0..N | This IE provides information on a transmitter detected for direct communication |  |
| timeOfFirstTransmission | DateTime | OC | 0..1 | This IE holds the time in UTC format for the first packet transmitted |  |
| timeOfFirstReception | DateTime | OC | 0..1 | This IE holds the time in UTC format for the first packet received. |  |

###### 6.1.6.2.x.5 Type CoverageInfo

Table 6.1.6.2.x.5-1: 5G ProSe Specified portion of type CoverageInfo

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| coverageStatus | boolean | OC | 0..1 | Whether the UE is served by NG-RAN or not |  |
| changeTime | DateTime | OC | 0..1 | The time when the coverage status changed to its current state. |  |
| locationInfo | array(LocationInfo) | OC | 0..N | It provides UE location Information. When in NG-RAN coverage, additionally includes a list of location changes |  |

###### 6.1.6.2.x.6 Type RadioParameterSetInfo

This clause is additional portion of the type RadioParameterSetInfo defined in clause 6.x.2.2 for 5G ProSe charging described in 3GPP TS 32.277[35].

Table 6.1.6.2.x.6-1: 5G ProSe Specified portion of type RadioParameterSetInfo

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| radioParameterSetValues | array(OctetString) | OC | 0..N | It provides the radio parameter set configured in the UE for direct communication. The format of the value is according to the SL-Preconfiguration data type. |  |
| changeTimestamp | DateTime | OC | 0..1 | The time when associated time stamp of when Radio Parameters became active. |  |

###### 6.1.6.2.x.7 Type TransmitterInfo

This clause is additional portion of the type TransmitterInfo defined in clause 6.x.2.2 for 5G ProSe charging described in 3GPP TS 32.277[35].

Table 6.1.6.2.x.7-1: 5G ProSe Specified portion of type TransmitterInfo

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| proseSourceIPAddress | string | OC | 0..1 | Source IP address of ProSe UE |  |

###### 6.1.6.2.x.8 Type ProseChargingInformation

Table 6.1.6.2.x.8-1: Definition of type ProseChargingInformation

| Attribute name | Data type | P | Cardinality | Description | Applicability |
| --- | --- | --- | --- | --- | --- |
| announcingPlmnID | PlmnId | OC | 0..1 | PLMN identity of the serving PLMN which signalled the carrier frequency. |  |
| announcingUeHplmnIdentifier | PlmnId | OM | 0..1 | PLMN identity of HPLMN for announcing UE. |  |
| announcingUeVplmnIdentifier | PlmnId | OC | 0..1 | PLMN identity of VPLMN for announcing UE |  |
| monitoringUeHplmnIdentifier | PlmnId | OC | 0..1 | PLMN identity of HPLMN for monitoring UE. |  |
| monitoringUeVplmnIdentifier | PlmnId | OC | 0..1 | PLMN identity of VPLMN for monitoring UE. |  |
| discovererUeHplmnIdentifier | PlmnId | OM | 0..1 | PLMN identity of Discoverer UE HPLMN. |  |
| discovererUeVplmnIdentifier | PlmnId | OC | 0..1 | PLMN identity of Discoverer UE VPLMN. |  |
| discovereeUeHplmnIdentifier | PlmnId | OC | 0..1 | PLMN identity of Discoveree UE HPLMN. |  |
| discovereeUeVplmnIdentifier | PlmnId | OC | 0..1 | PLMN identity of Discoveree UE VPLMN. |  |
| monitoredPlmnIdentifier | PlmnId | OC | 0..1 | Monitored PLMN ID in Match\_Report request |  |
| proseApplicationID | string | OC | 0..1 | The identities used for ProSe Direct Discovery, identifying application related information for the ProSe-enabled UE |  |
| applicationID | string | OC | 0..1 | A PLMN-specific, country-specific or global-specifc identifier identifying a specific 3rd party application. |  |
| applicationSpecificData | string | OC | 0..1 | This IE contains a data block provided by the application in the UE. |  |
| proseFunctionality | ProseFunctionality | OC | 0..1 | This IE holds the ProSe functionality UE is requesting |  |
| proseEventType | ProseEventType | OC | 0..1 | This IE holds the event which triggers the charging message delivery |  |
| directDiscoveryModel | DirectDiscoveryModel | OC | 0..1 | This IE holds the model of the Direct Discovery used by the UE. |  |
| validityPeriod | integer | OC | 0..1 | Time interval during which user is authorized for using ProSe Direct Discovery |  |
| roleOfUE | RoleOfUE | OC | 0..1 | Role of the UE using ProSe |  |
| proseRequestTimestamp | DateTime | OC | 0..1 | The time when ProSe Request is received from UE. |  |
| pC3ProtocolCause | integer | OC | 0..1 | This IE holds the particular reason why a DISCOVERY\_REQUEST or Match\_Report messages from the UE have been rejected by the 5G DDNMF in PC3 interface. |  |
| monitoringUEIdentifier | string | OM | 0..1 | Identifier of the party who initiate monitor/match report |  |
| requestedPLMNIdentifier | PlmnId | OC | 0..1 | The PLMN identifier of the user who is targeted in proximity request. |  |
| timeWindow | integer | OC | 0..1 | The time interval in minutes during which a proximity request is valid. |  |
| rangeClass | RangeClass | OC | 0..1 | A range class for the first proximity request. |  |
| proximityAlertIndication | Boolean | OC | 0..1 | Indication of whether proximity alert has been sent before proximity request cancellation. |  |
| proximityAlertTimestamp | DateTime | OC | 0..1 | The time stamp when proximity alert is sent, to indicate two UEs are in proximity. |  |
| proximityCancellationTimestamp | DateTime | OC | 0..1 | The time stamp when proximity request cancellation is requested. |  |
| relayIPAddress | string | OC | 0..1 | The IP address UE used as ProSe UE-to-Network Relay UE address |  |
| proseUEToNetworkRelayUEID | string | OC | 0..1 | A link layer identifier that uniquely represents the ProSe UE-to-Network Relay UE |  |
| proseDestinationLayer2ID | string | OC | 0..1 | The identifier of a link-layer that identifies a device or a group of devices that are recipients of ProSe communication frames. |  |
| pFIContainerInformation | array(pFIContainerInformation) | OC | 0..N | This field holds the PFI data container information |  |
| transmissionDataContainer | array(PC5DataContainer) | OC | 0..N | The container associated to a trigger conditions |  |
| receptionDataContainer | array(PC5DataContainer) | OC | 0..N | This field holds the container associated to a trigger conditions |  |

###### 6.1.6.2.x.9 Type PFIContainerInformation

This clause is additional portion of the type PFIContainerInformation defined in clause 6.x.2.2 for 5G ProSe charging described in 3GPP TS 32.277[35].

Table 6.1.6.2.x.9-1: 5G ProSe Specified portion of type PFIContainerInformation

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| pFI | Qfi | OM | 0..1 | PC5 QoS flow Identifier (PFI) |  |
| reportTime | DateTime | OM | 1 | the UTC time indicating time stamp when the QFI data container was closed |  |
| timeofFirstUsage | DateTime | OC | 0..1 | the UTC time indicating time stamp for the first IP packet to be transmitted and mapped to the PFI container |  |
| timeofLastUsage | DateTime | OC | 0..1 | the UTC time indicating time stamp for the last IP packet to be transmitted and mapped to the PFI container. |  |
| qoSInformation | QoSData | OC | 0..1 | the PC5 QoS applied to PFI container.  In case gbrUl or gbrDl are present for GBR QoS flow, the GBR targets are "GUARANTEED", otherwise, are " NOT\_GUARANTEED". |  |
| qoSCharacteristics | QosCharacteristics | OC | 0..1 | Map of PC5 QoS characteristics for non standard PQIs and non-preconfigured PQIs. |  |
| userLocationInformation | UserLocation | OC | 0..1 | provides information on the location |  |
| uetimeZone | TimeZone | OC | 0..1 | UE Time Zone the UE is currently located |  |
| presenceReportingAreaInformation | map(PresenceInfo) | OC | 0..N | the Presence Reporting Area status of UE during the PFI container interval. |  |

###### 6.1.6.2.x.10 Type PC5DataContainer

Table 6.1.6.2.x.10-1: 5G ProSe Specified portion of type PC5DataContainer

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| localSequenceNumber | string | OC | 0..1 | The sequence number of the Direct Communication data container |  |
| changeTime | DateTime | OC | 0..1 | The time when the container is closed and reported due to ProSe charging condition change. |  |
| coverageStatus | boolean | OC | 0..1 | Whether UE is served by NG-RAN or not |  |
| userLocationInformation | UserLocation | OC | 0..1 | The location of the UE |  |
| dataVolume | Uint64 | OC | 0..1 | This field holds the amount of volume transmitted or received |  |
| changeCondition | string | OC | 0..1 | ProSe specific reason for closing the container |  |
| usageInfoReportSN | string | OC | 0..1 | The sequence number of usage information report, which is used to generate the container. |  |
| radioResourcesId | RadioResourcesIndicator | OC | 0..1 | This IE identifies whether the operator-provided radio resources or the configured radio resources were used for ProSe direct communication. |  |
| radioFrequency | string | OC | 0..1 | This IE identifies the radio frequency used for ProSe direct communication |  |
| pC5RadioTechnology | string | OM | 0..1 | The PC5 radio technology used by UE |  |

|  |
| --- |
| **Next change** |

##### 6.1.6.3.4 Enumeration: NodeFunctionality

Table 6.1.6.3.4-1: Enumeration NodeFunctionality

|  |  |  |
| --- | --- | --- |
| Enumeration value | Description | Applicability |
| SMF | This field identifies that NF is a SMF. |  |
| AMF | This field identifies that NF is a AMF. |  |
| SMSF | This field identifies that NF service consumer is a SMSF. |  |
| PGW\_C\_SMF | This field identifies that NF is a SMF+PGW-C. |  |
| NEF | This field identifies that NF is a NEF. |  |
| SGW | This field identifies that node is an SGW, only applicable for interworking with EPC. |  |
| I\_SMF | This field identifies that node is an I-SMF, only applicable for PDU session served by SMF + I-SMF. | ETSUN |
| ePDG | This field identifies that node is an ePDG, only applicable for interworking with EPC/ePDG. | 5GIEPC\_CH |
| CEF | This field identifies that NF is a CEF. |  |
| MnS\_Producer | This field identifies that NF is a MnS Producer |  |
| SGSN | This field identifies that node is an SGSN, only applicable when SMF+PGW-C serves GERAN/UTRAN access. | TEI17\_NIESGU |
| 5G DDNMF | This field identifies that NF is a 5G DDNMF | 5G ProSe |

|  |
| --- |
| **Next change** |

##### 6.1.6.3.a Enumeration: ProseFunctionality

Table 6.1.6.3.a -1: Enumeration ProseFunctionality

|  |  |  |
| --- | --- | --- |
| Enumeration value | Description | Applicability |
| DIRECT\_DISCOVERY | Indicates the UE is requesting for ProSe direct discovery. |  |
| DIRECT\_COMMUNICATION | Indicates the UE is requesting for ProSe direct communication. |  |

##### 6.1.6.3.b Enumeration: ProseEventType

Table 6.1.6.3.b -1: Enumeration ProseEventType

|  |  |  |
| --- | --- | --- |
| Enumeration value | Description | Applicability |
| ANNOUNCING | Indicates the ProSe ProSe charging announcing event. |  |
| MONITORING | Indicates the ProSe ProSe charging monitoring event. |  |
| MATCH\_REPORT | Indicates the ProSe ProSe charging match report event. |  |

##### 6.1.6.3.c Enumeration: DirectDiscoveryModel

Table 6.1.6.3.c -1: Enumeration DirectDiscoveryModel

|  |  |  |
| --- | --- | --- |
| Enumeration value | Description | Applicability |
| MODEL\_A | Indicates model A of the Direct Discovery used by the UE |  |
| MODEL\_B | Indicates model B of the Direct Discovery used by the UE. |  |

##### 6.1.6.3.d Enumeration: RoleOfUE

Table 6.1.6.3.d -1: Enumeration RoleOfUE

|  |  |  |
| --- | --- | --- |
| Enumeration value | Description | Applicability |
| ANNOUNCING\_UE | Indicates role of the UE using ProSe for announcing. |  |
| MONITORING\_UE | Indicates role of the UE using ProSe for monitoring. |  |
| REQUESTOR\_UE | Indicates role of the UE using ProSe for sending requst. |  |
| REQUESTED\_UE | Indicates role of the UE using ProSe for receive requst. |  |

##### 6.1.6.3.e Enumeration: RangeClass

Table 6.1.6.3.e -1: Enumeration RangeClass

|  |  |  |
| --- | --- | --- |
| Enumeration value | Description | Applicability |
| RESERVED | This value is reserved |  |
| 50\_METER | Indicates a range class for a specific proximity request in 50m |  |
| 100\_METER | Indicates a range class for a specific proximity request in 100m |  |
| 200\_METER | Indicates a range class for a specific proximity request in 200m |  |
| 500\_METER | Indicates a range class for a specific proximity request in 500m |  |
| 1000\_METER | Indicates a range class for a specific proximity request in 1000m |  |
| UNUSED | Indicates a range class is not used. |  |

##### 6.1.6.3.f Enumeration: RadioResourcesIndicator

Table 6.1.6.3.f -1: Enumeration RadioResourcesIndicator

|  |  |  |
| --- | --- | --- |
| Enumeration value | Description | Applicability |
| OPERATOR\_PROVIDED | Indicates the operator-provided radio resources for direct communication. |  |
| CONFIGURED | Indicates the configured radio resources for direct communication. |  |

|  |
| --- |
| **Next change** |

### 6.1.8 Feature negotiation

The optional features in table 6.1.8-1 are defined for the Nchf\_ConvergedCharging API. They shall be negotiated using the extensibility mechanism defined in subclause 6.6 of 3GPP TS 29.500 [299].

Table 6.1.8-1: Supported Features

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Feature number | | Feature Name | | Description | |
| 1 | | CHFCQM | | CHF-controlled quota management i.e. support for temporary offline | |
| 2 | | AF\_Charging\_Identifier | | Indicates the support of long character strings as charging identifiers. | |
| 3 | | 5GIEPC\_CH | | 5GS interworking with EPC | |
| 4 | | ATSSS | | This feature indicates support of Access Traffic Steering, Switching, Splitting (ATSSS). | |
| 5 | | ETSUN | | This feature indicates support of Enhancing Topology of SMF and UPF in 5G Networks (ETSUN). | |
| 6 | | EnhancedDiagnostics | | Support the enhanced diagnostics | |
| 7 | | AMF\_subs\_PRA | | PRA(s) subscription by CHF in AMF | |
| 8 | | FilterRuleList | | Support of multiple filter rules in the final unit indication | |
| 9 | | TEI17\_NIESGU | | This feature indicates support of GERAN/UTRAN access | |
| 10 | | IMS | | This feature indicates support of IMS. | |
| 11 | | QoSMonitoring | | This feature indicates support of QoS Monitoring | |
| 12 | | Announcement | | This feature indicates support of announcements. | |
| 13 | | 5GLAN | | This feature indicates support of 5G LAN-type services. | |
| 13 | | URLLC | | This feature indicates support of URLLC. | |
| 14 | | NotifyInfoResponse | | This feature indicates support of response with information for a notification. | |
| 15 | | ES4xx | | Extended Support of HTTP 400, 403, 404 allowing use of either ChargingDataResponse or ProblemDetails in the response. | |
| 15 | | 5G\_PROSE\_CH | | This feature indicates support of 5G ProSe. | |

|  |
| --- |
| **End of changes** |