**3GPP TSG-SA5 Meeting #145-e *S5-225335rev1***

e-meeting, 15 - 24 August 2022

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** |  | **rev** | **1** | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network | **x** |

|  |
| --- |
|  |
| ***Title:***  | Rel-17 CR 28.622 Include already approved changes or enhancements of attribute properties for IOC ManagementDataCollection  |
|  |  |
| ***Source to WG:*** | Nokia, Nokia Shanghai Bell |
| ***Source to TSG:*** | S5 |
|  |  |
| ***Work item code:*** |  |  | ***Date:*** | 2022-08-05 |
|  |  |  |  |  |
| ***Category:*** |  |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | Modifications of attribute properties table in approved Rel-17 Input to draftCR S5-223626 has accidentally not been included in S5-223657 (MADCOL draftCR) and S5-223588 (MADCOL CR) |
|  |  |
| ***Summary of change:*** | * Include changes already approved in Input to draftCR S5-223626, which have been missed to include in MADCOL draftCR and MADCOL CR.
* Editorial corrections
 |
|  |  |
| ***Consequences if not approved:*** | Attribute properties of some attributes introduced in ManagmentDataCollection IOC are not or not correctly specified or are misaligned. |
|  |  |
| ***Clauses affected:*** | 4.3.43, 4.3.48.1, 4.4.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

***First change***

### 4.3.43 ManagementDataCollection

#### 4.3.43.1 Definition

This IOC represents a management data collection request job. The requested data could be of kind Trace, MDT (Minimization of Drive Test), RLF (Radio Link Failure) report, RCEF (RRC Connection Establishment Failure) report, PM (performance measurements), KPI (end-to-end key performance indicators) or a combination of these.

The attribute "managementData" defines the management data which shall be reported. This may either include a list of data categories or a list of management data identified with their name. For further details see clause 4.3.46.

The "targetNodeFilter" attribute can be used to target object instance(s) producing the required management data. It is assumed that the consumer may not have detailed knowledge of the network and hence may not identify the exact object instance producing the required management data. In this case consumer can request management data, specified by 3GPP, produced by certain network function(s) based on a particular location, the domain (CN or RAN) of the network function, and the handled traffic (CP or UP) of the network function.

To activate the production of the requested data, a MnS consumer has to create a "ManagementDataCollection" object instance on the MnS producer.

The MnS producer will derive multiple jobs ("PerfMetricJob", "TraceJob") from a single "ManagementDataCollection" job for collecting the required management data. Once it receives the measurement from multiple sources, it consolidate the data into a set of management data for reporting.

The attribute "collectionTimeWindow" specifies the time window for which the management data should be reported.

The attribute "reportingCtrl" specifies the method and associated control parameters for reporting the produced management data to MnS consumers. Three methods are available: file-based reporting with selection of the file location by the MnS producer, file-based reporting with selection of the file location by the MnS consumer and stream-based reporting.

The attribute "dataScope" configures, whether the management data should be reported per S-NSSAI or per 5QI, if applicable.

#### 4.3.43.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute Name** | **S** | **isReadable** | **isWritable** | **isInvariant** | **isNotifyable** |
| managementData | M | T | T | T | N/A |
| targetNodeFilter | M | T | T | T | N/A |
| collectionTimeWindow | M | T | T | T | N/A |
| reportingCtrl | M | T | T | T | N/A |
| dataScope | O | T | T | T | N/A |

#### 4.3.43.3 Attribute constraints

None.

#### 4.3.43.4 Notifications

The common notifications defined in clause 4.5 are valid for this IOC. In addition, the following set of notifications is also valid.

| **Name** | **S** | **Notes** |
| --- | --- | --- |
| notifyFileReady | M | -- |
| notifyFilePreparationError | M | -- |

### 4.3.44 TimeWindow <<dataType>>

#### 4.3.44.1 Definition

This data type defines the start time and end time for which the management data should be reported.

#### 4.3.44.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute name** | **S** | **isReadable** | **isWritable** | **isInvariant** | **isNotifyable** |
| startTime | M | T | T | T | T |
| endTime | M | T | T | T | T |

#### 4.3.44.3 Attribute constraints

None.

#### 4.3.44.4 Notifications

The clause 4.5 of the <<IOC>> using this <<dataType>> as one of its attributes, shall be applicable.

### 4.3.45 NodeFilter <<dataType>>

#### 4.3.45.1 Definition

This data type defines several selection criteria for the target node(s) i.e., the node(s) producing the requested management data.

The attribute "areaOfInterest" determines the location for which the management data is collected. The system translates the area into the target managed objects. The location is either configured by a list of TAI, a list of cells (identified either by NG-RAN CGI, E-UTRAN CGI or UTRAN CGI) or by a geographical area. The geographical area will be mapped to the cells providing coverage for this area. The cell coverage status at the time of the request is used for the mapping. Managed objects providing service to these cells are considered as target managed objects. Furthermore, an object which name contains or is associated to a managed object providing service to the considered cell, is considered as target managed object as well.

The attribute "networkDomain" is used to select a particular domain (e.g. RAN, CN) for which the management data is collected. The system translates this information into the target managed objects. Managed objects from this selected particular domain (e.g RAN, CN) are considered as target managed objects. Furthermore, an object which name contains or is associated to a managed object of that domain, is considered as target managed object as well.

The attribute "cpUpType" is used to select the traffic type (CP, UP) for which the management data is collected. The system translates this information into the target managed objects. Managed objects catering particular traffic type (CP, UP) are considered as target managed objects. Furthermore, an object which name contains or is associated to a managed object of that traffic type, shall be considered as target managed object as well.

The attribute "sst" is used to select the SST (Slice/Service Type)[22] for which the management data is collected. The system translates this information into the target managed objects. Managed objects related to particular SST will be considered as target managed objects.

If it is not possible to select the target node(s) (based on a particular selection criteria) deterministically, the selection criteria should not be used.

#### 4.3.45.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute name** | **S** | **isReadable** | **isWritable** | **isInvariant** | **isNotifyable** |
| areaOfInterest | O | T | T | T | N/A |
| networkDomain | O | T | T | T | N/A |
| cpUpType | O | T | T | T | N/A |
| sst | O | T | T | T | N/A |

#### 4.3.45.3 Attribute constraints

None.

#### 4.3.45.4 Notifications

The subclause 4.5 of the <<IOC>> using this <<dataType>> as one of its attributes, shall be applicable.

### 4.3.46 ManagementData <<choice>>

#### 4.3.46.1 Definition

This <<choice>> defines the management data which is requested. It is a choice between

- a list of data categories (attribute mgtDataCategory) This may include "COVERAGE", "CAPACITY", "MOBILITY", "ENERGY\_EFFICIENCY", "ACCESSIBILITY" etc. The mapping of exact measurement with the requested category will be done at the producer and is implementation specific.

- a list of management data identified with their name (attribute "mgtDataName"). The management data name presents a specific single measurement (e.g. by selecting "RRU.PrbTotDl", see TS 28.552 [20] or "immediateMdt.nr.m1", see TS 32.422 [30]) or a set of measurements (e.g. measurement families such as RRU (radio resource utilization) or MM (mobility management) in case of PM, see TS 28.552 [20], or group of measurements such as "immediateMdt.nr" in case of MDT, see TS 32.422 [30]).

#### 4.3.46.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute name** | **S** | **isReadable** | **isWritable** | **isInvariant** | **isNotifyable** |
| CHOICE\_1.1 mgtDataCategory | M | T | T | T | N/A |
| CHOICE\_2.1 mgtDataName | M | T | T | T | N/A |

### 4.3.47 AreaOfInterest <<choice>>

#### 4.3.47.1 Definition

This <<choice>> defines the area which shall be considered for the service.

#### 4.3.47.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute name** | **S** | **isReadable** | **isWritable** | **isInvariant** | **isNotifyable** |
| CHOICE\_1.1 geoAreaToCellMapping  | M | T | T | T | N/A |
| CHOICE\_2.1 taiList | M | T | T | T | N/A |
| CHOICE\_3.1 nrCellIdList | M | T | T | T | N/A |
| CHOICE\_4.1 eutraCellIdList | M | T | T | T | N/A |
| CHOICE\_5.1 utraCellIdList | M | T | T | T | N/A |

#### 4.3.47.3 Attribute constraints

|  |  |
| --- | --- |
| Name | Definition |
| CHOICE\_1.1 geoAreaToCellMapping | This attribute shall be supported, when a service is requested for a geographical area. |
| CHOICE\_2.1 taiList | This attribute shall be supported, when a service is requested for TAI. |
| CHOICE\_3.1 nrCellIdList | This attribute shall be supported, in case of NR cells. |
| CHOICE\_4.1 eutraCellIdList | This attribute shall be supported, in case of E-UTRAN cells. |
| CHOICE\_5.1 utraCellIdList | This attribute shall be supported, in case of UTRA cells. |

### 4.3.48 GeoAreaToCellMapping <<dataType>>

#### 4.3.48.1 Definition

This data type defines a geographical area by specifying the convex polygon in the attribute "convexGeoPolygon".

The MnS producer shall map the geographical area to cells. There are two evaluation criteria whether a cell belongs to a geographical area or not. If attribute "associationThreshold" is absent, the location of the base station antenna determines the belonging. If attribute "associationThreshold" is configured, the coverage area is considered. The attribute "associationThreshold" determines the lower boundary of the coverage ratio. For example, if the "associationThreshold" is configured to 60%, a cell shall be considered as included in the geographical area if at least 60% of the coverage area of that cell overlaps with the specified geographical area.

The mapping of the geographical area to cells is performed at instantiation of the IOC.

#### 4.3.48.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute name** | **S** | **isReadable** | **isWritable** | **isInvariant** | **isNotifyable** |
| convexGeoPolygon | M | T | T | T | N/A |
| associationThreshold | O | T | T | T | N/A |

### 4.3.49 GeoCoordinate <<dataType>>

#### 4.3.49.1 Definition

This data type defines a geographical location on earth.

#### 4.3.49.2 Attributes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | S | isReadable | isWritable | isInvariant | isNotifyable |
| latitude | M | T | T | F | T |
| longitude | M | T | T | F | T |

## 4.4 Attribute definitions

### 4.4.1 Attribute properties

The following table defines the properties of attributes specified in the present document.

| Attribute Name | Documentation and Allowed Values | Properties |
| --- | --- | --- |
| numberOfFiles | Number of files in a file collection.allowedValues: NA | Type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| fileLocation | Location of the file incl. the file transfer protocol, and the file name for the case the file content cannot be retrieved by reading the "fileContent" attribute.The allowed file transfer protocols are:- sftp- ftpes- httpsExamples:"sftp://companyA.com/datastore/fileName.xml","https://companyA.com/ManagedElement=1/Files=1/File=1allowedValues: NA | Type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| fileCompression | Name of the algorithm used for compressing the file. An empty or absent "fileCompression" parameter indicates the file is not compressed. The MnS producer selects the compression algorithm. It is encouraged to use popular algorithms such as GZIP.allowedValues: N/A | Type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| fileSize | Size of the file.Unit is byte.allowedValues: non-negative integers | Type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| fileDataType | Type of the management data stored in the file.AllowedValues:- "PERFORMANCE"- "TRACE"- "ANALYTICS"- "PROPRIETARY"The value "PERFORMANCE" refers to measurements and KPIs. | Type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| fileFormat | Identifier of the XML or ASN.1 schema (incl. its version) used to produce the file content.allowedValues: N/A | Type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| fileReadyTime | Date and time, when the file was closed (the last time) and made available on the MnS producer. The file content will not be changed anymore.allowedValues: N/A | Type: DateTimemultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| fileExpirationTime | Date and time after which the file may be deleted.allowedValues: N/A | Type: DateTimemultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| fileContent | File content.allowedValues: N/A | Type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| jobMonitor | Provides monitoring for the file download job. The data type of this attribute is the "ProcessMonitor" as defined in clause 4.3.43 with the specialisations defined in clause 4.3.44.1.allowedValues: N/A | Type: JobMonitormultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| cancelJob | Setting this attribute to "TRUE" cancels the file download job. As specified in the definition of "ProcessMonitor", cancellation is possible in the "NOT\_STARTED" and "RUNNING" state. Setting the attribute to "FALSE" has no observable result.allowedValues: TRUE, FALSE | Type: ENUMmultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: FALSEisNullable: False |
| FileDownloadJob.jobMonitor.resultStateInfo | Provides the following specialisation for the "resultStateInfo" attribute of the "ProcessMonitor" data type for the "FileDownloadJob".In the event the file download fails, and the "status" is equal to "FAILED", it provides the reason for the failure.allowedValues for "status" = "FAILED": - NULL - UNKNOWN - NO\_STORAGE - LOW\_MEMORY - NO\_CONNECTION\_TO\_REMOTE\_SERVER - FILE\_NOT\_AVAILABLE - DNS\_CANNOT\_BE\_RESOLVED - TIMER\_EXPIRED - OTHERThe allowed values for "FINISHED" or "CANCELLED" are vendor specific. | Type: Stringmultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| heartbeatNtfPeriod | Periodicity of the heartbeat notification emission. The value of zero has the special meaning of stopping the heartbeat notification emission.Unit is in seconds.AllowedValues: non-negative integers | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: 0isNullable: False |
| triggerHeartbeatNtf | Setting this attribute to TRUE triggers an immediate additional heartbeat notification emission. Setting the value to FALSE has no observable result.The periodicity of notifyHeartbeat emission is not changed.AllowedValues: TRUE, FALSE | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FALSE isNullable: False |
| notificationRecipientAddress | Address of the notification recipient.allowedValues: N/A | type: String multiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| notificationTypes | Notification types of notifications that are candidates for being forwarding to the notification recipient. If this attribute is absent, notifications of all types are candidates for being forwarding to the notification recipient.If the notificationFilter attribute is absent, all candidate notifications are forwarded to the notification recipient, otherwise the candidate notifications are discriminated by the filter specified by the notificationFilter attribute.Below is a list of notificationType values that are defined in 3GPP specifications. If the notificationType itself is supported by the system, it shall be supported in the NtfSubscriptionControl.notificationTypes attribute as well. Other notificationTypes defined by SDOs or enterprises may also be supported.AllowedValues: - notifyMOICreation- notifyMOIDeletion- notifyMOIAttributeValueChanges- notifyMOIChanges- notifyEvent- notifyNewAlarm- notifyChangedAlarm- notifyAckStateChanged- notifyComments- notifyCorrelatedNotificationChanged- notifyChangedAlarmGeneral- notifyClearedAlarm- notifyAlarmListRebuilt- notifyPotentialFaultyAlarmList- notifyFileReady- notifyFilePreparationError- notifyThresholdCrossing | type: ENUMmultiplicity: \*isOrdered: FalseisUnique: TruedefaultValue: NoneisNullable: False |
| notificationFilter | Filter to be applied to candidate notifications identified by the notificationTypes attribute. Only notifications that pass the filter criteria are forwarded to the notification recipient. All other notifications are discarded.The filter can be applied to any field of a notification.allowedValues: N/A | type: String multiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| scope | Scopes the managed object instances included in the notification subscription. If this attribute is absent, all objects below and including the base object are scoped.allowedValues: N/A | type: Scopemultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| scopeType | If the optional scopeLevel attribute is not supported or absent, allowed values of scopeType are BASE\_ONLY and BASE\_ALL.The value BASE\_ONLY indicates only the base object is selected.The value BASE\_ALL indicates the base object and all of its subordinate objects (incl. the leaf objects) are selected.If the scopeLevel attribute is supported and present, allowed values of scopeType are BASE\_NTH\_LEVEL and BASE\_SUBTREE.The value BASE\_NTH\_LEVEL indicates all objects on the level, which is specified by the scopeLevel attribute, below the base object are selected. The base object is at scopeLevel zero.The value BASE\_SUBTREE indicates the base object and all subordinate objects down to and including the objects on the level, which is specified by the scopeLevel attribute, are selected. The base object is at scopeLevel zero.allowedValues: N/A | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| scopeLevel | See definition of scopeType attribute.allowedValues: N/A | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| farEndEntity | The value of this attribute shall be the Distinguished Name of the far end network entity to which the reference point is related.As an example, with EP\_Iucs, if the instance of EP\_Iucs is contained by one RncFunction instance, the farEndEntity is the Distinguished Name of the MscServerFunction instance to which this Iucs reference point is related. allowedValues: N/A | type: DNmultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| linkType | This attribute defines the type of the link. allowedValues: Signalling, Bearer, OAM&P, Other or multiple combinations of this type. | type: Stringmultiplicity: 0..\*isOrdered: FalseisUnique: TruedefaultValue: None isNullable: False |
| locationName | The physical location of this entity (e.g. an address). allowedValues: N/A | type: Stringmultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| monitorGranularityPeriod | Granularity period used to monitor measurements for threshold crossings. The period is defined in seconds.See Note 5allowedValues: Integer with a minimum value of 1 | type: Integermultiplicity: 1isOrdered: N/AisUnique: TruedefaultValue: None isNullable: False |
| monitorGranularityPeriods | Granularity periods supported for the monitoring of associated measurement types for thresholds. The period is defined in seconds.allowedValues: Integer with a minimum value of 1 | type: Integermultiplicity: \*isOrdered: FalseisUnique: TruedefaultValue: NoneisNullable: False |
| thresholdInfoList | List of threshold infos. | type: ThresholdInfomultiplicity: 1..\*isOrdered: FalseisUnique: TruedefaultValue: NoneisNullable: False |
| thresholdValue | Value against which the monitored performance metric is compared at a threshold level in case the hysteresis is zero.allowedValues: float or integer | type: Unionmultiplicity: 1isOrdered: NAisUnique: NAdefaultValue: NoneisNullable: False |
| hysteresis | Hysteresis of a threshold. If this attribute is present the monitored performance metric is not compared against the threshold value as specified by the thresholdValue attribute but against a high and low threshold value given byhighThresholdValue- = thresholdValue + hysteresislowThresholdValue = thresholdValue - hysteresisWhen going up, the threshold is triggered when the performance metric reaches or crosses the high threshold value. When going down, the threshold is triggered when the performance metric reaches or crosses the low threshold value.A hysteresis may be present only when the monitored performance metric is not of type counter that can go up only. If present for a performance metric of type counter, it shall be ignored.allowedValues: non-negative float or integer | type: Unionmultiplicity: 0..1isOrdered: NAisUnique: NAdefaultValue: NoneisNullable: False |
| thresholdDirection | Direction of a threshold indicating the direction for which a threshold crossing triggers a threshold.When the threshold direction is configured to "UP", the associated treshold is triggered only when the performance metric value is going up upon reaching or crossing the threshold value. The treshold is not triggered, when the performance metric is going down upon reaching or crossing the threshold value.Vice versa, when the threshold direction is configured to "DOWN", the associated treshold is triggered only when the performance metric is going down upon reaching or crossing the threshold value. The treshold is not triggered, when the performance metric is going up upon reaching or crossing the threshold value.When the threshold direction is set to "UP\_AND\_DOWN" the treshold is active in both direcions.In case a threshold with hysteresis is configured, the threshold direction attribute shall be set to "UP\_AND\_DOWN".allowedValues:- UP- DOWN- UP\_AND\_DOWN | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| objectClass | Class of a managed object instance.allowedValues: N/A | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| objectInstance | Managed object instance identified by its DN.allowedValues: N/A | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| objectInstances | List of managed object instances. Each object instance is identified by its DN.allowedValues: N/A | type: Dnmultiplicity: \*isOrdered: FalseisUnique: TruedefaultValue: NoneisNullable: False |
| peeParametersList | This attribute contains the parameter list for the control and monitoring of power, energy and environmental parameters of ManagedFunction instance(s). This list contains the following parameters:- siteIdentification- siteLatitude (optional)- siteLongitude (optional)- siteAltitude (optional)- siteDescription - equipmentType- environmentType- powerInterface siteIdentification: The identification of the site where the ManagedFunction resides.allowedValues: N/AsiteLatitude: The latitude of the site where the ManagedFunction instance resides, based on World Geodetic System (1984 version) global reference frame (WGS 84). Positive values correspond to the northern hemisphere. This attribute is optional for BTSFunction, RNCFunction , GNBDUFunction and NRSectorCarrier instance(s).allowedValues: -90.0000 to +90.0000siteLongitude: The longitude of the site where the ManagedFunction instance resides, based on World Geodetic System (1984 version) global reference frame (WGS 84). Positive values correspond to degrees east of 0 degrees longitude. This attribute is optional for BTSFunction, RNCFunction, GNBDUFunction and NRSectorCarrier instance(s).allowedValues: -180.0000 to +180.0000siteAltitude: The altitude of the site where the ManagedFunction instance resides, in unit of meter. This attribute is optional for BTSFunction, RNCFunction, GNBDUFunction and NRSectorCarrier instance(s).siteDescription: An operator defined description of the site where the ManagedFunction instance resides.allowedValues: N/A equipmentType: The type of equipment where the managedFunction instance resides. allowedValues: see clause 4.4.1 of ETSI ES 202 336-12 [18].environmentType: The type of environment where the managedFunction instance resides. allowedValues: see clause 4.4.1 of ETSI ES 202 336-12 [18].powerInterface: The type of power.allowedValues: see clause 4.4.1 of ETSI ES 202 336-12 [18]. | type: Stringmultiplicity: 0..\*isOrdered: FalseisUnique: TruedefaultValue: NoneisNullable: True |
| priorityLabel | This is a label that consumer would assign a value on a concrete instance of the managed object. The management system takes the value of this attribute into account. The effect of this attribute value to the subject managed entity is not standardized | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| protocolVersion | Versions(s) and additional descriptive information for the protocol(s) used for the associated communication link. Syntax and semantic is not specified.allowedValues: N/A | type: Stringmultiplicity: \*isOrdered: FalseisUnique: TruedefaultValue: NoneisNullable: False |
| setOfMcc | Set of Mobile Country Code (MCC). The MCC uniquely identifies the country of domicile of the mobile subscriber. MCC is part of the IMSI (TS 23.003 [5])This list contains all the MCC values in subordinate object instances to this SubNetwork instance.allowedValues: See clause 2.3 of TS 23.003 [5] for MCC allocation principles. | type: Integermultiplicity: 1..\*isOrdered: FalseisUnique: TruedefaultValue: NoneisNullable: False |
| swVersion | The software version of the ManagementNode or ManagedElement (this is used for determining which version of the vendor specific information is valid for the ManagementNode or ManagedElement).allowedValues: N/A | type: Stringmultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| systemDN | Distinguished Name (DN) of a IRPAgent or a MnSAgent.allowedValues: N/A | type: DNmultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| userDefinedState | An operator defined state for operator specific usage.allowedValues: N/A | type: Stringmultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| userLabel | A user-friendly (and user assignable) name of this object.allowedValues: N/A | type: Stringmultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| vendorName | The name of the vendor.allowedValues: N/A | type: Stringmultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| vnfParametersList | This attribute contains the parameter set of the VNF instance(s) corresponding to an NE. Each entry in the list contains:- vnfInstanceId- vnfdId (optional)- flavourId (optional) - autoScalable (optional)vnfInstanceId: VNF instance identifier (vnfInstanceId, see section 9.4.2 of [16] and section B2.4.2.1.2.3 of [17]).See Note 1.vnfdId: Identifier of the VNFD on which the VNF instance is based, see section 9.4.2 of [16]. This attribute is optional.Note: the value of this attribute is identical to that of the same attribute in clause 9.4.2 of ETSI GS NFV-IFA 008 [16].flavourId: Identifier of the VNF Deployment Flavour applied to this VNF instance, see section 9.4.3 of [16]. This attribute is optional.Note: the value of this attribute is identical to that of the same attribute in clause 9.4.3 of ETSI GS NFV-IFA 008 [16].autoScalable: Indicator of whether the auto-scaling of this VNF instance is enabled or disabled. The type is Boolean. This attribute is optional.See Note2.The presence of this attribute indicates that the ManagedFunction represented by the MOI is a virtualized function. See Note 3.allowedValues: N/AA string length of zero for vnfInstanceId means the VNF instance(s) corresponding to the MOI does not exist (e.g. has not been instantiated yet, has already been terminated). | type: Stringmultiplicity: \*isOrdered: FalseisUnique: TruedefaultValue: NoneisNullable: True |
| vsData | Vendor specific attributes of the type vsDataType. The attribute definitions including constraints (value ranges, data types, etc.) are specified in a vendor specific data format file. allowedValues: -- | type: --multiplicity: --isOrdered: --isUnique: --defaultValue: --isNullable: False |
| vsDataFormatVersion | Name of the data format file, including version.allowedValues: N/A | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| vsDataType | Type of vendor specific data contained by this instance, e.g. relation specific algorithm parameters, cell specific parameters for power control or re-selection or a timer. The type itself is also vendor specific.allowedValues: N/A | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| supportedPerfMetricGroups | A set of performance metric groups. When this attribute is contained in a managed object it may define performance metrics for this object and all descendant objects.allowedValues: N/A | type: SupportedPerfMetricGroupmultiplicity: \*isOrdered: FalseisUnique: TruedefaultValue: NoneisNullable: False |
| performanceMetrics | List of performance metrics.Performance metrics include measurements defined in TS 28.552 [20] and KPIs defined in TS 28.554 [28]. Performance metrics can also be specified by other SDOs, or be vendor specific. Performance metrics are identified with their names.For measurements defined in TS 28.552 [20] the name is constructed as follows:- "family.measurementName.subcounter" for measurement types with subcounters- "family.measurementName" for measurement types without subcounters- "family" for measurement familiesFor KPIs defined in TS 28.554 [28] the name is defined in the KPI definitions template as the component designated with e).A name can also identify a vendor specific performance metric or a group of vendor specific performance metrics.allowedValues: N/A | type: Stringmultiplicity: \*isOrdered: FalseisUnique: TruedefaultValue: NoneisNullable: False |
| supportedTraceMetrics | List of trace metrics. When this attribute is contained in a managed object it defines the trace metrics supported for this object and all descendant objects.Trace metrics include trace messages, MDT measurements (Immediate MDT, Logged MDT, Logged MBSFN MDT), RLF and RCEF reports, see TS 32.422 [30]. Trace metrics are identified with their metric identifier. The metric identifier is constructed as defined in clause 10 of TS 32.422 [30].allowedValues: N/A | type: Stringmultiplicity: \*isOrdered: FalseisUnique: TruedefaultValue: NoneallowedValues: N/AisNullable: False |
| rootObjectInstances | List of object instances. Each object instance is identified by its DN and designates the root of a subtree that contains the root object and all descendant objects. | type: Dnmultiplicity: \*isOrdered: FalseisUnique: TruedefaultValue: NoneisNullable: False |
| reportingMethods | List of reporting methods for performance metricsallowedValues:  - "FILE\_BASED\_LOC\_SET\_BY\_PRODUCER", - "FILE\_BASED\_LOC\_SET\_BY\_CONSUMER", - "STREAM\_BASED" | type: ENUMmultiplicity: \*isOrdered: FalseisUnique: TruedefaultValue: NoneisNullable: False |
| nFServiceType | The parameter defines the type of the managed NF service instanceallowedValues: See clause 7.2 of TS 23.501[22] | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| operations | This parameter defines set of operations supported by the managed NF service instance.allowedValues: See TS 23.502[23] for supporting operations | type: Operationmultiplicity: 1..\*isOrdered: FalseisUnique: TruedefaultValue: NoneisNullable: False |
| Operation.name | This parameter defines the name of the operation of the managed NF service instance.allowedValues: N/A | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: True |
| allowedNFTypes | This parameter identifies the type of network functions allowed to access the operation of the managed NF service instance.allowedValues: See TS 23.501[22] for NF types | type: ENUMmultiplicity: 1..\*isOrdered: FalseisUnique: TruedefaultValue: NoneisNullable: False |
| operationSemantics | This paramerter identifies the semantics type of the operation. See TS 23.502[23]allowedValues: “Request/Response”, “Subscribe/Notify”.  | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| sAP | This parameter specifies the service access point of the managed NF service instance.allowedValues: N/A | type: SAPmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| host | This parameter specifies the host address of the managed NF service instance. It can be FQDN (See TS 23.003 [5]) or an IPv4 address (See RFC 791 [24]) or an IPv6 address (See RFC 2373 [25]).allowedValues: N/A | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| port | This parameter specifies the transport port of the managed NF service instance.allowedValues: 1 - 65535 | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| usageState | Usage state of a managed object instance. It describes whether the resource is actively in use at a specific instant, and if so, whether or not it has spare capacity for additional users at that instant. allowedValues: "IDLE", "ACTIVE", "BUSY".The meaning of these values is as defined in 3GPP TS 28.625 [21] and ITU-T X.731 [19]. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| registrationState | This parameter defines the registration status of the managed NF service instance.allowedValues: "Registered", "Deregistered". | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: DeregisteredisNullable: False |
| jobRef | Object instance of the "PerfMetricJob" or "TraceJob" that produced the file.allowedValues: NA | Type: Dnmultiplicity: 0..\*isOrdered: FalseisUnique: TruedefaultValue: NoneisNullable: False |
| jobId | Identifier of a PerfMetricJob job or a TraceJob. | type: Stringmultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| granularityPeriod | Granularity period used to produce measurements. The period is defined in seconds.See Note 4.allowedValues: Integer with a minimum value of 1 | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| granularityPeriods | Granularity periods supported for the production of associated measurement types. The period is defined in seconds.allowedValues: Integer with a minimum value of 1 | type: Integermultiplicity: \*isOrdered: False isUnique: TruedefaultValue: NoneisNullable: False |
| reportingCtrl | Selecting the reporting method and defining associated control parameters. | type: ReportingCtrlmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| fileReportingPeriod | For the file-based reporting method this is the time window during which collected measurements are stored into the same file before the file is closed and a new file is opened. The period is defined in minutes.allowedValues: Multiples of granularityPeriod | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| linkToCreatsSubscriptions | Link to the parent object below which "NtfSubscriptionControl" instances can be created. | type: Linkmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| \_linkToFiles | Link to a "Files" object.allowedValues: N/A | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| fileLocation | The location of a file. allowedValues: File URI [See RFC 8089 [49]). | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: True |
| streamTarget | The stream target for the stream-based reporting method.allowedValues: N/A | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: True |
| administrativeState | Administrative state of a managed object instance. The administrative state describes the permission to use or prohibition against using the object instance. The adminstrative state is set by the MnS consumer.allowedValues: LOCKED, UNLOCKED.  | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: LOCKEDisNullable: False |
| operationalState | Operational state of manged object instance. The operational state describes if an object instance is operable ("ENABLED") or inoperable ("DISABLED"). This state is set by the object instance or the MnS producer and is hence READ-ONLY.allowedValues: ENABLED, DISABLED. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: DISABLEDisNullable: False |
| alarmRecords | List of alarm recordsallowedValues: N/A | type: AlarmRecordmultiplicity: \*isOrdered: FalseisUnique: Truedefault value: NoneisNullable: True |
| numOfAlarmRecords | Number of alarm records in the AlarmList.allowedValues: 0 to x where x is vendor specific. | type: integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| lastModification | Time an alarm record was modified the last timeallowedValues: N/A | type: DateTimemultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| tjJobType | It specifies the MDT mode and it specifies also whether the TraceJob represents only MDT, Logged MBSFN MDT, Trace or a combined Trace and MDT job. The attribute is applicable for Trace, MDT, RCEF and RLF reporting.See the clause 5.9a of TS 32.422 [30] for additional details on the allowed values. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: TRACE\_ONLYisNullable: False |
| tjListOfInterfaces | It specifies the interfaces that need to be traced.The attribute is applicable only for Trace. In case this attribute is not used, it carries a null semantic.See the clause 5.5 of TS 32.422 [30] for additional details on the allowed values. | type: ENUMmultiplicity: 1..\*isOrdered: FalseisUnique: TruedefaultValue: NoneisNullable: True |
| tjListOfNeTypes | It specifies the network element types where the trace should be activated. The attribute is applicable only for Trace with Signalling Based Trace activation. In case this attribute is not used, it carries a null semantic.See the clause 5.4 of TS 32.422 [30] for additional details on the allowed values. | type: ENUMmultiplicity: 1..\*isOrdered: FalseisUnique: TruedefaultValue: NoneisNullable: True |
| tjPLMNTarget | It specifies which PLMN that the subscriber of the session to be recorded uses as selected PLMN. PLMN Target might differ from the PLMN specified in the Trace Reference.See the clause 5.9b of 3GPP TS 32.422 [30] for additional details on the allowed values. | type: PlmnIdmultiplicity: 1isOrdered: N/AisUnique: TruedefaultValue: None isNullable: True |
| tjStreamingTraceConsumerURI | It specifies the Uniform Resource Identifier (URI) of the Streaming Trace data reporting MnS consumer (a.k.a. streaming target).See the clause 5.9 c of TS 32.422 [30] for additional details on the allowed values. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: True |
| tjTraceCollectionEntityAddress | It specifies the address of the Trace Collection Entity when the attribute tjTraceReportingFormat is configured for the file-based reporting. The attribute is applicable for both Trace and MDT.See the clause 5.9 of TS 32.422 [30] for additional details on the allowed values. | type: IpAddressmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: True |
| tjTraceDepth | It specifies the trace depth. The attribute is applicable only for Trace. In case this attribute is not used, it carries a null semantic.See the clause 5.3 of 3GPP TS 32.422 [30] for additional details on the allowed values. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: MAXIMUM isNullable: True |
| tjTraceReference | A globally unique identifier, which uniquely identifies the Trace Session that is created by the TraceJob. In case of shared network, it is the MCC and MNC of the Participating Operator that request the trace session that shall be provided.The attribute is applicable for both Trace and MDT.See the clause 5.6 of 3GPP TS 32.422 [30] for additional details on the allowed values. | type: TraceReferencemultiplicity: 1isOrdered: TrueisUnique: TruedefaultValue: None isNullable: False |
| tjTraceRecordSessionReference | An identifier, which identifies the Trace Recording Session. The attribute is applicable for both Trace and MDT.See the clause 5.7 of 3GPP TS 32.422 [30] for additional details on the allowed values. | type: Stringmultiplicity: 1isOrdered: TrueisUnique: TruedefaultValue: None isNullable: False |
| tjTraceReportingFormat | It specifies the trace reporting format - streaming trace reporting or file-based trace reporting.See the clause 5.11 of 3GPP TS 32.422 [30] for additional details on the allowed values.AllowedValues: FILE-BASED, STREAMING | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FILE-BASED isNullable: False |
| tjTraceTarget | It specifies the target object of the Trace and MDT. The attribute is applicable for both Trace and MDT. This attribute includes the ID type of the target as an enumeration and the ID value(s).The tjTraceTarget shall be "PUBLIC\_ID" in case of a Management Based Activation is done to an SCSCFFunction (Serving Call Session Control Function) or PCSCFFunction (Proxy Call Session Control Function) (TS 28.705[44]). The tjTraceTarget shall be "UTRAN\_CELL" only in case of the UTRAN cell traffic trace function. The tjTraceTarget shall be "E-UTRAN\_CELL" only in case of E-UTRAN cell traffic trace function.The tjTraceTarget shall be "NG-RAN\_CELL" only in case of NR cell traffic trace function.The tjTraceTarget shall be either "IMSI", "IMEI" or "IMEISV" if the Trace Session is activated to any of the following ManagedEntity(ies):- HSSFunction (Home Subscriber Server) (TS 28.705 [44])- MscServerFunction (Mobile Switching Centre Server) (TS 28.702 [45])- SgsnFunction (Serving GPRS Support Node) (TS 28.702[45])- GgsnFunction (Gateway GPRS Support Node) (TS 28.702[45])- BmscFunction (Broadcast Multicast Service Centre) (TS 28.702[45])- RncFunction (Radio Network Controller) (TS 28.652[46])- MmeFunction (Mobility Management Entity) (TS 28.708[47])- ServingGWFunction (Serving Gateway) (TS 28.708[47])- PGWFunction (PDN Gateway) (TS 28.708[47]).The tjTraceTarget shall be either “SUPI” or “IMEISV” if the Trace Session is activated to any of the following ManagedEntity(ies) (TS 28.541[48]):- AFFunction- AMFFunction- AUSFunction- NEFFunction- NRFFunction- NSSFFunction- PCFFunction- SMFFunction- UPFFunction- UDMFunctionIn case of signalling based MDT, the tjTraceTarget attribute shall be able to carry "PUBLIC\_ID", "IMSI", "IMEI", "IMEISV)" or "SUPI".In case of management based Immediate MDT, the tjTraceTarget attribute shall be null value.In case of management based Logged MDT, the tjTraceTarget attribute shall carry an "eNB" or a "gNB" or an "RNC". The Logged MDT should be initiated on the specified eNB/gNB/RNC in tjTraceTarget. In case of RLF reporting, or RCEF reporting, the tjTraceTarget attribute shall be null value. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: No isNullable: True |
| tjTriggeringEvent | It specifies the triggering event parameter of the trace session. The attribute is applicable only for Trace. In case this attribute is not used, it carries a null semantic.See the clause 5.1 of 3GPP TS 32.422 [30] for additional details on the allowed values. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: True |
| tjMDTAnonymizationOfData | It specifies the level of anonymization for management based MDT.See the clause 5.10.12 of 3GPP TS 32.422 [30] for additional details on the allowed values. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NO\_IDENTITY isNullable: True |
| tjMDTAreaConfigurationForNeighCell | It specifies the area for which UE is requested to perform measurement logging for neighbour cells which have list of frequencies. If it is not configured, the UE shall perform measurement logging for all the neighbour cells.Applicable only to NR Logged MDT.See the clause 5.10.26 of 3GPP TS 32.422 [30] for additional details on the allowed values. | type: AreaConfigmultiplicity: 1..\*isOrdered: FalseisUnique: TruedefaultValue: None isNullable: True |
| tjMDTAreaScope | It specifies MDT area scope when activates an MDT job. For RLF and RCEF reporting it specifies the eNB/gNB or list of eNBs/gNBs where the RLF or RCEF reports should be collected.List of cells/TA/LA/RA for signalling based MDT or management based Logged MDT.List of cells for management based Immediate MDT.Cell, TA, LA, RA are mutually exclusive.One or list of eNBs/gNBs for RLF and RCEF reportingSee the clause 5.10.2 of 3GPP TS 32.422 [30] for additional details on the allowed values. | type: AreaScopemultiplicity: 1..\*isOrdered: FalseisUnique: TruedefaultValue: None isNullable: True |
| tjMDTCollectionPeriodRrmLte | It specifies the collection period for collecting RRM configured measurement samples for M3 in LTE. The attribute is applicable only for Immediate MDT. In case this attribute is not used, it carries a null semantic.See the clause 5.10.20 of 3GPP TS 32.422 [30] for additional details on the allowed values. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: True |
| tjMDTCollectionPeriodRrmUmts | It specifies the collection period for collecting RRM configured measurement samples for M3, M4, M5 in UMTS. The attribute is applicable only for Immediate MDT. In case this attribute is not used, it carries a null semantic.See the clause 5.10.21 of 3GPP TS 32.422 [30] for additional details on the allowed values. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: True |
| tjMDTEventListForTriggeredMeasurement | It specifies event types for event triggered measurement in the case of logged NR MDT. Each trace session may configure at most one event. The UE shall perform logging of measurements only upon certain condition being fulfilled:- Out of coverage.- A2 event.See the clause 5.10.28 of 3GPP TS 32.422 [30] for additional details on the allowed values. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: True |
| tjMDTEventThreshold | It specifies the threshold which should trigger the reporting in case A2 event reporting in LTE and NR or 1F/1l event in UMTS. The attribute is applicable only for Immediate MDT and when tjMDTReportingTrigger is configured for A2 event in LTE and NR or 1F event or 1l event in UMTS. In case this attribute is not used, it carries a null semantic.See the clauses 5.10.7 and 5.10.7a of 3GPP TS 32.422 [30] for additional details on the allowed values. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: True |
| tjMDTListOfMeasurements | It specifies the UE measurements that shall be collected in an Immediate MDT job. The attribute is applicable only for Immediate MDT. In case this attribute is not used, it carries a null semantic.See the clause 5.10.3 of 3GPP TS 32.422 [30] for additional details on the allowed values. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: True |
| tjMDTLoggingDuration | It specifies how long the MDT configuration is valid at the UE in case of Logged MDT. The attribute is applicable only for Logged MDT and Logged MBSFN MDT. In case this attribute is not used, it carries a null semantic.See the clause 5.10.9 of 3GPP TS 32.422 [30] for additional details on the allowed values. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: True |
| tjMDTLoggingInterval | It specifies the periodicty for Logged MDT. The attribute is applicable only for Logged MDT and Logged MBSFN MDT. In case this attribute is not Sused, it carries a null semantic.See the clause 5.10.8 of 3GPP TS 32.422 [30] for additional details on the allowed values. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: True |
| tjMDTLoggingEventThreshold | It specifies the threshold which should trigger the reporting in case of event based reporting of logged NR MDT. The attribute is applicable only for Logged MDT and when tjMDTReportType is configured for event triggered reporting and when tjMDTEventListForTriggeredMeasurement is configured for L1 event. In case this attribute is not used, it carries a null semantic.See the clause 5.10.36 of TS 32.422 [30] for additional details on the allowed values. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: True |
| tjMDTLoggedHysteresis | It specifies the hysteresis used within the entry and leave condition of the L1 event based reporting of logged NR MDT. The attribute is applicable only for Logged MDT, when tjMDTReportType is configured for event triggered reporting and when tjMDTEventListForTriggeredMeasurement is configured for L1 event. In case this attribute is not used, it carries a null semantic.See the clause 5.10.37 of TS 32.422 [30] for additional details on the allowed values. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: True |
| tjMDTLoggedTimeToTrigger | It specifies the threshold which should trigger the reporting in case of event based reporting of logged NR MDT. The attribute is applicable only for Logged MDT, when tjMDTReportType is configured for event triggered reporting and when tjMDTEventListForTriggeredMeasurement is configured for L1 event. In case this attribute is not used, it carries a null semantic.See the clauses 5.10.38 of TS 32.422 [30] for additional details on the allowed values. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: True |
| tjMDTMBSFNAreaList | The MBSFN Area consists of a MBSFN Area ID and Carrier Frequency (EARFCN). The target MBSFN area List can have up to 8 entries. This parameter is applicable only if the job type is Logged MBSFN MDT.See the clause 5.10.25 of TS 32.422 [30] for additional details on the allowed values. | type: MbsfnAreamultiplicity: 1..8isOrdered: FalseisUnique: TruedefaultValue: NoneisNullable: True |
| tjMDTMeasurementPeriodLTE | It specifies the collection period for the Data Volume (M4) and Scheduled IP throughput measurements (M5) for LTE MDT taken by the eNB. The attribute is applicable only for Immediate MDT. In case this attribute is not used, it carries a null semantic.See the clause 5.10.23 of TS 32.422 [30] for additional details on the allowed values. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: True |
| tjMDTCollectionPeriodM6Lte | It specifies the collection period for the Packet Delay measurement (M6) for MDT taken by the eNB. The attribute is applicable only for Immediate MDT. In case this attribute is not used, it carries a null semantic.See the clause 5.10.32 of TS 32.422 [30] for additional details on the allowed values. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: True |
| tjMDTCollectionPeriodM7Lte | It specifies the collection period for the Packet Loss Rate measurement (M7) for LTE MDT taken by the eNB. The attribute is applicable only for Immediate MDT. In case this attribute is not used, it carries a null semantic.See the clause 5.10.33 of TS 32.422 [30] for additional details on the allowed values. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: True |
| tjMDTMeasurementPeriodUMTS | It specifies the collection period for the Data Volume (M6) and Throughput measurements (M7) for UMTS MDT taken by RNC. The attribute is applicable only for Immediate MDT. In case this attribute is not used, it carries a null semantic.See the clause 5.10.22 of TS 32.422 [30] for additional details on the allowed values. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: True |
| tjMDTCollectionPeriodRrmNR | It specifies the collection period for collecting RRM configured measurement samples for M4, M5 in NR. The attribute is applicable only for Immediate MDT. In case this attribute is not used, it carries a null semantic.See the clause 5.10.30 of TS 32.422 [30] for additional details on the allowed values. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: True |
| tjMDTCollectionPeriodM6NR | It specifies the collection period for the Packet Delay measurement (M6) for NR MDT taken by the gNB. The attribute is applicable only for Immediate MDT. In case this attribute is not used, it carries a null semantic.See the clause 5.10.34 of TS 32.422 [30] for additional details on the allowed values. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: True |
| tjMDTCollectionPeriodM7NR | It specifies the collection period for the Packet Loss Rate measurement (M7) for NR MDT taken by the gNB. The attribute is applicable only for Immediate MDT. In case this attribute is not used, it carries a null semantic.See the clause 5.10.35 of TS 32.422 [30] for additional details on the allowed values. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: True |
| tjMDTBeamLevelMeasurement | This indicates whether the NR M1 beam level measurements shall be included or not. See the clause 5.10.40 of TS 32.422 [30] for additional details.The default value is "FALSE".allowedValues: TRUE, FALSE | type: Booleanmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: FALSE isNullable: False |
| tjMDTM4ThresholdUmts | It specifies the threshold which should trigger the reporting in case of event-triggered periodic reporting for M4 (UE power headroom measurement) in UMTS. In case this attribute is not used, it carries a null semantic.See the clause 5.10.39 of TS 32.422 [30] for additional details on the allowed values. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: True |
| tjMDTMeasurementQuantity | It specifies the measurements that are collected in an MDT job for a UMTS MDT configured for event triggered reporting.See the clause 5.10.15 of TS 32.422 [30] for additional details on the allowed values. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: True |
| tjMDTPLMNList | It indicates the PLMNs where measurement collection, status indication and log reporting are allowed.See the clause 5.10.24 of TS 32.422 [30] for additional details on the allowed values. | type: PlmnIdmultiplicity: 1..16isOrdered: FalseisUnique: TruedefaultValue: NoneisNullable: True |
| tjMDTPositioningMethod | It specifies what positioning method should be used in the MDT job.See the clause 5.10.19 of TS 32.422 [30] for additional details on the allowed values. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: True |
| tjMDTReportAmount | It specifies the number of measurement reports that shall be taken for periodic reporting while the UE is in connected. The attribute is applicable only for Immediate MDT and when tjMDTReportingTrigger is configured for periodical measurements. In case this attribute is not used, it carries a null semantic.See the clause 5.10.6 of TS 32.422 [30] for additional details on the allowed values. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: True |
| tjMDTReportingTrigger | It specifies whether periodic or event based measurements should be collected. The attribute is applicable only for Immediate MDT and when the tjMDTListOfMeasurements is configured for M1 (for UMTS, LTE and NR) or M2 (only for UMTS). In case this attribute is not used, it carries a null semantic.See the clause 5.10.4 of TS 32.422 [30] for additional details on the allowed values. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: True |
| tjMDTReportInterval | It specifies the interval between the periodical measurements that shall be taken when the UE is in connected mode. The attribute is applicable only for Immediate MDT and when tjMDTReportingTrigger is configured for periodical measurements. In case this attribute is not used, it carries a null semantic.See the clause 5.10.5 of TS 32.422 [30] for additional details on the allowed values. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: True |
| tjMDTReportType | It specifies report type for logged NR MDT as:- periodical.- event triggered.See the clause 5.10.27 of TS 32.422 [30] for additional details on the allowed values. | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: True |
| tjMDTSensorInformation | It specifies which sensor information shall be included in logged NR MDT and immediate NR MDT measurement if they are available. The following sensor measurement can be included or excluded for the UE: - Barometric pressure.- UE speed.- UE orientation.See the clause 5.10.29 of 3GPP TS 32.422 [30] for additional details on the allowed values. | type: ENUMmultiplicity: 1..\*isOrdered: FalseisUnique: TruedefaultValue: NoneisNullable: True |
| tjMDTTraceCollectionEntityID | It specifies the TCE Id which is sent to the UE in Logged MDT.See the clause 5.10.11 of 3GPP TS 32.422 [30] for additional details on the allowed values. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: True |
| mcc | Mobile Country CodeallowedValues: As defined by the data type | type: Mccmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| mnc | Mobile NetworkallowedValues: As defined by the data type | type: Mncmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| traceId | An identifier, which identifies the Trace (together with MCC and MNC). This is a 3 byte Octet String.See the clause 5.6 of 3GPP TS 32.422 [30] for additional details on the allowed values. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| freqInfo | It specifies the carrier frequency and bands used in a cell. | type: FreqInfomultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| arfcn | RF Reference Frequency as defined in TS 38.104 [35], clause 5.4.2.1. The frequency provided identifies the absolute frequency position of the reference resource block (Common RB 0) of the carrier. Its lowest subcarrier is also known as Point A.allowedValues: 0, 1, …,3279165 | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| freqBands | List of NR frequency operating bands. Primary NR Operating Band as defined in TS 38.104 [35], clause 5.4.2.3.The value 1 corresponds to n1, value 2 corresponds to NR operating band n2, etc.allowedValues: 1, 2, …,1024 | type: Integermultiplicity: 1..\*isOrdered: FalseisUnique: TruedefaultValue: NoneisNullable: False |
| pciList | List of neighbour cells subject for MDT scope.allowedValues: 0, 1, …,1007 | type: Integermultiplicity: 1..32isOrdered: FalseisUnique: TruedefaultValue: NoneisNullable: False |
| tac | Tracking Area CodeallowedValues: As defined by the data type | type: Tacmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| utraCellIdList | List of UTRAN cells identified by UTRAN CGIallowedValues: As defined by the data type | type: UtraCellIdmultiplicity: 1..32isOrdered: FalseisUnique: TruedefaultValue: NoneisNullable: False |
| eutraCellIdList | List of E-UTRAN cells identified by E-UTRAN-CGIallowedValues: As defined by the data type | type: EutraCellIdmultiplicity: 1..32isOrdered: FalseisUnique: TruedefaultValue: NoneisNullable: False |
| nrCellIdList | List of NR cells identified by NG-RAN CGIallowedValues: As defined by the data type | type: NrCellIdmultiplicity: 1..32isOrdered: FalseisUnique: TruedefaultValue: NoneisNullable: False |
| tacList | Tracking Area Code listallowedValues: As defined by the data type | type: Tacmultiplicity: 1..8isOrdered: FalseisUnique: TruedefaultValue: NoneisNullable: False |
| taiList | Tracking Area Identity listallowedValues: As defined by the data type | type: Taimultiplicity: 1..8isOrdered: FalseisUnique: TruedefaultValue: NoneisNullable: False |
| mbsfnAreaId | MBSFN Area IdentifierAllowedValues: 1, 2, … | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| earfcn | Carrier Frequency AllowedValues: 1, 2, … | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| mnsLabel | Human-readable name of management service. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| mnsType | Type of management service.allowedValues: ProvMnS, FaultSupervisionMnS, StreamingDataReportingMnS, FileDataReportingMnS | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| mnsVersion | Version of management service. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| mnsAddress | Addressing information for Management Service operations. | type: Stringmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| ProcessMonitor.id | Id of the process. It is unique within a single multivalue attribute of type ProcessMonitor. | Type: Stringmultiplicity: 1isOrdered: N/AisUnique: TruedefaultValue: NoneisNullable: False |
| ProcessMonitor.status | This attribute represents the status of the associated process, whether it fails, succeeds etc. It does not represent the returned values of a successfully finished process.allowedValues:- NOT\_STARTED- RUNNING- CANCELLING- FINISHED- FAILED- PARTIALLY\_FAILED- CANCELLED | Type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| ProcessMonitor.progressPercentage | Progress of the process as percentage.Allowed values: integer between 0 and 100 | Type: Integermultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: False |
| ProcessMonitor.progressStateInfo | Additional textual qualification of the states "NOT\_STARTED", "CANCELLING" and "RUNNING".For specific processes, specific well-defined strings (e.g. string patterns or enums) may be defined as a specialisation.allowedValues: N/A | Type: Stringmultiplicity: 0..\*isOrdered: TrueisUnique: FalsedefaultValue: NoneisNullable: False |
| ProcessMonitor.resultStateInfo | Additional textual qualification of the states "FINISHED", "FAILED", "PARTIALLY\_FAILED and "CANCELLED". For example, in the "FAILED" or "PARTIALLY\_FAILED" state this attribute may be used to provide error reasons.This attribute shall not be used to make the outcome of the process available for retrieval, if any. For this purpose, dedicated attributes shall be specified when specifying the representation of a specific process.For specific processes, specific well-defined strings (e.g. string patterns or enums) may be defined as a specialisation.allowedValues: N/A | Type: Stringmultiplicity: 0..1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| ProcessMonitor.startTime | Start time of the associated process, i.e. the time when the status changed from "NOT\_STARTED" to "RUNNING".allowedValues: N/A | Type: DateTimemultiplicity: 0.. 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| ProcessMonitor.endTime | Date and time when status changed to SUCCESS, CANCELLED, FAILED or PARTIALLY\_FAILED. If the time is in the future, it is the estimated time the process will end.allowedValues: N/A | Type: DateTimemultiplicity: 0.. 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| ProcessMonitor.timer | Time until the associated process is automatically cancelled. If set, the system decreases the timer with time. When it reaches zero the cancellation of the associated process is initiated by the MnS\_Producer. If not set, there is no time limit for the process.Once the timer is set, the consumer can not change it anymore. If the consumer has not set the timer the MnS Producer may set it.Unit is minutes.allowedValues: Positive integers | Type: Integermultiplicity: 0.. 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| mnsScope | This attribute list contains the DNs of the managed object instances that can be accessed using the Management Service. If a complete SubNetwork can be accessed using the Management Service, this attribute may contain the DN of the SubNetwork instead of the DNs of the individual managed entities within the SubNetwork. | type: DNmultiplicity: 1..\*isOrdered: FalseisUnique: TruedefaultValue: NoneisNullable: False |
| managementData | This attribute defines the list of management data that are requested.  | Type: ManagementDatamultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| mgtDataCategory | This attribute defines the management data that are requested. Allowed values for data category are COVERAGE, CAPACITY, ENERGY\_EFFICIENCY, MOBILITY, ACCESSIBILITY. The data categories will map to certain measurement families defined in TS 28.552 [2], see below. In addition to the below mappings, MnS producer may map the provided categories to any additional proprietary management data, as appropriate. The COVERAGE category will map to measurement families of MR (measurements related to Measurement Report) and L1M (measurements related to Layer 1 Measurement). The CAPACITY category will map to measurement family RRU (measurements related to Radio Resource Utilization). The ENERGY\_EFFICIENCY category will map to measurement family PEE (measurements related to Power, Energy and Environment). The MOBILITY category will map to measurement family MM (measurements related to Mobility Management). The ACCESSIBILITY category will map to measurement family CE (measurements related to Connection Establishment). | type: ENUMmultiplicity: 1..\*isOrdered: FalseisUnique: TruedefaultValue: NoneisNullable: True |
| mgtDataName | The list may include metrics or set of metrics defined in TS 28.552 [20], TS 28.554 [28] and TS 32.422 [30]. The metrics are identified with their names/identifiers. For performance measurements defined in TS 28.552 [20] the name is constructed as follows:- "family.measurementName.subcounter" for measurement types with subcounters- "family.measurementName" for measurement types without subcounters- "family" for measurement familiesFor KPIs defined in TS 28.554 [28] the name is defined according to the KPI definitions template as the component designated with a).For trace metrics (including trace messages, MDT measurements (Immediate MDT, Logged MDT, Logged MBSFN MDT), RLF and RCEF reports) defined in TS 32.422 [30], the name (metric identifier) is defined in clause 10 of TS 32.422 [30]. | type: stringmultiplicity: 1..\*isOrdered: FalseisUnique: TruedefaultValue: NoneisNullable: True |
| targetNodeFilter | Set of information to target the Object Instance to collect the measurements from. | type: NodeFiltermultiplicity: 1..\*isOrdered: N/AisUnique: N/AdefaultValue: NoisNullable: True |
| areaOfInterest | It specifies a location(s) from where the management data shall be collected. It is defined in terms of TAI(s). | type: Taimultiplicity: 1..\*isOrdered: N/AisUnique: N/AdefaultValue: NoisNullable: True |
| geoAreaToCellMapping | It specifies the geographical area from where the management data shall be collected and the mapping to cells. allowedValues: N/A | type: GeoAreaToCellMappingmultiplicity: 1..\*isOrdered: FalseisUnique: TruedefaultValue: None isNullable: True |
| convexGeoPolygon | It specifies the geographical area with a convex polygon. The convex polygon is specified by its corners.allowedValues: N/A | type: GeoCoordinatemultiplicity: 3..\*isOrdered: FalseisUnique: TruedefaultValue: None isNullable: True |
| latitude | Latitude based on World Geodetic System (1984 version) global reference frame (WGS 84). Positive values correspond to the northern hemisphere.AllowedValues: -90.0000, …+90.0000 | type: floatmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| longitude | Longitude based on World Geodetic System (1984 version) global reference frame (WGS 84). Positive values correspond to degrees east of 0 degrees longitude.AllowedValues: -180.0000, … +180.0000 | type: floatmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: NoneisNullable: False |
| associationThreshold | It specifies the threshold of coverage area in percentage whether a cell belongs to the geographical area or not.If this attribute is absent, the location of the base station antenna determines whether a cell belongs to the geographical area or not.Allowed values: 1,…,100 | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: None isNullable: True |
| networkDomain | It specifies the network domain of the target node. This will also result in collecting appropriate management data from the nodes belonging to the specified domain.Allowed Values: CN, RAN | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: N/AisNullable: True |
| cpUpType | It specifies the traffic type of the target node. This will also result in collecting appropriate management data from the nodes handling the specified traffic (e.g AMF for CP and UPF for UP).Allowed Values: CP, UP | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: N/AisNullable: True |
| sst | It specifies the slice service type (SST) of which the slice subnet should be targeted. Please refer to [22]. | type: Integermultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: N/AisNullable: True |
| collectionTimeWindow | Collection time window for which the management data should be reported. | type: TimeWindowmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: N/AisNullable: True |
| startTime | It specifies the start of collection period | type: DateTimemultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: N/AisNullable: True |
| endTime | It specifies the end of collection period | type: DateTimemultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: N/AisNullable: True |
| dataScope | It specifies whether the required data is reported per S-NSSAI or per 5QI.Allowed Value: SNSSAI, 5QI | type: ENUMmultiplicity: 1isOrdered: N/AisUnique: N/AdefaultValue: N/AisNullable: True |
| NOTE 1: The value of this attribute is identical to that of the same attribute in clause 9.4.2 of ETSI GS NFV-IFA 008 [16].NOTE 2: The value of this attribute is identical to that of the attribute isAutoscaleEnabled included in vnfConfigurableProperty in clause 9.4.2 of ETSI GS NFV-IFA 008 [16].NOTE 3: The presence of the attribute vnfParametersList, whose vnfInstanceId with a string length of zero, in createMO operation can trigger the instantiation of the related VNF/VNFC instances.NOTE 4: The GP defines the measurement data production rate. The supported rates are dependent on the capacity of the producer involved (e.g. the processing power of the producer, the complexity of the measurement type involved etc) and therefore, it cannot be standardized for all producers involved. The supported GPs reflects the agreement between producer and the consumer involved.NOTE 5: The monitoring granularity period defines the measurements monitoring period. The supported monitoring periods are dependent on the capacity of the producer involved (e.g. the processing power of the producer, the complexity of the measurement type involved etc) and therefore, it cannot be standardized for all producers involved. The supported monitoring GPs reflect the agreement between producer and the consumer involved.NOTE 6: The supported threshold levels are dependent on the capacity of the producer involved (e.g. the processing power of the producer, number of measurements being measured by the producer at the time, the complexity of the measurement type involved etc) and therefore, it cannot be standardized for all producers involved. The supported levels can only reflect the negotiated agreement between producer and the consumer involved. |

### 4.4.2 Constraints

None

***End of changes***