**3GPP TSG-SA5 Meeting #145-e *S5-225352***

**Online, , 15th Aug 2022 - 24th Aug 2022**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **28.623** | **CR** | **draftCR** | **rev** | **-** | **Current version:** | **17.2.2** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Rel-18 draftCR TS 28.623 Report Amount for M4, M5, M6 and M7 measurements in LTE |
|  |  |
| ***Source to WG:*** | China Telecomunication Corp., Huawei, Nokia, Nokia Shanghai Bell |
| ***Source to TSG:*** | S5 |
|  |  |
| ***Work item code:*** | DUMMY |  | ***Date:*** | 2022-08-05 |
|  |  |  |  |  |
| ***Category:*** | **C** |  | ***Release:*** | Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | To support report amount for MDT, this contribution proposes to add report amount for M4, M5, M6 and M7 measurements in LTE. |
|  |  |
| ***Summary of change:*** | Add Report Amount for M4, M5, M6 and M7 measurements in LTE. |
|  |  |
| ***Consequences if not approved:*** | Cannot support report amount for Immediate MDT or combined Immediate MDT and Trace. |
|  |  |
| ***Clauses affected:*** | A.2.2.13, C.4.3 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** | **X** |  |  O&M Specifications | TS 32.422 draftCRTS 28.622 draftCR |
|  |  |
| ***Other comments:*** | Forge Link: <https://forge.3gpp.org/rep/sa5/MnS/-/edit/TS28.623_Rel-18_draftCR_Report_amount_for_M4_M5_M6_and_M7_measurement_in_LTE_yaml/>; [https://forge.3gpp.org/rep/sa5/MnS/-/edit/TS28.623\_Rel-18\_draftCR\_Report\_amount\_for\_M4\_M5\_M6\_and\_M7\_measurement\_in\_LTE\_yang/](https://forge.3gpp.org/rep/sa5/MnS/-/edit/TS28.623_Rel-18_draftCR_Report_amount_for_M4_M5_M6_and_M7_measurement_in_LTE_yaml/) |
|  |  |
| ***This CR's revision history:*** |  |

|  |
| --- |
| **Start of changes** |

### A.2.2.13 IOC TraceJob

Mapping from NRM IOC TraceJob attributes to SS equivalent MOC TraceJob attributes

| IS Attributes | SS Attributes | SS Type |
| --- | --- | --- |
| tjJobType | tjJobType | tjJobType-Type |
| tjListOfInterfaces | tjListOfInterfaces | tjListOfInterfaces-Type |
| tjListOfNeTypes | tjListOfNeTypes | tjListOfNeTypes-Type |
| tjPLMNTarget | tjPLMNTarget | tjPLMNTarget-Type |
| tjStreamingTraceConsumerURI | tjTraceConsumer | StreamingTraceConsumerURI-Type |
| tjTraceCollectionEntityAddress | tjTraceConsumer | TraceCollectionEntityAddress-Type |
| tjTraceDepth | tjTraceDepth | tjTraceDepth-Type |
| tjTraceReference | tjTraceReference | tjTraceReference-Type |
| tjTraceReportingFormat | tjTraceReportingFormat | tjTraceReportingFormat-Type |
| tjTraceTarget | tjTraceTarget | tjTraceTarget-Type |
| tjTriggeringEvent | tjTriggeringEvent | tjTriggeringEvent-Type |
| tjMDTAnonymizationOfData | tjMDTAnonymizationOfData | tjMDTAnonymizationOfData-Type |
| tjMDTAreaConfigurationForNeighCell | tjMDTAreaConfigurationForNeighCell | tjMDTAreaConfigurationForNeighCell-Type |
| tjMDTAreaScope | tjMDTAreaScope | tjMDTAreaScope-Type |
| tjMDTCollectionPeriodRrmLte | tjMDTCollectionPeriodRrmLte | tjMDTCollectionPeriodRrmLte-Type |
| tjMDTCollectionPeriodRrmUmts | tjMDTCollectionPeriodRrmUmts | tjMDTCollectionPeriodRrmUmts-Type |
| tjMDTCollectionPeriodRrmNR | tjMDTCollectionPeriodRrmNR | tjMDTCollectionPeriodRrmNR-Type |
| tjMDTEventListForTriggeredMeasurement | tjMDTEventListForTriggeredMeasurement | tjMDTEventListForTriggeredMeasurement-Type |
| tjMDTEventThreshold | tjMDTEventThreshold | tjMDTEventThreshold-Type |
| tjMDTListOfMeasurements | tjMDTListOfMeasurements | tjMDTListOfMeasurements-Type |
| tjMDTLoggingDuration | tjMDTLoggingDuration | tjMDTLoggingDuration-Type |
| tjMDTLoggingInterval | tjMDTLoggingInterval | tjMDTLoggingInterval-Type |
| tjMDTMBSFNAreaList | tjMDTMBSFNAreaList | tjMDTMBSFNAreaList-Type |
| tjMDTMeasurementPeriodLTE | tjMDTMeasurementPeriodLTE | tjMDTMeasurementPeriodLTE-Type |
| tjMDTMeasurementPeriodUMTS | tjMDTMeasurementPeriodUMTS | tjMDTMeasurementPeriodUMTS-Type |
| tjMDTMeasurementQuantity | tjMDTMeasurementQuantity | tjMDTMeasurementQuantity-Type |
| tjMDTPLMList | tjMDTPLMList | tjMDTPLMList-Type |
| tjMDTPositioningMethod | tjMDTPositioningMethod | tjMDTPositioningMethod-Type |
| tjMDTReportAmount | tjMDTReportAmount | tjMDTReportAmount-Type |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
| tjMDTreportAmountM1LTE | tjMDTreportAmountM1LTE | tjMDTreportAmountM1LTE-Type |
| tjMDTreportAmountM4LTE | tjMDTreportAmountM4LTE | tjMDTreportAmountM1LTE-Type |
| tjMDTreportAmountM5LTE | tjMDTreportAmountM5LTE | tjMDTreportAmountM1LTE-Type |
| tjMDTreportAmountM6LTE | tjMDTreportAmountM6LTE | tjMDTreportAmountM1LTE-Type |
| tjMDTreportAmountM7LTE | tjMDTreportAmountM7LTE | tjMDTreportAmountM1LTE-Type |
| tjMDTReportingTrigger | tjMDTReportingTrigger | tjMDTReportingTrigger-Type |
| tjMDTReportInterval | tjMDTReportInterval | tjMDTReportInterval-Type |
| tjMDTReportType | tjMDTReportType | tjMDTReportType-Type |
| tjMDTSensorInformation | tjMDTSensorInformation | tjMDTSensorInformation-Type |
| tjMDTTraceCollectionEntityID | tjMDTTraceCollectionEntityID | tjMDTTraceCollectionEntityID-Type |

|  |
| --- |
| **next change** |

## C.4.3 OpenAPI document "TS28623\_GenericNrm.yaml"

openapi: 3.0.1

info:

 title: Generic NRM

 version: 17.2.0

 description: >-

 OAS 3.0.1 definition of the Generic NRM

 © 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

externalDocs:

 description: 3GPP TS 28.623; Generic NRM

 url: http://www.3gpp.org/ftp/Specs/archive/28\_series/28.623/

paths: {}

components:

 schemas:

#-------- Definition of types-----------------------------------------------------

 RegistrationState:

 type: string

 enum:

 - REGISTERED

 - DEREGISTERED

 VnfParameter:

 type: object

 properties:

 vnfInstanceId:

 type: string

 vnfdId:

 type: string

 flavourId:

 type: string

 autoScalable:

 type: boolean

 PeeParameter:

 type: object

 properties:

 siteIdentification:

 type: string

 siteDescription:

 type: string

 siteLatitude:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/Latitude'

 siteLongitude:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/Longitude'

 siteAltitude:

 type: number

 format: float

 equipmentType:

 type: string

 environmentType:

 type: string

 powerInterface:

 type: string

 ThresholdInfo:

 type: object

 properties:

 thresholdDirection:

 type: string

 enum:

 - UP

 - DOWN

 - UP\_AND\_DOWN

 thresholdValue:

 oneOf:

 - type: integer

 - $ref: 'TS28623\_ComDefs.yaml#/components/schemas/Float'

 hysteresis:

 oneOf:

 - type: integer

 minimum: 0

 - type: number

 format: float

 minimum: 0

 Operation:

 type: object

 properties:

 name:

 type: string

 allowedNFTypes:

 $ref: '#/components/schemas/NFType'

 operationSemantics:

 $ref: '#/components/schemas/OperationSemantics'

 NFType:

 type: string

 description: ' NF name defined in TS 23.501'

 enum:

 - NRF

 - UDM

 - AMF

 - SMF

 - AUSF

 - NEF

 - PCF

 - SMSF

 - NSSF

 - UDR

 - LMF

 - GMLC

 - 5G\_EIR

 - SEPP

 - UPF

 - N3IWF

 - AF

 - UDSF

 - DN

 OperationSemantics:

 type: string

 enum:

 - REQUEST\_RESPONSE

 - SUBSCRIBE\_NOTIFY

 SAP:

 type: object

 properties:

 host:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/HostAddr'

 port:

 type: integer

 NFServiceType:

 type: string

 enum:

 - Namf\_Communication

 - Namf\_EventExposure

 - Namf\_MT

 - Namf\_Location

 - Nsmf\_PDUSession

 - Nsmf\_EventExposure

 - Others

 TransportProtocol:

 anyOf:

 - type: string

 enum:

 - TCP

 - type: string

 SupportedPerfMetricGroup:

 type: object

 properties:

 performanceMetrics:

 type: array

 items:

 type: string

 granularityPeriods:

 type: array

 items:

 type: integer

 minimum: 1

 reportingMethods:

 type: array

 items:

 type: string

 enum:

 - FILE\_BASED\_LOC\_SET\_BY\_PRODUCER

 - FILE\_BASED\_LOC\_SET\_BY\_CONSUMER

 - STREAM\_BASED

 monitorGranularityPeriods:

 type: array

 items:

 type: integer

 minimum: 1

 ReportingCtrl:

 oneOf:

 - type: object

 properties:

 fileReportingPeriod:

 type: integer

 - type: object

 properties:

 fileReportingPeriod:

 type: integer

 fileLocation:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/Uri'

 - type: object

 properties:

 streamTarget:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/Uri'

 Scope:

 type: object

 properties:

 scopeType:

 type: string

 enum:

 - BASE\_ONLY

 - BASE\_ALL

 - BASE\_NTH\_LEVEL

 - BASE\_SUBTREE

 scopeLevel:

 type: integer

 ProcessMonitor:

 description: >-

 This data type is the "ProcessMonitor" data type without specialisations.

 type: object

 properties:

 jobId:

 type: string

 status:

 type: string

 enum:

 - NOT\_STARTED

 - RUNNING

 - FINSHED

 - FAILED

 - PARTIALLY\_FAILED

 - CANCELLING

 - CANCELLED

 progressPercentage:

 type: integer

 minimum: 0

 maximum: 100

 progressStateInfo:

 type: string

 resultStateInfo:

 type: string

 startTime:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DateTime'

 endTime:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DateTime'

 timer:

 type: integer

 FileDownloadJobProcessMonitor:

 description: >-

 This data type is the "ProcessMonitor" data type with specialisations

 for usage in the "FileDownloadJob".

 type: object

 properties:

 jobId:

 type: string

 status:

 type: string

 enum:

 - NOT\_STARTED

 - RUNNING

 - FINSHED

 - FAILED

 - CANCELLING

 - CANCELLED

 progressPercentage:

 type: integer

 minimum: 0

 maximum: 100

 progressStateInfo:

 type: string

 resultStateInfo:

 oneOf:

 - type: string

 enum:

 - NULL

 - UNKNOWN

 - NO\_STORAGE

 - LOW\_MEMROY

 - NO\_CONNECTION\_TO\_REMOTE\_SERVER

 - FILE\_NOT\_AVAILABLE

 - DNS\_CANNOT\_BE\_RESOLVED

 - TIMER\_EXPIRED

 - OTHER

 - type: string

 startTime:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DateTime'

 endTime:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DateTime'

 timer:

 type: integer

 AreaScope:

 oneOf:

 - type: array

 items:

 $ref: '#/components/schemas/EutraCellId'

 - type: array

 items:

 $ref: '#/components/schemas/NrCellId'

 - type: array

 items:

 $ref: '#/components/schemas/Tac'

 - type: array

 items:

 $ref: '#/components/schemas/Tai'

 Tai:

 type: object

 properties:

 mcc:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/Mcc'

 mnc:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/Mnc'

 tac:

 $ref: '#/components/schemas/Tac'

 AreaConfig:

 type: object

 properties:

 freqInfo:

 $ref: '#/components/schemas/FreqInfo'

 pciList:

 type: array

 items:

 type: integer

 FreqInfo:

 description: specifies the carrier frequency and bands used in a cell.

 type: object

 properties:

 arfcn:

 type: integer

 freqBands:

 type: array

 items:

 type: integer

 MbsfnArea:

 type: object

 properties:

 mbsfnAreaId:

 type: integer

 minimum: 1

 earfcn:

 type: integer

 minimum: 1

 Tac:

 type: string

 pattern: '(^[A-Fa-f0-9]{4}$)|(^[A-Fa-f0-9]{6}$)'

 EutraCellId:

 type: string

 pattern: '^[A-Fa-f0-9]{7}$'

 NrCellId:

 type: string

 pattern: '^[A-Fa-f0-9]{9}$'

 IpAddr:

 oneOf:

 - $ref: 'TS28623\_ComDefs.yaml#/components/schemas/Ipv4Addr'

 - $ref: 'TS28623\_ComDefs.yaml#/components/schemas/Ipv6Addr'

 ManagementData:

 oneOf:

 - type: array

 items:

 type: string

 enum:

 - COVERAGE

 - CAPACITY

 - ENERGY\_EFFICIENCY

 - MOBILITY

 - ACCESSIBILITY

 - type: array

 items:

 type: string

 NodeFilter:

 type: object

 properties:

 areaOfInterest:

 $ref: 'comDefs.yaml#/components/schemas/AreaOfInterest'

 networkDomain:

 type: string

 enum:

 - CN

 - RAN

 cpUpType:

 type: string

 enum:

 - CP

 - UP

 sst:

 type: integer

#-------- Definition of types used in Trace control NRM fragment------------------

 jobType-Type:

 type: string

 description: Specifies whether the TraceJob represents only MDT, Logged MBSFN MDT, Trace or a combined Trace and MDT job. Applicable for Trace, MDT, RCEF and RLF reporting. See 3GPP TS 32.422 clause 5.9a for additional details.

 enum:

 - IMMEDIATE\_MDT\_ONLY

 - LOGGED\_MDT\_ONLY

 - TRACE\_ONLY

 - IMMEDIATE\_MDT AND TRACE

 - RLF\_REPORT\_ONLY

 - RCEF\_REPORT\_ONLY

 - LOGGED\_MBSFN\_MDT

 listOfInterfaces-Type:

 description: The interfaces to be recorded in the Network Element. See 3GPP TS 32.422 clause 5.5 for additional details.

 type: object

 properties:

 MSCServerInterfaces:

 type: array

 items:

 type: string

 enum:

 - A

 - Iu-CS

 - Mc

 - MAP-G

 - MAP-B

 - MAP-E

 - MAP-F

 - MAP-D

 - MAP-C

 - CAP

 MGWInterfaces:

 type: array

 items:

 type: string

 enum:

 - Mc

 - Nb-UP

 - Iu-UP

 RNCInterfaces:

 type: array

 items:

 type: string

 enum:

 - Iu-CS

 - Iu-PS

 - Iur

 - Iub

 - Uu

 SGSNInterfaces:

 type: array

 items:

 type: string

 enum:

 - Gb

 - Iu-PS

 - Gn

 - MAP-Gr

 - MAP-Gd

 - MAP-Gf

 - Ge

 - Gs

 - S6d

 - S4

 - S3

 - S13

 GGSNInterfaces:

 type: array

 items:

 type: string

 enum:

 - Gn

 - Gi

 - Gmb

 S-CSCFInterfaces:

 type: array

 items:

 type: string

 enum:

 - Mw

 - Mg

 - Mr

 - Mi

 P-CSCFInterfaces:

 type: array

 items:

 type: string

 enum:

 - Gm

 - Mw

 I-CSCFInterfaces:

 type: array

 items:

 type: string

 enum:

 - Cx

 - Dx

 - Mg

 - Mw

 MRFCInterfaces:

 type: array

 items:

 type: string

 enum:

 - Mp

 - Mr

 MGCFInterfaces:

 type: array

 items:

 type: string

 enum:

 - Mg

 - Mj

 - Mn

 IBCFInterfaces:

 type: array

 items:

 type: string

 enum:

 - Ix

 - Mx

 E-CSCFInterfaces:

 type: array

 items:

 type: string

 enum:

 - Mw

 - Ml

 - Mm

 - Mi/Mg

 BGCFInterfaces:

 type: array

 items:

 type: string

 enum:

 - Mi

 - Mj

 - Mk

 ASInterfaces:

 type: array

 items:

 type: string

 enum:

 - Dh

 - Sh

 - ISC

 - Ut

 HSSInterfaces:

 type: array

 items:

 type: string

 enum:

 - MAP-C

 - MAP-D

 - Gc

 - Gr

 - Cx

 - S6d

 - S6a

 - Sh

 - N70

 - N71

 - NU1

 EIRInterfaces:

 type: array

 items:

 type: string

 enum:

 - MAP-F

 - S13

 - MAP-Gf

 BM-SCInterfaces:

 type: array

 items:

 type: string

 enum:

 - Gmb

 MMEInterfaces:

 type: array

 items:

 type: string

 enum:

 - S1-MME

 - S3

 - S6a

 - S10

 - S11

 - S13

 SGWInterfaces:

 type: array

 items:

 type: string

 enum:

 - S4

 - S5

 - S8

 - S11

 - Gxc

 PDN\_GWInterfaces:

 type: array

 items:

 type: string

 enum:

 - S2a

 - S2b

 - S2c

 - S5

 - S6b

 - Gx

 - S8

 - SGi

 eNBInterfaces:

 type: array

 items:

 type: string

 enum:

 - S1-MME

 - X2

 en-gNBInterfaces:

 type: array

 items:

 type: string

 enum:

 - S1-MME

 - X2

 - Uu

 - F1-C

 - E1

 AMFInterfaces:

 type: array

 items:

 type: string

 enum:

 - N1

 - N2

 - N8

 - N11

 - N12

 - N14

 - N15

 - N20

 - N22

 - N26

 AUSFInterfaces:

 type: array

 items:

 type: string

 enum:

 - N12

 - N13

 NEFInterfaces:

 type: array

 items:

 type: string

 enum:

 - N29

 - N30

 - N33

 NRFInterfaces:

 type: array

 items:

 type: string

 enum:

 - N27

 NSSFInterfaces:

 type: array

 items:

 type: string

 enum:

 - N22

 - N31

 PCFInterfaces:

 type: array

 items:

 type: string

 enum:

 - N5

 - N7

 - N15

 SMFInterfaces:

 type: array

 items:

 type: string

 enum:

 - N4

 - N7

 - N10

 - N11

 - S5-C

 SMSFInterfaces:

 type: array

 items:

 type: string

 enum:

 - N20

 - N21

 UDMInterfaces:

 type: array

 items:

 type: string

 enum:

 - N8

 - N10

 - N13

 - N21

 - NU1

 UPFInterfaces:

 type: array

 items:

 type: string

 enum:

 - N4

 ng-eNBInterfaces:

 type: array

 items:

 type: string

 enum:

 - NG-C

 - Xn-C

 - Uu

 gNB-CU-CPInterfaces:

 type: array

 items:

 type: string

 enum:

 - NG-C

 - Xn-C

 - Uu

 - F1-C

 - E1

 - X2-C

 gNB-CU-UPInterfaces:

 type: array

 items:

 type: string

 enum:

 - E1

 gNB-DUInterfaces:

 type: array

 items:

 type: string

 enum:

 - F1-C

 listOfNeTypes-Type:

 description: The Network Element types where Trace Session activation is needed. See 3GPP TS 32.422 clause 5.4 for additional details.

 type: array

 items:

 type: string

 enum:

 - MSC\_SERVER

 - SGSN

 - MGW

 - GGSN

 - RNC

 - BM\_SC

 - MME

 - SGW

 - PGW

 - ENB

 - EN\_GNB

 - GNB\_CU\_CP

 - GNB\_CU\_UP

 - GNB\_DU

 - AMF

 - PCF

 - SMF

 - UPF

 - AUSF

 - SMSF

 - HSS

 - UDM

 plmnTarget-Type:

 type: object

 description: The PLMN for which sessions shall be selected in the Trace Session in case of management based activation when several PLMNs are supported in the RAN (this means that shared cells and not shared cells are allowed for the specified PLMN. Note that the PLMN Target might differ from the PLMN specified in the Trace Reference, as that specifies the PLMN that is containing the management system requesting the Trace Session from the NE. See 3GPP TS 32.422 clause 5.9b for additional details.

 properties:

 mcc:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/Mcc'

 mnc:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/Mnc'

 required:

 - mcc

 - mnc

 traceDepth-Type:

 description: Specifies how detailed information should be recorded in the Network Element. The Trace Depth is a paremeter for Trace Session level, i.e., the Trace Depth is the same for all of the NEs to be traced in the same Trace Session. See 3GPP TS 32.422 clause 5.3 for additional details.

 type: string

 enum:

 - MINIMUM

 - MEDIUM

 - MAXIMUM

 - VENDORMINIMUM

 - VENDORMEDIUM

 - VENDORMAXIMUM

 traceReference-Type:

 type: object

 description: The Trace Reference parameter shall be globally unique, therefore the Trace Reference shall compose as follows - MCC+MNC+Trace ID, where the MCC and MNC are coming with the Trace activation request from the management system to identify one PLMN containing the management system, and Trace ID is a 3 byte Octet String. See 3GPP TS 32.422 clause 5.6 for additional details.

 properties:

 mcc:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/Mcc'

 mnc:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/Mnc'

 traceId:

 type: string

 required:

 - mcc

 - mnc

 - traceId

 traceReportingFormat-Type:

 type: string

 description: Specifies whether file-based or streaming reporting shall be used for this Trace Session. See 3GPP TS 32.422 clause 5.11 for additional details.

 enum:

 - FILE-BASED

 - STREAMING

 traceTarget-Type:

 type: object

 description: Trace target conveying both the type and value of the target ID. For additional details see 3GPP TS 32.422

 properties:

 TargetIdType:

 type: string

 enum:

 - IMSI

 - IMEI

 - IMEISV

 - PUBLIC\_ID

 - UTRAN\_CELL

 - E-UTRAN\_CELL

 - NG-RAN\_CELL

 - eNB

 - RNC

 - gNB

 - SUPI

 TargetIdValue:

 type: string

 required:

 - TargetIdType

 - TargetIdValue

 triggeringEvents-Type:

 type: object

 description: Specifies when to start a Trace Recording Session and which message shall be recorded first, when to stop a Trace Recording Session and which message shall be recorded last respectively. See 3GPP TS 32.422 clause 5.1 for additional detials.

 properties:

 MSC\_SERVER:

 type: array

 items:

 type: string

 enum:

 - MO\_MT\_CALLS

 - MO\_MT\_SMS

 - LU\_IMSIattach\_IMSIdetach

 - HANDOVER

 - SS

 SGSN:

 type: array

 items:

 type: string

 enum:

 - PDPcontext

 - MO\_MT\_SMS

 - RAU\_GPRSattach\_GPRSdetach

 - MBMScontext

 MGW:

 type: array

 items:

 type: string

 enum:

 - CONTEXT

 GGSN:

 type: array

 items:

 type: string

 enum:

 - PDPcontext

 - MBMScontext

 IMS:

 type: array

 items:

 type: string

 enum:

 - SIPsession\_StandaloneTransaction

 BM\_SC:

 type: array

 items:

 type: string

 enum:

 - MBMSactivation

 MME:

 type: array

 items:

 type: string

 enum:

 - UEinitiatedPDNconnectivityRequest

 - ServiceRequest

 - InitialAttach\_TAU\_Detach

 - UEinitiatedPDNdisconnection

 - BearerActivationModificationDeletion

 - Handover

 SGW:

 type: array

 items:

 type: string

 enum:

 - PDNconnectionCreation

 - PDNconnectionTermination

 - BearerActivationModificationDeletion

 PGW:

 type: array

 items:

 type: string

 enum:

 - PDNconnectionCreation

 - PDNconnectionTermination

 - BearerActivationModificationDeletion

 AMF:

 type: array

 items:

 type: string

 enum:

 - Registration

 - ServiceRequest

 - Handover

 - UEderegistration

 - NetworkDeregistration

 - UEMobilityFromEPC

 - UEMobilityToEPC

 SMF:

 type: array

 items:

 type: string

 enum:

 - PDUsessionEstablishment

 - PDUsessionModification

 - PDUsessionRelease

 - PDUsessionUPactivationDeactivation

 - MobilityBtw3gppAndN3gppTo5GC

 - MobilityFromEpc

 PCF:

 type: array

 items:

 type: string

 enum:

 - AMpolicy

 - SMpolicy

 - Authorization

 - BDTpolicy

 UPF:

 type: array

 items:

 type: string

 enum:

 - N4Session

 AUSF:

 type: array

 items:

 type: string

 enum:

 - UEauthentication

 NEF:

 type: array

 items:

 type: string

 enum:

 - EventExposure

 - PFDmanagement

 - ParameterProvision

 - Trigger

 NRF:

 type: array

 items:

 type: string

 enum:

 - NFmanagement

 - NFdiscovery

 NSSF:

 type: array

 items:

 type: string

 enum:

 - NSSelection

 - NSSAI

 SMSF:

 type: array

 items:

 type: string

 enum:

 - SMservice

 UDM:

 type: array

 items:

 type: string

 enum:

 - UEcontext

 - SubscriberData

 - UEauthentication

 - EventExposure

 anonymizationOfMdtData-Type:

 description: Specifies level of MDT anonymization. For additional details see 3GPP TS 32.422 clause 5.10.12.

 type: string

 enum:

 - NO\_IDENTITY

 - TAC\_OF\_IMEI

 beamLevelMeasurement-Type:

 description: Determines whether beam level measurements shall be included in case of immediate MDT M1 measurement in NR. For additional details see 3GPP TS 32.422 clause 5.10.40.

 type: boolean

 collectionPeriodRrmLte-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.20.

 type: string

 enum:

 - 100ms

 - 1000ms

 - 1024ms

 - 1280ms

 - 2048ms

 - 2560ms

 - 5120ms

 - 10000ms

 - 10240ms

 - 60000ms

 collectionPeriodM6Lte-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.32.

 type: string

 enum:

 - 1024ms

 - 2048ms

 - 5120ms

 - 10240ms

 collectionPeriodM7Lte-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.33.

 type: integer

 minimum: 1

 maximum: 60

 collectionPeriodRrmUmts-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.21.

 type: string

 enum:

 - 100ms

 - 250ms

 - 500ms

 - 1000ms

 - 2000ms

 - 3000ms

 - 4000ms

 - 6000ms

 collectionPeriodRrmNr-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.30.

 type: string

 enum:

 - 1024ms

 - 2048ms

 - 5120ms

 - 10240ms

 - 60000ms

 collectionPeriodM6Nr-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.34.

 type: string

 enum:

 - 120ms

 - 240ms

 - 480ms

 - 640ms

 - 1024ms

 - 2048ms

 - 5120ms

 - 10240ms

 - 20480ms

 - 40960ms

 - 1min

 - 6min

 - 12min

 - 30min

 collectionPeriodM7Nr-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.35.

 type: integer

 minimum: 1

 maximum: 60

 eventListForEventTriggeredMeasurement-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.28.

 type: string

 enum:

 - OUT\_OF\_COVERAGE

 - A2\_EVENT

 eventThreshold-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.7, 5.10.7a, 5.10.13 and 5.10.14.

 type: object

 properties:

 EventThresholdRSRP:

 oneOf:

 - type: integer

 minimum: 0

 maximum: 97

 - type: integer

 minimum: 0

 maximum: 127

 EventThresholdRSRQ:

 oneOf:

 - type: integer

 minimum: 0

 maximum: 34

 - type: integer

 minimum: 0

 maximum: 127

 EventThreshold1F:

 type: object

 properties:

 CPICH\_RSCP:

 type: integer

 minimum: -120

 maximum: 25

 CPICH\_EcNo:

 type: integer

 minimum: -24

 maximum: 0

 PathLoss:

 type: integer

 minimum: 30

 maximum: 165

 EventThreshold1I:

 type: integer

 minimum: -120

 maximum: 25

 listOfMeasurements-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.3 for details.

 type: object

 properties:

 UMTS:

 type: array

 items:

 type: string

 enum:

 - M1

 - M2

 - M3

 - M4

 - M5

 - M6\_DL

 - M6\_UL

 - M7\_DL

 - M7\_UL

 LTE:

 type: array

 items:

 type: string

 enum:

 - M1

 - M2

 - M3

 - M4

 - M5

 - M1\_EVENT\_TRIGGERED

 - M6

 - M7

 - M8

 - M9

 NR:

 type: array

 items:

 type: string

 enum:

 - M1

 - M2

 - M3

 - M4

 - M5

 - M6

 - M7

 - M1\_EVENT\_TRIGGERED

 - M8

 - M9

 loggingDuration-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.9.

 type: string

 enum:

 - 600s

 - 1200s

 - 2400s

 - 3600s

 - 5400s

 - 7200s

 loggingInterval-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.8.

 type: object

 properties:

 UMTS:

 type: array

 items:

 type: string

 enum:

 - 1.28s

 - 2.56s

 - 5.12s

 - 10.24s

 - 20.48s

 - 30.72s

 - 40.96s

 - 61.44s

 LTE:

 type: array

 items:

 type: string

 enum:

 - 1.28s

 - 2.56s

 - 5.12s

 - 10.24s

 - 20.48s

 - 30.72s

 - 40.96s

 - 61.44s

 NR:

 type: array

 items:

 type: string

 enum:

 - 0.32s

 - 0.64s

 - 1.28s

 - 2.56s

 - 5.12s

 - 10.24s

 - 20.48s

 - 30.72s

 - 40.96s

 - 61.44s

 - INFINITY

 eventThresholdL1-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.X.

 type: object

 properties:

 RSRP:

 type: integer

 minimum: 0

 maximum: 127

 RSRQ:

 type: integer

 minimum: 0

 maximum: 127

 hysteresisL1-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.Y.

 type: integer

 minimum: 0

 maximum: 30

 timeToTriggerL1-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.Z.

 type: string

 enum:

 - 0ms

 - 40ms

 - 64ms

 - 80ms

 - 100ms

 - 128ms

 - 160ms

 - 256ms

 - 320ms

 - 480ms

 - 512ms

 - 640ms

 - 1024ms

 - 1280ms

 - 2560ms

 - 5120ms

 measurementPeriodLte-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.23.

 type: string

 enum:

 - 1024ms

 - 2048ms

 - 5120ms

 - 10240ms

 - 1min

 measurementPeriodUmts-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.22.

 type: string

 enum:

 - 1000ms

 - 2000ms

 - 3000ms

 - 4000ms

 - 6000ms

 - 8000ms

 - 12000ms

 - 16000ms

 - 20000ms

 - 24000ms

 - 28000ms

 - 32000ms

 - 64000ms

 measurementQuantity-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.15.

 type: string

 enum:

 - CPICH\_EcNo

 - CPICH\_RSCP

 - PathLoss

 eventThresholdUphUmts-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.A.

 type: integer

 minimum: 0

 maximum: 31

 plmnList-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.24.

 type: array

 items:

 type: object

 properties:

 mcc:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/Mcc'

 mnc:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/Mnc'

 required:

 - mcc

 - mnc

 maxItems: 16

 positioningMethod-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.19.

 type: string

 enum:

 - GNSS

 - E-CELL\_ID

 reportAmount-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.6.

 type: string

 enum:

 - 1

 - 2

 - 4

 - 8

 - 16

 - 32

 - 64

 - INFINITY

 reportAmountM1LTE-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.x.

 type: string

 enum:

 - 1

 - 2

 - 4

 - 8

 - 16

 - 32

 - 64

 - INFINITY

 reportAmountM4LTE-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.y.

 type: string

 enum:

 - 1

 - 2

 - 4

 - 8

 - 16

 - 32

 - 64

 - INFINITY

 reportAmountM5LTE-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.z.

 type: string

 enum:

 - 1

 - 2

 - 4

 - 8

 - 16

 - 32

 - 64

 - INFINITY

 reportAmountM6LTE-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.a.

 type: string

 enum:

 - 1

 - 2

 - 4

 - 8

 - 16

 - 32

 - 64

 - INFINITY

 reportAmountM7LTE-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.b.

 type: string

 enum:

 - 1

 - 2

 - 4

 - 8

 - 16

 - 32

 - 64

 - INFINITY

 reportingTrigger-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.4.

 type: array

 items:

 type: string

 enum:

 - PERIODICAL

 - A2\_FOR\_LTE\_NR

 - 1F\_FOR\_UMTS

 - 1I\_FOR\_UMTS\_MCPS\_TDD

 - A2\_TRIGGERED\_PERIODIC\_FOR\_LTE\_NR

 - ALL\_CONFIGURED\_RRM\_FOR\_LTE\_NR

 - ALL\_CONFIGURED\_RRM\_FOR\_UMTS

 reportInterval-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.5.

 type: object

 properties:

 UMTS:

 type: array

 items:

 type: string

 enum:

 - 250ms

 - 500ms

 - 1000ms

 - 2000ms

 - 3000ms

 - 4000ms

 - 6000ms

 - 8000ms

 - 12000ms

 - 16000ms

 - 20000ms

 - 24000ms

 - 28000ms

 - 32000ms

 - 64000ms

 LTE:

 type: array

 items:

 type: string

 enum:

 - 120ms

 - 240ms

 - 480ms

 - 640ms

 - 1024ms

 - 2048ms

 - 5120ms

 - 10240ms

 - 60000ms

 - 360000ms

 - 720000ms

 - 1800000ms

 - 3600000ms

 NR:

 type: array

 items:

 type: string

 enum:

 - 120ms

 - 240ms

 - 480ms

 - 640ms

 - 1024ms

 - 2048ms

 - 5120ms

 - 10240ms

 - 20480ms

 - 40960ms

 - 60000ms

 - 360000ms

 - 720000ms

 - 1800000ms

 reportType-Type:

 description: Report type for logged NR MDT. See details in 3GPP TS 32.422 clause 5.10.27.

 type: string

 enum:

 - PERIODICAL

 - EVENT\_TRIGGERED

 sensorInformation-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.29.

 type: array

 items:

 type: string

 enum:

 - BAROMETRIC\_PRESSURE

 - UE\_SPEED

 - UE\_ORIENTATION

 traceCollectionEntityId-Type:

 description: See details in 3GPP TS 32.422 clause 5.10.11. Only TCE Id value may be sent over the air to the UE being configured for Logged MDT.

 type: integer

#-------- end of Definition of types used in Trace control NRM fragment ----------

#-------- Definition of abstract IOC Top -----------------------------------------

 Top-Attr:

 # This definition will be deprecated, when all occurances of Top-Attr

 # are replaced by Top.

 type: object

 properties:

 id:

 type: string

 nullable: true

 objectClass:

 type: string

 objectInstance:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/Dn'

 VsDataContainer:

 $ref: '#/components/schemas/VsDataContainer-Multiple'

 required:

 - id

 Top:

 type: object

 properties:

 id:

 type: string

 nullable: true

 objectClass:

 type: string

 objectInstance:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/Dn'

 VsDataContainer:

 $ref: '#/components/schemas/VsDataContainer-Multiple'

 required:

 - id

#-------- Definition of IOCs with new name-containments defined in other TS ------

 SubNetwork-Attr:

 type: object

 properties:

 dnPrefix:

 type: string

 userLabel:

 type: string

 userDefinedNetworkType:

 type: string

 setOfMcc:

 type: array

 items:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/Mcc'

 priorityLabel:

 type: integer

 supportedPerfMetricGroups:

 type: array

 items:

 $ref: '#/components/schemas/SupportedPerfMetricGroup'

 supportedTraceMetrics:

 type: array

 items:

 type: string

 ManagedElement-Attr:

 type: object

 properties:

 dnPrefix:

 type: string

 managedElementTypeList:

 type: array

 items:

 type: string

 userLabel:

 type: string

 locationName:

 type: string

 managedBy:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnList'

 vendorName:

 type: string

 userDefinedState:

 type: string

 swVersion:

 type: string

 priorityLabel:

 type: integer

 supportedPerfMetricGroups:

 type: array

 items:

 $ref: '#/components/schemas/SupportedPerfMetricGroup'

 supportedTraceMetrics:

 type: array

 items:

 type: string

 SubNetwork-ncO:

 type: object

 properties:

 ManagementNode:

 $ref: '#/components/schemas/ManagementNode-Multiple'

 MnsAgent:

 $ref: '#/components/schemas/MnsAgent-Multiple'

 MeContext:

 $ref: '#/components/schemas/MeContext-Multiple'

 PerfMetricJob:

 $ref: '#/components/schemas/PerfMetricJob-Multiple'

 ThresholdMonitor:

 $ref: '#/components/schemas/ThresholdMonitor-Multiple'

 TraceJob:

 $ref: '#/components/schemas/TraceJob-Multiple'

 ManagementDataCollection:

 $ref: '#/components/schemas/ManagementDataCollection-Multiple'

 NtfSubscriptionControl:

 $ref: '#/components/schemas/NtfSubscriptionControl-Multiple'

 AlarmList:

 $ref: '#/components/schemas/AlarmList-Single'

 Files:

 $ref: '#/components/schemas/Files-Multiple'

 FileDownloadJob:

 $ref: '#/components/schemas/FileDownloadJob-Multiple'

 MnsRegistry:

 $ref: '#/components/schemas/MnsRegistry-Single'

 ManagedElement-ncO:

 type: object

 properties:

 MnsAgent:

 $ref: '#/components/schemas/MnsAgent-Multiple'

 PerfMetricJob:

 $ref: '#/components/schemas/PerfMetricJob-Multiple'

 ThresholdMonitor:

 $ref: '#/components/schemas/ThresholdMonitor-Multiple'

 TraceJob:

 $ref: '#/components/schemas/TraceJob-Multiple'

 NtfSubscriptionControl:

 $ref: '#/components/schemas/NtfSubscriptionControl-Multiple'

 AlarmList:

 $ref: '#/components/schemas/AlarmList-Single'

 FileDownloadJob:

 $ref: '#/components/schemas/FileDownloadJob-Multiple'

 Files:

 $ref: '#/components/schemas/Files-Multiple'

#-------- Definition of abstract IOCs --------------------------------------------

 ManagedFunction-Attr:

 type: object

 properties:

 userLabel:

 type: string

 vnfParametersList:

 type: array

 items:

 $ref: '#/components/schemas/VnfParameter'

 peeParametersList:

 type: array

 items:

 $ref: '#/components/schemas/PeeParameter'

 priorityLabel:

 type: integer

 supportedPerfMetricGroups:

 type: array

 items:

 $ref: '#/components/schemas/SupportedPerfMetricGroup'

 supportedTraceMetrics:

 type: array

 items:

 type: string

 EP\_RP-Attr:

 type: object

 properties:

 userLabel:

 type: string

 farEndEntity:

 type: string

 supportedPerfMetricGroups:

 type: array

 items:

 $ref: '#/components/schemas/SupportedPerfMetricGroup'

 TraceJob-Attr:

 type: object

 description: abstract class used as a container of all TraceJob attributes

 properties:

 jobType:

 $ref: '#/components/schemas/jobType-Type'

 listOfInterfaces:

 $ref: '#/components/schemas/listOfInterfaces-Type'

 listOfNeTypes:

 $ref: '#/components/schemas/listOfNeTypes-Type'

 plmnTarget:

 $ref: '#/components/schemas/plmnTarget-Type'

 traceReportingConsumerUri:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/Uri'

 traceCollectionEntityIpAddress:

 $ref: '#/components/schemas/IpAddr'

 traceDepth:

 $ref: '#/components/schemas/traceDepth-Type'

 traceReference:

 $ref: '#/components/schemas/traceReference-Type'

 traceRecordingSessionReference:

 type: string

 jobId:

 type: string

 traceReportingFormat:

 $ref: '#/components/schemas/traceReportingFormat-Type'

 traceTarget:

 $ref: '#/components/schemas/traceTarget-Type'

 triggeringEvents:

 $ref: '#/components/schemas/triggeringEvents-Type'

 anonymizationOfMdtData:

 $ref: '#/components/schemas/anonymizationOfMdtData-Type'

 areaConfigurationForNeighCell:

 $ref: '#/components/schemas/AreaConfig'

 areaScope:

 type: array

 items:

 $ref: '#/components/schemas/AreaScope'

 beamLevelMeasurement:

 $ref: '#/components/schemas/beamLevelMeasurement-Type'

 collectionPeriodRrmLte:

 $ref: '#/components/schemas/collectionPeriodRrmLte-Type'

 collectionPeriodM6Lte:

 $ref: '#/components/schemas/collectionPeriodM6Lte-Type'

 collectionPeriodM7Lte:

 $ref: '#/components/schemas/collectionPeriodM7Lte-Type'

 collectionPeriodRrmUmts:

 $ref: '#/components/schemas/collectionPeriodRrmUmts-Type'

 collectionPeriodRrmNr:

 $ref: '#/components/schemas/collectionPeriodRrmNr-Type'

 collectionPeriodM6Nr:

 $ref: '#/components/schemas/collectionPeriodM6Nr-Type'

 collectionPeriodM7Nr:

 $ref: '#/components/schemas/collectionPeriodM7Nr-Type'

 eventListForEventTriggeredMeasurement:

 $ref: '#/components/schemas/eventListForEventTriggeredMeasurement-Type'

 eventThreshold:

 $ref: '#/components/schemas/eventThreshold-Type'

 listOfMeasurements:

 $ref: '#/components/schemas/listOfMeasurements-Type'

 loggingDuration:

 $ref: '#/components/schemas/loggingDuration-Type'

 loggingInterval:

 $ref: '#/components/schemas/loggingInterval-Type'

 eventThresholdL1:

 $ref: '#/components/schemas/eventThresholdL1-Type'

 hysteresisL1:

 $ref: '#/components/schemas/hysteresisL1-Type'

 timeToTriggerL1:

 $ref: '#/components/schemas/timeToTriggerL1-Type'

 mbsfnAreaList:

 type: array

 items:

 $ref: '#/components/schemas/MbsfnArea'

 measurementPeriodLte:

 $ref: '#/components/schemas/measurementPeriodLte-Type'

 measurementPeriodUmts:

 $ref: '#/components/schemas/measurementPeriodUmts-Type'

 measurementQuantity:

 $ref: '#/components/schemas/measurementQuantity-Type'

 eventThresholdUphUmts:

 $ref: '#/components/schemas/eventThresholdUphUmts-Type'

 plmnList:

 $ref: '#/components/schemas/plmnList-Type'

 positioningMethod:

 $ref: '#/components/schemas/positioningMethod-Type'

 reportAmount:

 $ref: '#/components/schemas/reportAmount-Type'

 reportAmountM1LTE:

 $ref: '#/components/schemas/reportAmountM1LTE-Type'

 reportAmountM4LTE:

 $ref: '#/components/schemas/reportAmountM4LTE-Type'

 reportAmountM5LTE:

 $ref: '#/components/schemas/reportAmountM5LTE-Type'

 reportAmountM6LTE:

 $ref: '#/components/schemas/reportAmountM6LTE-Type'

 reportAmountM7LTE:

 $ref: '#/components/schemas/reportAmountM7LTE-Type'

 reportingTrigger:

 $ref: '#/components/schemas/reportingTrigger-Type'

 reportInterval:

 $ref: '#/components/schemas/reportInterval-Type'

 reportType:

 $ref: '#/components/schemas/reportType-Type'

 sensorInformation:

 $ref: '#/components/schemas/sensorInformation-Type'

 traceCollectionEntityId:

 $ref: '#/components/schemas/traceCollectionEntityId-Type'

 ManagedFunction-ncO:

 type: object

 properties:

 PerfMetricJob:

 $ref: '#/components/schemas/PerfMetricJob-Multiple'

 ThresholdMonitor:

 $ref: '#/components/schemas/ThresholdMonitor-Multiple'

 ManagedNFService:

 $ref: '#/components/schemas/ManagedNFService-Multiple'

 TraceJob:

 $ref: '#/components/schemas/TraceJob-Multiple'

 MnsRegistry-Single:

 type: object

 properties:

 MnsInfo:

 $ref: '#/components/schemas/MnsInfo-Multiple'

#-------- Definition of concrete IOCs --------------------------------------------

 VsDataContainer-Single:

 type: object

 properties:

 id:

 type: string

 attributes:

 type: object

 properties:

 vsDataType:

 type: string

 vsDataFormatVersion:

 type: string

 vsData:

 nullable: true

 VsDataContainer:

 $ref: '#/components/schemas/VsDataContainer-Multiple'

 ManagedNFService-Single:

 allOf:

 - $ref: '#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 type: object

 properties:

 userLabel:

 type: string

 nFServiceType:

 $ref: '#/components/schemas/NFServiceType'

 sAP:

 $ref: '#/components/schemas/SAP'

 operations:

 type: array

 items:

 $ref: '#/components/schemas/Operation'

 administrativeState:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/AdministrativeState'

 operationalState:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/OperationalState'

 usageState:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/UsageState'

 registrationState:

 $ref: '#/components/schemas/RegistrationState'

 ManagementNode-Single:

 allOf:

 - $ref: '#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 type: object

 properties:

 userLabel:

 type: string

 managedElements:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnList'

 vendorName:

 type: string

 userDefinedState:

 type: string

 locationName:

 type: string

 swVersion:

 type: string

 MnsAgent:

 $ref: '#/components/schemas/MnsAgent-Multiple'

 MnsAgent-Single:

 allOf:

 - $ref: '#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 type: object

 properties:

 systemDN:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/Dn'

 MeContext-Single:

 allOf:

 - $ref: '#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 type: object

 properties:

 dnPrefix:

 type: string

 PerfMetricJob-Single:

 allOf:

 - $ref: '#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 type: object

 properties:

 administrativeState:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/AdministrativeState'

 operationalState:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/OperationalState'

 jobId:

 type: string

 performanceMetrics:

 type: array

 items:

 type: string

 granularityPeriod:

 type: integer

 minimum: 1

 objectInstances:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnList'

 rootObjectInstances:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnList'

 reportingCtrl:

 $ref: '#/components/schemas/ReportingCtrl'

 Files:

 $ref: '#/components/schemas/Files-Multiple'

 ThresholdMonitor-Single:

 allOf:

 - $ref: '#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 type: object

 properties:

 administrativeState:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/AdministrativeState'

 operationalState:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/OperationalState'

 performanceMetrics:

 type: array

 items:

 type: string

 thresholdInfoList:

 type: array

 items:

 $ref: '#/components/schemas/ThresholdInfo'

 monitorGranularityPeriod:

 type: integer

 minimum: 1

 objectInstances:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnList'

 rootObjectInstances:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DnList'

 NtfSubscriptionControl-Single:

 allOf:

 - $ref: '#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 type: object

 properties:

 notificationRecipientAddress:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/Uri'

 notificationTypes:

 type: array

 items:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/NotificationType'

 scope:

 $ref: '#/components/schemas/Scope'

 notificationFilter:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/Filter'

 HeartbeatControl:

 $ref: '#/components/schemas/HeartbeatControl-Single'

 HeartbeatControl-Single:

 allOf:

 - $ref: '#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 type: object

 properties:

 heartbeatNtfPeriod:

 type: integer

 minimum: 0

 triggerHeartbeatNtf:

 type: boolean

 TraceJob-Single:

 allOf:

 - $ref: '#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 $ref: '#/components/schemas/TraceJob-Attr'

 Files:

 $ref: '#/components/schemas/Files-Multiple'

 ManagementDataCollection-Single:

 allOf:

 - $ref: '#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 type: object

 properties:

 managementData:

 $ref: '#/components/schemas/ManagementData'

 targetNodeFilter:

 $ref: '#/components/schemas/NodeFilter'

 collectionTimeWindow:

 $ref: 'comDefs.yaml#/components/schemas/TimeWindow'

 reportingCtrl:

 type: string

 dataScope:

 type: string

 enum:

 - SNSSAI

 - 5QI

 AlarmList-Single:

 allOf:

 - $ref: '#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 type: object

 properties:

 administrativeState:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/AdministrativeState'

 operationalState:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/OperationalState'

 numOfAlarmRecords:

 type: integer

 lastModification:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DateTime'

 alarmRecords:

 description: >-

 This resource represents a map of alarm records.

 The alarmIds are used as keys in the map.

 type: object

 additionalProperties:

 $ref: 'TS28532\_FaultMnS.yaml#/components/schemas/AlarmRecord'

 FileDownloadJob-Single:

 allOf:

 - $ref: '#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 type: object

 properties:

 fileLocation:

 type: string

 notificationRecipientAddress:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/Uri'

 cancelJob:

 type: string

 enum:

 - TRUE

 - FALSE

 jobMonitor:

 $ref: '#/components/schemas/FileDownloadJobProcessMonitor'

 Files-Single:

 allOf:

 - $ref: '#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 type: object

 properties:

 numberOfFiles:

 type: integer

 jobRef:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/Dn'

 jobId:

 type: string

 File:

 $ref: '#/components/schemas/File-Multiple'

 File-Single:

 allOf:

 - $ref: '#/components/schemas/Top'

 - type: object

 properties:

 attributes:

 type: object

 properties:

 fileLocation:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/Uri'

 fileCompression:

 type: string

 fileSize:

 type: integer

 fileDataType:

 type: string

 enum:

 - PERFORMANCE

 - TRACE

 - ANALYTICS

 - PROPRIETARY

 fileFormat:

 type: string

 fileReadyTime:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DateTime'

 fileExpirationTime:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/DateTime'

 fileContent:

 type: string

 jobRef:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/Dn'

 jobId:

 type: string

 MnsInfo-Single:

 type: object

 properties:

 mnsLabel:

 type: string

 mnsType:

 type: string

 enum:

 - ProvMnS

 - FaultSupervisionMnS

 - StreamingDataReportingMnS

 - FileDataReportingMnS

 mnsVersion:

 type: string

 mnsAddress:

 description: Resource URI as defined in the relevant Technical Specification

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/Uri'

 mnsScope:

 description: >-

 List of the managed object instances that can be accessed using the MnS.

 If a complete SubNetwork can be accessed using the MnS, this attribute may contain the

 DN of the SubNetwork instead of the DNs of the individual managed entities within the

 SubNetwork.

 type: array

 items:

 $ref: 'TS28623\_ComDefs.yaml#/components/schemas/Dn'

#-------- Definition of YAML arrays for name-contained IOCs ----------------------

 VsDataContainer-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/VsDataContainer-Single'

 ManagedNFService-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/ManagedNFService-Single'

 ManagementNode-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/ManagementNode-Single'

 MnsAgent-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/MnsAgent-Single'

 MeContext-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/MeContext-Single'

 PerfMetricJob-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/PerfMetricJob-Single'

 ThresholdMonitor-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/ThresholdMonitor-Single'

 TraceJob-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/TraceJob-Single'

 ManagementDataCollection-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/ManagementDataCollection-Single'

 NtfSubscriptionControl-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/NtfSubscriptionControl-Single'

 FileDownloadJob-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/FileDownloadJob-Single'

 Files-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/Files-Single'

 File-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/File-Single'

 MnsInfo-Multiple:

 type: array

 items:

 $ref: '#/components/schemas/MnsInfo-Single'

#-------- Definitions in TS 28.623 for TS 28.532 ---------------------------------

 resources-genericNrm:

 oneOf:

 - $ref: '#/components/schemas/VsDataContainer-Single'

 - $ref: '#/components/schemas/ManagementNode-Single'

 - $ref: '#/components/schemas/MnsAgent-Single'

 - $ref: '#/components/schemas/MeContext-Single'

 - $ref: '#/components/schemas/ManagedNFService-Single'

 - $ref: '#/components/schemas/PerfMetricJob-Single'

 - $ref: '#/components/schemas/ThresholdMonitor-Single'

 - $ref: '#/components/schemas/TraceJob-Single'

 - $ref: '#/components/schemas/ManagementDataCollection-Single'

 - $ref: '#/components/schemas/NtfSubscriptionControl-Single'

 - $ref: '#/components/schemas/HeartbeatControl-Single'

 - $ref: '#/components/schemas/AlarmList-Single'

 - $ref: '#/components/schemas/FileDownloadJob-Single'

 - $ref: '#/components/schemas/Files-Single'

 - $ref: '#/components/schemas/File-Single'

 - $ref: '#/components/schemas/MnsRegistry-Single'

 - $ref: '#/components/schemas/MnsInfo-Single'

|  |
| --- |
| **3rd modified section** |

## D.2.10 module \_3gpp-common-trace.yang

<CODE BEGINS>

module \_3gpp-common-trace {

 yang-version 1.1;

 namespace "urn:3gpp:sa5:\_3gpp-common-trace";

 prefix "trace3gpp";

 import \_3gpp-common-top { prefix top3gpp; }

 import \_3gpp-common-yang-types {prefix types3gpp; }

 import ietf-inet-types { prefix inet; }

 organization "3GPP SA5";

 contact "https://www.3gpp.org/DynaReport/TSG-WG--S5--officials.htm?Itemid=464";

 description "Trace handling";

 reference "3GPP TS 28.623

 Generic Network Resource Model (NRM)

 Integration Reference Point (IRP);

 Solution Set (SS) definitions

 3GPP TS 28.622

 Generic Network Resource Model (NRM)

 Integration Reference Point (IRP);

 Information Service (IS)";

 revision 2022-04-27 { reference "CR-0159"; }

 revision 2021-10-18 { reference "CR-0139"; }

 revision 2021-07-22 { reference "CR-0137"; }

 revision 2021-01-25 { reference "CR-0122"; }

 revision 2020-11-16 { reference "CR-0117"; }

 revision 2020-08-06 { reference "CR-0102"; }

 grouping TraceJobGrp {

 leaf tjJobType {

 type enumeration {

 enum IMMEDIATE\_MDT\_ONLY;

 enum LOGGED\_MDT\_ONLY;

 enum TRACE\_ONLY;

 enum IMMEDIATE\_MDT\_AND\_TRACE;

 enum RLF\_REPORT\_ONLY;

 enum RCEF\_REPORT\_ONLY;

 enum LOGGED\_MBSFN\_MDT;

 }

 default TRACE\_ONLY;

 description "Specifies the MDT mode and it specifies also whether the

 TraceJob represents only MDT, Logged MBSFN MDT, Trace or a combined

 Trace and MDT job. The attribute is applicable for Trace, MDT, RCEF and

 RLF reporting.";

 reference "Clause 5.9a of 3GPP TS 32.422 for additional details on the

 allowed values.";

 }

 list tjListOfInterfaces {

 key idx;

 must 'count(MSCServerInterfaces)+count(MGWInterfaces)+count(RNCInterfaces)'

 +'+count(SGSNInterfaces)+count(GGSNInterfaces)+count(S-CSCFInterfaces)'

 +'+count(P-CSCFInterfaces)+count(I-CSCFInterfaces)+count(MRFCInterfaces)'

 +'+count(MGCFInterfaces)+count(IBCFInterfaces)+count(E-CSCFInterfaces)'

 +'+count(BGCFInterfaces)+count(ASInterfaces)+count(HSSInterfaces)'

 +'+count(EIRInterfaces)+count(BM-SCInterfaces)+count(MMEInterfaces)'

 +'+count(SGWInterfaces)+count(PDN\_GWInterfaces)+count(eNBInterfaces)'

 +'+count(en-gNBInterfaces)+count(AMFInterfaces)+count(AUSFInterfaces)'

 +'+count(NEFInterfaces)+count(NRFInterfaces)+count(NSSFInterfaces)'

 +'+count(PCFInterfaces)+count(SMFInterfaces)+count(SMSFInterfaces)'

 +'+count(UDMInterfaces)+count(UPFInterfaces)+count(ng-eNBInterfaces)'

 +'+count(gNB-CU-CPInterfaces)+count(gNB-CU-UPInterfaces)'

 +'+count(gNB-DUInterfaces)';

 description "Specifies the interfaces that need to be traced in the given

 ManagedEntityFunction.The attribute is applicable only for Trace. In

 case this attribute is not used, it carries a null semantic.";

 reference "Clause 5.5 of 3GPP TS 32.422 for additional details on the

 allowed values.";

 leaf idx { type uint32 ; }

 leaf-list MSCServerInterfaces {

 type enumeration {

 enum A ;

 enum Iu-CS ;

 enum Mc ;

 enum MAP-G ;

 enum MAP-B ;

 enum MAP-E ;

 enum MAP-F ;

 enum MAP-D ;

 enum MAP-C ;

 enum CAP ;

 }

 }

 leaf-list MGWInterfaces {

 type enumeration {

 enum Mc ;

 enum Nb-UP ;

 enum Iu-UP ;

 }

 }

 leaf-list RNCInterfaces {

 type enumeration {

 enum Iu-CS ;

 enum Iu-PS ;

 enum Iur ;

 enum Iub ;

 enum Uu ;

 }

 }

 leaf-list SGSNInterfaces {

 type enumeration {

 enum Gb ;

 enum Iu-PS ;

 enum Gn ;

 enum MAP-Gr ;

 enum MAP-Gd ;

 enum MAP-Gf ;

 enum Ge ;

 enum Gs ;

 enum S6d ;

 enum S4 ;

 enum S3 ;

 enum S13 ;

 }

 }

 leaf-list GGSNInterfaces {

 type enumeration {

 enum Gn ;

 enum Gi ;

 enum Gmb ;

 }

 }

 leaf-list S-CSCFInterfaces {

 type enumeration {

 enum Mw ;

 enum Mg ;

 enum Mr ;

 enum Mi ;

 }

 }

 leaf-list P-CSCFInterfaces {

 type enumeration {

 enum Gm ;

 enum Mw ;

 }

 }

 leaf-list I-CSCFInterfaces {

 type enumeration {

 enum Cx ;

 enum Dx ;

 enum Mg ;

 enum Mw ;

 }

 }

 leaf-list MRFCInterfaces {

 type enumeration {

 enum Mp ;

 enum Mr ;

 }

 }

 leaf-list MGCFInterfaces {

 type enumeration {

 enum Mg ;

 enum Mj ;

 enum Mn ;

 }

 }

 leaf-list IBCFInterfaces {

 type enumeration {

 enum Ix ;

 enum Mx ;

 }

 }

 leaf-list E-CSCFInterfaces {

 type enumeration {

 enum Mw ;

 enum Ml ;

 enum Mm ;

 enum Mi-Mg ;

 }

 }

 leaf-list BGCFInterfaces {

 type enumeration {

 enum Mi ;

 enum Mj ;

 enum Mk ;

 }

 }

 leaf-list ASInterfaces {

 type enumeration {

 enum Dh ;

 enum Sh ;

 enum ISC ;

 enum Ut ;

 }

 }

 leaf-list HSSInterfaces {

 type enumeration {

 enum MAP-C ;

 enum MAP-D ;

 enum Gc ;

 enum Gr ;

 enum Cx ;

 enum S6d ;

 enum S6a ;

 enum Sh ;

 }

 }

 leaf-list EIRInterfaces {

 type enumeration {

 enum MAP-F ;

 enum S13 ;

 enum MAP-Gf ;

 }

 }

 leaf-list BM-SCInterfaces {

 type enumeration {

 enum Gmb ;

 }

 }

 leaf-list MMEInterfaces {

 type enumeration {

 enum S1-MME ;

 enum S3 ;

 enum S6a ;

 enum S10 ;

 enum S11 ;

 enum S13 ;

 }

 }

 leaf-list SGWInterfaces {

 type enumeration {

 enum S4 ;

 enum S5 ;

 enum S8 ;

 enum S11 ;

 enum Gxc ;

 }

 }

 leaf-list PDN\_GWInterfaces {

 type enumeration {

 enum S2a ;

 enum S2b ;

 enum S2c ;

 enum S5 ;

 enum S6b ;

 enum Gx ;

 enum S8 ;

 enum SGi ;

 }

 }

 leaf-list eNBInterfaces {

 type enumeration {

 enum S1-MME ;

 enum X2 ;

 }

 }

 leaf-list en-gNBInterfaces {

 type enumeration {

 enum S1-MME ;

 enum X2 ;

 enum Uu ;

 enum F1-C ;

 enum E1 ;

 }

 }

 leaf-list AMFInterfaces {

 type enumeration {

 enum N1 ;

 enum N2 ;

 enum N8 ;

 enum N11 ;

 enum N12 ;

 enum N14 ;

 enum N15 ;

 enum N20 ;

 enum N22 ;

 enum N26 ;

 }

 }

 leaf-list AUSFInterfaces {

 type enumeration {

 enum N12 ;

 enum N13 ;

 }

 }

 leaf-list NEFInterfaces {

 type enumeration {

 enum N29 ;

 enum N30 ;

 enum N33 ;

 }

 }

 leaf-list NRFInterfaces {

 type enumeration {

 enum N27 ;

 }

 }

 leaf-list NSSFInterfaces {

 type enumeration {

 enum N22 ;

 enum N31 ;

 }

 }

 leaf-list PCFInterfaces {

 type enumeration {

 enum N5 ;

 enum N7 ;

 enum N15 ;

 }

 }

 leaf-list SMFInterfaces {

 type enumeration {

 enum N4 ;

 enum N7 ;

 enum N10 ;

 enum N11 ;

 enum S5-C ;

 }

 }

 leaf-list SMSFInterfaces {

 type enumeration {

 enum N20 ;

 enum N21 ;

 }

 }

 leaf-list UDMInterfaces {

 type enumeration {

 enum N8 ;

 enum N10 ;

 enum N13 ;

 enum N21 ;

 }

 }

 leaf-list UPFInterfaces {

 type enumeration {

 enum N4 ;

 }

 }

 leaf-list ng-eNBInterfaces {

 type enumeration {

 enum NG-C ;

 enum Xn-C ;

 enum Uu ;

 }

 }

 leaf-list gNB-CU-CPInterfaces {

 type enumeration {

 enum NG-C ;

 enum Xn-C ;

 enum Uu ;

 enum F1-C ;

 enum E1 ;

 enum X2-C ;

 }

 }

 leaf-list gNB-CU-UPInterfaces {

 type enumeration {

 enum E1 ;

 }

 }

 leaf-list gNB-DUInterfaces {

 type enumeration {

 enum F1-C ;

 }

 }

 }

 leaf-list tjListOfNeTypes {

 type enumeration {

 enum MSC\_SERVER;

 enum SGSN;

 enum MGW;

 enum GGSN;

 enum RNC;

 enum BM\_SC;

 enum MME;

 enum SGW;

 enum PGW;

 enum ENB;

 enum EN\_GNB;

 enum GNB\_CU\_CP;

 enum GNB\_CU\_UP;

 enum GNB\_DU;

 }

 description "Specifies in which type of ManagedFunction the trace should

 be activated. The attribute is applicable only for Trace with

 Signalling Based Trace activation. In case this attribute is not used,

 it carries a null semantic";

 reference "Clause 5.4 of 3GPP TS 32.422 for additional details on the

 allowed values";

 }

 leaf tjPLMNTarget {

 type string;

 mandatory true;

 description "Specifies which PLMN that the subscriber of the session to

 be recorded uses as selected PLMN. PLMN Target might differ from the

 PLMN specified in the Trace Reference";

 reference "Clause 5.9b of 3GPP TS 32.422";

 }

 leaf tjStreamingTraceConsumerURI {

 when '../tjTraceReportingFormat = "STREAMING"';

 type inet:uri;

 mandatory true;

 description "URI of the Streaming Trace data reporting MnS consumer

 (a.k.a. streaming target).

 This attribute shall be present if file based trace data reporting is

 supported and tjTraceReportingFormat set to 'file based' or when

 tjJobType is set to Logged MDT or Logged MBSFN MDT.";

 reference "Clause 5.9 of 3GPP TS 32.422";

 }

 leaf tjTraceCollectionEntityAddress {

 when '../tjTraceReportingFormat = "FILE\_BASED" or '

 +'../tjJobType = "LOGGED\_MDT\_ONLY" or ../tjJobType = "LOGGED\_MBSFN\_MDT"';

 type union {

 type inet:uri;

 type inet:ip-address;

 }

 mandatory true;

 description "Specifies the address of the Trace Collection Entity when

 the attribute tjTraceReportingFormat is configured for the file-based

 reporting. The attribute is applicable for both Trace and MDT.";

 reference "Clause 5.9 of 3GPP TS 32.422";

 }

 leaf tjTraceDepth {

 when '../tjJobType = "TRACE\_ONLY"'

 + ' or ../tjJobType = "IMMEDIATE\_MDT\_AND\_TRACE"';

 type enumeration {

 enum MINIMUM;

 enum MEDIUM;

 enum MAXIMUM;

 enum VENDORMINIMUM;

 enum VENDORMEDIUM;

 enum VENDORMAXIMUM;

 }

 default MAXIMUM;

 description "Specifies how detailed information should be recorded in the

 Network Element. The Trace Depth is a paremeter for Trace Session level,

 i.e., the Trace Depth is the same for all of the NEs to be traced in

 the same Trace Session.

 The attribute is applicable only for Trace, otherwise it carries a null

 semantic.";

 reference "Clause 5.3 of 3GPP TS 32.422";

 }

 leaf tjTraceReference {

 type uint64;

 mandatory true;

 description "A globally unique identifier, which uniquely identifies the

 Trace Session that is created by the TraceJob.

 In case of shared network, it is the MCC and MNC of the Participating

 Operator that request the trace session that shall be provided.

 The attribute is applicable for both Trace and MDT.";

 }

 leaf tjTraceRecordSessionReference {

 type string;

 mandatory true;

 description "An identifier, which identifies the Trace Recording Session.

 The attribute is applicable for both Trace and MDT.

 See the clause 5.7 of 3GPP TS 32.422 for additional details on the

 allowed values.";

 }

 leaf tjTraceReportingFormat {

 type enumeration {

 enum FILE\_BASED;

 enum STREAMING;

 }

 default FILE\_BASED;

 description "Specifies the trace reporting format - streaming trace

 reporting or file-based trace reporting";

 reference "3GPP TS 32.422 clause 5.11";

 }

 list tjTraceTarget {

 key "targetIdType targetIdValue";

 max-elements 1;

 leaf targetIdType {

 type enumeration {

 enum IMSI;

 enum IMEI;

 enum IMEISV;

 enum PUBLIC\_ID;

 enum UTRAN\_CELL;

 enum E\_UTRAN\_CELL;

 enum NG\_RAN\_CELL;

 enum ENB;

 enum RNC;

 enum GNB;

 enum SUPI;

 }

 }

 leaf targetIdValue {

 type string;

 }

 description "Specifies the target object of the Trace and MDT. The

 attribute is applicable for both Trace and MDT. This attribute

 includes the ID type of the target as an enumeration and the ID value.

 The tjTraceTarget shall be public ID in case of a Management Based

 Activation is done to an ScscfFunction. The tjTraceTarget shall be

 cell only in case of the UTRAN cell traffic trace function.

 The tjTraceTarget shall be E-UtranCell only in case of E-UTRAN cell

 traffic trace function.The tjTraceTarget shall be either IMSI or

 IMEI(SV) if the Trace Session is activated to any of the following

 ManagedEntity(ies):

 - HssFunction

 - MscServerFunction

 - SgsnFunction

 - GgsnFunction

 - BmscFunction

 - RncFunction

 - MmeFunction

 The tjTraceTarget shall be IMSI if the Trace Session is activated to a

 ManagedEntity playing a role of ServinGWFunction.

 In case of signaling based Trace/MDT, the tjTraceTarget attribute shall

 be able to carry (IMSI or IMEI(SV)or SUPI), the tjMDTAreaScope attribute

 shall be able to carry a list of (cell or E-UtranCell or NRCellDU or

 TA/LA/RA).

 In case of management based Immediate MDT, the tjTraceTarget attribute

 shall be null value, the tjMDTAreaScope attribute shall carry a list of

 (Utrancell or E-UtranCell or NRCellDU).

 In case of management based Logged MDT, the tjTraceTarget attribute

 shall carry an eBs or a RNC or gNBs. The Logged MDT should be initiated

 on the specified eNB or RNC or gNB in tjTraceTarget. The tjMDTAreaScope

 attribute shall carry a list of (Utrancell or E-UtranCell or NRCellDU or

 TA/LA/RA).

 In case of RLF reporting, or RCEF reporting, the tjTraceTarget

 attribute shall be null value, the tjMDTAreaScope attribute shall carry

 one or list of eNBs/gNBs";

 reference "3GPP TS 32.422";

 }

 leaf tjTriggeringEvent {

 when '../tjJobType = "TRACE\_ONLY" or ../tjJobType = "IMMEDIATE\_MDT\_AND\_TRACE"';

 type string ;

 mandatory true;

 description "Specifies the triggering event parameter of the trace session.

 The attribute is applicable only for Trace. In case this attribute is

 not used, it carries a null semantic.";

 reference "Clause 5.1 of 3GPP TS 32.422";

 }

 leaf tjMDTAnonymizationOfData {

 when ../tjMDTAreaScope ;

 type enumeration {

 enum NO\_IDENTITY;

 enum TAC\_OF\_IMEI;

 }

 default NO\_IDENTITY;

 description "Specifies level of MDT anonymization.";

 reference "3GPP TS 32.422 clause 5.10.12.";

 }

 list tjMDTAreaConfigurationForNeighCell {

 when '../tjJobType = "LOGGED\_MDT\_ONLY"';

 key "idx";

 min-elements 1;

 leaf idx { type uint32 ; }

 description "It specifies the area for which UE is requested to perform

 measurement logging for neighbour cells which have list of frequencies.

 If it is not configured, the UE shall perform measurement logging for

 all the neighbour cells.

 Applicable only to NR Logged MDT.";

 reference "3GPP TS 32.422 clause 5.10.26.";

 leaf frequency {

 type string;

 }

 leaf cell {

 type string;

 }

 }

 leaf-list tjMDTAreaScope {

 type string;

 description "specifies MDT area scope when activates an MDT job.

 For RLF and RCEF reporting it specifies the eNB or list of eNBs where the

 RLF or RCEF reports should be collected.

 List of cells/TA/LA/RA for signaling based MDT or management based Logged

 MDT.

 List of cells for management based Immediate MDT.

 Cell, TA, LA, RA are mutually exclusive.

 One or list of eNBs for RLF and RCEFreporting";

 reference "Clause 5.10.2 of 3GPP TS 32.422";

 }

 leaf tjMDTCollectionPeriodRrmLte {

 when '../tjJobType = "IMMEDIATE\_MDT\_ONLY"'

 + ' or ../tjJobType = "IMMEDIATE\_MDT\_AND\_TRACE"';

 type uint32 {

 range "250|500|1000|2000|3000|4000|6000|8000|12000|16000|20000|"

 +"24000|28000|32000|64000";

 }

 units milliseconds;

 description "Specifies the collection period for collecting RRM configured

 measurement samples for M2, M3 in LTE. The attribute is applicable only

 for Immediate MDT. In case this attribute is not used, it carries a

 null semantic.";

 reference "Clause 5.10.20 of 3GPP TS 32.422";

 }

 leaf tjMDTCollectionPeriodM6Lte {

 when '../tjJobType = "IMMEDIATE\_MDT\_ONLY"'

 + ' or ../tjJobType = "IMMEDIATE\_MDT\_AND\_TRACE"';

 type uint32 {

 range "1024|2048|5120|10240";

 }

 units milliseconds;

 description "Specifies the collection period for the Packet Delay

 measurement (M6) for MDT taken by the eNB. The attribute is applicable

 only for Immediate MDT. In case this attribute is not used,

 it carries a null semantic.";

 reference "Clause 5.10.32 of TS 32.422 ";

 }

 leaf tjMDTCollectionPeriodM7Lte {

 when '../tjJobType = "IMMEDIATE\_MDT\_ONLY"'

 + ' or ../tjJobType = "IMMEDIATE\_MDT\_AND\_TRACE"';

 type uint16 {

 range 1..60 ;

 }

 description "It specifies the collection period for the Data Volume (M6)

 and Throughput measurements (M7) for UMTS MDT taken by RNC. The

 attribute is applicable only for Immediate MDT. In case this attribute

 is not used, it carries a null semantic.";

 reference "Clause 5.10.22 of TS 32.422 .";

 }

 leaf tjMDTCollectionPeriodRrmUmts {

 when '../tjJobType = "IMMEDIATE\_MDT\_ONLY"'

 + ' or ../tjJobType = "IMMEDIATE\_MDT\_AND\_TRACE"';

 type uint32 {

 range "1024|1280|2048|2560|5120|"

 +"10240|60000";

 }

 units milliseconds;

 description "Specifies the collection period for collecting RRM configured

 measurement samples for M3, M4, M5 in UMTS. The attribute is applicable

 only for Immediate MDT. In case this attribute is not used, it carries

 a null semantic";

 reference "Clause 5.10.21 of 3GPP TS 32.422";

 }

 leaf tjMDTCollectionPeriodRrmNR {

 when '../tjJobType = "IMMEDIATE\_MDT\_ONLY"'

 + ' or ../tjJobType = "IMMEDIATE\_MDT\_AND\_TRACE"';

 type uint32 {

 range "1024|2048|5120|10240|60000";

 }

 units milliseconds;

 description "Specifies the collection period for collecting RRM

 configured measurement samples for M4, M5 in NR. The attribute is

 applicable only for Immediate MDT. In case this attribute is not

 used, it carries a null semantic.";

 reference "Clause 5.10.30 of 3GPP TS 32.422";

 }

 leaf tjMDTCollectionPeriodM6NR {

 when '../tjJobType = "IMMEDIATE\_MDT\_ONLY"'

 + ' or ../tjJobType = "IMMEDIATE\_MDT\_AND\_TRACE"';

 type enumeration {

 enum 120ms;

 enum 240ms;

 enum 480ms;

 enum 640ms;

 enum 1024ms;

 enum 2048ms;

 enum 5120ms;

 enum 10240ms;

 enum 20480ms;

 enum 40960ms;

 enum 1min;

 enum 6min;

 enum 12min;

 enum 30min;

 }

 description "It specifies the collection period for the Packet Delay

 measurement (M6) for NR MDT taken by the gNB. The attribute is

 applicable only for Immediate MDT. In case this attribute is not used,

 it carries a null semantic.";

 reference "clause 5.10.34 of TS 32.422";

 }

 leaf tjMDTCollectionPeriodM7NR {

 when '../tjJobType = "IMMEDIATE\_MDT\_ONLY"'

 + ' or ../tjJobType = "IMMEDIATE\_MDT\_AND\_TRACE"';

 type uint32 {

 range "1..60";

 }

 description "It specifies the collection period for the Packet Loss Rate

 measurement (M7) for NR MDT taken by the gNB. The attribute is

 applicable only for Immediate MDT. In case this attribute is not used,

 it carries a null semantic.";

 reference "clause 5.10.35 of TS 32.422";

 }

 leaf tjMDTEventListForTriggeredMeasurement {

 when '../tjJobType = "LOGGED\_MDT\_ONLY"';

 type enumeration {

 enum OUT\_OF\_COVERAGE ;

 enum A2\_EVENT ;

 }

 mandatory true;

 description "Specifies event types for event triggered measurement in the

 case of logged NR MDT. Each trace session may configure at most one

 event. The UE shall perform logging of measurements only upon certain

 condition being fulfilled:

 - Out of coverage.

 - A2 event.";

 reference "Clause 5.10.28 of 3GPP TS 32.422";

 }

 leaf tjMDTEventThreshold {

 type int64;

 description "Specifies the threshold which should trigger the reporting

 in case A2 event reporting in LTE or 1F/1l event in UMTS. The attribute

 is applicable only for Immediate MDT and when reportingTrigger is

 configured for A2 event in LTE or 1F event or 1l event in UMTS. In

 case this attribute is not used, it carries a null semantic.";

 reference "Clauses 5.10.7 and 5.10.7a of 3GPP TS 32.422";

 }

 leaf tjMDTListOfMeasurements {

 when '../tjJobType = "IMMEDIATE\_MDT\_ONLY"';

 type int64;

 mandatory true;

 description "It specifies the UE measurements that shall be collected in

 an Immediate MDT job. The attribute is applicable only for Immediate MDT.

 In case this attribute is not used, it carries a null semantic.";

 reference "3GPP TS 32.422 clause 5.10.3";

 }

 leaf tjMDTLoggingDuration {

 when '../tjJobType = "LOGGED\_MDT\_ONLY" or ../tjJobType = "LOGGED\_MBSFN\_MDT"';

 type uint32 {

 range "600|1200|2400|3600|5400|7200";

 }

 units seconds;

 mandatory true;

 description "Specifies how long the MDT configuration is valid at the

 UE in case of Logged MDT. The attribute is applicable only for

 Logged MDT and Logged MBSFN MDT. In case this attribute is not used, it

 carries a null semantic.";

 reference "5.10.9 of 3GPP TS 32.422";

 }

 leaf tjMDTLoggingInterval {

 when '../tjJobType = "LOGGED\_MDT\_ONLY" or ../tjJobType = "LOGGED\_MBSFN\_MDT"';

 type uint32 {

 range "1280|2560|5120|10240|20480|"

 +"30720|40960|61440";

 }

 units milliseconds;

 mandatory true;

 description "Specifies the periodicty for Logged MDT. The attribute is

 applicable only for Logged MDT and Logged MBSFN MDT. In case this

 attribute is not used, it carries a null semantic";

 reference "5.10.8 of 3GPP TS 32.422";

 }

 leaf tjMDTLoggingEventThreshold {

 when '../tjJobType = "LOGGED\_MDT\_ONLY" or ../tjJobType = "LOGGED\_MBSFN\_MDT"';

 type uint32 {

 range "0..127";

 }

 description "It specifies the threshold which should trigger

 the reporting in case of event based reporting of logged NR MDT.

 The attribute is applicable only for Logged MDT and when tjMDTReportType

 is configured for event triggered reporting and when

 tjMDTEventListForTriggeredMeasurement is configured for L1 event.

 In case this attribute is not used, it carries a null semantic.";

 reference "clause 5.10.36 of TS 32.422";

 }

 leaf tjMDTLoggedHysteresis {

 when '../tjJobType = "LOGGED\_MDT\_ONLY" or ../tjJobType = "LOGGED\_MBSFN\_MDT"';

 type uint32 {

 range "0..30";

 }

 description "It specifies the hysteresis used within the entry and leave

 condition of the L1 event based reporting of logged NR MDT.

 The attribute is applicable only for Logged MDT, when tjMDTReportType

 is configured for event triggered reporting and when

 tjMDTEventListForTriggeredMeasurement is configured for L1 event.

 In case this attribute is not used, it carries a null semantic.";

 reference "clause 5.10.37 of TS 32.422";

 }

 leaf tjMDTLoggedTimeToTrigger {

 when '../tjJobType = "LOGGED\_MDT\_ONLY" or ../tjJobType = "LOGGED\_MBSFN\_MDT"';

 type int32 ;

 description "It specifies the threshold which should trigger

 the reporting in case of event based reporting of logged NR MDT.

 The attribute is applicable only for Logged MDT, when tjMDTReportType

 is configured for event triggered reporting and when

 tjMDTEventListForTriggeredMeasurement is configured for L1 event.

 In case this attribute is not used, it carries a null semantic.";

 reference "clauses 5.10.38 of TS 32.422";

 }

 leaf-list tjMDTMBSFNAreaList {

 when '../tjJobType = "LOGGED\_MBSFN\_MDT"';

 type string;

 min-elements 1;

 max-elements 8;

 description "The MBSFN Area consists of a MBSFN Area ID and Carrier

 Frequency (EARFCN). The target MBSFN area List can have up to 8 entries.

 This parameter is applicable only if the job type is Logged MBSFN MDT.";

 reference "5.10.25 of 3GPP TS 32.422";

 }

 leaf tjMDTMeasurementPeriodLTE {

 when '../tjJobType = "IMMEDIATE\_MDT\_ONLY"'

 + ' or ../tjJobType = "IMMEDIATE\_MDT\_AND\_TRACE"';

 type uint32 {

 range "1024|1280|2048|2560|5120|"

 +"10240|60000";

 }

 units milliseconds;

 mandatory true;

 description "It specifies the measurement period for the Data Volume and

 Scheduled IP throughput measurements for MDT taken by the eNB.

 The attribute is applicable only for Immediate MDT. In case this

 attribute is not used, it carries a null semantic.";

 reference "Clause 5.10.23 of 3GPP TS 32.422";

 }

 leaf tjMDTMeasurementPeriodUMTS {

 when '../tjJobType = "IMMEDIATE\_MDT\_ONLY"'

 + 'or ../tjJobType = "IMMEDIATE\_MDT\_AND\_TRACE"';

 type uint32 {

 range "250|500|1000|2000|3000|4000|6000|8000|12000|16000|20000|"

 +"24000|28000|32000|64000";

 }

 units milliseconds;

 mandatory true;

 description "It specifies the measurement period for the Data Volume and

 Throughput measurements for MDT taken by RNC.

 The attribute is applicable only for Immediate MDT. In case this

 attribute is not used, it carries a null semantic.";

 reference "Clause 5.10.22 of 3GPP TS 32.422";

 }

 leaf tjMDTMeasurementQuantity {

 when '../tjJobType = "IMMEDIATE\_MDT\_ONLY"'

 + ' or ../tjJobType = "IMMEDIATE\_MDT\_AND\_TRACE"';

 type uint64 ;

 mandatory true;

 description "It specifies the measurements that are collected in an MDT

 job for a UMTS MDT configured for event triggered reporting.";

 reference "Clause 5.10.15 of 3GPP TS 32.422";

 }

 leaf tjMDTM4ThresholdUmts {

 when '../tjJobType = "IMMEDIATE\_MDT\_ONLY"'

 + ' or ../tjJobType = "IMMEDIATE\_MDT\_AND\_TRACE"';

 type uint16 {

 range 0..31 ;

 }

 description "It specifies the threshold which should trigger

 the reporting in case of event-triggered periodic reporting for M4

 (UE power headroom measurement) in UMTS. In case this attribute is

 not used, it carries a null semantic.";

 reference "3GPP TS 32.422 clause 5.10.A";

 }

 list tjMDTPLMList {

 when '../tjJobType = "LOGGED\_MDT\_ONLY"';

 key "mcc mnc";

 uses types3gpp:PLMNId;

 min-elements 1;

 max-elements 16;

 description "It indicates the PLMNs where measurement collection, status

 indication and log reporting is allowed.";

 reference "Clause 5.10.24 of 3GPP TS 32.422";

 }

 leaf tjMDTPositioningMethod {

 when '../tjJobType = "IMMEDIATE\_MDT\_ONLY"'

 + ' or ../tjJobType = "IMMEDIATE\_MDT\_AND\_TRACE"';

 type enumeration {

 enum GNSS;

 enum E\_CELL\_ID;

 }

 mandatory true;

 description "It specifies what positioning method should be used in the

 MDT job.";

 reference "Clause 5.10.19 of 3GPP TS 32.422";

 }

 leaf tjMDTReportAmount {

 when '../tjJobType = "IMMEDIATE\_MDT\_ONLY"'

 + ' and ./tjMDTReportingTrigger = "PERIODICAL"';

 type union {

 type uint32 {

 range "1|4|8|16|32|64" ;

 }

 type enumeration {

 enum INFINITY;

 }

 }

 mandatory true;

 description "It specifies the number of measurement reports in NR and UMTS that shall be

 taken for periodic reporting while the UE is in connected.

 The attribute is applicable only for Immediate MDT and when

 tjMDTReportingTrigger is configured for periodical measurements. In

 case this attribute is not used, it carries a null semantic.";

 reference "Clause 5.10.6 of 3GPP TS 32.422";

 }

 leaf tjMDTreportAmountM1LTE {

 when '../tjJobType = "IMMEDIATE\_MDT\_ONLY"'

 + ' and ./tjMDTReportingTrigger = "PERIODICAL"';

 type union {

 type uint32 {

 range "1|4|8|16|32|64" ;

 }

 type enumeration {

 enum INFINITY;

 }

 }

 mandatory true;

 description "It specifies the number of measurement reports for M1 in LTE that shall be

 taken for periodic reporting while the UE is in connected.

 The attribute is applicable only for Immediate MDT and when

 tjMDTReportingTrigger is configured for periodical measurements. In

 case this attribute is not used, it carries a null semantic.";

 reference "Clause 5.10.x of 3GPP TS 32.422";

 }

 leaf tjMDTreportAmountM4LTE {

 when '../tjJobType = "IMMEDIATE\_MDT\_ONLY"'

 + ' and ./tjMDTReportingTrigger = "PERIODICAL"';

 type union {

 type uint32 {

 range "1|4|8|16|32|64" ;

 }

 type enumeration {

 enum INFINITY;

 }

 }

 mandatory true;

 description "It specifies the number of measurement reports for M4 in LTE that shall be

 taken for periodic reporting while the UE is in connected.

 The attribute is applicable only for Immediate MDT and when

 tjMDTReportingTrigger is configured for periodical measurements. In

 case this attribute is not used, it carries a null semantic.";

 reference "Clause 5.10.y of 3GPP TS 32.422";

 }

 leaf tjMDTreportAmountM5LTE {

 when '../tjJobType = "IMMEDIATE\_MDT\_ONLY"'

 + ' and ./tjMDTReportingTrigger = "PERIODICAL"';

 type union {

 type uint32 {

 range "1|4|8|16|32|64" ;

 }

 type enumeration {

 enum INFINITY;

 }

 }

 mandatory true;

 description "It specifies the number of measurement reports for M5 in LTE that shall be

 taken for periodic reporting while the UE is in connected.

 The attribute is applicable only for Immediate MDT and when

 tjMDTReportingTrigger is configured for periodical measurements. In

 case this attribute is not used, it carries a null semantic.";

 reference "Clause 5.10.z of 3GPP TS 32.422";

 }

 leaf tjMDTreportAmountM6LTE {

 when '../tjJobType = "IMMEDIATE\_MDT\_ONLY"'

 + ' and ./tjMDTReportingTrigger = "PERIODICAL"';

 type union {

 type uint32 {

 range "1|4|8|16|32|64" ;

 }

 type enumeration {

 enum INFINITY;

 }

 }

 mandatory true;

 description "It specifies the number of measurement reports for M6 in LTE that shall be

 taken for periodic reporting while the UE is in connected.

 The attribute is applicable only for Immediate MDT and when

 tjMDTReportingTrigger is configured for periodical measurements. In

 case this attribute is not used, it carries a null semantic.";

 reference "Clause 5.10.a of 3GPP TS 32.422";

 }

 leaf tjMDTreportAmountM7LTE {

 when '../tjJobType = "IMMEDIATE\_MDT\_ONLY"'

 + ' and ./tjMDTReportingTrigger = "PERIODICAL"';

 type union {

 type uint32 {

 range "1|4|8|16|32|64" ;

 }

 type enumeration {

 enum INFINITY;

 }

 }

 mandatory true;

 description "It specifies the number of measurement reports for M7 in LTE that shall be

 taken for periodic reporting while the UE is in connected.

 The attribute is applicable only for Immediate MDT and when

 tjMDTReportingTrigger is configured for periodical measurements. In

 case this attribute is not used, it carries a null semantic.";

 reference "Clause 5.10.b of 3GPP TS 32.422";

 }

 leaf tjMDTReportingTrigger {

 when '../tjJobType = "IMMEDIATE\_MDT\_ONLY"';

 type enumeration {

 enum PERIODICAL;

 enum A2\_FOR\_LTE;

 enum 1F\_FOR\_UMTS;

 enum 1I\_FOR\_UMTS\_MCPS\_TDD;

 enum A2\_TRIGGERED\_PERIODIC\_FOR\_LTE;

 enum ALL\_CONFIGURED\_RRM\_FOR\_LTE;

 enum ALL\_CONFIGURED\_RRM\_FOR\_UMTS;

 }

 description "It specifies whether periodic or event based measurements

 should be collected.

 The attribute is applicable only for Immediate MDT and when the

 tjMDTListOfMeasurements is configured for M1 (for both UMTS and LTE)

 or M2 (only for UMTS). In case this attribute is not used, it carries

 a null semantic.";

 reference "Clause 5.10.4 of 3GPP TS 32.422";

 }

 leaf tjMDTReportInterval {

 when '../tjJobType = "IMMEDIATE\_MDT\_ONLY"'

 + ' and ../tjMDTReportingTrigger = "PERIODICAL"';

 type uint32 {

 range "120|240|250|480|500|640|1000|1024|2000|2048|3000|4000|"

 +"5120|6000|8000|10240|12000|16000|20000|"

 +"24000|28000|32000|60000|64000|"

 +"360000|720000|1800000|3600000";

 }

 units milliseconds;

 mandatory true;

 description "It specifies the interval between the periodical measurements

 that shall be taken when the UE is in connected mode.

 The attribute is applicable only for Immediate MDT and when

 tjMDTReportingTrigger is configured for periodical measurements. In case

 this attribute is not used, it carries a null semantic.";

 reference "5.10.5 of 3GPP TS 32.422";

 }

 leaf tjMDTReportType {

 when '../tjJobType = "LOGGED\_MDT\_ONLY"';

 type enumeration {

 enum PERIODICAL;

 enum EVENT\_TRIGGERED;

 }

 mandatory true;

 description "It specifies report type for logged NR MDT";

 reference "Clause 5.10.27 of 3GPP TS 32.422";

 }

 leaf tjMDTSensorInformation {

 type bits {

 bit BAROMETRIC\_PRESSURE;

 bit UE\_SPEED;

 bit UE\_ORIENTATION;

 }

 default "";

 description "It specifies which sensor information shall be included in

 logged NR MDT and immediate NR MDT measurement if they are available.

 The following sensor measurement can be included or excluded for

 the UE.";

 reference "Clause 5.10.29 of 3GPP TS 32.422";

 }

 leaf tjMDTTraceCollectionEntityID {

 when '../tjJobType = "LOGGED\_MDT\_ONLY" or ../tjJobType = "LOGGED\_MBSFN\_MDT"';

 type uint8;

 mandatory true;

 description "It specifies the TCE Id which is sent to the UE in

 Logged MDT.";

 reference "Clause 5.10.11 of 3GPP TS 32.422";

 }

 }

 grouping TraceSubtree {

 description "Contains classes that manage Tracing.

 Should be used in all classes (or classes inheriting from)

 - SubNnetwork

 - ManagedElement

 - ManagedFunction

 If a YANG module wants to augment these classes/list/groupings they must

 augment all user classes!";

 list TraceJob {

 description "Represents the Trace Control and Configuration parameters of a

 particular Trace Job (see TS 32.421 and TS 32.422 for details).

 It can be name-contained by SubNetwork, ManagedElement, ManagedFunction

 or NetworkSliceSubnet.

 To activate Trace Jobs, a MnS consumer has to create TraceJob object

 instances on the MnS producer. A MnS consumer can activate a Trace Job

 for another MnS consumer since it is not required the value of

 tjTraceCollectionEntityAddress or tjStreamingTraceConsumerUri to be his

 own.

 When a MnS consumer wishes to deactivate a Trace Job, the MnS consumer

 shall delete the corresponding TraceJob instance.

 For details of management Trace Job activation/deactivation see clause

 4.1.1.1.2 of TS 32.422.

 The attribute tjJobType specifies the kind of data to collect. Dependent

 on the selected type various parameters shall be available. The

 attributes tjJobType, tjTraceReference, tjTraceRecordSessionReference,

 tjTraceCollectionEntityAddress and tjTraceReportingFormat are mandatory

 for all job types. If streaming reporting is selected for

 tjTraceReportingFormat, tjStreamingTraceConsumerURI shall be present

 additionally. The attribute tjPLMNTarget shall be present if trace

 activation method is management based.

 For the different job types the attributes are differentiated as follows:

 - In case of TRACE\_ONLY additionally the following attributes shall be

 available: tjListOfNeTypes, tjTraceDepth, tjTraceTarget and

 tjTriggeringEvent.

 For this case the optional attribute tjListOfInterfaces allows to

 specify the interfaces to be recorded.

 - In case of IMMEDIATE\_MDT\_ONLY additionally the following attributes

 shall be available:

 - tjTraceTarget

 - tjMDTAnonymizationOfData,

 - tjMDTListOfMeasurements,

 - tjMDTCollectionPeriodRrmUmts (conditional for M3, M4 and M5 in UMTS),

 - tjMDTMeasurementPeriodUMTS (conditional for M6 and M7 in UMTS),

 - tjMDTCollectionPeriodRrmLte (conditional for M2 and M3 in LTE),

 - tjMDTMeasurementPeriodLTE (conditional for M4 and M5 in LTE),

 - tjMDTCollectionPeriodM6Lte (conditional for M6 in LTE),

 - tjMDTCollectionPeriodM7Lte (conditional for M7 in LTE),

 - tjMDTCollectionPeriodRrmNR (conditional for M4 and M5 in NR),

 - tjMDTCollectionPeriodM6NR (conditional for M6 in NR),

 - tjMDTCollectionPeriodM7NR (conditional for M7 in NR),

 - tjMDTReportInterval (conditional for M1 in LTE or NR and M1/M2 in

 UMTS),

 - tjMDTReportAmount (conditional for M1 in NR and M1/M2 in

 UMTS),

 - tjMDTreportAmountM1LTE (conditional for M1 in LTE),

 - tjMDTreportAmountM4LTE (conditional for M4 in LTE),

 - tjMDTreportAmountM5LTE (conditional for M5 in LTE),

 - tjMDTreportAmountM6LTE (conditional for M6 in LTE),

 - tjMDTreportAmountM7LTE (conditional for M7 in LTE),

 - tjMDTReportingTrigger (conditional for M1 in LTE or NR and M1/M2 in

 UMTS),

 - tjMDTEventThreshold (conditional for A2 event reporting or A2 event

 triggered periodic reporting),

 - tjMDTMeasurementQuantity (conditional for 1F event reporting).

 For this case the optional attribute tjMDTAreaScope allows to specify

 the area in terms of cells or Tracking Area/Routing Area/Location area

 where the MDT data collection shall take place and the optional

 attributes tjMDTPositioningMethod, tjMDTSensorInformation allow to

 specify the positioning methods to use or the sensor information to

 include.

 - In case of IMMEDIATE\_MDT\_AND\_TRACE both additional attributes of

 TRACE\_ONLY and IMMEDIATE\_MDT\_ONLY shall apply.

 - In case of LOGGED\_MDT\_ONLY additionally the following attributes

 shall be available: tjTraceTarget, tjMDTAnonymizationOfData,

 tjMDTTraceCollectionEntityID, tjMDTLoggingInterval,

 tjMDTLoggingDuration, tjMDTReportType,

 tjMDTEventListForTriggeredMeasurements.

 For this case the optional attribute tjMDTAreaScope allows to specify

 the area in terms of cells or Tracking Area/Routing Area/Location area

 where the MDT data collection shall take place, the optional attribute

 tjMDTPLMNList allows to specify the PLMNs where measurement collection,

 status indication and log reporting is allowed, the optional attribute

 tjMDTAreaConfigurationForNeighCell allows to specify the area for

 which UE is requested to perform measurements logging for neighbour

 cells which have list of frequencies and the optional attribute

 tjMDTSensorInformation allows to specify the sensor information to

 include.

 - In case of RLF\_REPORT\_ONLY and RCEF\_REPORT\_ONLY additionally the

 attribute tjTraceTarget shall be available, the optional attribute

 tjMDTAreaScope allows to specify the eNB or list of eNBs or gNB or

 list of gNBs where the reports should be collected.

 - In case of LOGGED\_MBSFN\_MDT additionally the following attributes

 shall be available: tjMDTAnonymizationOfData, tjMDTLoggingInterval,

 tjMDTLoggingDuration, tjMDTMBSFNAreaList.

 Creation and deletion of TraceJob instances by MnS consumers is optional;

 when not supported, the TraceJob instances may be created and deleted by

 the system or be pre-installed.";

 key id;

 uses top3gpp:Top\_Grp ;

 container attributes {

 uses TraceJobGrp ;

 }

 }

 }

}<CODE ENDS>

|  |
| --- |
| **end of changes** |