**3GPP TSG-SA5 Meeting #145-e *S5-225732***

**e-meeting, 15 - 24 August 2022**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.0* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **32.291** | **CR** | **0429** | **rev** | **-** | **Current version:** | **17.3.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Update Open API version | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Huawei | | | | | | | | | |
| ***Source to TSG:*** | S5 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | TEI16, 5GS\_Ph1-SBI\_CH | | | | |  | ***Date:*** | | | 2022-08-25 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **A** |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) Rel-12 (Release 12)* *Rel-13 (Release 13) Rel-14 (Release 14) Rel-15 (Release 15) Rel-16 (Release 16)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | CRs modifying the Nchf\_ ConvergedCharging API have been agreed and the version number of the corresponding OpenAPI file thus needs to be incremented following the rules in TS 29.501, subclause 4.3.1.  For Converged Charging Service in A.2:  - S5-225745 CR 0413 Backward compatible corrections  - S5-225741 CR 0408 Backward compatible corrections  - S5-225742 CR 0409 Backward compatible corrections  - S5-225740 CR 0416 Backward compatible corrections  - [S5-225279](https://www.3gpp.org/ftp/TSG_SA/WG5_TM/TSGS5_145e/Docs/S5-225279.zip) CR 0418 Backward compatible corrections  - [S5-225771](https://www.3gpp.org/ftp/TSG_SA/WG5_TM/TSGS5_145e/Docs/S5-225441.zip) CR 0423 Backward compatible corrections  - [S5-225451](https://www.3gpp.org/ftp/TSG_SA/WG5_TM/TSGS5_145e/Docs/S5-225451.zip) CR 0425 Backward compatible corrections  - [S5-225455](https://www.3gpp.org/ftp/TSG_SA/WG5_TM/TSGS5_145e/Docs/S5-225455.zip) CR 0427 Backward compatible corrections | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | For converged Charging Service:  - Nchf\_ ConvergedCharging Service version number is incremented from "3.1.0" to "3.1.1"  - TS 32.291 version number is incremented from "17.3.0" to "17.4.0". | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Wrong version info in OpenAPI. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | A.2 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

|  |
| --- |
| **First change** |

## A.2 Nchf\_ConvergedCharging API

openapi: 3.0.0

info:

title: Nchf\_ConvergedCharging

version: 3.1.1

description: |

ConvergedCharging Service © 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: >

3GPP TS 32.291 V17.4.0: Telecommunication management; Charging management;

5G system, charging service; Stage 3.

url: 'http://www.3gpp.org/ftp/Specs/archive/32\_series/32.291/'

servers:

- url: '{apiRoot}/nchf-convergedcharging/v3'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in subclause 4.4 of 3GPP TS 29.501.

security:

- {}

- oAuth2ClientCredentials:

- nchf-convergedcharging

paths:

/chargingdata:

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/ChargingDataRequest'

responses:

'201':

description: Created

content:

application/json:

schema:

$ref: '#/components/schemas/ChargingDataResponse'

'400':

description: Bad request

content:

application/problem+json:

schema:

oneOf:

- $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

- $ref: '#/components/schemas/ChargingDataResponse'

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

description: Forbidden

content:

application/problem+json:

schema:

oneOf:

- $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

- $ref: '#/components/schemas/ChargingDataResponse'

'404':

description: Not Found

content:

application/problem+json:

schema:

oneOf:

- $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

- $ref: '#/components/schemas/ChargingDataResponse'

'405':

$ref: 'TS29571\_CommonData.yaml#/components/responses/405'

'408':

$ref: 'TS29571\_CommonData.yaml#/components/responses/408'

'410':

$ref: 'TS29571\_CommonData.yaml#/components/responses/410'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

callbacks:

chargingNotification:

'{$request.body#/notifyUri}':

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/ChargingNotifyRequest'

responses:

'200':

description: OK.

content:

application/ json:

schema:

$ref: '#/components/schemas/ChargingNotifyResponse'

'204':

description: 'No Content, Notification was succesfull'

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

description: Bad request

content:

application/problem+json:

schema:

oneOf:

- $ref: TS29571\_CommonData.yaml#/components/schemas/ProblemDetails

- $ref: '#/components/schemas/ChargingNotifyResponse'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

'/chargingdata/{ChargingDataRef}/update':

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/ChargingDataRequest'

parameters:

- name: ChargingDataRef

in: path

description: a unique identifier for a charging data resource in a PLMN

required: true

schema:

type: string

responses:

'200':

description: OK. Updated Charging Data resource is returned

content:

application/json:

schema:

$ref: '#/components/schemas/ChargingDataResponse'

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

description: Bad request

content:

application/problem+json:

schema:

oneOf:

- $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

- $ref: '#/components/schemas/ChargingDataResponse'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

description: Forbidden

content:

application/problem+json:

schema:

oneOf:

- $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

- $ref: '#/components/schemas/ChargingDataResponse'

'404':

description: Not Found

content:

application/problem+json:

schema:

oneOf:

- $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

- $ref: '#/components/schemas/ChargingDataResponse'

'405':

$ref: 'TS29571\_CommonData.yaml#/components/responses/405'

'408':

$ref: 'TS29571\_CommonData.yaml#/components/responses/408'

'410':

$ref: 'TS29571\_CommonData.yaml#/components/responses/410'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

'/chargingdata/{ChargingDataRef}/release':

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/ChargingDataRequest'

parameters:

- name: ChargingDataRef

in: path

description: a unique identifier for a charging data resource in a PLMN

required: true

schema:

type: string

responses:

'204':

description: No Content.

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'404':

description: Not Found

content:

application/problem+json:

schema:

oneOf:

- $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

- $ref: '#/components/schemas/ChargingDataResponse'

'410':

$ref: 'TS29571\_CommonData.yaml#/components/responses/410'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{nrfApiRoot}/oauth2/token'

scopes:

nchf-convergedcharging: Access to the Nchf\_ConvergedCharging API

schemas:

ChargingDataRequest:

type: object

properties:

subscriberIdentifier:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

tenantIdentifier:

type: string

chargingId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ChargingId'

mnSConsumerIdentifier:

type: string

nfConsumerIdentification:

$ref: '#/components/schemas/NFIdentification'

invocationTimeStamp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

invocationSequenceNumber:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

retransmissionIndicator:

type: boolean

oneTimeEvent:

type: boolean

oneTimeEventType:

$ref: '#/components/schemas/oneTimeEventType'

notifyUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

supportedFeatures:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

serviceSpecificationInfo:

type: string

multipleUnitUsage:

type: array

items:

$ref: '#/components/schemas/MultipleUnitUsage'

minItems: 0

triggers:

type: array

items:

$ref: '#/components/schemas/Trigger'

minItems: 0

pDUSessionChargingInformation:

$ref: '#/components/schemas/PDUSessionChargingInformation'

roamingQBCInformation:

$ref: '#/components/schemas/RoamingQBCInformation'

sMSChargingInformation:

$ref: '#/components/schemas/SMSChargingInformation'

nEFChargingInformation:

$ref: '#/components/schemas/NEFChargingInformation'

registrationChargingInformation:

$ref: '#/components/schemas/RegistrationChargingInformation'

n2ConnectionChargingInformation:

$ref: '#/components/schemas/N2ConnectionChargingInformation'

locationReportingChargingInformation:

$ref: '#/components/schemas/LocationReportingChargingInformation'

nSPAChargingInformation:

$ref: '#/components/schemas/NSPAChargingInformation'

nSMChargingInformation:

$ref: '#/components/schemas/NSMChargingInformation'

mMTelChargingInformation:

$ref: '#/components/schemas/MMTelChargingInformation'

iMSChargingInformation:

$ref: '#/components/schemas/IMSChargingInformation'

edgeInfrastructureUsageChargingInformation':

$ref: '#/components/schemas/EdgeInfrastructureUsageChargingInformation'

eASDeploymentChargingInformation:

$ref: '#/components/schemas/EASDeploymentChargingInformation'

directEdgeEnablingServiceChargingInformation:

$ref: '#/components/schemas/NEFChargingInformation'

exposedEdgeEnablingServiceChargingInformation:

$ref: '#/components/schemas/NEFChargingInformation'

proSeChargingInformation:

$ref: '#/components/schemas/ProseChargingInformation'

required:

- nfConsumerIdentification

- invocationTimeStamp

- invocationSequenceNumber

ChargingDataResponse:

type: object

properties:

invocationTimeStamp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

invocationSequenceNumber:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

invocationResult:

$ref: '#/components/schemas/InvocationResult'

sessionFailover:

$ref: '#/components/schemas/SessionFailover'

supportedFeatures:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

multipleUnitInformation:

type: array

items:

$ref: '#/components/schemas/MultipleUnitInformation'

minItems: 0

triggers:

type: array

items:

$ref: '#/components/schemas/Trigger'

minItems: 0

pDUSessionChargingInformation:

$ref: '#/components/schemas/PDUSessionChargingInformation'

roamingQBCInformation:

$ref: '#/components/schemas/RoamingQBCInformation'

locationReportingChargingInformation:

$ref: '#/components/schemas/LocationReportingChargingInformation'

required:

- invocationTimeStamp

- invocationSequenceNumber

ChargingNotifyRequest:

type: object

properties:

notificationType:

$ref: '#/components/schemas/NotificationType'

reauthorizationDetails:

type: array

items:

$ref: '#/components/schemas/ReauthorizationDetails'

minItems: 0

required:

- notificationType

ChargingNotifyResponse:

type: object

properties:

invocationResult:

$ref: '#/components/schemas/InvocationResult'

NFIdentification:

type: object

properties:

nFName:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

nFIPv4Address:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

nFIPv6Address:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

nFPLMNID:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

nodeFunctionality:

$ref: '#/components/schemas/NodeFunctionality'

nFFqdn:

type: string

required:

- nodeFunctionality

MultipleUnitUsage:

type: object

properties:

ratingGroup:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatingGroup'

requestedUnit:

$ref: '#/components/schemas/RequestedUnit'

usedUnitContainer:

type: array

items:

$ref: '#/components/schemas/UsedUnitContainer'

minItems: 0

uPFID:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

multihomedPDUAddress:

$ref: '#/components/schemas/PDUAddress'

required:

- ratingGroup

InvocationResult:

type: object

properties:

error:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

failureHandling:

$ref: '#/components/schemas/FailureHandling'

Trigger:

type: object

properties:

triggerType:

$ref: '#/components/schemas/TriggerType'

triggerCategory:

$ref: '#/components/schemas/TriggerCategory'

timeLimit:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

volumeLimit:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

volumeLimit64:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

eventLimit:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

maxNumberOfccc:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

tariffTimeChange:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

required:

- triggerType

- triggerCategory

MultipleUnitInformation:

type: object

properties:

resultCode:

$ref: '#/components/schemas/ResultCode'

ratingGroup:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatingGroup'

grantedUnit:

$ref: '#/components/schemas/GrantedUnit'

triggers:

type: array

items:

$ref: '#/components/schemas/Trigger'

minItems: 0

validityTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

quotaHoldingTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

finalUnitIndication:

$ref: '#/components/schemas/FinalUnitIndication'

timeQuotaThreshold:

type: integer

volumeQuotaThreshold:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

unitQuotaThreshold:

type: integer

uPFID:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

announcementInformation:

$ref: '#/components/schemas/AnnouncementInformation'

required:

- ratingGroup

RequestedUnit:

type: object

properties:

time:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

totalVolume:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

uplinkVolume:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

downlinkVolume:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

serviceSpecificUnits:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

UsedUnitContainer:

type: object

properties:

serviceId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ServiceId'

quotaManagementIndicator:

$ref: '#/components/schemas/QuotaManagementIndicator'

triggers:

type: array

items:

$ref: '#/components/schemas/Trigger'

minItems: 0

triggerTimestamp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

time:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

totalVolume:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

uplinkVolume:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

downlinkVolume:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

serviceSpecificUnits:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

eventTimeStamps:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

minItems: 0

localSequenceNumber:

type: integer

pDUContainerInformation:

$ref: '#/components/schemas/PDUContainerInformation'

nSPAContainerInformation:

$ref: '#/components/schemas/NSPAContainerInformation'

pC5ContainerInformation:

$ref: '#/components/schemas/PC5ContainerInformation'

required:

- localSequenceNumber

GrantedUnit:

type: object

properties:

tariffTimeChange:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

time:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

totalVolume:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

uplinkVolume:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

downlinkVolume:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

serviceSpecificUnits:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

FinalUnitIndication:

type: object

properties:

finalUnitAction:

$ref: '#/components/schemas/FinalUnitAction'

restrictionFilterRule:

$ref: '#/components/schemas/IPFilterRule'

restrictionFilterRuleList:

type: array

items:

$ref: '#/components/schemas/IPFilterRule'

minItems: 1

filterId:

type: string

filterIdList:

type: array

items:

type: string

minItems: 1

redirectServer:

$ref: '#/components/schemas/RedirectServer'

required:

- finalUnitAction

RedirectServer:

type: object

properties:

redirectAddressType:

$ref: '#/components/schemas/RedirectAddressType'

redirectServerAddress:

type: string

required:

- redirectAddressType

- redirectServerAddress

ReauthorizationDetails:

type: object

properties:

serviceId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ServiceId'

ratingGroup:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatingGroup'

quotaManagementIndicator:

$ref: '#/components/schemas/QuotaManagementIndicator'

PDUSessionChargingInformation:

type: object

properties:

chargingId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ChargingId'

homeProvidedChargingId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ChargingId'

userInformation:

$ref: '#/components/schemas/UserInformation'

userLocationinfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

mAPDUNon3GPPUserLocationInfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

non3GPPUserLocationTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

mAPDUNon3GPPUserLocationTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

presenceReportingAreaInformation:

type: object

additionalProperties:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

minProperties: 0

uetimeZone:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

pduSessionInformation:

$ref: '#/components/schemas/PDUSessionInformation'

unitCountInactivityTimer:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'  
 rANSecondaryRATUsageReport:

$ref: '#/components/schemas/RANSecondaryRATUsageReport'

UserInformation:

type: object

properties:

servedGPSI:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

servedPEI:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Pei'

unauthenticatedFlag:

type: boolean

roamerInOut:

$ref: '#/components/schemas/RoamerInOut'

PDUSessionInformation:

type: object

properties:

networkSlicingInfo:

$ref: '#/components/schemas/NetworkSlicingInfo'

pduSessionID:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PduSessionId'

pduType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PduSessionType'

sscMode:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SscMode'

hPlmnId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

servingNetworkFunctionID:

$ref: '#/components/schemas/ServingNetworkFunctionID'

ratType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

mAPDUNon3GPPRATType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

dnnId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

dnnSelectionMode:

$ref: '#/components/schemas/dnnSelectionMode'

chargingCharacteristics:

type: string

pattern: '^[0-9a-fA-F]{1,4}$'

chargingCharacteristicsSelectionMode:

$ref: '#/components/schemas/ChargingCharacteristicsSelectionMode'

startTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

stopTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

3gppPSDataOffStatus:

$ref: '#/components/schemas/3GPPPSDataOffStatus'

sessionStopIndicator:

type: boolean

pduAddress:

$ref: '#/components/schemas/PDUAddress'

diagnostics:

$ref: '#/components/schemas/Diagnostics'

authorizedQoSInformation:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/AuthorizedDefaultQos'

subscribedQoSInformation:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SubscribedDefaultQos'

authorizedSessionAMBR:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ambr'

subscribedSessionAMBR:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ambr'

servingCNPlmnId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

mAPDUSessionInformation:

$ref: '#/components/schemas/MAPDUSessionInformation'

enhancedDiagnostics:

$ref: '#/components/schemas/EnhancedDiagnostics5G'

redundantTransmissionType:

$ref: '#/components/schemas/RedundantTransmissionType'

pDUSessionPairID:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

5GLANTypeService:

$ref: '#/components/schemas/5GLANTypeService'

required:

- pduSessionID

- dnnId

PDUContainerInformation:

type: object

properties:

timeofFirstUsage:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

timeofLastUsage:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

qoSInformation:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/QosData'

qoSCharacteristics:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/QosCharacteristics'

afChargingIdentifier:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ChargingId'

afChargingIdString:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationChargingId'

userLocationInformation:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

uetimeZone:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

rATType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

servingNodeID:

type: array

items:

$ref: '#/components/schemas/ServingNetworkFunctionID'

minItems: 0

presenceReportingAreaInformation:

type: object

additionalProperties:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

minProperties: 0

3gppPSDataOffStatus:

$ref: '#/components/schemas/3GPPPSDataOffStatus'

sponsorIdentity:

type: string

applicationserviceProviderIdentity:

type: string

chargingRuleBaseName:

type: string

mAPDUSteeringFunctionality:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/SteeringFunctionality'

mAPDUSteeringMode:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/SteeringMode'

trafficForwardingWay:

$ref: '#/components/schemas/TrafficForwardingWay'

qosMonitoringReport:

type: array

items:

$ref: '#/components/schemas/QosMonitoringReport'

minItems: 0

NSPAContainerInformation:

type: object

properties:

latency:

type: integer

throughput:

$ref: '#/components/schemas/Throughput'

maximumPacketLossRate:

type: string

serviceExperienceStatisticsData:

$ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/ServiceExperienceInfo'

theNumberOfPDUSessions:

type: integer

theNumberOfRegisteredSubscribers:

type: integer

loadLevel:

$ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/NsiLoadLevelInfo'

NSPAChargingInformation:

type: object

properties:

singleNSSAI:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

required:

- singleNSSAI

NetworkSlicingInfo:

type: object

properties:

sNSSAI:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

required:

- sNSSAI

PDUAddress:

type: object

properties:

pduIPv4Address:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

pduIPv6AddresswithPrefix:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

pduAddressprefixlength:

type: integer

iPv4dynamicAddressFlag:

type: boolean

iPv6dynamicPrefixFlag:

type: boolean

addIpv6AddrPrefixes:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Prefix'

ServingNetworkFunctionID:

type: object

properties:

servingNetworkFunctionInformation:

$ref: '#/components/schemas/NFIdentification'

aMFId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/AmfId'

required:

- servingNetworkFunctionInformation

RoamingQBCInformation:

type: object

properties:

multipleQFIcontainer:

type: array

items:

$ref: '#/components/schemas/MultipleQFIcontainer'

minItems: 0

uPFID:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

roamingChargingProfile:

$ref: '#/components/schemas/RoamingChargingProfile'

MultipleQFIcontainer:

type: object

properties:

triggers:

type: array

items:

$ref: '#/components/schemas/Trigger'

minItems: 0

triggerTimestamp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

time:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

totalVolume:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

uplinkVolume:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

downlinkVolume:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

localSequenceNumber:

type: integer

qFIContainerInformation:

$ref: '#/components/schemas/QFIContainerInformation'

required:

- localSequenceNumber

QFIContainerInformation:

type: object

properties:

qFI:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Qfi'

reportTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

timeofFirstUsage:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

timeofLastUsage:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

qoSInformation:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/QosData'

qoSCharacteristics:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/QosCharacteristics'

userLocationInformation:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

uetimeZone:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

presenceReportingAreaInformation:

type: object

additionalProperties:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

minProperties: 0

rATType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

servingNetworkFunctionID:

type: array

items:

$ref: '#/components/schemas/ServingNetworkFunctionID'

minItems: 0

3gppPSDataOffStatus:

$ref: '#/components/schemas/3GPPPSDataOffStatus'

3gppChargingId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ChargingId'

diagnostics:

$ref: '#/components/schemas/Diagnostics'

enhancedDiagnostics:

type: array

items:

type: string

required:

- reportTime

RoamingChargingProfile:

type: object

properties:

triggers:

type: array

items:

$ref: '#/components/schemas/Trigger'

minItems: 0

partialRecordMethod:

$ref: '#/components/schemas/PartialRecordMethod'

SMSChargingInformation:

type: object

properties:

originatorInfo:

$ref: '#/components/schemas/OriginatorInfo'

recipientInfo:

type: array

items:

$ref: '#/components/schemas/RecipientInfo'

minItems: 0

userEquipmentInfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Pei'

roamerInOut:

$ref: '#/components/schemas/RoamerInOut'

userLocationinfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

uetimeZone:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

rATType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

sMSCAddress:

type: string

sMDataCodingScheme:

type: integer

sMMessageType:

$ref: '#/components/schemas/SMMessageType'

sMReplyPathRequested:

$ref: '#/components/schemas/ReplyPathRequested'

sMUserDataHeader:

type: string

sMStatus:

type: string

pattern: '^[0-7]?[0-9a-fA-F]$'

sMDischargeTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

numberofMessagesSent:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

sMServiceType:

$ref: '#/components/schemas/SMServiceType'

sMSequenceNumber:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

sMSresult:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

submissionTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

sMPriority:

$ref: '#/components/schemas/SMPriority'

messageReference:

type: string

messageSize:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

messageClass:

$ref: '#/components/schemas/MessageClass'

deliveryReportRequested:

$ref: '#/components/schemas/DeliveryReportRequested'

OriginatorInfo:

type: object

properties:

originatorSUPI:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

originatorGPSI:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

originatorOtherAddress:

$ref: '#/components/schemas/SMAddressInfo'

originatorReceivedAddress:

$ref: '#/components/schemas/SMAddressInfo'

originatorSCCPAddress:

type: string

sMOriginatorInterface:

$ref: '#/components/schemas/SMInterface'

sMOriginatorProtocolId:

type: string

RecipientInfo:

type: object

properties:

recipientSUPI:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

recipientGPSI:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

recipientOtherAddress:

$ref: '#/components/schemas/SMAddressInfo'

recipientReceivedAddress:

$ref: '#/components/schemas/SMAddressInfo'

recipientSCCPAddress:

type: string

sMDestinationInterface:

$ref: '#/components/schemas/SMInterface'

sMrecipientProtocolId:

type: string

SMAddressInfo:

type: object

properties:

sMaddressType:

$ref: '#/components/schemas/SMAddressType'

sMaddressData:

type: string

sMaddressDomain:

$ref: '#/components/schemas/SMAddressDomain'

RecipientAddress:

type: object

properties:

recipientAddressInfo:

$ref: '#/components/schemas/SMAddressInfo'

sMaddresseeType:

$ref: '#/components/schemas/SMAddresseeType'

MessageClass:

type: object

properties:

classIdentifier:

$ref: '#/components/schemas/ClassIdentifier'

tokenText:

type: string

SMAddressDomain:

type: object

properties:

domainName:

type: string

3GPPIMSIMCCMNC:

type: string

SMInterface:

type: object

properties:

interfaceId:

type: string

interfaceText:

type: string

interfacePort:

type: string

interfaceType:

$ref: '#/components/schemas/InterfaceType'

RANSecondaryRATUsageReport:

type: object

properties:

rANSecondaryRATType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

qosFlowsUsageReports:

type: array

items:

$ref: '#/components/schemas/QosFlowsUsageReport'

Diagnostics:

type: integer

IPFilterRule:

type: string

QosFlowsUsageReport:

type: object

properties:

qFI:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Qfi'

startTimestamp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

endTimestamp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

uplinkVolume:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

downlinkVolume:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

5GLANTypeService:

type: object

properties:

internalGroupIdentifier:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

NEFChargingInformation:

type: object

properties:

externalIndividualIdentifier:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

externalGroupIdentifier:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ExternalGroupId'

groupIdentifier:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

aPIDirection:

$ref: '#/components/schemas/APIDirection'

aPITargetNetworkFunction:

$ref: '#/components/schemas/NFIdentification'

aPIResultCode:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

aPIName:

type: string

aPIReference:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

aPIContent:

type: string

required:

- aPIName

RegistrationChargingInformation:

type: object

properties:

registrationMessagetype:

$ref: '#/components/schemas/RegistrationMessageType'

userInformation:

$ref: '#/components/schemas/UserInformation'

userLocationinfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

pSCellInformation:

$ref: '#/components/schemas/PSCellInformation'

uetimeZone:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

rATType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

5GMMCapability:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Bytes'

mICOModeIndication:

$ref: '#/components/schemas/MICOModeIndication'

smsIndication:

$ref: '#/components/schemas/SmsIndication'

taiList:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Tai'

minItems: 0

serviceAreaRestriction:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ServiceAreaRestriction'

minItems: 0

requestedNSSAI:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

minItems: 0

allowedNSSAI:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

minItems: 0

rejectedNSSAI:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

minItems: 0

nSSAIMapList:

type: array

items:

$ref: '#/components/schemas/NSSAIMap'

minItems: 0

amfUeNgapId:

type: integer

ranUeNgapId:

type: integer

ranNodeId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GlobalRanNodeId'

required:

- registrationMessagetype

PSCellInformation:

type: object

properties:

nrcgi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ncgi'

ecgi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ecgi'

NSSAIMap:

type: object

properties:

servingSnssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

homeSnssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

required:

- servingSnssai

- homeSnssai

N2ConnectionChargingInformation:

type: object

properties:

n2ConnectionMessageType:

$ref: '#/components/schemas/N2ConnectionMessageType'

userInformation:

$ref: '#/components/schemas/UserInformation'

userLocationinfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

pSCellInformation:

$ref: '#/components/schemas/PSCellInformation'

uetimeZone:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

rATType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

amfUeNgapId:

type: integer

ranUeNgapId:

type: integer

ranNodeId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GlobalRanNodeId'

restrictedRatList:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

minItems: 0

forbiddenAreaList:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Area'

minItems: 0

serviceAreaRestriction:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ServiceAreaRestriction'

minItems: 0

restrictedCnList:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/CoreNetworkType'

minItems: 0

allowedNSSAI:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

minItems: 0

rrcEstCause:

type: string

pattern: '^[0-9a-fA-F]+$'

required:

- n2ConnectionMessageType

LocationReportingChargingInformation:

type: object

properties:

locationReportingMessageType:

$ref: '#/components/schemas/LocationReportingMessageType'

userInformation:

$ref: '#/components/schemas/UserInformation'

userLocationinfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

pSCellInformation:

$ref: '#/components/schemas/PSCellInformation'

uetimeZone:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

rATType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

presenceReportingAreaInformation:

type: object

additionalProperties:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

minProperties: 0

required:

- locationReportingMessageType

N2ConnectionMessageType:

type: integer

LocationReportingMessageType:

type: integer

NSMChargingInformation:

type: object

properties:

managementOperation:

$ref: '#/components/schemas/ManagementOperation'

idNetworkSliceInstance:

type: string

listOfserviceProfileChargingInformation:

type: array

items:

$ref: '#/components/schemas/ServiceProfileChargingInformation'

minItems: 0

managementOperationStatus:

$ref: '#/components/schemas/ManagementOperationStatus'

# To be introduced once the reference to 'generic.yaml is resolved

# managementOperationalState:

# $ref: 'genericNrm.yaml#/components/schemas/OperationalState'

# managementAdministrativeState:

# $ref: 'genericNrm.yaml#/components/schemas/AdministrativeState'

required:

- managementOperation

ServiceProfileChargingInformation:

type: object

properties:

serviceProfileIdentifier:

type: string

sNSSAIList:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

minItems: 0

# To be introduced once the reference to 'nrNrm.yaml is resolved

# sST:

# $ref: 'nrNrm.yaml#/components/schemas/Sst'

latency:

type: integer

availability:

type: number

# To be introduced once the reference to sliceNrm.yaml is resolved

# resourceSharingLevel:

# $ref: 'sliceNrm.yaml#/components/schemas/SharingLevel'

jitter:

type: integer

reliability:

type: string

maxNumberofUEs:

type: integer

coverageArea:

type: string

# To be introduced once the reference to sliceNrm.yaml is resolved

# uEMobilityLevel:

# $ref: 'sliceNrm.yaml#/components/schemas/MobilityLevel'

# delayToleranceIndicator:

# $ref: 'sliceNrm.yaml#/components/schemas/Support'

dLThptPerSlice:

$ref: '#/components/schemas/Throughput'

dLThptPerUE:

$ref: '#/components/schemas/Throughput'

uLThptPerSlice:

$ref: '#/components/schemas/Throughput'

uLThptPerUE:

$ref: '#/components/schemas/Throughput'

maxNumberofPDUsessions:

type: integer

kPIMonitoringList:

type: string

supportedAccessTechnology:

type: integer

# To be introduced once the reference to sliceNrm.yaml is resolved

# v2XCommunicationModeIndicator:

# $ref: 'sliceNrm.yaml#/components/schemas/Support'

addServiceProfileInfo:

type: string

Throughput:

type: object

properties:

guaranteedThpt:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

maximumThpt:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

MAPDUSessionInformation:

type: object

properties:

mAPDUSessionIndicator:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/MaPduIndication'

aTSSSCapability:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/AtsssCapability'

EnhancedDiagnostics5G:

$ref: '#/components/schemas/RanNasCauseList'

RanNasCauseList:

type: array

items:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/RanNasRelCause'

QosMonitoringReport:

description: Contains reporting information on QoS monitoring.

type: object

properties:

ulDelays:

type: array

items:

type: integer

minItems: 0

dlDelays:

type: array

items:

type: integer

minItems: 0

rtDelays:

type: array

items:

type: integer

minItems: 0

AnnouncementInformation:

type: object

properties:

announcementIdentifier:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

announcementReference:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

variableParts:

type: array

items:

$ref: '#/components/schemas/VariablePart'

minItems: 0

timeToPlay:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

quotaConsumptionIndicator:

$ref: '#/components/schemas/QuotaConsumptionIndicator'

announcementPriority:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

playToParty:

$ref: '#/components/schemas/PlayToParty'

announcementPrivacyIndicator:

$ref: '#/components/schemas/AnnouncementPrivacyIndicator'

Language:

$ref: '#/components/schemas/Language'

VariablePart:

type: object

properties:

variablePartType:

$ref: '#/components/schemas/VariablePartType'

variablePartValue:

type: array

items:

type: string

minItems: 1

variablePartOrder:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

required:

- variablePartType

- variablePartValue

Language:

type: string

MMTelChargingInformation:

type: object

properties:

supplementaryServices:

type: array

items:

$ref: '#/components/schemas/SupplementaryService'

minItems: 1

SupplementaryService:

type: object

properties:

supplementaryServiceType:

$ref: '#/components/schemas/SupplementaryServiceType'

supplementaryServiceMode:

$ref: '#/components/schemas/SupplementaryServiceMode'

numberOfDiversions:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

associatedPartyAddress:

type: string

conferenceId:

type: string

participantActionType:

$ref: '#/components/schemas/ParticipantActionType'

changeTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

numberOfParticipants:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

cUGInformation:

$ref: '#/components/schemas/OctetString'

IMSChargingInformation:

type: object

properties:

eventType:

$ref: '#/components/schemas/SIPEventType'

iMSNodeFunctionality:

$ref: '#/components/schemas/IMSNodeFunctionality'

roleOfNode:

$ref: '#/components/schemas/RoleOfIMSNode'

userInformation:

$ref: '#/components/schemas/UserInformation'

userLocationInfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

ueTimeZone:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

3gppPSDataOffStatus:

$ref: '#/components/schemas/3GPPPSDataOffStatus'

isupCause:

$ref: '#/components/schemas/ISUPCause'

controlPlaneAddress:

$ref: '#/components/schemas/IMSAddress'

vlrNumber:

$ref: '#/components/schemas/E164'

mscAddress:

$ref: '#/components/schemas/E164'

userSessionID:

type: string

outgoingSessionID:

type: string

sessionPriority:

$ref: '#/components/schemas/IMSSessionPriority'

callingPartyAddresses:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

minItems: 1

calledPartyAddress:

type: string

numberPortabilityRoutinginformation:

type: string

carrierSelectRoutingInformation:

type: string

alternateChargedPartyAddress:

type: string

requestedPartyAddress:

type: array

items:

type: string

minItems: 1

calledAssertedIdentities:

type: array

items:

type: string

minItems: 1

calledIdentityChanges:

type: array

items:

$ref: '#/components/schemas/CalledIdentityChange'

minItems: 1

associatedURI:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

minItems: 1

timeStamps:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

applicationServerInformation:

type: array

items:

type: string

minItems: 1

interOperatorIdentifier:

type: array

items:

$ref: '#/components/schemas/InterOperatorIdentifier'

minItems: 1

imsChargingIdentifier:

type: string

relatedICID:

type: string

relatedICIDGenerationNode:

type: string

transitIOIList:

type: array

items:

type: string

minItems: 1

earlyMediaDescription:

type: array

items:

$ref: '#/components/schemas/EarlyMediaDescription'

minItems: 1

sdpSessionDescription:

type: array

items:

type: string

minItems: 1

sdpMediaComponent:

type: array

items:

$ref: '#/components/schemas/SDPMediaComponent'

minItems: 1

servedPartyIPAddress:

$ref: '#/components/schemas/IMSAddress'

serverCapabilities:

$ref: '#/components/schemas/ServerCapabilities'

trunkGroupID:

$ref: '#/components/schemas/TrunkGroupID'

bearerService:

type: string

imsServiceId:

type: string

messageBodies:

type: array

items:

$ref: '#/components/schemas/MessageBody'

minItems: 1

accessNetworkInformation:

type: array

items:

type: string

minItems: 1

additionalAccessNetworkInformation:

type: string

cellularNetworkInformation:

type: string

accessTransferInformation:

type: array

items:

$ref: '#/components/schemas/AccessTransferInformation'

minItems: 1

accessNetworkInfoChange:

type: array

items:

$ref: '#/components/schemas/AccessNetworkInfoChange'

minItems: 1

imsCommunicationServiceID:

type: string

imsApplicationReferenceID:

type: string

causeCode:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

reasonHeader:

type: array

items:

type: string

minItems: 1

initialIMSChargingIdentifier:

type: string

nniInformation:

type: array

items:

$ref: '#/components/schemas/NNIInformation'

minItems: 1

fromAddress:

type: string

imsEmergencyIndication:

type: boolean

imsVisitedNetworkIdentifier:

type: string

sipRouteHeaderReceived:

type: string

sipRouteHeaderTransmitted:

type: string

tadIdentifier:

$ref: '#/components/schemas/TADIdentifier'

feIdentifierList:

type: string

EdgeInfrastructureUsageChargingInformation:

type: object

properties:

meanVirtualCPUUsage:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

meanVirtualMemoryUsage:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

meanVirtualDiskUsage:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

durationStartTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

durationEndTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

EASDeploymentChargingInformation:

type: object

properties:

# To be introduced once the reference to EdgeNrm.yaml is resolved

# eEASDeploymentRequirements:

# $ref: 'EdgeNrm.yaml#/components/schemas/EASRequirements'

lCMStartTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

lCMEndTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

PC5ContainerInformation:

type: object

properties:

coverageInfoList:

type: array

items:

$ref: '#/components/schemas/CoverageInfo'

radioParameterSetInfoList:

type: array

items:

$ref: '#/components/schemas/RadioParameterSetInfo'

transmitterInfoList:

type: array

items:

$ref: '#/components/schemas/TransmitterInfo'

minItems: 0

timeOfFirst Transmission:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

timeOfFirst Reception:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

CoverageInfo:

type: object

properties:

coverageStatus:

type: boolean

changeTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

locationInfo:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

minItems: 0

RadioParameterSetInfo:

type: object

properties:

radioParameterSetValues:

type: array

items:

$ref: '#/components/schemas/OctetString'

minItems: 0

changeTimestamp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

TransmitterInfo:

type: object

properties:

proseSourceIPAddress:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/IpAddr'

proseSourceL2Id:

type: string

ProseChargingInformation:

type: object

properties:

announcingPlmnID:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

announcingUeHplmnIdentifier:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

announcingUeVplmnIdentifier:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

monitoringUeHplmnIdentifier:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

monitoringUeVplmnIdentifier:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

discovererUeHplmnIdentifier:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

discovererUeVplmnIdentifier:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

discovereeUeHplmnIdentifier:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

discovereeUeVplmnIdentifier:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

monitoredPlmnIdentifier:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

proseApplicationID:

type: string

ApplicationId:

type: string

applicationSpecificDataList:

type: array

items:

type: string

minItems: 0

proseFunctionality:

$ref: '#/components/schemas/ProseFunctionality'

proseEventType:

$ref: '#/components/schemas/ProseEventType'

directDiscoveryModel:

$ref: '#/components/schemas/DirectDiscoveryModel'

validityPeriod:

type: integer

roleOfUE:

$ref: '#/components/schemas/RoleOfUE'

proseRequestTimestamp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

pC3ProtocolCause:

type: integer

monitoringUEIdentifier:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

requestedPLMNIdentifier:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

timeWindow:

type: integer

rangeClass:

$ref: '#/components/schemas/RangeClass'

proximityAlertIndication:

type: boolean

proximityAlertTimestamp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

proximityCancellationTimestamp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

relayIPAddress:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/IpAddr'

proseUEToNetworkRelayUEID :

type: string

proseDestinationLayer2ID:

type: string

pFIContainerInformation:

type: array

items:

$ref: '#/components/schemas/PFIContainerInformation'

minItems: 0

transmissionDataContainer:

type: array

items:

$ref: '#/components/schemas/PC5DataContainer'

minItems: 0

receptionDataContainer:

type: array

items:

$ref: '#/components/schemas/PC5DataContainer'

minItems: 0

required:

- aPIName

PFIContainerInformation:

type: object

properties:

pFI:

type: string

reportTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

timeofFirstUsage:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

timeofLastUsage:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

qoSInformation:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/QosData'

qoSCharacteristics:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/QosCharacteristics'

userLocationInformation:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

uetimeZone:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

presenceReportingAreaInformation:

type: object

additionalProperties:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

minProperties: 0

PC5DataContainer:

type: object

properties:

localSequenceNumber:

type: string

changeTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

coverageStatus:

type: boolean

userLocationInformation:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

dataVolume:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

changeCondition:

type: string

radioResourcesId:

$ref: '#/components/schemas/RadioResourcesId'

radioFrequency:

type: string

pC5RadioTechnology:

type: string

OctetString:

type: string

pattern: '^[0-9a-fA-F]+$'

E164:

type: string

pattern: '^[0-9a-fA-F]+$'

IMSAddress:

type: object

properties:

ipv4Addr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

ipv6Addr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

e164:

$ref: '#/components/schemas/E164'

anyOf:

- required: [ ipv4Addr ]

- required: [ ipv6Addr ]

- required: [ e164 ]

ServingNodeAddress:

type: object

properties:

ipv4Addr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

ipv6Addr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

anyOf:

- required: [ ipv4Addr ]

- required: [ ipv6Addr ]

SIPEventType:

type: object

properties:

sIPMethod:

type: string

eventHeader:

type: string

expiresHeader:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

ISUPCause:

type: object

properties:

iSUPCauseLocation:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

iSUPCauseValue:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

iSUPCauseDiagnostics:

$ref: '#/components/schemas/OctetString'

CalledIdentityChange:

type: object

properties:

calledIdentity:

type: string

changeTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

InterOperatorIdentifier:

type: object

properties:

originatingIOI:

type: string

terminatingIOI:

type: string

EarlyMediaDescription:

type: object

properties:

sDPTimeStamps:

$ref: '#/components/schemas/SDPTimeStamps'

sDPMediaComponent:

type: array

items:

$ref: '#/components/schemas/SDPMediaComponent'

minItems: 0

sDPSessionDescription:

type: array

items:

type: string

minItems: 0

SDPTimeStamps:

type: object

properties:

sDPOfferTimestamp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

sDPAnswerTimestamp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

SDPMediaComponent:

type: object

properties:

sDPMediaName:

type: string

SDPMediaDescription:

type: array

items:

type: string

minItems: 0

localGWInsertedIndication:

type: boolean

ipRealmDefaultIndication:

type: boolean

transcoderInsertedIndication:

type: boolean

mediaInitiatorFlag:

$ref: '#/components/schemas/MediaInitiatorFlag'

mediaInitiatorParty:

type: string

threeGPPChargingId:

$ref: '#/components/schemas/OctetString'

accessNetworkChargingIdentifierValue:

$ref: '#/components/schemas/OctetString'

sDPType:

$ref: '#/components/schemas/SDPType'

ServerCapabilities:

type: object

properties:

mandatoryCapability:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

minItems: 0

optionalCapability :

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

minItems: 0

serverName:

type: array

items:

type: string

minItems: 0

TrunkGroupID:

type: object

properties:

incomingTrunkGroupID:

type: string

outgoingTrunkGroupID:

type: string

MessageBody:

type: object

properties:

contentType:

type: string

contentLength:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

contentDisposition:

type: string

originator:

$ref: '#/components/schemas/OriginatorPartyType'

required:

- contentType

- contentLength

AccessTransferInformation:

type: object

properties:

accessTransferType:

$ref: '#/components/schemas/AccessTransferType'

accessNetworkInformation:

type: array

items:

$ref: '#/components/schemas/OctetString'

minItems: 0

cellularNetworkInformation:

$ref: '#/components/schemas/OctetString'

interUETransfer:

$ref: '#/components/schemas/UETransferType'

userEquipmentInfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Pei'

instanceId:

type: string

relatedIMSChargingIdentifier:

type: string

relatedIMSChargingIdentifierNode:

$ref: '#/components/schemas/IMSAddress'

changeTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

AccessNetworkInfoChange:

type: object

properties:

accessNetworkInformation:

type: array

items:

$ref: '#/components/schemas/OctetString'

minItems: 0

cellularNetworkInformation:

$ref: '#/components/schemas/OctetString'

changeTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

NNIInformation:

type: object

properties:

sessionDirection:

$ref: '#/components/schemas/NNISessionDirection'

nNIType:

$ref: '#/components/schemas/NNIType'

relationshipMode:

$ref: '#/components/schemas/NNIRelationshipMode'

neighbourNodeAddress:

$ref: '#/components/schemas/IMSAddress'

NotificationType:

anyOf:

- type: string

enum:

- REAUTHORIZATION

- ABORT\_CHARGING

- type: string

NodeFunctionality:

anyOf:

- type: string

enum:

- AMF

- SMF

- SMS

- PGW\_C\_SMF

- NEFF # Included for backwards compatibility, shall not be used

- SGW

- I\_SMF

- ePDG

- CEF

- NEF

- MnS\_Producer

- SGSN

- type: string

ChargingCharacteristicsSelectionMode:

anyOf:

- type: string

enum:

- HOME\_DEFAULT

- ROAMING\_DEFAULT

- VISITING\_DEFAULT

- type: string

TriggerType:

anyOf:

- type: string

enum:

- QUOTA\_THRESHOLD

- QHT

- FINAL

- QUOTA\_EXHAUSTED

- VALIDITY\_TIME

- OTHER\_QUOTA\_TYPE

- FORCED\_REAUTHORISATION

- UNUSED\_QUOTA\_TIMER # Included for backwards compatibility, shall not be used

- UNIT\_COUNT\_INACTIVITY\_TIMER

- ABNORMAL\_RELEASE

- QOS\_CHANGE

- VOLUME\_LIMIT

- TIME\_LIMIT

- EVENT\_LIMIT

- PLMN\_CHANGE

- USER\_LOCATION\_CHANGE

- RAT\_CHANGE

- SESSION\_AMBR\_CHANGE

- UE\_TIMEZONE\_CHANGE

- TARIFF\_TIME\_CHANGE

- MAX\_NUMBER\_OF\_CHANGES\_IN\_CHARGING\_CONDITIONS

- MANAGEMENT\_INTERVENTION

- CHANGE\_OF\_UE\_PRESENCE\_IN\_PRESENCE\_REPORTING\_AREA

- CHANGE\_OF\_3GPP\_PS\_DATA\_OFF\_STATUS

- SERVING\_NODE\_CHANGE

- REMOVAL\_OF\_UPF

- ADDITION\_OF\_UPF

- INSERTION\_OF\_ISMF

- REMOVAL\_OF\_ISMF

- CHANGE\_OF\_ISMF

- START\_OF\_SERVICE\_DATA\_FLOW

- ECGI\_CHANGE

- TAI\_CHANGE

- HANDOVER\_CANCEL

- HANDOVER\_START

- HANDOVER\_COMPLETE

- GFBR\_GUARANTEED\_STATUS\_CHANGE

- ADDITION\_OF\_ACCESS

- REMOVAL\_OF\_ACCESS

- START\_OF\_SDF\_ADDITIONAL\_ACCESS

- REDUNDANT\_TRANSMISSION\_CHANGE

- CGI\_SAI\_CHANGE

- RAI\_CHANGE

- type: string

FinalUnitAction:

anyOf:

- type: string

enum:

- TERMINATE

- REDIRECT

- RESTRICT\_ACCESS

- type: string

RedirectAddressType:

anyOf:

- type: string

enum:

- IPV4

- IPV6

- URL

- URI

- type: string

TriggerCategory:

anyOf:

- type: string

enum:

- IMMEDIATE\_REPORT

- DEFERRED\_REPORT

- type: string

QuotaManagementIndicator:

anyOf:

- type: string

enum:

- ONLINE\_CHARGING

- OFFLINE\_CHARGING

- QUOTA\_MANAGEMENT\_SUSPENDED

- type: string

FailureHandling:

anyOf:

- type: string

enum:

- TERMINATE

- CONTINUE

- RETRY\_AND\_TERMINATE

- type: string

SessionFailover:

anyOf:

- type: string

enum:

- FAILOVER\_NOT\_SUPPORTED

- FAILOVER\_SUPPORTED

- type: string

3GPPPSDataOffStatus:

anyOf:

- type: string

enum:

- ACTIVE

- INACTIVE

- type: string

ResultCode:

anyOf:

- type: string

enum:

- SUCCESS

- END\_USER\_SERVICE\_DENIED

- QUOTA\_MANAGEMENT\_NOT\_APPLICABLE

- QUOTA\_LIMIT\_REACHED

- END\_USER\_SERVICE\_REJECTED

- USER\_UNKNOWN

- RATING\_FAILED

- QUOTA\_MANAGEMENT

- type: string

PartialRecordMethod:

anyOf:

- type: string

enum:

- DEFAULT

- INDIVIDUAL

- type: string

RoamerInOut:

anyOf:

- type: string

enum:

- IN\_BOUND

- OUT\_BOUND

- type: string

SMMessageType:

anyOf:

- type: string

enum:

- SUBMISSION

- DELIVERY\_REPORT

- SM\_SERVICE\_REQUEST

- DELIVERY

- type: string

SMPriority:

anyOf:

- type: string

enum:

- LOW

- NORMAL

- HIGH

- type: string

DeliveryReportRequested:

anyOf:

- type: string

enum:

- YES

- NO

- type: string

InterfaceType:

anyOf:

- type: string

enum:

- UNKNOWN

- MOBILE\_ORIGINATING

- MOBILE\_TERMINATING

- APPLICATION\_ORIGINATING

- APPLICATION\_TERMINATING

- type: string

ClassIdentifier:

anyOf:

- type: string

enum:

- PERSONAL

- ADVERTISEMENT

- INFORMATIONAL

- AUTO

- type: string

SMAddressType:

anyOf:

- type: string

enum:

- EMAIL\_ADDRESS

- MSISDN

- IPV4\_ADDRESS

- IPV6\_ADDRESS

- NUMERIC\_SHORTCODE

- ALPHANUMERIC\_SHORTCODE

- OTHER

- IMSI

- type: string

SMAddresseeType:

anyOf:

- type: string

enum:

- TO

- CC

- BCC

- type: string

SMServiceType:

anyOf:

- type: string

enum:

- VAS4SMS\_SHORT\_MESSAGE\_CONTENT\_PROCESSING

- VAS4SMS\_SHORT\_MESSAGE\_FORWARDING

- VAS4SMS\_SHORT\_MESSAGE\_FORWARDING\_MULTIPLE\_SUBSCRIPTIONS

- VAS4SMS\_SHORT\_MESSAGE\_FILTERING

- VAS4SMS\_SHORT\_MESSAGE\_RECEIPT

- VAS4SMS\_SHORT\_MESSAGE\_NETWORK\_STORAGE

- VAS4SMS\_SHORT\_MESSAGE\_TO\_MULTIPLE\_DESTINATIONS

- VAS4SMS\_SHORT\_MESSAGE\_VIRTUAL\_PRIVATE\_NETWORK(VPN)

- VAS4SMS\_SHORT\_MESSAGE\_AUTO\_REPLY

- VAS4SMS\_SHORT\_MESSAGE\_PERSONAL\_SIGNATURE

- VAS4SMS\_SHORT\_MESSAGE\_DEFERRED\_DELIVERY

- type: string

ReplyPathRequested:

anyOf:

- type: string

enum:

- NO\_REPLY\_PATH\_SET

- REPLY\_PATH\_SET

- type: string

oneTimeEventType:

anyOf:

- type: string

enum:

- IEC

- PEC

- type: string

dnnSelectionMode:

anyOf:

- type: string

enum:

- VERIFIED

- UE\_DNN\_NOT\_VERIFIED

- NW\_DNN\_NOT\_VERIFIED

- type: string

APIDirection:

anyOf:

- type: string

enum:

- INVOCATION

- NOTIFICATION

- type: string

RegistrationMessageType:

anyOf:

- type: string

enum:

- INITIAL

- MOBILITY

- PERIODIC

- EMERGENCY

- DEREGISTRATION

- type: string

MICOModeIndication:

anyOf:

- type: string

enum:

- MICO\_MODE

- NO\_MICO\_MODE

- type: string

SmsIndication:

anyOf:

- type: string

enum:

- SMS\_SUPPORTED

- SMS\_NOT\_SUPPORTED

- type: string

ManagementOperation:

anyOf:

- type: string

enum:

- CreateMOI

- ModifyMOIAttributes

- DeleteMOI

- type: string

ManagementOperationStatus:

anyOf:

- type: string

enum:

- OPERATION\_SUCCEEDED

- OPERATION\_FAILED

- type: string

RedundantTransmissionType:

anyOf:

- type: string

enum:

- NON\_TRANSMISSION

- END\_TO\_END\_USER\_PLANE\_PATHS

- N3/N9

- TRANSPORT\_LAYER

- type: string

VariablePartType:

anyOf:

- type: string

enum:

- INTEGER

- NUMBER

- TIME

- DATE

- CURRENCY

- type: string

QuotaConsumptionIndicator:

anyOf:

- type: string

enum:

- QUOTA\_NOT\_USED

- QUOTA\_IS\_USED

- type: string

PlayToParty:

anyOf:

- type: string

enum:

- SERVED

- REMOTE

- type: string

AnnouncementPrivacyIndicator:

anyOf:

- type: string

enum:

- NOT\_PRIVATE

- PRIVATE

- type: string

SupplementaryServiceType:

anyOf:

- type: string

enum:

- OIP

- OIR

- TIP

- TIR

- HOLD

- CB

- CDIV

- CW

- MWI

- CONF

- FA

- CCBS

- CCNR

- MCID

- CAT

- CUG

- PNM

- CRS

- ECT

- type: string

SupplementaryServiceMode:

anyOf:

- type: string

enum:

- CFU

- CFB

- CFNR

- CFNL

- CD

- CFNRC

- ICB

- OCB

- ACR

- BLIND\_TRANFER

- CONSULTATIVE\_TRANFER

- type: string

ParticipantActionType:

anyOf:

- type: string

enum:

- CREATE

- JOIN

- INVITE\_INTO

- QUIT

- type: string

TrafficForwardingWay:

anyOf:

- type: string

enum:

- N6

- N19

- LOCAL\_SWITCH

- type: string

IMSNodeFunctionality:

anyOf:

- type: string

enum:

- S\_CSCF

- P\_CSCF

- I\_CSCF

- MRFC

- MGCF

- BGCF

- AS

- IBCF

- S-GW

- P-GW

- HSGW

- E-CSCF

- MME

- TRF

- TF

- ATCF

- PROXY

- EPDG

- TDF

- TWAG

- SCEF

- IWK\_SCEF

- type: string

RoleOfIMSNode:

anyOf:

- type: string

enum:

- ORIGINATING

- TERMINATING

- FORWARDING

- type: string

IMSSessionPriority:

anyOf:

- type: string

enum:

- PRIORITY\_0

- PRIORITY\_1

- PRIORITY\_2

- PRIORITY\_3

- PRIORITY\_4

- type: string

MediaInitiatorFlag:

anyOf:

- type: string

enum:

- CALLED\_PARTY

- CALLING\_PARTY

- UNKNOWN

- type: string

SDPType:

anyOf:

- type: string

enum:

- OFFER

- ANSWER

- type: string

OriginatorPartyType:

anyOf:

- type: string

enum:

- CALLING

- CALLED

- type: string

AccessTransferType:

anyOf:

- type: string

enum:

- PS\_TO\_CS

- CS\_TO\_PS

- PS\_TO\_PS

- CS\_TO\_CS

- type: string

UETransferType:

anyOf:

- type: string

enum:

- INTRA\_UE

- INTER\_UE

- type: string

NNISessionDirection:

anyOf:

- type: string

enum:

- INBOUND

- OUTBOUND

- type: string

NNIType:

anyOf:

- type: string

enum:

- NON\_ROAMING

- ROAMING\_NO\_LOOPBACK

- ROAMING\_LOOPBACK

- type: string

NNIRelationshipMode:

anyOf:

- type: string

enum:

- TRUSTED

- NON\_TRUSTED

- type: string

TADIdentifier:

anyOf:

- type: string

enum:

- CS

- PS

- type: string

ProseFunctionality:

anyOf:

- type: string

enum:

- DIRECT\_DISCOVERY

- DIRECT\_COMMUNICATION

- type: string

ProseEventType:

anyOf:

- type: string

enum:

- ANNOUNCING

- MONITORING

- MATCH\_REPORT

- type: string

DirectDiscoveryModel:

anyOf:

- type: string

enum:

- MODEL\_A

- MODEL\_B

- type: string

RoleOfUE:

anyOf:

- type: string

enum:

- ANNOUNCING\_UE

- MONITORING\_UE

- REQUESTOR\_UE

- REQUESTED\_UE

- type: string

RangeClass:

anyOf:

- type: string

enum:

- RESERVED

- 50\_METER

- 100\_METER

- 200\_METER

- 500\_METER

- 1000\_METER

- UNUSED

- type: string

RadioResourcesId:

anyOf:

- type: string

enum:

- OPERATOR\_PROVIDED

- CONFIGURED

- type: string

|  |
| --- |
| **End of change** |