**3GPP TSG-SA WG6 Meeting #42-bis-e S6-21xxxx**

**e-meeting, 12th – 20th April 2021 (revision of S6-210928)**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **23.286** | **CR** | **0057** | **rev** | **1** | **Current version:** | **17.1.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Alignment of Get V2X UE service discovery response with request |
|  |  |
| ***Source to WG:*** | Huawei, Hisilicon |
| ***Source to TSG:*** | S6 |
|  |  |
| ***Work item code:*** | eV2XAPP |  | ***Date:*** | 2021-04-05 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | The Get V2X UE service discovery request is enabled between VAE servers as specified in clause 9.9.2.1. So, correspondingly Get V2X.UE service discovery response should be aligned. |
|  |  |
| ***Summary of change:*** | Update the information flow for Get V2X.UE service discovery response. |
|  |  |
| ***Consequences if not approved:*** | Request-Response messages will not be aligned. |
|  |  |
| ***Clauses affected:*** | 9.9.2.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **N** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **N** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **N** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

\* \* \* First Change \* \* \* \*

#### 9.9.2.2 Get V2X UE service discovery response

Table 9.9.2.2-1 describes the information flow get V2X UE service discovery response from the VAE server to the VAE client and between VAE servers.

Table 9.9.2.2-1: Get V2X UE service discovery response

|  |  |  |
| --- | --- | --- |
| Information element | Status | Description |
| Result | M | Indicates the success or failure of getting the service discovery information |
| V2X UE service discovery information  | O (NOTE) | The V2X UE service discovery data includes:- List of available V2X services identified by V2X service IDs - Mapping of the V2X services to V2X application server address as specified in 3GPP TS 23.285 [5] |
| NOTE: If the Result information element indicates failure then V2X UE service discovery information element is not included. |