**3GPP TSG-SA WG6 Meeting #43 S6-211xxx**

**e-meeting, 24th May – 2nd June 2021 (revision of S6-211154)**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **23.282** | **CR** | **0276**  | **rev** | **1** | **Current version:** | **17.6.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | EN resolutions in clause 6 |
|  |  |
| ***Source to WG:*** | at&t |
| ***Source to TSG:*** | S6 |
|  |  |
| ***Work item code:*** | eMCData3 |  | ***Date:*** | 05-17-2021 |
|  |  |  |  |  |
| ***Category:*** | F |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | Provide resolutions to the EN in clause 6 |
|  |  |
| ***Summary of change:*** | 1. The EN in 6.6.1 has been realized in the recent additions in 7.5.2.2.4 for file upload procedure and in S6-210961, approved in SA6 #42 e-meeting, for file download procedure. It is removed.
 |
|  |  |
| ***Consequences if not approved:*** | It could confuse the readers and the stage 3 development. |
|  |  |
| ***Clauses affected:*** | 6.6.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

\* \* \* First Change \* \* \* \*

### 6.6.1 On-network functional model

Figure 6.6.1-1 shows the application plane functional model for file distribution.



Figure 6.6.1-1: Application plane functional model for file distribution

In the model shown in figure 6.6.1-1, the following apply:

- MCData-FD-1 reference point is primarily used for MCData application signalling for establishing a session in support of MCData file distribution. Secondarily, MCData-FD-1 reference point is also used for both uplink and downlink unicast data (e.g., URL associated to file, file download completed report).

- MCData-FD-2 reference point carries uplink and downlink unicast file data between the FD functions of the MCData server and the MCData UE.

- MCData-FD-3 reference point carries downlink multicast file data from the FD function of the MCData server to the FD function of the MCData UE.

- MCData-FD-4 reference point carries uplink and downlink unicast file data between the media storage function of the MCData Content server and the media storage client of the MCData UE.

- MCData-FD-5 reference point supports the MCData server to access the stored files in the MCData content server for certain file distribution functions, such as retrieval a file to be distributed through multicast etc. This reference points also supports any necessary operational requirements.

- MCData-FD-7 reference point supports the upload and download of file data between MCData content server and MCData message store.

NOTE: The security aspects of MCData-FD-5 and MCData-FD-7 reference points are the responsibility of SA3 and thus outside the scope of the present document.

\* \* \* Next Change \* \* \* \*