**3GPP TSG-SA WG6 Meeting #44 S6-211697Rev2**

**e-meeting, 12th – 20th July 2021 (revision of S6-21xxxx)**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** | **295** | **rev** | **1** | **Current version:** | **17.7.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  |  Corrections to Location Information table in 10.9.2.3 |
|  |  |
| ***Source to WG:*** | at&t |
| ***Source to TSG:*** | S6 |
|  |  |
| ***Work item code:*** | Enh3MCPTT |  | ***Date:*** | 2021-07-06 |
|  |  |  |  |  |
| ***Category:*** | F |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | The IEs in tables in 10.9.2.3 need corrections. |
|  |  |
| ***Summary of change:*** | 1. When a location information request is sent from the LMS to LMC, the the MC service ID is used to identify the MC service user whose location is being requested.
2. The second MC service ID IE is changed to the identity of the requesting MC service user to avoid duplicating to the first MC service ID on the table.
3. FA IE is not used and thus removed.
4. The second 10.9.2.3-2 table should be 10.9.2.3-3.
 |
|  |  |
| ***Consequences if not approved:*** | Will give wrong guidance to stage 3 development. |
|  |  |
| ***Clauses affected:*** | 10.9.2.3 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

\* \* First Change \* \* \*

#### 10.9.2.3 Location information request

Tables 10.9.2.3-1, 10.9.2.3-2 and 10.9.2.3-3 describe the information flow from the MC service server to the location management server and from the location management server to the location management client and from location management client to location management server respectively for requesting an immediate location information report.

Table 10.9.2.3-1: Location information request (MC service server to location management server)

|  |  |  |
| --- | --- | --- |
| Information element | Status | Description |
| MC service ID list | O(see NOTE) | List of MC service users whose location information is requested |
| Functional alias | O(see NOTE) | Location information of MC service users who have activated this functional alias is requested |
| NOTE: Either the MC service ID list or the functional alias must be present. |

Table 10.9.2.3-2: Location information request (Location management server to location management client)

|  |  |  |
| --- | --- | --- |
| Information element | Status | Description |
| MC service ID | M | Identity of MC service user whose location information is requested |
| MC service ID | O | Identity of the requesting MC service user (e.g. MCPTT ID, MCVideo ID, MCData ID) |
|  |  |  |

Table 10.9.2.3-3: Location information request (Location management client to location management server)

|  |  |  |
| --- | --- | --- |
| Information element | Status | Description |
| MC service ID | M | Identity of the requesting authorized MC service user (e.g. MCPTT ID, MCVideo ID, MCData ID) |
| MC service ID list | O(see NOTE) | List of MC service users whose location information is requested |
| Functional alias | O | Functional alias that corresponds to the requesting MC service user (e.g. MCPTT ID, MCVideo ID, MCData ID) |
| Functional alias | O(see NOTE) | Functional alias that corresponds to the requested MC service user(s) (e.g. MCPTT ID, MCVideo ID, MCData ID) |
| NOTE: Either the MC service ID list or the functional alias must be present. |