**3GPP TSG-CT WG3 Meeting #136 *C3-244244***

**Maastricht, NL, 19 - 23 August, 2024 (Revision of C3-24xxxx)**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** |  | **rev** |  | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Enhance Roaming SMS |
|  |  |
| ***Source to WG:*** | Ericsson, Nokia, Huawei |
| ***Source to TSG:*** | CT3 |
|  |  |
| ***Work item code:*** | TEI19\_RVAS |  | ***Date:*** | 2024-08-08 |
|  |  |  |  |  |
| ***Category:*** | B |  | ***Release:*** | Rel-19 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | As specified in TS 23.502 clause 4.15.3.1:*NOTE 2: Roaming status means whether the UE is in HPLMN or VPLMN based on the most recently received registration state in the UDM. Following parameters may be included as part of event report:**1) Equipment identifier (PEI)* *2) Subscription identifiers (e.g., GPSI)*  *This event can be used by AF to implement certain capabilities, for e.g., send welcome SMS to subscriber, etc.*The PEI and GPSI shall be added into Roaming Status Report to support welcome SMS. |
|  |  |
| ***Summary of change:*** | Add the PEI and GPSI in the Roaming Status Report supported by new feature. |
|  |  |
| ***Consequences if not approved:*** | Stage 2 requirements on support of welcome SMS is not addressed. |
|  |  |
| ***Clauses affected:*** | 5.3.2.1.1, 5.3.2.3.2, 5.3.4, A.3 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This CR introduces a backwards compatible feature in the OpenAPI file of MonitoringEvent API. |
|  |  |
| ***This CR's revision history:*** |  |

\*\*\* 1st Change \*\*\*

##### 5.3.2.1.1 Introduction

This clause defines data structures to be used in resource representations, including subscription resources.

Table 5.3.2.1.1-1 specifies data types re-used by the MonitoringEvent API from other specifications, including a reference to their respective specifications and when needed, a short description of their use within the MonitoringEvent API.

Table 5.3.2.1.1-1: MonitoringEvent API re-used Data Types

|  |  |  |
| --- | --- | --- |
| Data type | Reference | Comments |
| 2DRelativeLocation | 3GPP TS 29.572 [42] | Represents 2D local co-ordinates with origin corresponding to another known point. |
| 3DRelativeLocation | 3GPP TS 29.572 [42] | Represents 3D local co-ordinates with origin corresponding to another known point. |
| AccuracyFulfilmentIndicator | 3GPP TS 29.572 [42] | The indication whether the obtained location estimate satisfies the requested QoS or not. |
| AgeOfLocationEstimate | 3GPP TS 29.572 [42] | Age of the location estimate for change of location type or motion type of Location deferred report. |
| Angle | 3GPP TS 29.572 [42] | Indicates value of angle |
| ApplicationlayerId | 3GPP TS 29.571 [45] | Represents the Application Layer ID. |
| CivicAddress | 3GPP TS 29.572 [42] | Civic address. |
| CodeWord | 3GPP TS 29.515 [65] | Code word. |
| DddTrafficDescriptor | 3GPP TS 29.571 [45] | Traffic Descriptor of source of downlink data. |
| DlDataDeliveryStatus | 3GPP TS 29.571 [45] | Traffic Descriptor of source of downlink data notifications. |
| Dnn | 3GPP TS 29.571 [45] | Identifies a DNN. |
| Fqdn | 3GPP TS 29.571 [45] | Identifies a FQDN. |
| GeographicArea | 3GPP TS 29.572 [42] | Identifies the geographical information of the user(s). |
| Gpsi | 3GPP TS 29.571 [45] | Represents a GPSI. |
| IpAddr | 3GPP TS 29.571 [45] | UE IP Address. |
| LdrType | 3GPP TS 29.572 [42] | Location deferred requested event type. |
| LinearDistance | 3GPP TS 29.572 [42] | This IE shall be present and set to true if a location estimate is required for motion event report. |
| LocationQoS | 3GPP TS 29.572 [42] | Requested location QoS. |
| MacAddr48 | 3GPP TS 29.571 [45] | MAC Address. |
| MinorLocationQoS | 3GPP TS 29.572 [42] | Minor Location QoS. |
| NetworkAreaInfo | 3GPP TS 29.554 [50] | Identifies a network area information. |
| VelocityRequested | 3GPP TS 29.572 [42] | Velocity of the target UE requested. |
| PatchItem | 3GPP TS 29.571 [45] | Contains the list of changes to be made to a resource according to the JSON PATCH format specified in IETF RFC 6902 [67]. |
| PduSessionInformation | 3GPP TS 29.523 [70] | Represents PDU session identification information. |
| Pei | 3GPP TS 29.571 [45] | Represents a PEI. |
| PositioningMethod | 3GPP TS 29.572 [42] | Identifies the positioning method used to obtain the location estimate of the UE. |
| RangeDirection | 3GPP TS 29.572 [42] | Represents the range and direction between two points. |
| RangingSlResult | 3GPP TS 29.572 [42] | Represents the requested result type for ranging and sidelink positioning |
| RelatedUe | 3GPP TS 29.572 [42] | Represents information on the related UE for ranging and sidelink positioning |
| SACEventStatus | 3GPP TS 29.571 [45] | Contains the network slice status information related to network slice admission control. |
| SACInfo | 3GPP TS 29.571 [45] | Represents network slice admission control information to control the triggering of notifications or convey network slice status information. |
| Snssai | 3GPP TS 29.571 [45] | Contains a S-NSSAI. |
| SupportedFeatures | 3GPP TS 29.571 [45] | Used to negotiate the applicability of the optional features defined in table 5.3.4-1. |
| ServiceIdentiy | 3GPP TS 29.515 [65] | Service identity. |
| SupportedGADShapes | 3GPP TS 29.572 [42] | Supported Geographical Area Description shapes. |
| TrafficInformation | 3GPP TS 29.520 [73] | Traffic information including UL/DL data rate and/or Traffic volume. |
| UcPurpose | 3GPP TS 29.503 [63] | Represents the purpose of a user consent. |
| Uinteger | 3GPP TS 29.571 [45] | Represents an unsigned Integer. |
| Uncertainty | 3GPP TS 29.572 [42] | Indicates value of uncertainty. |
| Uri | 5.2.1.3.2 | Represents a URI. |
| UserLocation | 3GPP TS 29.571 [6] | Represents a user location. |
| VelocityEstimate | 3GPP TS 29.572 [42] | UE velocity, if requested and available. |

Table 5.3.2.1.1-2 specifies the data types defined for the MonitoringEvent API.

Table 5.3.2.1.1-2: MonitoringEvent API specific Data Types

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Clause defined | Description | Applicability |
| Accuracy | 5.3.2.4.7 | Represents a desired granularity of accuracy for the requested location information. | Location\_notification,eLCS, EDGEAPP |
| ApiCapabilityInfo | 5.3.2.3.9 | Represents the availability information of supported API. | API\_support\_capability\_notification |
| AppliedParameterConfiguration | 5.3.2.3.8 | Represents the parameter configuration applied in the network. | Enhanced\_param\_config |
| AssociationType | 5.3.2.4.6 | Represents an IMEI or IMEISV to IMSI association. | Change\_of\_IMSI\_IMEI\_association\_notification |
| ConsentRevocNotif | 5.3.2.3.12 | Represents the user consent revocation information conveyed in a user consent revocation notification. | UserConsentRevocation |
| ConsentRevoked | 5.3.2.3.13 | Represents the information related to revoked user consent(s). | UserConsentRevocation |
| FailureCause | 5.3.2.3.6 | Represents the reason of communication failure. | Communication\_failure\_notification |
| GroupMembListChanges | 5.3.2.3.13 | Represents information on the change(s) to a group members list. | GMEC |
| IdleStatusInfo | 5.3.2.3.3 | Represents the information relevant to when the UE transitions into idle mode. | Ue-reachability\_notification,Availability\_after\_DDN\_failure\_notification |
| InterfaceIndication | 5.3.2.4.10 | Represents the network entity used for data delivery towards the SCS/AS. | Pdn\_connectivity\_status |
| LocationFailureCause | 5.3.2.4.11 | Represents the cause of location/positioning failure. | eLCS |
| LocationInfo | 5.3.2.3.5 | Represents the user location information. | Location\_notification, eLCS |
| LocationType | 5.3.2.4.5 | Represents a location type. | Location\_notification, Number\_of\_UEs\_in\_an\_area\_notification, Number\_of\_UEs\_in\_an\_area\_notification\_5G,eLCS |
| MonitoringEventReport | 5.3.2.3.2 | Represents an event monitoring report. |  |
| MonitoringEventReports | 5.3.2.3.10 | Represents one or multiple event monitoring report(s). | enNB |
| MonitoringEventSubscription | 5.3.2.1.2 | Represents a subscription to event(s) monitoring. |  |
| MonitoringNotification | 5.3.2.2.2 | Represents an event monitoring notification. |  |
| MonitoringType | 5.3.2.4.3 | Represents a monitoring event type. |  |
| PdnConnectionInformation | 5.3.2.3.7 | Represents the PDN connection information of the UE. | Pdn\_connectivity\_status |
| PdnConnectionStatus | 5.3.2.4.8 | Represents the PDN connection status. | Pdn\_connectivity\_status |
| PdnType | 5.3.2.4.9 | Represents a PDN connection type. |  |
| ReachabilityType | 5.3.2.4.4 | Represents a reachability type. | Ue-reachability\_notification |
| SACRepFormat | 5.3.2.4.13 | Represents the NSAC reporting format. | NSAC |
| SubType | 5.3.2.4.12 | Represents a subscription type. | UAV |
| UavPolicy | 5.3.2.3.11 | Represents the policy information included in the UAV presence monitoring request. | UAV |
| UePerLocationReport | 5.3.2.3.4 | Represents the number of UEs found at the indicated location. | Number\_of\_UEs\_in\_an\_area\_notification, Number\_of\_UEs\_in\_an\_area\_notification\_5G |
| UpCumEvtRep | 5.3.2.3.18 | Represents the cumulative event report for events reported via user plane. | eLCS\_en |
| UpLocRepAddrAfRm | 5.3.2.3.17 | Represents the user plane addressing information. | eLCS\_en |

\*\*\* 2nd Change \*\*\*

##### 5.3.2.3.2 Type: MonitoringEventReport

This data type represents a monitoring event notification which is sent from the SCEF to the SCS/AS.

Table 5.3.2.3.2-1: Definition of type MonitoringEventReport

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | Cardinality | Description | Applicability (NOTE 1) |
| imeiChange | AssociationType | 0..1 | If "monitoringType" is "CHANGE\_OF\_IMSI\_IMEI\_ASSOCIATION", this parameter shall be included to identify the event of change of IMSI-IMEI or IMSI-IMEISV association is detected.Refer to 3GPP TS 29.336 [11] Clause 8.4.22. | Change\_of\_IMSI\_IMEI\_association\_notification |
| externalId | ExternalId | 0..1 | Contains the external identifier.This attribute may also be present in the monitoring event subscription one-time response message, if the "UEId\_retrieval" feature is supported and the corresponding request message includes the "ueIpAddr" attribute or the "ueMacAddr" attribute.This attribute may also be present when the "RVAS\_5G" fetaure is supported and the reported event within the "monitoringType" attribute is "ROAMING\_STATUS".(NOTE 2) |  |
| appId | string | 0..1 | Contains the identifier of the detected application. (NOTE 4) | AppDetection\_5G |
| pduSessInfo | PduSessionInformation | 0..1 | Represents the PDU session information related to the detected application.If "monitoringType" is "APPLICATION\_START" and/or "APPLICATION\_STOP", this attribute shall be present, if available, to indicate the application traffic detection details. | AppDetection\_5G |
| idleStatusInfo | IdleStatusInfo | 0..1 | If "idleStatusIndication" in the "MonitoringEventSubscription"sets to "true", this parameter shall be included to indicate the information when the UE transitions into idle mode. | Ue-reachability\_notification,Availability\_after\_DDN\_failure\_notification |
| locationInfo | LocationInfo | 0..1 | If "monitoringType" is "LOCATION\_REPORTING", this parameter shall be included to indicate the user location related information. | Location\_notification, eLCS |
| locFailureCause | LocationFailureCause | 0..1 | Indicates the location positioning failure cause. | eLCS |
| lossOfConnectReason | integer | 0..1 | If "monitoringType" is "LOSS\_OF\_CONNECTIVITY", this parameter shall be included if available to identify the reason why loss of connectivity is reported.Refer to 3GPP TS 29.336 [11] Clause 8.4.58. | Loss\_of\_connectivity\_notification |
| unavailPerDur | DurationSec | 0..1 | If "monitoringType" is "LOSS\_OF\_CONNECTIVITY", then this parameter shall be included if available to identify the UE’s Unavailability Period Duration. | Loss\_of\_connectivity\_notification\_5G |
| maxUEAvailabilityTime | DateTime | 0..1 | If "monitoringType" is "UE\_REACHABILITY", this parameter may be included to identify the timestamp until which a UE using a power saving mechanism is expected to be reachable for SM delivery.Refer to Clause 5.3.3.22 of 3GPP TS 29.338 [34]. | Ue-reachability\_notification |
| msisdn | Msisdn | 0..1 | Identifies the MS internal PSTN/ISDN number.This attribute may also be present when the "RVAS\_5G" fetaure is supported and the reported event within the "monitoringType" attribute is "ROAMING\_STATUS".(NOTE 2) |  |
| monitoringType | MonitoringType | 1 | Identifies the type of monitoring type as defined in clause 5.3.2.4.3. |  |
| uePerLocationReport | UePerLocationReport | 0..1 | If "monitoringType" is "NUMBER\_OF\_UES\_IN\_AN\_AREA", this parameter shall be included to indicate the number of UEs found at the location.If "subType" indicates "AERIAL\_UE" subscription type, this parameter shall be included to indicate the number of UAV’s found at the location. | Number\_of\_UEs\_in\_an\_area\_notification, Number\_of\_UEs\_in\_an\_area\_notification\_5G |
| plmnId | PlmnId | 0..1 | If "monitoringType" is "ROAMING\_STATUS" and "plmnIIndication" in the "MonitoringEventSubscription" sets to "true", this parameter shall be included to indicate the UE's serving PLMN. | Roaming\_status\_notification |
| pei | Pei | 0..1 | Contains the PEI.This attribute may be present only when the reported event within the "monitoringType" attribute is "ROAMING\_STATUS". | RVAS\_5G |
| reachabilityType | ReachabilityType | 0..1 | If "monitoringType" is "UE\_REACHABILITY", this parameter shall be included to identify the reachability of the UE.Refer to 3GPP TS 29.336 [11] Clause 8.4.20. | Ue-reachability\_notification |
| roamingStatus | boolean | 0..1 | If "monitoringType" is "ROAMING\_STATUS", this parameter shall be set to "true" if the new serving PLMN is different from the HPLMN. Set to false or omitted otherwise. | Roaming\_status\_notification |
| failureCause | FailureCause | 0..1 | If "monitoringType" is "COMMUNICATION\_FAILURE", this parameter shall be included to indicate the reason of communication failure. | Communication\_failure\_notification |
| eventTime | DateTime | 0..1 | Identifies when the event is detected or received.Shall be included for each group of UEs. |  |
| pdnConnInfoList | array(PdnConnectionInformation) | 0..N | If "monitoringType" is "PDN\_CONNECTIVITY\_STATUS", this parameter shall be included to indicate the PDN connection details. | Pdn\_connectivity\_status |
| dddStatus | DlDataDeliveryStatus | 0..1 | If "monitoringType" is "DOWNLINK\_DATA\_DELIVERY\_STATUS", this parameter shall be included to identify the downlink data delivery status detected by the network. | Downlink\_data\_delivery\_status\_5G |
| dddTrafDescriptor | DddTrafficDescriptor | 0..1 | If "monitoringType" is "DOWNLINK\_DATA\_DELIVERY\_STATUS", this parameter shall be included to identify the downlink data descriptor impacted by the downlink data delivery status change. | Downlink\_data\_delivery\_status\_5G  |
| maxWaitTime | DateTime | 0..1 | If "monitoringType" is "DOWNLINK\_DATA\_DELIVERY\_STATUS", this parameter may be included to identify the time before which the data will be buffered. | Downlink\_data\_delivery\_status\_5G |
| apiCaps | array(ApiCapabilityInfo) | 0..N | If "monitoringType" is "API\_SUPPORT\_CAPABILITY", this parameter shall be included to indicate the availability of all APIs supported by the serving network or the availability of interested APIs, indicated by the "apiNames" attribute in "MonitoringEventSubscription", supported by the serving network. If no API is supported by the serving network, an empty apiCaps shall be provided. | API\_support\_capability\_notification |
| nSStatusInfo | SACEventStatus | 0..1 | If the "monitoringType" attribute is set to "NUM\_OF\_REGD\_UES" or "NUM\_OF\_ESTD\_PDU\_SESSIONS", this parameter shall be included to indicate the current network slice status information for the concerned network slice. (NOTE 3) | NSAC |
| afServiceId | string | 0..1 | Contains the identifier of the service to which the NSAC reporting is related.It shall be provided only if it is present in the related NSAC subscription request and the "monitoringType" attribute is set to either "NUM\_OF\_REGD\_UES" or "NUM\_OF\_ESTD\_PDU\_SESSIONS". | NSAC |
| servLevelDevId | string | 0..1 | If "monitoringType" is "AREA\_OF\_INTEREST" or "NUMBER\_OF\_UES\_IN\_AN\_AREA" and "subType" indicate "AERIAL\_UE", this parameter may be included to identify the UAV. | UAV |
| uavPresInd | boolean | 0..1 | If "monitoringType" is "AREA\_OF\_INTEREST", this parameter shall be set to true if the specified UAV is in the monitoring area. Set to false or omitted otherwise. | UAV |
| groupMembListChanges | GroupMembListChanges | 0..1 | Contains information on the change(s) to the group members list.This attribute shall be present only if the "monitoringType" attribute is set to "GROUP\_MEMBER\_LIST\_CHANGE". | GMEC |
| sessInactiveTime | DurationSec | 0..1 | The value of the session inactivity timer.This attribute shall be present only if the "monitoringType" attribute is set to "SESSION\_INACTIVITY\_TIME". | DataTransfer |
| trafficInfo | TrafficInformation | 0..1 | The value of the UL/DL data rate and/or Traffic volume.This attribute shall be present only if the "monitoringType" attribute is set to "TRAFFIC\_VOLUME” and/or "UL\_DL\_DATA\_RATE". | DataTransfer |
| NOTE 1: Properties marked with a feature as defined in clause 5.3.4 are applicable as described in clause 5.2.7. If no features are indicated, the related property applies for all the features.NOTE 2: Identifies the user for which the event occurred. At least one of the properties shall be included.NOTE 3: If the "eNSAC" feature is supported, the "SACEventStatus" data type shall include an indication to report either the current number of registered UEs or the current number of UEs with at least one PDU session/PDN connection.NOTE 4: When the "AppDetection\_5G" feature is supported and the "monitoringType" attribute is set to either "APPLICATION\_START" or "APPLICATION\_STOP", the "appId" attribute shall be present only if the "appIds" attribute within the corresponding subscription resource contains more than one array element (i.e., more than one application identifier). |

\*\*\* 3rd Change \*\*\*

### 5.3.4 Used Features

The table below defines the features applicable to the MonitoringEvent API. Those features are negotiated as described in clause 5.2.7.

Table 5.3.4-1: Features used by MonitoringEvent API

|  |  |  |
| --- | --- | --- |
| Feature Number | Feature | Description |
| 1 | Loss\_of\_connectivity\_notification | The SCS/AS is notified when the 3GPP network detects that the UE is no longer reachable for signalling or user plane communication |
| 2 | Ue-reachability\_notification | The SCS/AS is notified when the UE becomes reachable for sending either SMS or downlink data to the UE |
| 3 | Location\_notification | The SCS/AS is notified of the current location or the last known location of the UE |
| 4 | Change\_of\_IMSI\_IMEI\_association\_notification | The SCS/AS is notified when the association of an ME (IMEI(SV)) that uses a specific subscription (IMSI) is changed |
| 5 | Roaming\_status\_notification | The SCS/AS is notified when the UE's roaming status changes |
| 6 | Communication\_failure\_notification | The SCS/AS is notified of communication failure events |
| 7 | Availability\_after\_DDN\_failure\_notification | The SCS/AS is notified when the UE has become available after a DDN failure |
| 8 | Number\_of\_UEs\_in\_an\_area\_notification | The SCS/AS is notified the number of UEs present in a given geographic areaThe feature supports pre-5G (e.g. 4G) requirement. |
| 9 | Notification\_websocket | The delivery of notifications over Websocket is supported according to clause 5.2.5.4. This feature requires that the Notification\_test\_event featute is also supported. |
| 10 | Notification\_test\_event | The testing of notification connection is supported according to clause 5.2.5.3. |
| 11 | Subscription\_modification | Modifications of an individual subscription resource. |
| 12 | Number\_of\_UEs\_in\_an\_area\_notification\_5G | The AF is notified the number of UEs present in a given geographic area.The feature supports the 5G requirement. This feature may only be supported in 5G. |
| 13 | Pdn\_connectivity\_status | The SCS/AS requests to be notified when the 3GPP network detects that the UE’s PDN connection is set up or torn down. |
| 14 | Downlink\_data\_delivery\_status\_5G | The AF requests to be notified when the 3GPP network detects that the downlink data delivery status is changed. The feature is not applicable to pre-5G. |
| 15 | Availability\_after\_DDN\_failure\_notification\_enhancement | The AF is notified when the UE has become available after a DDN failure and the traffic matches the packet filter provided by the AF. The feature is not applicable to pre-5G. |
| 16 | Enhanced\_param\_config | This feature supports the co-existence of multiple event configurations for target UE(s) if there are parameters affecting periodic RAU/TAU timer and/or Active Time. Supporting this feature also requires the support of feature number 1 or 2. |
| 17 | API\_support\_capability\_notification | The SCS/AS is notified of the availability of support of service APIs. This feature is only applicable in interworking SCEF+NEF scenario. |
| 18 | eLCS | This feature supports the enhanced location exposure service (e.g. location information preciser than cell level).The feature is not applicable to pre-5G (e.g. 4G). |
| 19 | NSAC | This feature controls the support of the Network Slice Admission Control (NSAC) functionalities.The feature is not applicable to pre-5G (e.g. 4G). |
| 20 | Partial\_group\_modification | This feature supports the partial cancellation and/or partial addition to the group member(s) within the grouped event monitoring subscription. |
| 21 | UAV | The SCS/AS requests to be notified of the UAV presence status in a specific geographic area. This feature is only applicable in interworking SCEF+NEF scenario, or standalone 5G scenario.This feature requires that Number\_of\_UEs\_in\_an\_area\_notification and Number\_of\_UEs\_in\_an\_area\_notification\_5G features are also supported. |
| 22 | MULTIQOS | This feature indicates the support for "Multiple QoS Class" which enables to support more than one Location QoS during LCS procedures.This feature requires that the eLCS feature is also supported. |
| 23 | Session\_Management\_Enhancement | This feature supports Session Management enhancement with requested DNN and/or S-NSSAI. This feature requires that the Pdn\_connectivity\_status feature or Downlink\_data\_delivery\_status\_5G feature is also supported. |
| 24 | enNB | Indicates the support of enhancements to the northbound interfaces. |
| 25 | EDGEAPP | This feature controls the support of EDGE applications related functionalities (e.g. support the civic address as a possible location granularity).The feature is not applicable to pre-5G (e.g. 4G). |
| 26 | UEId\_retrieval | This feature supports AF specific UE ID retrieval which is not applicable to pre-5G (e.g. 4G). |
| 27 | UserConsentRevocation | This feature indicates the support of user consent revocation management and enforcement (e.g. stop data processing) for EDGE applications. |
| 28 | Subscription\_Patch | This feature indicates the support of the PATCH method for partial modification of an existing event monitoring subscription. |
| 29 | GMEC | This feature indicates the support of Generic Group Management, Exposure and Communication Enhancements.The following functionalities are supported:- Support Group Members List Change event reporting.This feature is not applicable to pre-5G (e.g., 4G). |
| 30 | Loss\_of\_connectivity\_notification\_5G | The AF is notified when the 3GPP network detects that the UE is no longer reachable for signalling or user plane communication.This feature is not applicable to pre-5G (e.g. 4G). |
| 31 | enNB1 | Indicates the support of enhancements to this northbound API in Rel-18. |
| 32 | AppDetection\_5G | This feature indicates the support of Application traffic detection (e.g., start and stop) monitoring event.This feature is not applicable to pre-5G (e.g., 4G). |
| 33 | enNB1\_5G | Indicates the support of enhancements to this northbound API for 5G in Rel-18.This feature is not applicable to pre-5G (e.g. 4G). |
| 34 | eLCS\_en | This feature indicates the support of the enhancements to the eLCS feature.The following functionalities are supported:- Support the error handling related to the area event reporting for the case where the requested location area is not allowed.- Support location reporting over user plane between UE and AF.This feature is not applicable to pre-5G (e.g. 4G). |
| 35 | eNSAC | This feature indicates the support of the enhancements to the NSAC feature. The following functionalities are supported:- Support the status notification of the current number of UEs with at least one PDU session/PDN connection.This feature is not applicable to pre-5G (e.g. 4G). |
| 36 | Ranging\_SL | This feature indicates the support of the ranging and sidelink positioning functionality.The following functionalities are supported:- Support the ranging and sidelink input/output parameters.This feature requires the support of eLCS feature.This feature is not applicable to pre-5G (e.g. 4G). |
| 37 | DataTransfer | This feature indicates the support of Session inactivity time, Traffic volume and UL/DL data rate events for data transfer and measurement.This feature is not applicable to pre-5G (e.g. 4G). |
| 38 | RVAS\_5G | This feature indicates the support of the 5G Roaming Value-Added Services (RVAS).The following functionalities are supported:- Support the reporting of the equipment and subscription identifers as part of the roaming status report in order to support the RVAS Welcome SMS functionality.This feature requires the support of "Roaming\_status\_notification" feature.This feature is not applicable to pre-5G (e.g., 4G). |
| Feature: A short name that can be used to refer to the bit and to the feature, e.g. "Notification".Description: A clear textual description of the feature. |

\*\*\* 4th Change \*\*\*

# A.3 MonitoringEvent API

openapi: 3.0.0

info:

 title: 3gpp-monitoring-event

 version: 1.3.0

 description: |

 API for Monitoring Event.

 © 2024, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

externalDocs:

 description: 3GPP TS 29.122 V18.6.0 T8 reference point for Northbound APIs

 url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.122/'

security:

 - {}

 - oAuth2ClientCredentials: []

servers:

 - url: '{apiRoot}/3gpp-monitoring-event/v1'

 variables:

 apiRoot:

 default: https://example.com

 description: apiRoot as defined in clause 5.2.4 of 3GPP TS 29.122.

paths:

 /{scsAsId}/subscriptions:

 get:

 summary: Read all or queried active subscriptions for the SCS/AS.

 operationId: FetchAllMonitoringEventSubscriptions

 tags:

 - Monitoring Event Subscriptions

 parameters:

 - name: scsAsId

 in: path

 description: Identifier of the SCS/AS

 required: true

 schema:

 type: string

 - name: ip-addrs

 in: query

 description: The IP address(es) of the requested UE(s).

 required: false

 content:

 application/json:

 schema:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/IpAddr'

 minItems: 1

 - name: ip-domain

 in: query

 description: >

 The IPv4 address domain identifier. The attribute may only be provided if IPv4 address

 is included in the ip-addrs query parameter.

 required: false

 schema:

 type: string

 - name: mac-addrs

 in: query

 description: The MAC address(es) of the requested UE(s).

 required: false

 schema:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

 minItems: 1

 responses:

 '200':

 description: OK (Successful get all or queried active subscriptions for the SCS/AS)

 content:

 application/json:

 schema:

 type: array

 items:

 $ref: '#/components/schemas/MonitoringEventSubscription'

 minItems: 0

 description: Monitoring event subscriptions

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '406':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/406'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 post:

 summary: Creates a new subscription resource for monitoring event notification.

 operationId: CreateMonitoringEventSubscription

 tags:

 - Monitoring Event Subscriptions

 parameters:

 - name: scsAsId

 in: path

 description: Identifier of the SCS/AS

 required: true

 schema:

 type: string

 requestBody:

 description: Subscription for notification about monitoring event

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/MonitoringEventSubscription'

 callbacks:

 notificationDestination:

 '{$request.body#/notificationDestination}':

 post:

 requestBody: # contents of the callback message

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/MonitoringNotification'

 responses:

 '204':

 description: No Content (successful notification)

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 UserConsentRevocationNotif:

 '{$request.body#/revocationNotifUri}':

 post:

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/ConsentRevocNotif'

 responses:

 '204':

 description: No Content (successful notification).

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 responses:

 '201':

 description: Created (Successful creation of subscription)

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/MonitoringEventSubscription'

 headers:

 Location:

 description: 'Contains the URI of the newly created resource'

 required: true

 schema:

 type: string

 '200':

 description: The operation is successful and immediate report is included.

 content:

 application/json:

 schema:

 oneOf:

 - $ref: '#/components/schemas/MonitoringEventReport'

 - $ref: '#/components/schemas/MonitoringEventReports'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 /{scsAsId}/subscriptions/{subscriptionId}:

 get:

 summary: Read an active subscriptions for the SCS/AS and the subscription Id.

 operationId: FetchIndMonitoringEventSubscription

 tags:

 - Individual Monitoring Event Subscription

 parameters:

 - name: scsAsId

 in: path

 description: Identifier of the SCS/AS

 required: true

 schema:

 type: string

 - name: subscriptionId

 in: path

 description: Identifier of the subscription resource

 required: true

 schema:

 type: string

 responses:

 '200':

 description: OK (Successful get the active subscription)

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/MonitoringEventSubscription'

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '406':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/406'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 put:

 summary: Updates/replaces an existing subscription resource.

 operationId: UpdateIndMonitoringEventSubscription

 tags:

 - Individual Monitoring Event Subscription

 parameters:

 - name: scsAsId

 in: path

 description: Identifier of the SCS/AS

 required: true

 schema:

 type: string

 - name: subscriptionId

 in: path

 description: Identifier of the subscription resource

 required: true

 schema:

 type: string

 requestBody:

 description: Parameters to update/replace the existing subscription

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/MonitoringEventSubscription'

 responses:

 '200':

 description: OK (Successful update of the subscription)

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/MonitoringEventSubscription'

 '204':

 description: No Content (Successful update of the subscription)

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 patch:

 summary: Modifies an existing subscription of monitoring event.

 operationId: ModifyIndMonitoringEventSubscription

 tags:

 - Individual Monitoring Event Subscription

 parameters:

 - name: scsAsId

 in: path

 description: Identifier of the SCS/AS.

 required: true

 schema:

 type: string

 - name: subscriptionId

 in: path

 description: Identifier of the subscription resource.

 required: true

 schema:

 type: string

 requestBody:

 description: >

 This is used for PATCH request for partial cancellation and/or partial addition of certain

 UE(s) within an active group.

 required: true

 content:

 application/json-patch+json:

 schema:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PatchItem'

 minItems: 1

 responses:

 '204':

 description: The resource was modified successfully.

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 delete:

 summary: Deletes an already existing monitoring event subscription.

 operationId: DeleteIndMonitoringEventSubscription

 tags:

 - Individual Monitoring Event Subscription

 parameters:

 - name: scsAsId

 in: path

 description: Identifier of the SCS/AS

 required: true

 schema:

 type: string

 - name: subscriptionId

 in: path

 description: Identifier of the subscription resource

 required: true

 schema:

 type: string

 responses:

 '204':

 description: No Content (Successful deletion of the existing subscription)

 '200':

 description: OK (Successful deletion of the existing subscription)

 content:

 application/json:

 schema:

 type: array

 items:

 $ref: '#/components/schemas/MonitoringEventReport'

 minItems: 1

 description: >

 The subscription was terminated successfully, the monitoring event report(s)

 shall be included if received.

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

 securitySchemes:

 oAuth2ClientCredentials:

 type: oauth2

 flows:

 clientCredentials:

 tokenUrl: '{tokenUrl}'

 scopes: {}

 schemas:

 MonitoringEventSubscription:

 description: Represents a subscription to event(s) monitoring.

 type: object

 properties:

 self:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

 supportedFeatures:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 mtcProviderId:

 type: string

 description: Identifies the MTC Service Provider and/or MTC Application.

 appIds:

 type: array

 items:

 type: string

 description: Identifies the Application Identifier(s)

 minItems: 1

 externalId:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalId'

 msisdn:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Msisdn'

 addedExternalIds:

 type: array

 items:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalId'

 minItems: 1

 description: Indicates the added external Identifier(s) within the active group.

 addedMsisdns:

 type: array

 items:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Msisdn'

 minItems: 1

 description: Indicates the added MSISDN(s) within the active group.

 excludedExternalIds:

 type: array

 items:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalId'

 minItems: 1

 description: Indicates cancellation of the external Identifier(s) within the active group.

 excludedMsisdns:

 type: array

 items:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Msisdn'

 minItems: 1

 description: Indicates cancellation of the MSISDN(s) within the active group.

 externalGroupId:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalGroupId'

 addExtGroupId:

 type: array

 items:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalGroupId'

 minItems: 2

 ipv4Addr:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Ipv4Addr'

 ipv6Addr:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Ipv6Addr'

 dnn:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 notificationDestination:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

 requestTestNotification:

 type: boolean

 description: >

 Set to true by the SCS/AS to request the SCEF to send a test notification

 as defined in clause 5.2.5.3. Set to false by the SCS/AS indicates not request SCEF to

 send a test notification, default false if omitted otherwise.

 websockNotifConfig:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/WebsockNotifConfig'

 monitoringType:

 $ref: '#/components/schemas/MonitoringType'

 maximumNumberOfReports:

 type: integer

 minimum: 1

 description: >

 Identifies the maximum number of event reports to be generated by the HSS, MME/SGSN

 as specified in clause 5.6.0 of 3GPP TS 23.682.

 monitorExpireTime:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/DateTime'

 repPeriod:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

 groupReportGuardTime:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

 maximumDetectionTime:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

 reachabilityType:

 $ref: '#/components/schemas/ReachabilityType'

 maximumLatency:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

 maximumResponseTime:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

 suggestedNumberOfDlPackets:

 type: integer

 minimum: 0

 description: >

 If "monitoringType" is "UE\_REACHABILITY", this parameter may be included to identify

 the number of packets that the serving gateway shall buffer in case that

 the UE is not reachable.

 idleStatusIndication:

 type: boolean

 description: >

 If "monitoringType" is set to "UE\_REACHABILITY" or "AVAILABILITY\_AFTER\_DDN\_FAILURE",

 this parameter may be included to indicate the notification of when a UE, for which PSM

 is enabled, transitions into idle mode. "true" indicates enabling of notification;

 "false" indicate no need to notify. Default value is "false" if omitted.

 locationType:

 $ref: '#/components/schemas/LocationType'

 accuracy:

 $ref: '#/components/schemas/Accuracy'

 minimumReportInterval:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

 maxRptExpireIntvl:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

 samplingInterval:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

 reportingLocEstInd:

 type: boolean

 description: >

 Indicates whether to request the location estimate for event reporting. If

 "monitoringType" is "LOCATION\_REPORTING", this parameter may be included to indicate

 whether event reporting requires the location information. If set to true, the location

 estimation information shall be included in event reporting. If set to "false",

 indicates the location estimation information shall not be included in event reporting.

 Default "false" if omitted.

 linearDistance:

 $ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/LinearDistance'

 locQoS:

 $ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/LocationQoS'

 svcId:

 $ref: 'TS29515\_Ngmlc\_Location.yaml#/components/schemas/ServiceIdentity'

 ldrType:

 $ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/LdrType'

 velocityRequested:

 $ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/VelocityRequested'

 maxAgeOfLocEst:

 $ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/AgeOfLocationEstimate'

 locTimeWindow:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeWindow'

 supportedGADShapes:

 type: array

 items:

 $ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/SupportedGADShapes'

 codeWord:

 $ref: 'TS29515\_Ngmlc\_Location.yaml#/components/schemas/CodeWord'

 upLocRepIndAf:

 description: >

 Indicates whether location reporting over user plane is requested or not.

 "true" indicates the location reporting over user plane is requested.

 "false" indicates the location reporting over user plane is not requested.

 Default value is "false" if omitted.

 type: boolean

 default: false

 upLocRepAddrAf:

 $ref: '#/components/schemas/UpLocRepAddrAfRm'

 associationType:

 $ref: '#/components/schemas/AssociationType'

 plmnIndication:

 type: boolean

 description: >

 If "monitoringType" is "ROAMING\_STATUS", this parameter may be included to indicate the

 notification of UE's Serving PLMN ID. Value "true" indicates enabling of notification;

 "false" indicates disabling of notification. Default value is "false" if omitted.

 locationArea:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/LocationArea'

 locationArea5G:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/LocationArea5G'

 dddTraDescriptors:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DddTrafficDescriptor'

 minItems: 1

 dddStati:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DlDataDeliveryStatus'

 minItems: 1

 apiNames:

 type: array

 items:

 type: string

 minItems: 1

 monitoringEventReport:

 $ref: '#/components/schemas/MonitoringEventReport'

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 tgtNsThreshold:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SACInfo'

 nsRepFormat:

 $ref: '#/components/schemas/SACRepFormat'

 afServiceId:

 type: string

 immediateRep:

 type: boolean

 description: >

 Indicates whether an immediate reporting is requested or not.

 "true" indicate an immediate reporting is requested.

 "false" indicate an immediate reporting is not requested.

 Default value "false" if omitted.

 uavPolicy:

 $ref: '#/components/schemas/UavPolicy'

 sesEstInd:

 type: boolean

 description: >

 Set to true by the SCS/AS so that only UAV's with "PDU session established for DNN(s)

 subject to aerial service" are to be listed in the Event report. Set to false or default

 false if omitted otherwise.

 subType:

 $ref: '#/components/schemas/SubType'

 addnMonTypes:

 type: array

 items:

 $ref: '#/components/schemas/MonitoringType'

 addnMonEventReports:

 type: array

 items:

 $ref: '#/components/schemas/MonitoringEventReport'

 ueIpAddr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/IpAddr'

 ueMacAddr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

 revocationNotifUri:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Uri'

 reqRangSlRes:

 type: array

 items:

 $ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/RangingSlResult'

 minItems: 1

 relatedUes:

 type: object

 additionalProperties:

 $ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/RelatedUe'

 minProperties: 1

 description: >

 Contains a list of the related UE(s) for the ranging and sidelink positioning and the

 corresponding information.

 The key of the map shall be a any unique string set to the value.

 required:

 - notificationDestination

 - monitoringType

 anyOf:

 - required: [maximumNumberOfReports]

 - required: [monitorExpireTime]

 MonitoringNotification:

 description: Represents an event monitoring notification.

 type: object

 properties:

 subscription:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

 configResults:

 type: array

 items:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/ConfigResult'

 minItems: 1

 description: Each element identifies a notification of grouping configuration result.

 monitoringEventReports:

 type: array

 items:

 $ref: '#/components/schemas/MonitoringEventReport'

 minItems: 1

 description: Monitoring event reports.

 addedExternalIds:

 type: array

 items:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalId'

 minItems: 1

 description: >

 Identifies the added external Identifier(s) within the active group via

 the "externalGroupId" attribute within the MonitoringEventSubscription data type.

 addedMsisdns:

 type: array

 items:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Msisdn'

 minItems: 1

 description: >

 Identifies the added MSISDN(s) within the active group via the "externalGroupId"

 attribute within the MonitoringEventSubscription data type.

 cancelExternalIds:

 type: array

 items:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalId'

 minItems: 1

 description: >

 Identifies the cancelled external Identifier(s) within the active group via

 the "externalGroupId" attribute within the MonitoringEventSubscription data type.

 cancelMsisdns:

 type: array

 items:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Msisdn'

 minItems: 1

 description: >

 Identifies the cancelled MSISDN(s) within the active group via the "externalGroupId"

 attribute within the MonitoringEventSubscription data type.

 cancelInd:

 type: boolean

 description: >

 Indicates whether to request to cancel the corresponding monitoring subscription.

 Set to false or omitted otherwise.

 appliedParam:

 $ref: '#/components/schemas/AppliedParameterConfiguration'

 required:

 - subscription

 MonitoringEventReport:

 description: Represents an event monitoring report.

 type: object

 properties:

 imeiChange:

 $ref: '#/components/schemas/AssociationType'

 externalId:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalId'

 appId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationId'

 pduSessInfo:

 $ref: 'TS29523\_Npcf\_EventExposure.yaml#/components/schemas/PduSessionInformation'

 idleStatusInfo:

 $ref: '#/components/schemas/IdleStatusInfo'

 locationInfo:

 $ref: '#/components/schemas/LocationInfo'

 locFailureCause:

 $ref: '#/components/schemas/LocationFailureCause'

 lossOfConnectReason:

 type: integer

 description: >

 If "monitoringType" is "LOSS\_OF\_CONNECTIVITY", this parameter shall be included

 if available to identify the reason why loss of connectivity is reported.

 Refer to 3GPP TS 29.336 clause 8.4.58.

 unavailPerDur:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

 maxUEAvailabilityTime:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/DateTime'

 msisdn:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Msisdn'

 monitoringType:

 $ref: '#/components/schemas/MonitoringType'

 uePerLocationReport:

 $ref: '#/components/schemas/UePerLocationReport'

 plmnId:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/PlmnId'

 reachabilityType:

 $ref: '#/components/schemas/ReachabilityType'

 roamingStatus:

 type: boolean

 description: >

 If "monitoringType" is "ROAMING\_STATUS", this parameter shall be set to "true"

 if the new serving PLMN is different from the HPLMN. Set to false or

 omitted otherwise.

 pei:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Pei'

 failureCause:

 $ref: '#/components/schemas/FailureCause'

 eventTime:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/DateTime'

 pdnConnInfoList:

 type: array

 items:

 $ref: '#/components/schemas/PdnConnectionInformation'

 minItems: 1

 dddStatus:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DlDataDeliveryStatus'

 dddTrafDescriptor:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DddTrafficDescriptor'

 maxWaitTime:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/DateTime'

 apiCaps:

 type: array

 items:

 $ref: '#/components/schemas/ApiCapabilityInfo'

 minItems: 0

 nSStatusInfo:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SACEventStatus'

 afServiceId:

 type: string

 servLevelDevId:

 type: string

 description: >

 If "monitoringType" is "AREA\_OF\_INTEREST", this parameter may be included

 to identify the UAV.

 uavPresInd:

 type: boolean

 description: >

 If "monitoringType" is "AREA\_OF\_INTEREST", this parameter shall be set to true

 if the specified UAV is in the monitoring area. Set to false or omitted otherwise.

 groupMembListChanges:

 $ref: '#/components/schemas/GroupMembListChanges'

 sessInactiveTime:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

 trafficInfo:

 $ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/TrafficInformation'

 required:

 - monitoringType

 MonitoringEventReports:

 description: Represents a set of event monitoring reports.

 type: object

 properties:

 monitoringEventReports:

 type: array

 items:

 $ref: '#/components/schemas/MonitoringEventReport'

 minItems: 1

 required:

 - monitoringEventReports

 IdleStatusInfo:

 description: Represents the information relevant to when the UE transitions into idle mode.

 type: object

 properties:

 activeTime:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

 edrxCycleLength:

 format: float

 type: number

 minimum: 0

 suggestedNumberOfDlPackets:

 type: integer

 minimum: 0

 description: >

 Identifies the number of packets shall be buffered in the serving gateway.

 It shall be present if the idle status indication is requested by the SCS/AS

 with "idleStatusIndication" in the "monitoringEventSubscription" sets to "true".

 idleStatusTimestamp:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/DateTime'

 periodicAUTimer:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

 UePerLocationReport:

 description: Represents the number of UEs found at the indicated location.

 type: object

 properties:

 ueCount:

 type: integer

 minimum: 0

 description: Identifies the number of UEs.

 externalIds:

 type: array

 items:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalId'

 minItems: 1

 description: Each element uniquely identifies a user.

 msisdns:

 type: array

 items:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Msisdn'

 minItems: 1

 description: Each element identifies the MS internal PSTN/ISDN number allocated for a UE.

 servLevelDevIds:

 type: array

 items:

 type: string

 minItems: 1

 description: Each element uniquely identifies a UAV.

 required:

 - ueCount

 LocationInfo:

 description: Represents the user location information.

 type: object

 properties:

 ageOfLocationInfo:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationMin'

 cellId:

 type: string

 description: >

 Indicates the Cell Global Identification of the user which identifies the cell the UE

 is registered.

 enodeBId:

 type: string

 description: Indicates the eNodeB in which the UE is currently located.

 routingAreaId:

 type: string

 description: Identifies the Routing Area Identity of the user where the UE is located.

 trackingAreaId:

 type: string

 description: Identifies the Tracking Area Identity of the user where the UE is located.

 plmnId:

 type: string

 description: Identifies the PLMN Identity of the user where the UE is located.

 twanId:

 type: string

 description: Identifies the TWAN Identity of the user where the UE is located.

 userLocation:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 geographicArea:

 $ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/GeographicArea'

 civicAddress:

 $ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/CivicAddress'

 positionMethod:

 $ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/PositioningMethod'

 qosFulfilInd:

 $ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/AccuracyFulfilmentIndicator'

 ueVelocity:

 $ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/VelocityEstimate'

 ldrType:

 $ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/LdrType'

 achievedQos:

 $ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/MinorLocationQoS'

 relAppLayerId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationlayerId'

 rangeDirection:

 $ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/RangeDirection'

 twoDRelLoc:

 $ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/2DRelativeLocation'

 threeDRelLoc:

 $ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/3DRelativeLocation'

 relVelocity:

 $ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/VelocityEstimate'

 upCumEvtRep:

 $ref: '#/components/schemas/UpCumEvtRep'

 FailureCause:

 description: Represents the reason of communication failure.

 type: object

 properties:

 bssgpCause:

 type: integer

 description: >

 Identifies a non-transparent copy of the BSSGP cause code. Refer to 3GPP TS 29.128.

 causeType:

 type: integer

 description: Identify the type of the S1AP-Cause. Refer to 3GPP TS 29.128.

 gmmCause:

 type: integer

 description: >

 Identifies a non-transparent copy of the GMM cause code. Refer to 3GPP TS 29.128.

 ranapCause:

 type: integer

 description: >

 Identifies a non-transparent copy of the RANAP cause code. Refer to 3GPP TS 29.128.

 ranNasCause:

 type: string

 description: >

 Indicates RAN and/or NAS release cause code information, TWAN release cause code

 information or untrusted WLAN release cause code information. Refer to 3GPP TS 29.214.

 s1ApCause:

 type: integer

 description: >

 Identifies a non-transparent copy of the S1AP cause code. Refer to 3GPP TS 29.128.

 smCause:

 type: integer

 description: >

 Identifies a non-transparent copy of the SM cause code. Refer to 3GPP TS 29.128.

 PdnConnectionInformation:

 description: Represents the PDN connection information of the UE.

 type: object

 properties:

 status:

 $ref: '#/components/schemas/PdnConnectionStatus'

 apn:

 type: string

 description: >

 Identify the APN, it is depending on the SCEF local configuration whether or

 not this attribute is sent to the SCS/AS.

 pdnType:

 $ref: '#/components/schemas/PdnType'

 interfaceInd:

 $ref: '#/components/schemas/InterfaceIndication'

 ipv4Addr:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Ipv4Addr'

 ipv6Addrs:

 type: array

 items:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Ipv6Addr'

 minItems: 1

 macAddrs:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

 minItems: 1

 required:

 - status

 - pdnType

 AppliedParameterConfiguration:

 description: Represents the parameter configuration applied in the network.

 type: object

 properties:

 externalIds:

 type: array

 items:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalId'

 minItems: 1

 description: Each element uniquely identifies a user.

 msisdns:

 type: array

 items:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Msisdn'

 minItems: 1

 description: Each element identifies the MS internal PSTN/ISDN number allocated for a UE.

 maximumLatency:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

 maximumResponseTime:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

 maximumDetectionTime:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

 ApiCapabilityInfo:

 description: Represents the availability information of supported API.

 type: object

 properties:

 apiName:

 type: string

 suppFeat:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 required:

 - apiName

 - suppFeat

 UavPolicy:

 description: >

 Represents the policy information included in the UAV presence monitoring request.

 type: object

 properties:

 uavMoveInd:

 type: boolean

 revokeInd:

 type: boolean

 required:

 - uavMoveInd

 - revokeInd

 ConsentRevocNotif:

 description: >

 Represents the user consent revocation information conveyed in a user consent

 revocation notification.

 type: object

 properties:

 subscriptionId:

 type: string

 consentsRevoked:

 type: array

 items:

 $ref: '#/components/schemas/ConsentRevoked'

 minItems: 1

 required:

 - subscriptionId

 - consentsRevoked

 ConsentRevoked:

 description: Represents the information related to a revoked user consent.

 type: object

 properties:

 ucPurpose:

 $ref: 'TS29503\_Nudm\_SDM.yaml#/components/schemas/UcPurpose'

 externalId:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalId'

 msisdn:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Msisdn'

 required:

 - ucPurpose

 oneOf:

 - required: [externalId]

 - required: [msisdn]

 GroupMembListChanges:

 description: Represents information on the change(s) to a group's members list.

 type: object

 properties:

 addedUEs:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 minItems: 1

 removedUEs:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 minItems: 1

 anyOf:

 - required: [addedUEs]

 - required: [removedUEs]

 UpLocRepAddrAfRm:

 description: Represents the user plane addressing information.

 type: object

 properties:

 ipv4Addrs:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 minItems: 1

 ipv6Addrs:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

 minItems: 1

 fqdn:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Fqdn'

 nullable: true

 anyOf:

 - required: [ipv4Addrs]

 - required: [ipv6Addrs]

 - required: [fqdn]

 UpCumEvtRep:

 description: Represents the cumulative event report.

 type: object

 properties:

 upLocRepStat:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

#

# ENUMS

#

 MonitoringType:

 anyOf:

 - type: string

 enum:

 - LOSS\_OF\_CONNECTIVITY

 - UE\_REACHABILITY

 - LOCATION\_REPORTING

 - CHANGE\_OF\_IMSI\_IMEI\_ASSOCIATION

 - ROAMING\_STATUS

 - COMMUNICATION\_FAILURE

 - AVAILABILITY\_AFTER\_DDN\_FAILURE

 - NUMBER\_OF\_UES\_IN\_AN\_AREA

 - PDN\_CONNECTIVITY\_STATUS

 - DOWNLINK\_DATA\_DELIVERY\_STATUS

 - API\_SUPPORT\_CAPABILITY

 - NUM\_OF\_REGD\_UES

 - NUM\_OF\_ESTD\_PDU\_SESSIONS

 - AREA\_OF\_INTEREST

 - GROUP\_MEMBER\_LIST\_CHANGE

 - APPLICATION\_START

 - APPLICATION\_STOP

 - SESSION\_INACTIVITY\_TIME

 - TRAFFIC\_VOLUME

 - UL\_DL\_DATA\_RATE

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: |

 Represents a monitoring event type.

 Possible values are

 - LOSS\_OF\_CONNECTIVITY: The SCS/AS requests to be notified when the 3GPP network detects

 that the UE is no longer reachable for signalling or user plane communication

 - UE\_REACHABILITY: The SCS/AS requests to be notified when the UE becomes reachable for

 sending either SMS or downlink data to the UE

 - LOCATION\_REPORTING: The SCS/AS requests to be notified of the current location or

 the last known location of the UE

 - CHANGE\_OF\_IMSI\_IMEI\_ASSOCIATION: The SCS/AS requests to be notified when the association

 of an ME (IMEI(SV)) that uses a specific subscription (IMSI) is changed

 - ROAMING\_STATUS: The SCS/AS queries the UE's current roaming status and requests to get

 notified when the status changes

 - COMMUNICATION\_FAILURE: The SCS/AS requests to be notified of communication failure events

 - AVAILABILITY\_AFTER\_DDN\_FAILURE: The SCS/AS requests to be notified when the UE has become

 available after a DDN failure

 - NUMBER\_OF\_UES\_IN\_AN\_AREA: The SCS/AS requests to be notified the number of UEs in a given

 geographic area

 - PDN\_CONNECTIVITY\_STATUS: The SCS/AS requests to be notified when the 3GPP network detects

 that the UE’s PDN connection is set up or torn down

 - DOWNLINK\_DATA\_DELIVERY\_STATUS: The AF requests to be notified when the 3GPP network

 detects that the downlink data delivery status is changed.

 - API\_SUPPORT\_CAPABILITY: The SCS/AS requests to be notified of the availability of support

 of service APIs.

 - NUM\_OF\_REGD\_UES: The AF requests to be notified of the current number of registered UEs

 for a network slice.

 - NUM\_OF\_ESTD\_PDU\_SESSIONS: The AF requests to be notified of the current number of

 established PDU Sessions for a network slice.

 - AREA\_OF\_INTEREST: The SCS/AS requests to be notified when the UE(i.e. UAV) moves in or

 out of the geographic area.

 - GROUP\_MEMBER\_LIST\_CHANGE: The AF requests to be notified of the changes to a group members

 list.

 - APPLICATION\_START: The AF requests to be notified about the start of application traffic

 has been detected.

 - APPLICATION\_STOP: The AF requests to be notified about the stop of application traffic

 has been detected.

 - SESSION\_INACTIVITY\_TIME: The AF requests to be notified of session inactivity time of the

 measured UE PDU Session.

 - TRAFFIC\_VOLUME: The AF requests to be notified of traffic volume of the measured UE.

 - UL\_DL\_DATA\_RATE: The AF requests to be notified of uplink and downlink data rate of the

 measured UE.

 ReachabilityType:

 anyOf:

 - type: string

 enum:

 - SMS

 - DATA

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: |

 Represents a reachability type.

 Possible values are

 - SMS: The SCS/AS requests to be notified when the UE becomes reachable for sending SMS

 to the UE

 - DATA: The SCS/AS requests to be notified when the UE becomes reachable for sending

 downlink data to the UE.

 LocationType:

 anyOf:

 - type: string

 enum:

 - CURRENT\_LOCATION

 - LAST\_KNOWN\_LOCATION

 - CURRENT\_OR\_LAST\_KNOWN\_LOCATION

 - INITIAL\_LOCATION

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: |

 Represents a location type.

 Possible values are

 - CURRENT\_LOCATION: The SCS/AS requests to be notified for current location

 - LAST\_KNOWN\_LOCATION: The SCS/AS requests to be notified for last known location

 - CURRENT\_OR\_LAST\_KNOWN\_LOCATION: The AF requests the current or last known location

 - INITIAL\_LOCATION: The AF requests the initial location

 AssociationType:

 anyOf:

 - type: string

 enum:

 - IMEI

 - IMEISV

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: |

 Represents an IMEI or IMEISV to IMSI association.

 Possible values are

 - IMEI: The value shall be used when the change of IMSI-IMEI association shall be detected

 - IMEISV: The value shall be used when the change of IMSI-IMEISV association shall be

 detected

 Accuracy:

 anyOf:

 - type: string

 enum:

 - CGI\_ECGI

 - ENODEB

 - TA\_RA

 - PLMN

 - TWAN\_ID

 - GEO\_AREA

 - CIVIC\_ADDR

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: |

 Represents a desired granularity of accuracy of the requested location information.

 Possible values are

 - CGI\_ECGI: The SCS/AS requests to be notified using cell level location accuracy.

 - ENODEB: The SCS/AS requests to be notified using eNodeB level location accuracy.

 - TA\_RA: The SCS/AS requests to be notified using TA/RA level location accuracy.

 - PLMN: The SCS/AS requests to be notified using PLMN level location accuracy.

 - TWAN\_ID: The SCS/AS requests to be notified using TWAN identifier level location accuracy.

 - GEO\_AREA: The SCS/AS requests to be notified using the geographical area accuracy.

 - CIVIC\_ADDR: The SCS/AS requests to be notified using the civic address accuracy.

 PdnConnectionStatus:

 anyOf:

 - type: string

 enum:

 - CREATED

 - RELEASED

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: |

 Represents the PDN connection status.

 Possible values are

 - CREATED: The PDN connection is created.

 - RELEASED: The PDN connection is released.

 PdnType:

 anyOf:

 - type: string

 enum:

 - IPV4

 - IPV6

 - IPV4V6

 - NON\_IP

 - ETHERNET

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: |

 Represents the PDN connection type.

 Possible values are

 - IPV4: PDN connection of IPv4 type.

 - IPV6: PDN connection of IPv6 type.

 - IPV4V6: PDN connection of IPv4v6 type.

 - NON\_IP: PDN connection of non-IP type.

 - ETHERNET: PDN connection of Ethernet type.

 InterfaceIndication:

 anyOf:

 - type: string

 enum:

 - EXPOSURE\_FUNCTION

 - PDN\_GATEWAY

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: |

 Represents the network entity used for data delivery towards the SCS/AS.

 Possible values are

 - EXPOSURE\_FUNCTION: SCEF is used for the PDN connection towards the SCS/AS.

 - PDN\_GATEWAY: PDN gateway is used for the PDN connection towards the SCS/AS.

 LocationFailureCause:

 anyOf:

 - type: string

 enum:

 - POSITIONING\_DENIED

 - UNSUPPORTED\_BY\_UE

 - NOT\_REGISTED\_UE

 - UNSPECIFIED

 - REQUESTED\_AREA\_NOT\_ALLOWED

 - type: string

 description: >

 This string provides forward-compatibility with future extensions to the enumeration but

 is not used to encode content defined in the present version of this API.

 description: >

 Represents the cause of location positioning failure.

 Possible values are:

 - POSITIONING\_DENIED: Positioning is denied.

 - UNSUPPORTED\_BY\_UE: Positioning is not supported by UE.

 - NOT\_REGISTED\_UE: UE is not registered.

 - UNSPECIFIED: Unspecified.

 - REQUESTED\_AREA\_NOT\_ALLOWED: The location request is rejected because the location area

 requested by the AF for area event reporting is not allowed.

 SubType:

 anyOf:

 - type: string

 enum:

 - AERIAL\_UE

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: |

 Represents a subscription type.

 Possible values are

 - AERIAL\_UE: The UE has Aerial subscription.

 SACRepFormat:

 anyOf:

 - type: string

 enum:

 - NUMERICAL

 - PERCENTAGE

 - type: string

 description: >

 This string provides forward-compatibility with future extensions to the enumeration but

 is not used to encode content defined in the present version of this API.

 description: Indicates the NSAC reporting format.

\*\*\* End of Changes \*\*\*