3GPP TSG-RAN WG4 Meeting #111 R4-2410217

Fukuoka City, Fukuoka , Japan, 20th – 24th May, 2024

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  | **38.133** | **CR** | **4369** | **rev** | **1** | **Current version:** | **15.25.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | (NR\_newRAT-Perf) Inter-RAT measurement for UE capable of independentGapConfig (Cat-F Rel-15) |
|  |  |
| ***Source to WG:*** | Qualcomm Incorporated |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NR\_newRAT-Perf |  | ***Date:*** | 2024-05-20 |
|  |  |  |  |  |
| ***Category:*** | F |  | ***Release:*** | Rel-15 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19) Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | In the following test cases, no differentiation about UE capability of per-FR gap is needed since no FR2 cell is present.* A.8.4.2.1, A.8.4.2.2, A.8.4.2.3, A.8.4.2.4

In the following test cases, a UE capable of per-FR gap (*independentGapConfig*) does not need a measurement gap since there is not an FR2 serving cell in the sub-test(s).* A.8.4.2.5, A.8.4.2.6, A.8.4.2.7, A.8.4.2.8
 |
|  |  |
| ***Summary of change:*** | Removed incorrect per-FG gap configuration from the following test cases.* A.8.4.2.1, A.8.4.2.2, A.8.4.2.3, A.8.4.2.4

Removed measurement gap configuration for a UE capable of per-FR gap from the following test cases.* A.8.4.2.5, A.8.4.2.6, A.8.4.2.7, A.8.4.2.8
 |
|  |  |
| ***Consequences if not approved:*** | The test cases might not be correctly implemented by RAN5. |
|  |  |
| ***Clauses affected:*** | A.8.4.2.1, A.8.4.2.2, A.8.4.2.3, A.8.4.2.4, A.8.4.2.5, A.8.4.2.6, A.8.4.2.7, A.8.4.2.8 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **x** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** | **x** |  |  Test specifications | TS 38.533 |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

<Start of Change 1>

### A.8.4.2 E-UTRA – NR Inter-RAT Measurements

#### A.8.4.2.1 NR Inter-RAT event triggered reporting tests for FR1 without SSB time index detection when DRX is not used

##### A.8.4.2.1.1 Test Purpose and Environment

The purpose of this test is to verify that the UE makes correct reporting of an event. This test will partly verify the NR inter-RAT cell search requirements in clause 8.1.2.4.21 of TS 36.133 [15] for E-UTRAN FDD-NR measurements and clause 8.1.2.4.22 of TS 36.133 [15] for E-UTRAN TDD-NR measurements.

In this test, there are two cells: E-UTRA cell 1 as PCell on E-UTRA RF channel 1 and NR cell 2 as neighbour cell in FR1 on NR RF channel 1. The test parameters are given in Tables A.8.4.2.1.1-1, A.8.4.2.1.1-2, A.8.4.2.1.1-3 and A.8.4.2.1.1-4.

Measurement gap pattern configuration is defined in Table A.8.4.2.1.1-2.

In the measurement control information, it is indicated to the UE that event-triggered reporting with Event B2 (PCell becomes worse than threshold1 and inter RAT neighbour becomes better than threshold2) [16] is used. The test consists of two successive time periods, with time duration of T1, and T2 respectively. During time duration T1, the UE shall not have any timing information of NR cell 2.

Table A.8.4.2.1.1-1: NR inter-RAT event triggered reporting tests without SSB index reading for FR1

|  |  |
| --- | --- |
| Configuration | Description |
| 1 | LTE FDD, NR 15 kHz SSB SCS, 10 MHz bandwidth, FDD duplex mode |
| 2 | LTE FDD, NR 15 kHz SSB SCS, 10 MHz bandwidth, TDD duplex mode |
| 3 | LTE FDD, NR 30 kHz SSB SCS, 40 MHz bandwidth, TDD duplex mode |
| 4 | LTE TDD, NR 15 kHz SSB SCS, 10 MHz bandwidth, FDD duplex mode |
| 5 | LTE TDD, NR 15 kHz SSB SCS, 10 MHz bandwidth, TDD duplex mode |
| 6 | LTE TDD, NR 30 kHz SSB SCS, 40 MHz bandwidth, TDD duplex mode |
| Note 1: The UE is only required to be tested in one of the supported test configurations. |

Table A.8.4.2.1.1-2: General test parameters for NR inter-RAT event triggered reporting for FR1 without SSB time index detection

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Parameter | Unit | Test configuration | Value | Comment |
| E-UTRA RF Channel Number |  | 1, 2, 3, 4, 5, 6 | 1 | One E-UTRAcarrier frequency is used. |
| NR RF Chanel Number |  | 1, 2, 3, 4, 5, 6 | 1 | One FR1 NR carrier frequency is used. |
| Active cell |  | 1, 2, 3, 4, 5, 6 | E-UTRA cell 1 (PCell) | E-UTRA cell 1 is on E-UTRA RF channel number 1. |
| Neighbour cell |  | 1, 2, 3, 4, 5, 6 | NR cell 2 | NR cell 2 is on NR RF channel number 1. |
| Gap Pattern Id |  | 1, 2, 3, 4, 5, 6 | 0 | As specified in clause Table 8.1.2.1-1 of TS 36.133 [15]. |
| Measurement gap offset |  | 1, 2, 3, 4, 5, 6 | 39 | As specified in TS 36.331 [16]. |
| b2-Threshold1 | dBm | 1, 2, 3, 4, 5, 6 | Note 1 | E-UTRA RSRP threshold for E-UTRA RSRP measurement on cell 1 for event B2 [16] |
| b2-Threshold2NR | dBm | 1, 2, 3, 4, 5, 6 | Note 2 | SS-RSRP threshold for SS-RSRP measurement on cell 2 for event B2 [16] |
| Hysteresis | dB | 1, 2, 3, 4, 5, 6 | 0 |  |
| CP length |  | 1, 2, 3, 4, 5, 6 | Normal |  |
| TimeToTrigger | s | 1, 2, 3, 4, 5, 6 | 0 |  |
| Filter coefficient |  | 1, 2, 3, 4, 5, 6 | 0 | L3 filtering is not used |
| DRX |  | 1, 2, 3, 4, 5, 6 | OFF | DRX is not used |
| Time offset between serving and neighbour cells |  | 1, 4 | 3ms | Asynchronous cells.The timing of Cell 2 is 3ms later than the timing of Cell 1. |
|  | 2, 3, 5, 6 | 3μs | Synchronous cells. |
| T1 | s | 1, 2, 3, 4, 5, 6 | 5 |  |
| T2 | s | 1, 2, 3, 4, 5, 6 | 1 |  |
| Note 1: The value of b2-Threshold1 is defined in Table A.8.4.2.1.1-3Note 2: The value of b2-Threshold2NR is defined in Table A.8.4.2.1.1-4 |

Table A.8.4.2.1.1-3: E-UTRAN PCell specific test parameters for NR inter-RAT event triggered reporting in non-DRX with NR neigbour cell in FR1 without SSB time index detection

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | Unit | Configuration | Cell 1 |
| T1 | T2 |
| RF channel number |  | 1, 2, 3, 4, 5, 6 | 1 |
| Duplex mode |  | 1, 2, 3 | FDD |
| 4, 5, 6 | TDD |
| TDD special subframe configurationNote1 |  | 4, 5, 6 | 6 |
| TDD uplink-downlink configurationNote1 |  | 4, 5, 6 | 1 |
| BWchannel | MHz | 1, 2, 3, 4, 5, 6 | 5 MHz: NRB,c = 2510 MHz: NRB,c = 5020 MHz: NRB,c = 100 |
| PDSCH parameters:DL Reference Measurement ChannelNote2 |  | 1, 2, 3 | 5 MHz: R.7 FDD10 MHz: R.3 FDD20 MHz: R.6 FDD |
| 4, 5, 6 | 5 MHz: R.4 TDD10 MHz: R.0 TDD20 MHz: R.3 TDD |
| PCFICH/PDCCH/PHICH parameters:DL Reference Measurement ChannelNote2 |  | 1, 2, 3 | 5 MHz: R.11 FDD10 MHz: R.6 FDD20 MHz: R.10 FDD |
| 4, 5, 6 | 5 MHz: R.11 TDD10 MHz: R.6 TDD20 MHz: R.10 TDD |
| OCNG PatternsNote2 |  | 1, 2, 3 | 5 MHz: OP.20 FDD10 MHz: OP.10 FDD20 MHz: OP.17 FDD |
| 4, 5, 6 | 5 MHz: OP.9 TDD10 MHz: OP.1 TDD20 MHz: OP.7 TDD |
| b2-Threshold1 | dBm | 1, 2, 3, 4, 5, 6 | -79 |
| PBCH\_RA | dB | 1, 2, 3, 4, 5, 6 | 0 |
| PBCH\_RB |
| PSS\_RA |
| SSS\_RA |
| PCFICH\_RB |
| PHICH\_RA |
| PHICH\_RB |
| PDCCH\_RA |
| PDCCH\_RB |
| PDSCH\_RA |
| PDSCH\_RB |
| OCNG\_RANote3 |
| OCNG\_RBNote3 |
| NocNote4 | dBm/15kHz | 1, 2, 3, 4, 5, 6 | -104 |
| Ês/Noc | dB | 1, 2, 3, 4, 5, 6 | 17 | 17 |
| Ês/IotNote5 | dB | 1, 2, 3, 4, 5, 6 | 17 | 17 |
| RSRPNote5 | dBm/15kHz | 1, 2, 3, 4, 5, 6 | -87 | -87 |
| SCH\_RPNote5 | dBm/15kHz | 1, 2, 3, 4, 5, 6 | -87 | -87 |
| IoNote5 | dBm/9MHz | 1, 2, 3, 4, 5, 6 | -59.13+10log (NRB,c /50) | -59.13+10log (NRB,c /50) |
| Propagation Condition Note6 |  | 1, 2, 3, 4, 5, 6 | AWGN |
| Antenna Configuration and Correlation Matrix Note6 |  | 1, 2, 3, 4, 5, 6 | 1x2 |
| Note 1: Special subframe and uplink-downlink configurations are specified in table 4.2-1 in TS 36.211 [23].Note 2: DL RMCs and OCNG patterns are specified in clauses A 3.1 and A 3.2 of TS 36.133 [15] respectively.Note 3: OCNG shall be used such that all cells are fully allocated and a constant total transmitted power spectral density is achieved for all OFDM symbols.Note 4: Interference from other cells and noise sources not specified in the test is assumed to be constant over subcarriers and time and shall be modelled as AWGN of appropriate power for Noc to be fulfilled.Note 5: Ês/Iot, RSRP, SCH\_RP and Io levels have been derived from other parameters for information purposes. They are not settable parameters themselves.Note 6: Propagation condition and correlation matrix are defined in clause B.2 in TS 36.101 [25]. |

Table A.8.4.2.1.1-4: NR neighbour cell specific test parameters for NR inter-RAT event triggered reporting for FR1 without SSB time index detection

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | Unit | Test configuration | Cell 2 |
| T1 | T2 |
| NR RF Channel Number |  | 1, 2, 3, 4, 5, 6 | 1 |
| Duplex mode |  | 1, 4 | FDD |
| 2, 3, 5, 6 | TDD |
| TDD configuration |  | 2, 5 | TDDConf.1.1 |
| 3, 6 | TDDConf.2.1 |
| BWchannel | MHz | 1, 2, 4, 5 | 10: NRB,c = 52 |
| 3, 6 | 40: NRB,c = 106  |
| OCNG Patterns defined in A.3.2.1.1 (OP.1)  |  | 1, 2, 3, 4, 5, 6 | OP.1 |
| SMTC configuration defined in A.3.11.1 and A.3.11.2 |  | 1, 4 | SMTC.2 |
| 2, 3, 5, 6 | SMTC.1 |
| PDSCH/PDCCH subcarrier spacing | kHz | 1, 2, 4, 5 | 15 |
| 3, 6 | 30 |
| b2-Threshold2NR | dBm/SCS | 1, 2, 4, 5 | -101 |
| 3, 6 | -98 |
| EPRE ratio of PSS to SSS |  | 1, 2, 3, 4, 5, 6 | 0 |
| EPRE ratio of PBCH DMRS to SSS |  |
| EPRE ratio of PBCH to PBCH DMRS |  |
| EPRE ratio of PDCCH DMRS to SSS |  |
| EPRE ratio of PDCCH to PDCCH DMRS |  |
| EPRE ratio of PDSCH DMRS to SSS  |  |
| EPRE ratio of PDSCH to PDSCH  |  |
| EPRE ratio of OCNG DMRS to SSS (Note 1) |  |
| EPRE ratio of OCNG to OCNG DMRS (Note 1) |  |
| Note2 | dBm/15kHz | 1, 2, 3, 4, 5, 6 | -98 |
| Note2 | dBm/SCS | 1, 2, 4, 5 | -98 |
| 3, 6 | -95 |
| SS-RSRP Note 3 | dBm/SCS | 1, 2, 4, 5 | -Infinity | -91 |
| 3, 6 | -Infinity | -88 |
|  | dB | 1, 2, 3, 4, 5, 6 | -Infinity | 7 |
|  | dB | 1, 2, 3, 4, 5, 6 | -Infinity | 7 |
| IoNote3 | dBm/9.36MHz | 1, 2, 4, 5 | -70.05 | -62.26 |
| dBm/38.16MHz | 3, 6 | -63.95 | -56.16 |
| Propagation Condition  |  | 1, 2, 3, 4, 5, 6 | AWGN  |
| Antenna Configuration and Correlation Matrix |  | 1, 2, 3, 4, 5, 6 | 1x2 |
| Note 1: OCNG shall be used such that the cell is fully allocated and a constant total transmitted power spectral density is achieved for all OFDM symbols.Note 2: Interference from other cells and noise sources not specified in the test is assumed to be constant over subcarriers and time and shall be modelled as AWGN of appropriate power for  to be fulfilled.Note 3: SS-RSRP and Io levels have been derived from other parameters for information purposes. They are not settable parameters themselves.Note 4: SS-RSRP minimum requirements are specified assuming independent interference and noise at each receiver antenna port. |

##### A.8.4.2.1.2 Test Requirements

The UE shall send one Event B2 triggered measurement report, with a measurement reporting delay less than 920 ms from the beginning of time period T2. The UE shall not send event triggered measurement reports, as long as the reporting criteria are not fulfilled. The rate of correct events observed during repeated tests shall be at least 90%.

The UE is not required to report SSB time index.

NOTE: The actual overall delays measured in the test may be up to 2xTTIDCCH higher than the measurement reporting delays above because of TTI insertion uncertainty of the measurement report in DCCH.

#### A.8.4.2.2 NR Inter-RAT event triggered reporting tests for FR1 without SSB time index detection when DRX is used

##### A.8.4.2.2.1 Test Purpose and Environment

The purpose of this test is to verify that the UE makes correct reporting of an event. This test will partly verify the NR inter-RAT cell search requirements in clause 8.1.2.4.21 of TS 36.133 [15] for E-UTRAN FDD-NR measurements and clause 8.1.2.4.22 of TS 36.133 [15] for E-UTRAN TDD-NR measurements.

In this test, there are two cells: E-UTRA cell 1 as PCell on E-UTRA RF channel 1 and NR cell 2 as neighbour cell in FR1 on NR RF channel 1. The test parameters are given in Tables A.8.4.2.2.1-1, A.8.4.2.2.1-2, A.8.4.2.2.1-3 and A.8.4.2.2.1-4.

In tests 1 and 2, measurement gap pattern configuration is defined in Table A.8.4.2.2.1-2.

In the measurement control information, it is indicated to the UE that event-triggered reporting with Event B2 (PCell becomes worse than threshold1 and inter RAT neighbour becomes better than threshold2) [16] is used. The test consists of two successive time periods, with time duration of T1, and T2 respectively. During time duration T1, the UE shall not have any timing information of NR cell 2.

Table A.8.4.2.2.1-1: NR inter-RAT event triggered reporting tests without SSB index reading for FR1

|  |  |
| --- | --- |
| Configuration | Description |
| 1 | LTE FDD, NR 15 kHz SSB SCS, 10 MHz bandwidth, FDD duplex mode |
| 2 | LTE FDD, NR 15 kHz SSB SCS, 10 MHz bandwidth, TDD duplex mode |
| 3 | LTE FDD, NR 30 kHz SSB SCS, 40 MHz bandwidth, TDD duplex mode |
| 4 | LTE TDD, NR 15 kHz SSB SCS, 10 MHz bandwidth, FDD duplex mode |
| 5 | LTE TDD, NR 15 kHz SSB SCS, 10 MHz bandwidth, TDD duplex mode |
| 6 | LTE TDD, NR 30 kHz SSB SCS, 40 MHz bandwidth, TDD duplex mode |
| Note 1: The UE is only required to be tested in one of the supported test configurations. |

Table A.8.4.2.2.1-2: General test parameters for NR inter-RAT event triggered reporting for FR1 without SSB time index detection

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Parameter | Unit | Test configuration | Value | Comment |
| Test 1 | Test 2 |
| E-UTRA RF Channel Number |  | 1, 2, 3, 4, 5, 6 | 1 | One E-UTRA carrier frequency is used. |
| NR RF Channel Number |  | 1, 2, 3, 4, 5, 6 | 1 | One FR1 NR carrier frequency is used. |
| Active cell |  | 1, 2, 3, 4, 5, 6 | E-UTRA cell 1 (PCell) | E-UTRA cell 1 is on E-UTRA RF channel number 1. |
| Neighbour cell |  | 1, 2, 3, 4, 5, 6 | NR cell 2 | NR cell 2 is on NR RF channel number 1. |
| Gap Pattern Id |  | 1, 2, 3, 4, 5, 6 | 0 | As specified in clause Table 8.1.2.1-1 of TS 36.133 [15]. |
| Measurement gap offset |  | 1, 2, 3, 4, 5, 6 | 39 | As specified in TS 36.331 [16]. |
| b2-Threshold1 | dBm | 1, 2, 3, 4, 5, 6 | Note 1 | E-UTRA RSRP threshold for E-UTRA RSRP measurement on cell 1 for event B2 [16] |
| b2-Threshold2NR | dBm | 1, 2, 3, 4, 5, 6 | Note 2 | SS-RSRP threshold for SS-RSRP measurement on cell 2 for event B2 [16] |
| Hysteresis | dB | 1, 2, 3, 4, 5, 6 | 0 |  |
| CP length |  | 1, 2, 3, 4, 5, 6 | Normal |  |
| TimeToTrigger | s | 1, 2, 3, 4, 5, 6 | 0 |  |
| Filter coefficient |  | 1, 2, 3, 4, 5, 6 | 0 | L3 filtering is not used |
| DRX |  | 1, 2, 3, 4, 5, 6 | DRX.9 | DRX.12 | As specified in clause A.3.3 |
| Time offset between serving and neighbour cells |  | 1, 4 | 3ms | Asynchronous cells.The timing of Cell 2 is 3ms later than the timing of Cell 1. |
|  | 2, 3, 5, 6 | 3μs | Synchronous cells. |
| T1 | s | 1, 2, 3, 4, 5, 6 | 5 |  |
| T2 | s | 1, 2, 3, 4, 5, 6 | 2 | 11 |  |
| Note 1: The value of b2-Threshold1 is defined in Table A.8.4.2.2.1-3Note 2: The value of b2-Threshold2NR is defined in Table A.8.4.2.2.1-4 |

Table A.8.4.2.2.1-3: E-UTRAN PCell specific test parameters for NR inter-RAT event triggered reporting in non-DRX with NR neigbour cell in FR1 without SSB time index detection

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | Unit | Configuration | Cell 1 |
| T1 | T2 |
| RF channel number |  | 1, 2, 3, 4, 5, 6 | 1 |
| Duplex mode |  | 1, 2, 3 | FDD |
| 4, 5, 6 | TDD |
| TDD special subframe configurationNote1 |  | 4, 5, 6 | 6 |
| TDD uplink-downlink configurationNote1 |  | 4, 5, 6 | 1 |
| BWchannel | MHz | 1, 2, 3, 4, 5, 6 | 5 MHz: NRB,c = 2510 MHz: NRB,c = 5020 MHz: NRB,c = 100 |
| PDSCH parameters:DL Reference Measurement ChannelNote2 |  | 1, 2, 3 | 5 MHz: R.7 FDD10 MHz: R.3 FDD20 MHz: R.6 FDD |
| 4, 5, 6 | 5 MHz: R.4 TDD10 MHz: R.0 TDD20 MHz: R.3 TDD |
| PCFICH/PDCCH/PHICH parameters:DL Reference Measurement ChannelNote2 |  | 1, 2, 3 | 5 MHz: R.11 FDD10 MHz: R.6 FDD20 MHz: R.10 FDD |
| 4, 5, 6 | 5 MHz: R.11 TDD10 MHz: R.6 TDD20 MHz: R.10 TDD |
| OCNG PatternsNote2 |  | 1, 2, 3 | 5 MHz: OP.20 FDD10 MHz: OP.10 FDD20 MHz: OP.17 FDD |
| 4, 5, 6 | 5 MHz: OP.9 TDD10 MHz: OP.1 TDD20 MHz: OP.7 TDD |
| b2-Threshold1 | dBm | 1, 2, 3, 4, 5, 6 | -77 |
| PBCH\_RA | dB | 1, 2, 3, 4, 5, 6 | 0 |
| PBCH\_RB |
| PSS\_RA |
| SSS\_RA |
| PCFICH\_RB |
| PHICH\_RA |
| PHICH\_RB |
| PDCCH\_RA |
| PDCCH\_RB |
| PDSCH\_RA |
| PDSCH\_RB |
| OCNG\_RANote3 |
| OCNG\_RBNote3 |
| NocNote4 | dBm/15kHz | 1, 2, 3, 4, 5, 6 | -104 |
| Ês/Noc | dB | 1, 2, 3, 4, 5, 6 | 17 | 17 |
| Ês/IotNote5 | dB | 1, 2, 3, 4, 5, 6 | 17 | 17 |
| RSRPNote5 | dBm/15kHz | 1, 2, 3, 4, 5, 6 | -87 | -87 |
| SCH\_RPNote5 | dBm/15kHz | 1, 2, 3, 4, 5, 6 | -87 | -87 |
| IoNote5 | dBm/9MHz | 1, 2, 3, 4, 5, 6 | -59.13+10log (NRB,c /50) | -59.13+10log (NRB,c /50) |
| Propagation Condition Note6 |  | 1, 2, 3, 4, 5, 6 | AWGN |
| Antenna Configuration and Correlation Matrix Note6 |  | 1, 2, 3, 4, 5, 6 | 1x2 |
| Note 1: Special subframe and uplink-downlink configurations are specified in table 4.2-1 in TS 36.211 [23].Note 2: DL RMCs and OCNG patterns are specified in clauses A 3.1 and A 3.2 of TS 36.133 [15] respectively.Note 3: OCNG shall be used such that all cells are fully allocated and a constant total transmitted power spectral density is achieved for all OFDM symbols.Note 4: Interference from other cells and noise sources not specified in the test is assumed to be constant over subcarriers and time and shall be modelled as AWGN of appropriate power for Noc to be fulfilled.Note 5: Ês/Iot, RSRP, SCH\_RP and Io levels have been derived from other parameters for information purposes. They are not settable parameters themselves.Note 6: Propagation condition and correlation matrix are defined in clause B.2 in TS 36.101 [25]. |

Table A.8.4.2.2.1-4: NR neighbour cell specific test parameters for NR inter-RAT event triggered reporting for FR1 without SSB time index detection

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | Unit | Test configuration | Cell 2 |
| T1 | T2 |
| NR RF Channel Number |  | 1, 2, 3, 4, 5, 6 | 1 |
| Duplex mode |  | 1, 4 | FDD |
| 2, 3, 5, 6 | TDD |
| TDD configuration |  | 2, 5 | TDDConf.1.1 |
| 3, 6 | TDDConf.2.1 |
| BWchannel | MHz | 1, 2, 4, 5 | 10: NRB,c = 52 |
| 3, 6 | 40: NRB,c = 106  |
| OCNG Patterns defined in A.3.2.1.1 (OP.1)  |  | 1, 2, 3, 4, 5, 6 | OP.1 |
| SMTC configuration defined in A.3.11.1 and A.3.11.2 |  | 1, 4 | SMTC.2 |
| 2, 3, 5, 6 | SMTC.1 |
| PDSCH/PDCCH subcarrier spacing | kHz | 1, 2, 4, 5 | 15 |
| 3, 6 | 30 |
| b2-Threshold2NR | dBm/SCS | 1, 2, 4, 5 | -101 |
| 3, 6 | -98 |
| EPRE ratio of PSS to SSS |  | 1, 2, 3, 4, 5, 6 | 0 |
| EPRE ratio of PBCH DMRS to SSS |  |
| EPRE ratio of PBCH to PBCH DMRS |  |
| EPRE ratio of PDCCH DMRS to SSS |  |
| EPRE ratio of PDCCH to PDCCH DMRS |  |
| EPRE ratio of PDSCH DMRS to SSS  |  |
| EPRE ratio of PDSCH to PDSCH  |  |
| EPRE ratio of OCNG DMRS to SSS (Note 1) |  |
| EPRE ratio of OCNG to OCNG DMRS (Note 1) |  |
| Note2 | dBm/15kHz | 1, 2, 3, 4, 5, 6 | -98 |
| Note2 | dBm/SCS | 1, 2, 4, 5 | -98 |
| 3, 6 | -95 |
| SS-RSRP Note 3 | dBm/SCS | 1, 2, 4, 5 | -Infinity | -91 |
| 3, 6 | -Infinity | -88 |
|  | dB | 1, 2, 3, 4, 5, 6 | -Infinity | 7 |
|  | dB | 1, 2, 3, 4, 5, 6 | -Infinity | 7 |
| IoNote3 | dBm/9.36MHz | 1, 2, 4, 5 | -70.05 | -62.26 |
| dBm/38.16MHz | 3, 6 | -63.95 | -56.16 |
| Propagation Condition  |  | 1, 2, 3, 4, 5, 6 | AWGN  |
| Antenna Configuration and Correlation Matrix |  | 1, 2, 3, 4, 5, 6 | 1x2 |
| Note 1: OCNG shall be used such that the cell is fully allocated and a constant total transmitted power spectral density is achieved for all OFDM symbols.Note 2: Interference from other cells and noise sources not specified in the test is assumed to be constant over subcarriers and time and shall be modelled as AWGN of appropriate power for  to be fulfilled.Note 3: SS-RSRP and Io levels have been derived from other parameters for information purposes. They are not settable parameters themselves.Note 4: SS-RSRP minimum requirements are specified assuming independent interference and noise at each receiver antenna port. |

##### A.8.4.2.2.2 Test Requirements

In test 1 with per-UE gap, the UE shall send one Event B2 triggered measurement report, with a measurement reporting delay less than 1080 ms from the beginning of time period T2. The UE shall not send event triggered measurement reports, as long as the reporting criteria are not fulfilled. The rate of correct events observed during repeated tests shall be at least 90%.

In test 2 with per-UE gap, the UE shall send one Event B2 triggered measurement report, with a measurement reporting delay less than 10240 ms from the beginning of time period T2. The UE shall not send event triggered measurement reports, as long as the reporting criteria are not fulfilled. The rate of correct events observed during repeated tests shall be at least 90%.

In tests 1 and 2, the UE is not required to report SSB time index.

NOTE: The actual overall delays measured in the test may be up to 2xTTIDCCH higher than the measurement reporting delays above because of TTI insertion uncertainty of the measurement report in DCCH.

#### A.8.4.2.3 NR Inter-RAT event triggered reporting tests for FR1 with SSB time index detection when DRX is not used

##### A.8.4.2.3.1 Test Purpose and Environment

The purpose of this test is to verify that the UE makes correct reporting of an event. This test will partly verify the NR inter-RAT cell search requirements in clause 8.1.2.4.21of TS 36.133 [15] for E-UTRAN FDD-NR measurements and clause 8.1.2.4.22 of TS 36.133 [15] for E-UTRAN TDD-NR measurements.

In this test, there are two cells: E-UTRA cell 1 as PCell on E-UTRA RF channel 1 and NR cell 2 as neighbour cell in FR1 on NR RF channel 1. The test parameters are given in Tables A.8.4.2.3.1-1, A.8.4.2.3.1-2, A.8.4.2.3.1-3 and A.8.4.2.3.1-4.

Measurement gap pattern configuration is defined in Table A.8.4.2.3.1-2.

In the measurement control information, it is indicated to the UE that event-triggered reporting with Event B2 (PCell becomes worse than threshold1 and inter RAT neighbour becomes better than threshold2) [16] is used. In the measurement configuration the UE shall be indicated to report the SSB index of the identified NR cell. The test consists of two successive time periods, with time duration of T1, and T2 respectively. During time duration T1, the UE shall not have any timing information of NR cell 2.

Table A.8.4.2.3.1-1: NR inter-RAT event triggered reporting tests without SSB index reading for FR1

|  |  |
| --- | --- |
| Configuration | Description |
| 1 | LTE FDD, NR 15 kHz SSB SCS, 10 MHz bandwidth, FDD duplex mode |
| 2 | LTE FDD, NR 15 kHz SSB SCS, 10 MHz bandwidth, TDD duplex mode |
| 3 | LTE FDD, NR 30 kHz SSB SCS, 40 MHz bandwidth, TDD duplex mode |
| 4 | LTE TDD, NR 15 kHz SSB SCS, 10 MHz bandwidth, FDD duplex mode |
| 5 | LTE TDD, NR 15 kHz SSB SCS, 10 MHz bandwidth, TDD duplex mode |
| 6 | LTE TDD, NR 30 kHz SSB SCS, 40 MHz bandwidth, TDD duplex mode |
| Note 1: The UE is only required to be tested in one of the supported test configurations. |

Table A.8.4.2.3.1-2: General test parameters for NR inter-RAT event triggered reporting for FR1 without SSB time index detection

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Parameter | Unit | Test configuration | Value | Comment |
| E-UTRA RF Channel Number |  | 1, 2, 3, 4, 5, 6 | 1 | One E-UTRA carrier frequency is used. |
| NR RF Channel Number |  | 1, 2, 3, 4, 5, 6 | 1 | One FR1 NR carrier frequency is used. |
| Active cell |  | 1, 2, 3, 4, 5, 6 | E-UTRA cell 1 (PCell) | E-UTRA cell 1 is on E-UTRA RF channel number 1. |
| Neighbour cell |  | 1, 2, 3, 4, 5, 6 | NR cell 2 | NR cell 2 is on NR RF channel number 1. |
| Gap Pattern Id |  | 1, 2, 3, 4, 5, 6 | 0 | As specified in clause Table 8.1.2.1-1 of TS 36.133 [15]. |
| Measurement gap offset |  | 1, 2, 3, 4, 5, 6 | 39 | As specified in TS 36.331 [16]. |
| b2-Threshold1 | dBm | 1, 2, 3, 4, 5, 6 | Note 1 | E-UTRA RSRP threshold for E-UTRA RSRP measurement on cell 1 for event B2 [16] |
| b2-Threshold2NR | dBm | 1, 2, 3, 4, 5, 6 | Note 2 | SS-RSRP threshold for SS-RSRP measurement on cell 2 for event B2 [16] |
| Hysteresis | dB | 1, 2, 3, 4, 5, 6 | 0 |  |
| CP length |  | 1, 2, 3, 4, 5, 6 | Normal |  |
| TimeToTrigger | s | 1, 2, 3, 4, 5, 6 | 0 |  |
| Filter coefficient |  | 1, 2, 3, 4, 5, 6 | 0 | L3 filtering is not used |
| DRX |  | 1, 2, 3, 4, 5, 6 | OFF | DRX is not used |
| Time offset between serving and neighbour cells |  | 1, 4 | 3ms | Asynchronous cells.The timing of Cell 2 is 3 ms later than the timing of Cell 1. |
|  | 2, 3, 5, 6 | 3μs | Synchronous cells. |
| T1 | s | 1, 2, 3, 4, 5, 6 | 5 |  |
| T2 | s | 1, 2, 3, 4, 5, 6 | 2 |  |
| Note 1: The value of b2-Threshold1 is defined in Table A.8.4.2.3.1-3Note 2: The value of b2-Threshold2NR is defined in Table A.8.4.2.3.1-4 |

Table A.8.4.2.3.1-3: E-UTRAN PCell specific test parameters for NR inter-RAT event triggered reporting in non-DRX with NR neigbour cell in FR1 without SSB time index detection

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | Unit | Configuration | Cell 1 |
| T1 | T2 |
| RF channel number |  | 1, 2, 3, 4, 5, 6 | 1 |
| Duplex mode |  | 1, 2, 3 | FDD |
| 4, 5, 6 | TDD |
| TDD special subframe configurationNote1 |  | 4, 5, 6 | 6 |
| TDD uplink-downlink configurationNote1 |  | 4, 5, 6 | 1 |
| BWchannel | MHz | 1, 2, 3, 4, 5, 6 | 5 MHz: NRB,c = 2510 MHz: NRB,c = 5020 MHz: NRB,c = 100 |
| PDSCH parameters:DL Reference Measurement ChannelNote2 |  | 1, 2, 3 | 5 MHz: R.7 FDD10 MHz: R.3 FDD20 MHz: R.6 FDD |
| 4, 5, 6 | 5 MHz: R.4 TDD10 MHz: R.0 TDD20 MHz: R.3 TDD |
| PCFICH/PDCCH/PHICH parameters:DL Reference Measurement ChannelNote2 |  | 1, 2, 3 | 5 MHz: R.11 FDD10 MHz: R.6 FDD20 MHz: R.10 FDD |
| 4, 5, 6 | 5 MHz: R.11 TDD10 MHz: R.6 TDD20 MHz: R.10 TDD |
| OCNG PatternsNote2 |  | 1, 2, 3 | 5 MHz: OP.20 FDD10 MHz: OP.10 FDD20 MHz: OP.17 FDD |
| 4, 5, 6 | 5 MHz: OP.9 TDD10 MHz: OP.1 TDD20 MHz: OP.7 TDD |
| b2-Threshold1 | dBm | 1, 2, 3, 4, 5, 6 | -77 |
| PBCH\_RA | dB | 1, 2, 3, 4, 5, 6 | 0 |
| PBCH\_RB |
| PSS\_RA |
| SSS\_RA |
| PCFICH\_RB |
| PHICH\_RA |
| PHICH\_RB |
| PDCCH\_RA |
| PDCCH\_RB |
| PDSCH\_RA |
| PDSCH\_RB |
| OCNG\_RANote3 |
| OCNG\_RBNote3 |
| NocNote4 | dBm/15kHz | 1, 2, 3, 4, 5, 6 | -104 |
| Ês/Noc | dB | 1, 2, 3, 4, 5, 6 | 17 | 17 |
| Ês/IotNote5 | dB | 1, 2, 3, 4, 5, 6 | 17 | 17 |
| RSRPNote5 | dBm/15kHz | 1, 2, 3, 4, 5, 6 | -87 | -87 |
| SCH\_RPNote5 | dBm/15kHz | 1, 2, 3, 4, 5, 6 | -87 | -87 |
| IoNote5 | dBm/9MHz | 1, 2, 3, 4, 5, 6 | -59.13+10log (NRB,c /50) | -59.13+10log (NRB,c /50) |
| Propagation Condition Note6 |  | 1, 2, 3, 4, 5, 6 | AWGN |
| Antenna Configuration and Correlation Matrix Note6 |  | 1, 2, 3, 4, 5, 6 | 1x2 |
| Note 1: Special subframe and uplink-downlink configurations are specified in table 4.2-1 in TS 36.211 [23].Note 2: DL RMCs and OCNG patterns are specified in clauses A 3.1 and A 3.2 of TS 36.133 [15] respectively.Note 3: OCNG shall be used such that all cells are fully allocated and a constant total transmitted power spectral density is achieved for all OFDM symbols.Note 4: Interference from other cells and noise sources not specified in the test is assumed to be constant over subcarriers and time and shall be modelled as AWGN of appropriate power for Noc to be fulfilled.Note 5: Ês/Iot, RSRP, SCH\_RP and Io levels have been derived from other parameters for information purposes. They are not settable parameters themselves.Note 6: Propagation condition and correlation matrix are defined in clause B.2 in TS 36.101 [25]. |

Table A.8.4.2.3.1-4: NR neighbour cell specific test parameters for NR inter-RAT event triggered reporting for FR1 without SSB time index detection

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | Unit | Test configuration | Cell 2 |
| T1 | T2 |
| NR RF Channel Number |  | 1, 2, 3, 4, 5, 6 | 1 |
| Duplex mode |  | 1, 4 | FDD |
| 2, 3, 5, 6 | TDD |
| TDD configuration |  | 2, 5 | TDDConf.1.1 |
| 3, 6 | TDDConf.2.1 |
| BWchannel | MHz | 1, 2, 4, 5 | 10: NRB,c = 52 |
| 3, 6 | 40: NRB,c = 106  |
| OCNG Patterns defined in A.3.2.1.1 (OP.1)  |  | 1, 2, 3, 4, 5, 6 | OP.1 |
| SMTC configuration defined in A.3.11.1 and A.3.11.2 |  | 1, 4 | SMTC.2 |
| 2, 3, 5, 6 | SMTC.1 |
| PDSCH/PDCCH subcarrier spacing | kHz | 1, 2, 4, 5 | 15 |
| 3, 6 | 30 |
| b2-Threshold2NR | dBm/SCS | 1, 2, 4, 5 | -101 |
| 3, 6 | -98 |
| EPRE ratio of PSS to SSS |  | 1, 2, 3, 4, 5, 6 | 0 |
| EPRE ratio of PBCH DMRS to SSS |  |
| EPRE ratio of PBCH to PBCH DMRS |  |
| EPRE ratio of PDCCH DMRS to SSS |  |
| EPRE ratio of PDCCH to PDCCH DMRS |  |
| EPRE ratio of PDSCH DMRS to SSS  |  |
| EPRE ratio of PDSCH to PDSCH  |  |
| EPRE ratio of OCNG DMRS to SSS (Note 1) |  |
| EPRE ratio of OCNG to OCNG DMRS (Note 1) |  |
| Note2 | dBm/15kHz | 1, 2, 3, 4, 5, 6 | -98 |
| Note2 | dBm/SCS | 1, 2, 4, 5 | -98 |
| 3, 6 | -95 |
| SS-RSRP Note 3 | dBm/SCS | 1, 2, 4, 5 | -Infinity | -91 |
| 3, 6 | -Infinity | -88 |
|  | dB | 1, 2, 3, 4, 5, 6 | -Infinity | 7 |
|  | dB | 1, 2, 3, 4, 5, 6 | -Infinity | 7 |
| IoNote3 | dBm/9.36MHz | 1, 2, 4, 5 | -70.05 | -62.26 |
| dBm/38.16MHz | 3, 6 | -63.95 | -56.16 |
| Propagation Condition  |  | 1, 2, 3, 4, 5, 6 | AWGN |
| Antenna Configuration and Correlation Matrix |  | 1, 2, 3, 4, 5, 6 | 1x2 |
| Note 1: OCNG shall be used such that the cell is fully allocated and a constant total transmitted power spectral density is achieved for all OFDM symbols.Note 2: Interference from other cells and noise sources not specified in the test is assumed to be constant over subcarriers and time and shall be modelled as AWGN of appropriate power for  to be fulfilled.Note 3: SS-RSRP and Io levels have been derived from other parameters for information purposes. They are not settable parameters themselves.Note 4: SS-RSRP minimum requirements are specified assuming independent interference and noise at each receiver antenna port. |

##### A.8.4.2.3.2 Test Requirements

The UE shall send one Event B2 triggered measurement report, with a measurement reporting delay less than 1040 ms from the beginning of time period T2. The UE shall not send event triggered measurement reports, as long as the reporting criteria are not fulfilled. The rate of correct events observed during repeated tests shall be at least 90%.

The UE is required to report SSB time index.

NOTE: The actual overall delays measured in the test may be up to 2xTTIDCCH higher than the measurement reporting delays above because of TTI insertion uncertainty of the measurement report in DCCH.

#### A.8.4.2.4 NR Inter-RAT event triggered reporting tests for FR1 with SSB time index detection when DRX is used

##### A.8.4.2.4.1 Test Purpose and Environment

The purpose of this test is to verify that the UE makes correct reporting of an event. This test will partly verify the NR inter-RAT cell search requirements in clause 8.1.2.4.21of TS 36.133 [15] for E-UTRAN FDD-NR measurements and clause 8.1.2.4.22 of TS 36.133 [15] for E-UTRAN TDD-NR measurements.

In this test, there are two cells: E-UTRA cell 1 as PCell on E-UTRA RF channel 1 and NR cell 2 as neighbour cell in FR1 on NR RF channel 1. The test parameters are given in Tables A.8.4.2.4.1-1, A.8.4.2.4.1-2, A.8.4.2.4.1-3 and A.8.4.2.4.1-4.

In tests 1 and 2, measurement gap pattern configuration is defined in Table A.8.4.2.4.1-2.

In the measurement control information, it is indicated to the UE that event-triggered reporting with Event B2 (PCell becomes worse than threshold1 and inter RAT neighbour becomes better than threshold2) [16] is used. In the measurement configuration the UE shall be indicated to report the SSB index of the identified NR cell. The test consists of two successive time periods, with time duration of T1, and T2 respectively. During time duration T1, the UE shall not have any timing information of NR cell 2.

Table A.8.4.2.4.1-1: NR inter-RAT event triggered reporting tests without SSB index reading for FR1

|  |  |
| --- | --- |
| Configuration | Description |
| 1 | LTE FDD, NR 15 kHz SSB SCS, 10 MHz bandwidth, FDD duplex mode |
| 2 | LTE FDD, NR 15 kHz SSB SCS, 10 MHz bandwidth, TDD duplex mode |
| 3 | LTE FDD, NR 30 kHz SSB SCS, 40 MHz bandwidth, TDD duplex mode |
| 4 | LTE TDD, NR 15 kHz SSB SCS, 10 MHz bandwidth, FDD duplex mode |
| 5 | LTE TDD, NR 15 kHz SSB SCS, 10 MHz bandwidth, TDD duplex mode |
| 6 | LTE TDD, NR 30 kHz SSB SCS, 40 MHz bandwidth, TDD duplex mode |
| Note 1: The UE is only required to be tested in one of the supported test configurations. |

Table A.8.4.2.4.1-2: General test parameters for NR inter-RAT event triggered reporting for FR1 without SSB time index detection

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Parameter | Unit | Test configuration | Value | Comment |
| Test 1 | Test 2 |
| E-UTRA RF Channel Number |  | 1, 2, 3, 4, 5, 6 | 1 | One E-UTRA carrier frequency is used. |
| NR RF Channel Number |  | 1, 2, 3, 4, 5, 6 | 1 | One FR1 NR carrier frequency is used. |
| Active cell |  | 1, 2, 3, 4, 5, 6 | E-UTRA cell 1 (PCell) | E-UTRA cell 1 is on E-UTRA RF channel number 1. |
| Neighbour cell |  | 1, 2, 3, 4, 5, 6 | NR cell 2 | NR cell 2 is on NR RF channel number 1. |
| Gap Pattern Id |  | 1, 2, 3, 4, 5, 6 | 0 | As specified in clause Table 8.1.2.1-1 of TS 36.133 [15]. |
| Measurement gap offset |  | 1, 2, 3, 4, 5, 6 | 39 | As specified in TS 36.331 [16]. |
| b2-Threshold1 | dBm | 1, 2, 3, 4, 5, 6 | Note 1 | E-UTRA RSRP threshold for E-UTRA RSRP measurement on cell 1 for event B2 [16] |
| b2-Threshold2NR | dBm | 1, 2, 3, 4, 5, 6 | Note 2 | SS-RSRP threshold for SS-RSRP measurement on cell 2 for event B2 [16] |
| Hysteresis | dB | 1, 2, 3, 4, 5, 6 | 0 |  |
| CP length |  | 1, 2, 3, 4, 5, 6 | Normal |  |
| TimeToTrigger | s | 1, 2, 3, 4, 5, 6 | 0 |  |
| Filter coefficient |  | 1, 2, 3, 4, 5, 6 | 0 | L3 filtering is not used |
| DRX |  | 1, 2, 3, 4, 5, 6 | DRX.9 | DRX.12 | As specified in clause A.3.3 |
| Time offset between serving and neighbour cells |  | 1, 4 | 3ms | Asynchronous cells.The timing of Cell 2 is 3ms later than the timing of Cell 1. |
|  | 2, 3, 5, 6 | 3μs | Synchronous cells. |
| T1 | s | 1, 2, 3, 4, 5, 6 | 5 |  |
| T2 | s | 1, 2, 3, 4, 5, 6 | 2 | 13 |  |
| Note 1: The value of b2-Threshold1 is defined in Table A.8.4.2.4.1-3Note 2: The value of b2-Threshold2NR is defined in Table A.8.4.2.4.1-4 |

Table A.8.4.2.4.1-3: E-UTRAN PCell specific test parameters for NR inter-RAT event triggered reporting in non-DRX with NR neigbour cell in FR1 without SSB time index detection

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | Unit | Configuration | Cell 1 |
| T1 | T2 |
| RF channel number |  | 1, 2, 3, 4, 5, 6 | 1 |
| Duplex mode |  | 1, 2, 3 | FDD |
| 4, 5, 6 | TDD |
| TDD special subframe configurationNote1 |  | 4, 5, 6 | 6 |
| TDD uplink-downlink configurationNote1 |  | 4, 5, 6 | 1 |
| BWchannel | MHz | 1, 2, 3, 4, 5, 6 | 5 MHz: NRB,c = 2510 MHz: NRB,c = 5020 MHz: NRB,c = 100 |
| PDSCH parameters:DL Reference Measurement ChannelNote2 |  | 1, 2, 3 | 5 MHz: R.7 FDD10 MHz: R.3 FDD20 MHz: R.6 FDD |
| 4, 5, 6 | 5 MHz: R.4 TDD10 MHz: R.0 TDD20 MHz: R.3 TDD |
| PCFICH/PDCCH/PHICH parameters:DL Reference Measurement ChannelNote2 |  | 1, 2, 3 | 5 MHz: R.11 FDD10 MHz: R.6 FDD20 MHz: R.10 FDD |
| 4, 5, 6 | 5 MHz: R.11 TDD10 MHz: R.6 TDD20 MHz: R.10 TDD |
| OCNG PatternsNote2 |  | 1, 2, 3 | 5 MHz: OP.20 FDD10 MHz: OP.10 FDD20 MHz: OP.17 FDD |
| 4, 5, 6 | 5 MHz: OP.9 TDD10 MHz: OP.1 TDD20 MHz: OP.7 TDD |
| b2-Threshold1 | dBm | 1, 2, 3, 4, 5, 6 | -77 |
| PBCH\_RA | dB | 1, 2, 3, 4, 5, 6 | 0 |
| PBCH\_RB |
| PSS\_RA |
| SSS\_RA |
| PCFICH\_RB |
| PHICH\_RA |
| PHICH\_RB |
| PDCCH\_RA |
| PDCCH\_RB |
| PDSCH\_RA |
| PDSCH\_RB |
| OCNG\_RANote3 |
| OCNG\_RBNote3 |
| NocNote4 | dBm/15kHz | 1, 2, 3, 4, 5, 6 | -104 |
| Ês/Noc | dB | 1, 2, 3, 4, 5, 6 | 17 | 17 |
| Ês/IotNote5 | dB | 1, 2, 3, 4, 5, 6 | 17 | 17 |
| RSRPNote5 | dBm/15kHz | 1, 2, 3, 4, 5, 6 | -87 | -87 |
| SCH\_RPNote5 | dBm/15kHz | 1, 2, 3, 4, 5, 6 | -87 | -87 |
| IoNote5 | dBm/9MHz | 1, 2, 3, 4, 5, 6 | -59.13+10log (NRB,c /50) | -59.13+10log (NRB,c /50) |
| Propagation Condition Note6 |  | 1, 2, 3, 4, 5, 6 | AWGN |
| Antenna Configuration and Correlation Matrix Note6 |  | 1, 2, 3, 4, 5, 6 | 1x2 |
| Note 1: Special subframe and uplink-downlink configurations are specified in table 4.2-1 in TS 36.211 [23].Note 2: DL RMCs and OCNG patterns are specified in clauses A 3.1 and A 3.2 of TS 36.133 [15] respectively.Note 3: OCNG shall be used such that all cells are fully allocated and a constant total transmitted power spectral density is achieved for all OFDM symbols.Note 4: Interference from other cells and noise sources not specified in the test is assumed to be constant over subcarriers and time and shall be modelled as AWGN of appropriate power for Noc to be fulfilled.Note 5: Ês/Iot, RSRP, SCH\_RP and Io levels have been derived from other parameters for information purposes. They are not settable parameters themselves.Note 6: Propagation condition and correlation matrix are defined in clause B.2 in TS 36.101 [25]. |

Table A.8.4.2.4.1-4: NR neighbour cell specific test parameters for NR inter-RAT event triggered reporting for FR1 without SSB time index detection

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | Unit | Test configuration | Cell 2 |
| T1 | T2 |
| NR RF Channel Number |  | 1, 2, 3, 4, 5, 6 | 1 |
| Duplex mode |  | 1, 4 | FDD |
| 2, 3, 5, 6 | TDD |
| TDD configuration |  | 2, 5 | TDDConf.1.1 |
| 3, 6 | TDDConf.2.1 |
| BWchannel | MHz | 1, 2, 4, 5 | 10: NRB,c = 52 |
| 3, 6 | 40: NRB,c = 106  |
| OCNG Patterns defined in A.3.2.1.1 (OP.1)  |  | 1, 2, 3, 4, 5, 6 | OP.1 |
| SMTC configuration defined in A.3.11.1 and A.3.11.2 |  | 1, 4 | SMTC.2 |
| 2, 3, 5, 6 | SMTC.1 |
| PDSCH/PDCCH subcarrier spacing | kHz | 1, 2, 4, 5 | 15 |
| 3, 6 | 30 |
| b2-Threshold2NR | dBm/SCS | 1, 2, 4, 5 | -101 |
| 3, 6 | -98 |
| EPRE ratio of PSS to SSS |  | 1, 2, 3, 4, 5, 6 | 0 |
| EPRE ratio of PBCH DMRS to SSS |  |
| EPRE ratio of PBCH to PBCH DMRS |  |
| EPRE ratio of PDCCH DMRS to SSS |  |
| EPRE ratio of PDCCH to PDCCH DMRS |  |
| EPRE ratio of PDSCH DMRS to SSS  |  |
| EPRE ratio of PDSCH to PDSCH  |  |
| EPRE ratio of OCNG DMRS to SSS (Note 1) |  |
| EPRE ratio of OCNG to OCNG DMRS (Note 1) |  |
| Note2 | dBm/15kHz | 1, 2, 3, 4, 5, 6 | -98 |
| Note2 | dBm/SCS | 1, 2, 4, 5 | -98 |
| 3, 6 | -95 |
| SS-RSRP Note 3 | dBm/SCS | 1, 2, 4, 5 | -Infinity | -91 |
| 3, 6 | -Infinity | -88 |
|  | dB | 1, 2, 3, 4, 5, 6 | -Infinity | 7 |
|  | dB | 1, 2, 3, 4, 5, 6 | -Infinity | 7 |
| IoNote3 | dBm/9.36MHz | 1, 2, 4, 5 | -70.05 | -62.26 |
| dBm/38.16MHz | 3, 6 | -63.95 | -56.16 |
| Propagation Condition  |  | 1, 2, 3, 4, 5, 6 | AWGN |
| Antenna Configuration and Correlation Matrix |  | 1, 2, 3, 4, 5, 6 | 1x2 |
| Note 1: OCNG shall be used such that the cell is fully allocated and a constant total transmitted power spectral density is achieved for all OFDM symbols.Note 2: Interference from other cells and noise sources not specified in the test is assumed to be constant over subcarriers and time and shall be modelled as AWGN of appropriate power for  to be fulfilled.Note 3: SS-RSRP and Io levels have been derived from other parameters for information purposes. They are not settable parameters themselves.Note 4: SS-RSRP minimum requirements are specified assuming independent interference and noise at each receiver antenna port. |

##### A.8.4.2.4.2 Test Requirements

In test 1 with per-UE gap, the UE shall send one Event B2 triggered measurement report, with a measurement reporting delay less than 1280 ms from the beginning of time period T2. The UE shall not send event triggered measurement reports, as long as the reporting criteria are not fulfilled. The rate of correct events observed during repeated tests shall be at least 90%.

In test 2 with per-UE gap, the UE shall send one Event B2 triggered measurement report, with a measurement reporting delay less than 12160 ms from the beginning of time period T2. The UE shall not send event triggered measurement reports, as long as the reporting criteria are not fulfilled. The rate of correct events observed during repeated tests shall be at least 90%.

In tests 1 and 2, the UE is required to report SSB time index.

NOTE: The actual overall delays measured in the test may be up to 2xTTIDCCH higher than the measurement reporting delays above because of TTI insertion uncertainty of the measurement report in DCCH.

#### A.8.4.2.5 NR Inter-RAT event triggered reporting tests for FR2 without SSB time index detection when DRX is not used

##### A.8.4.2.5.1 Test Purpose and Environment

The purpose of this test is to verify that the UE makes correct reporting of an event. This test will partly verify the NR inter-RAT cell search requirements in clause 8.1.2.4.21of TS 36.133 [15] for E-UTRAN FDD-NR measurements and clause 8.1.2.4.22 of TS 36.133 [15] for E-UTRAN TDD-NR measurements.

In this test, there are two cells: E-UTRA cell 1 as PCell on E-UTRA RF channel 1 and NR cell 2 as neighbour cell in FR2 on NR RF channel 1. The test parameters are given in Tables A.8.4.2.5.1-1, A.8.4.2.5.1-2 and A.8.4.2.5.1-3.

The cell specific test parameters for E-UTRA cell1 as PCell are defined in clause A.3.7.2.2.

Measurement gap pattern configuration defined in Table A.8.4.2.5.1-2 is provided for a UE that does not support per-FR gap, and no gap pattern (Gap Pattern Id and Measurement gap offset) is configured for a UE capable of per-FR gap.

In the measurement control information, it is indicated to the UE that event-triggered reporting with Event B1 (Inter RAT neighbour becomes better than threshold) [16] is used. The test consists of two successive time periods, with time duration of T1, and T2 respectively. During time duration T1, the UE shall not have timing information of NR cell 2.

Table A.8.4.2.5.1-1: NR inter-RAT event triggered reporting test without SSB index reading for FR2 in non-DRX

|  |  |
| --- | --- |
| Configuration | Description |
| 1 | LTE FDD, NR 120 kHz SSB SCS, 100 MHz bandwidth, TDD duplex mode |
| 2 | LTE TDD, NR 120 kHz SSB SCS, 100 MHz bandwidth, TDD duplex mode |
| Note 1: The UE is only required to be tested in one of the supported test configurations. |

Table A.8.4.2.5.1-2: General test parameters for NR inter-RAT event triggered reporting for FR2 without SSB time index detection in non-DRX

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Parameter | Unit | Test configuration | Value | Comment |
| E-UTRA RF Channel Number |  | 1, 2 | 1 | One E-UTRA carrier frequency is used. |
| NR RF Channel Number |  | 1, 2 | 1 | One FR2 NR carrier frequency is used. |
| Active cell |  | 1, 2 | E-UTRA cell 1 (PCell) | E-UTRA cell 1 is on E-UTRA RF channel number 1 as defined in clause A.3.7.2.2. |
| Neighbour cell |  | 1, 2 | NR cell 2 | NR cell 2 is on NR RF channel number 1. |
| Gap Pattern Id |  | 1, 2 | 0 | As specified in clause Table 8.1.2.1-1 of TS 36.133 [15]. |
| Measurement gap offset |  | 1, 2 | 39 | As specified in TS 36.331 [16]. |
| b1-ThresholdNR | dBm | 1, 2 | Note 1 | SS-RSRP threshold for SS-RSRP measurement on cell 2 for event B1 [16] |
| Hysteresis | dB | 1, 2 | 0 |  |
| CP length |  | 1, 2 | Normal |  |
| TimeToTrigger | s | 1, 2 | 0 |  |
| Filter coefficient |  | 1, 2 | 0 | L3 filtering is not used |
| DRX |  | 1, 2 | OFF | DRX is not used |
| Time offset between serving and neighbour cells |  | 1 | 3ms | Asynchronous cells.The timing of Cell 2 is 3ms later than the timing of Cell 1. |
|  | 2 | 3μs | Synchronous cells. |
| T1 | s | 1, 2 | 10 |  |
| T2 | s | 1, 2 | 6 |  |
| Note 1: The value of b1-ThresholdNR is defined in Table A.8.4.2.5.1-3 |

Table A.8.4.2.5.1-3: NR neighbour cell specific test parameters for NR inter-RAT event triggered reporting for FR2 without SSB time index detection in non-DRX

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | Unit | Test configuration | Cell 2 |
| T1 | T2 |
| AoA setup defined in A.3.15.2.1 |  | 1, 2 | Setup 2a |
| Assumption for UE beamsNote 5 |  | 1, 2 | Rough |
| NR RF Channel Number |  | 1, 2 | 1 |
| Duplex mode |  | 1, 2 | TDD |
| TDD configuration |  | 1, 2 | TDDConf.3.1 |
| BWchannel | MHz | 1, 2 | 100: NRB,c = 24 |
| OCNG patterns defined in A.3.2.1.3 |  | 1, 2 | OP.3 |
| SMTC configuration defined in A.3.11.1 and A.3.11.2 |  | 1 | SMTC.2 |
| 2 | SMTC.1 |
| PDSCH/PDCCH subcarrier spacing | kHz | 1, 2 | 120 |
| b1-ThresholdNR | UE power class 3 | dBm/SCS | 1, 2 | -112 |
| EPRE ratio of PSS to SSS |  | 1, 2 | 0 |
| EPRE ratio of PBCH DMRS to SSS |  |
| EPRE ratio of PBCH to PBCH DMRS |  |
| EPRE ratio of PDCCH DMRS to SSS |  |
| EPRE ratio of PDCCH to PDCCH DMRS |  |
| EPRE ratio of PDSCH DMRS to SSS  |  |
| EPRE ratio of PDSCH to PDSCH  |  |
| EPRE ratio of OCNG DMRS to SSS (Note 1) |  |
| EPRE ratio of OCNG to OCNG DMRS (Note 1) |  |
|  Ês | dBm/SCS | 1, 2 | -Infinity | -80.6 |
| SSB-RP Note 3 | dBm/SCS | 1, 2 | -Infinity | -80.6 |
| BB Note 6 | dB | 1, 2 | -Infinity | 8.3 |
| IoNote3 | dBm/95.04MHz | 1, 2 | -Infinity | -56.0 |
| Propagation Condition |  | 1, 2 | AWGN |
| Note 1: OCNG shall be used such that a constant total transmitted power spectral density is achieved for all OFDM symbols.Note 2: VoidNote 3: SSB-RP and Io levels have been derived from other parameters for information purposes. They are not settable parameters themselves.Note 4: VoidNote 5: Information about types of UE beam is given in B.2.1.3, and does not limit UE implementation or test system implementationNote 6: Calculation of Es/IotBB includes the effect of UE internal noise up to the value assumed for the associated Refsens requirement in clause 7.3.2 of TS 36.101-2 [19], and an allowance of 1dB for UE multi-band relaxation factor ΔMBP from TS 38.101-2 [19] Table 6.2.1.3-4. |

##### A.8.4.2.5.2 Test Requirements

The UE shall send one Event B1 triggered measurement report, with a measurement reporting delay less than D1 ms and D2 ms from the beginning of time period T2 for a UE incapable of per-FR gap and for a UE capable of per-FR gap, respectively. The UE shall not send event triggered measurement reports, as long as the reporting criteria are not fulfilled. The rate of correct events observed during repeated tests shall be at least 90%.

The UE is not required to report SSB time index.

Table A.8.4.2.5.2-1: Test requirements for NR inter-RAT event triggered reporting for FR2 without SSB time index detection in non-DRX

|  |  |
| --- | --- |
| Test case | Measurement reporting delay (ms) |
| D1 ms | D2 ms |
| UE power class 3 | 3200 | 1600 |

NOTE: The actual overall delays measured in the test may be up to 2xTTIDCCH higher than the measurement reporting delays above because of TTI insertion uncertainty of the measurement report in DCCH.

#### A.8.4.2.6 NR Inter-RAT event triggered reporting tests for FR2 without SSB time index detection when DRX is used

##### A.8.4.2.6.1 Test Purpose and Environment

The purpose of this test is to verify that the UE makes correct reporting of an event. This test will partly verify the NR inter-RAT cell search requirements in clause 8.1.2.4.21 of TS 36.133 [15] for E-UTRAN FDD-NR measurements and clause 8.1.2.4.22 of TS 36.133 [15] for E-UTRAN TDD-NR measurements.

In this test, there are two cells: E-UTRA cell 1 as PCell on E-UTRA RF channel 1 and NR cell 2 as neighbour cell in FR2 on NR RF channel 1. The test parameters are given in Tables A.8.4.2.6.1-1, A.8.4.2.6.1-2 and A.8.4.2.6.1-3.

The cell specific test parameters for E-UTRA cell1 as PCell are defined in clause A.3.7.2.2.

Measurement gap pattern configuration defined in Table A.8.4.2.6.1-2 is provided for a UE that does not support per-FR gap, and no gap pattern (Gap Pattern Id and Measurement gap offset) is configured for a UE capable of per-FR gap.

In the measurement control information, it is indicated to the UE that event-triggered reporting with Event B1 (Inter RAT neighbour becomes better than threshold) [16] is used. The test consists of two successive time periods, with time duration of T1, and T2 respectively. During time duration T1, the UE shall not have timing information of NR cell 2.

Table A.8.4.2.6.1-1: NR inter-RAT event triggered reporting tests without SSB index reading for FR2 in DRX

|  |  |
| --- | --- |
| **Configuration** | **Description** |
| 1 | LTE FDD, NR 120 kHz SSB SCS, 100 MHz bandwidth, TDD duplex mode |
| 2 | LTE TDD, NR 120 kHz SSB SCS, 100 MHz bandwidth, TDD duplex mode |
| Note 1: The UE is only required to be tested in one of the supported test configurations. |

Table A.8.4.2.6.1-2: General test parameters for NR inter-RAT event triggered reporting for FR2 without SSB time index detection in DRX

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Parameter | Unit | Test configuration | Value | Comment |
| Test 1 | Test 2 |
| E-UTRA RF Channel Number |  | 1, 2 | 1 | One E-UTRA carrier frequency is used. |
| NR RF Channel Number |  | 1, 2 | 1 | One FR2 NR carrier frequency is used. |
| Active cell |  | 1, 2, 3, 4, 5, 6 | E-UTRA cell 1 (PCell) | E-UTRA cell 1 is on E-UTRA RF channel number 1 as defined in clause A.3.7.2.2. |
| Neighbour cell |  | 1, 2, 3, 4, 5, 6 | NR cell 2 | NR cell 2 is on NR RF channel number 1. |
| Gap Pattern Id |  | 1, 2, 3, 4, 5, 6 | 0 | As specified in clause Table 8.1.2.1-1 of TS 36.133 [15]. |
| Measurement gap offset |  | 1, 2, 3, 4, 5, 6 | 39 | As specified in TS 36.331 [16]. |
| b1-ThresholdNR | dBm | 1, 2 | Note 1 | SS-RSRP threshold for SS-RSRP measurement on cell 2 for event B1 [16] |
| Hysteresis | dB | 1, 2, 3, 4, 5, 6 | 0 |  |
| CP length |  | 1, 2, 3, 4, 5, 6 | Normal |  |
| TimeToTrigger | s | 1, 2, 3, 4, 5, 6 | 0 |  |
| Filter coefficient |  | 1, 2, 3, 4, 5, 6 | 0 | L3 filtering is not used |
| DRX |  | 1, 2, 3, 4, 5, 6 | DRX.9 | DRX.12 | As specified in clause A.3.3 |
| Time offset between serving and neighbour cells |  | 1 | 3ms | Asynchronous cells.The timing of Cell 2 is 3ms later than the timing of Cell 1. |
|  | 2 | 3μs | Synchronous cells. |
| T1 | s | 1, 2, 3, 4, 5, 6 | 5 |  |
| T2 | s | 1, 2, 3, 4, 5, 6 | 6 | 83 |  |
| Note 1: The value of b1-ThresholdNR is defined in Table A.8.4.2.6.1-3 |

Table A.8.4.2.6.1-3: NR neighbour cell specific test parameters for NR inter-RAT event triggered reporting for FR2 without SSB time index detection in DRX

|  |  |  |  |
| --- | --- | --- | --- |
| **Parameter** | **Unit** | **Test configuration** | **Cell 2** |
| **T1** | **T2** |
| AoA setup defined in A.3.15.1 |  | 1, 2 | Setup 1 |
| Assumption for UE beamsNote 5 |  | 1, 2 | Rough |
| NR RF Channel Number |  | 1, 2 | 1 |
| Duplex mode |  | 1, 2 | TDD |
| TDD configuration |  | 1, 2 | TDDConf.3.1 |
| BWchannel | MHz | 1, 2 | 100: NRB,c = 66 |
| OCNG patterns defined in A.3.2.1.1 (OP.1)  |  | 1, 2 | OP.1 |
| SMTC configuration defined in A.3.11.1 and A.3.11.2 |  | 1 | SMTC.2 |
| 2 | SMTC.1 |
| PDSCH/PDCCH subcarrier spacing | kHz | 1, 2 | 120 |
| b1-ThresholdNR | UE power class 3 | dBm/SCS | 1, 2 | -106 |
| EPRE ratio of PSS to SSS |  | 1, 2 | 0 |
| EPRE ratio of PBCH DMRS to SSS |  |
| EPRE ratio of PBCH to PBCH DMRS |  |
| EPRE ratio of PDCCH DMRS to SSS |  |
| EPRE ratio of PDCCH to PDCCH DMRS |  |
| EPRE ratio of PDSCH DMRS to SSS  |  |
| EPRE ratio of PDSCH to PDSCH  |  |
| EPRE ratio of OCNG DMRS to SSS (Note 1) |  |
| EPRE ratio of OCNG to OCNG DMRS (Note 1) |  |
| Note2 | dBm/15kHz | 1, 2 | -104.7 |
| Note2 | dBm/SCS | 1, 2 | -95.7 |
| SS-RSRP Note 3 | dBm/SCS | 1, 2 | -Infinity | -87.7 |
|  | dB | 1, 2 | -Infinity | 8 |
|  | dB | 1, 2 | -Infinity | 8 |
| IoNote3 | dBm/95.04MHz | 1, 2 | -66.7 | -58.0 |
| Propagation Condition  |  | 1, 2 | AWGN |
| Note 1: OCNG shall be used such that the cell is fully allocated and a constant total transmitted power spectral density is achieved for all OFDM symbols.Note 2: Interference from other cells and noise sources not specified in the test is assumed to be constant over subcarriers and time and shall be modelled as AWGN of appropriate power for to be fulfilled.Note 3: SS-RSRP and Io levels have been derived from other parameters for information purposes. They are not settable parameters themselves.Note 4: SS-RSRP minimum requirements are specified assuming independent interference and noise at each receiver antenna port.Note 5: Information about types of UE beam is given in B.2.1.3, and does not limit UE implementation or test system implementation |

##### A.8.4.2.6.2 Test Requirements

In test 1, the UE shall send one Event B1 triggered measurement report, with a measurement reporting delay less than D1 ms and D3 ms from the beginning of time period T2 for a UE incapable of per-FR gap and for a UE capable of per-FR gap, respectively. The UE shall not send event triggered measurement reports, as long as the reporting criteria are not fulfilled. The rate of correct events observed during repeated tests shall be at least 90%.

In test 2, the UE shall send one Event B1 triggered measurement report, with a measurement reporting delay less than D2 ms and D4 ms from the beginning of time period T2 for a UE incapable of per-FR gap and for a UE capable of per-FR gap, respectively. The UE shall not send event triggered measurement reports, as long as the reporting criteria are not fulfilled. The rate of correct events observed during repeated tests shall be at least 90%.

In tests 1 and 2, the UE is not required to report SSB time index.

Table A.8.4.2.6.2-1: Test requirements for NR inter-RAT event triggered reporting for FR2 without SSB time index detection in DRX

|  |  |
| --- | --- |
| Test case | Measurement reporting delay (ms) |
| D1 ms | D2 ms | D3 ms | D4 ms |
| UE power class 3 | 4800 | 51200 | 4800 | 51200 |

NOTE: The actual overall delays measured in the test may be up to 2xTTIDCCH higher than the measurement reporting delays above because of TTI insertion uncertainty of the measurement report in DCCH.

#### A.8.4.2.7 NR Inter-RAT event triggered reporting tests for FR2 with SSB time index detection when DRX is not used

##### A.8.4.2.7.1 Test Purpose and Environment

The purpose of this test is to verify that the UE makes correct reporting of an event. This test will partly verify the NR inter-RAT cell search requirements in clause 8.1.2.4.21 of TS 36.133 [15] for E-UTRAN FDD-NR measurements and clause 8.1.2.4.22 of TS 36.133 [15] for E-UTRAN TDD-NR measurements.

In this test, there are two cells: E-UTRA cell 1 as PCell on E-UTRA RF channel 1 and NR cell 2 as neighbour cell in FR2 on NR RF channel 1. The test parameters are given in Tables A.8.4.2.7.1-1, A.8.4.2.7.1-2 and A.8.4.2.7.1-3.

The cell specific test parameters for E-UTRA cell1 as PCell are defined in clause A.3.7.2.2.

Measurement gap pattern configuration defined in Table A.8.4.2.7.1-2 is provided for a UE that does not support per-FR gap, and no gap pattern (Gap Pattern Id and Measurement gap offset) is configured for a UE capable of per-FR gap.

In the measurement control information, it is indicated to the UE that event-triggered reporting with Event B1 (Inter RAT neighbour becomes better than threshold) [16] is used. In the measurement configuration the UE shall be indicated to report the SSB index of the identified NR cell. The test consists of two successive time periods, with time duration of T1, and T2 respectively. During time duration T1, the UE shall not have any timing information of NR cell 2.

Table A.8.4.2.7.1-1: NR inter-RAT event triggered reporting test with SSB index reading for FR2 in non-DRX

|  |  |
| --- | --- |
| Configuration | Description |
| 1 | LTE FDD, NR 120 kHz SSB SCS, 100 MHz bandwidth, TDD duplex mode |
| 2 | LTE TDD, NR 120 kHz SSB SCS, 100 MHz bandwidth, TDD duplex mode |
| Note 1: The UE is only required to be tested in one of the supported test configurations. |

Table A.8.4.2.7.1-2: General test parameters for NR inter-RAT event triggered reporting for FR2 with SSB time index detection in non-DRX

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Parameter | Unit | Test configuration | Value | Comment |
| E-UTRA RF Channel Numbers |  | 1, 2 | 1 | One E-UTRA carrier frequency is used. |
| NR RF Channel Numbers |  | 1, 2 | 1 | One FR2 NR carrier frequency is used. |
| Active cell |  | 1, 2 | E-UTRA cell 1 (PCell) | E-UTRA cell 1 is on E-UTRA RF channel number 1 as defined in clause A.3.7.2.2. |
| Neighbour cell |  | 1, 2 | NR cell 2 | NR cell 2 is on NR RF channel number 1. |
| Gap Pattern Id |  | 1, 2 | 0 | As specified in clause Table 8.1.2.1-1 of TS 36.133 [15]. |
| Measurement gap offset |  | 1, 2 | 39 | As specified in TS 36.331 [16]. |
| b1-ThresholdNR | dBm | 1, 2 | Note 1 | SS-RSRP threshold for SS-RSRP measurement on cell 2 for event B1 [16] |
| Hysteresis | dB | 1, 2 | 0 |  |
| CP length |  | 1, 2 | Normal |  |
| TimeToTrigger | s | 1, 2 | 0 |  |
| Filter coefficient |  | 1, 2 | 0 | L3 filtering is not used |
| DRX |  | 1, 2 | OFF | DRX is not used |
| Time offset between serving and neighbour cells |  | 1 | 3ms | Asynchronous cells.The timing of Cell 2 is 3ms later than the timing of Cell 1. |
|  | 2 | 3μs | Synchronous cells. |
| T1 | s | 1, 2 | 5 |  |
| T2 | s | 1, 2 | 5 |  |
| Note 1: The value of b1-ThresholdNR is defined in Table A.8.4.2.7.1-3 |

Table A.8.4.2.7.1-3: NR neighbour cell specific test parameters for NR inter-RAT event triggered reporting for FR2 with SSB time index detection in non-DRX

|  |  |  |  |
| --- | --- | --- | --- |
| **Parameter** | **Unit** | **Test configuration** | **Cell 2** |
| **T1** | **T2** |
| AoA setup defined in A.3.15.1 |  | 1, 2 | Setup 1 |
| Assumption for UE beamsNote 5 |  | 1, 2 | Rough |
| NR RF Channel Number |  | 1, 2 | 1 |
| Duplex mode |  | 1, 2 | TDD |
| TDD configuration |  | 1, 2 | TDDConf.3.1 |
| BWchannel | MHz | 1, 2 | 100: NRB,c = 66 |
| OCNG patterns defined in A.3.2.1.1  |  | 1, 2 | OP.1 |
| SMTC configuration defined in A.3.11.1 and A.3.11.2 |  | 1 | SMTC.2 |
| 2 | SMTC.1 |
| PDSCH/PDCCH subcarrier spacing | kHz | 1, 2 | 120 |
| b1-ThresholdNR | UE power class 3 | dBm/SCS | 1, 2 | -106 |
| EPRE ratio of PSS to SSS |  | 1, 2 | 0 |
| EPRE ratio of PBCH DMRS to SSS |  |
| EPRE ratio of PBCH to PBCH DMRS |  |
| EPRE ratio of PDCCH DMRS to SSS |  |
| EPRE ratio of PDCCH to PDCCH DMRS |  |
| EPRE ratio of PDSCH DMRS to SSS  |  |
| EPRE ratio of PDSCH to PDSCH  |  |
| EPRE ratio of OCNG DMRS to SSS (Note 1) |  |
| EPRE ratio of OCNG to OCNG DMRS (Note 1) |  |
| Note2 | dBm/15kHz | 1, 2 | -104.7 |
| Note2 | dBm/SCS | 1, 2 | -95.7 |
| SS-RSRP Note 3 | dBm/SCS | 1, 2 | -Infinity | -87.7 |
|  | dB | 1, 2 | -Infinity | 8 |
|  | dB | 1, 2 | -Infinity | 8 |
| IoNote3 | dBm/95.04MHz | 1, 2 | -66.7 | -58.0 |
| Propagation Condition  |  | 1, 2 | AWGN |
| Note 1: OCNG shall be used such that the cell is fully allocated and a constant total transmitted power spectral density is achieved for all OFDM symbols.Note 2: Interference from other cells and noise sources not specified in the test is assumed to be constant over subcarriers and time and shall be modelled as AWGN of appropriate power for to be fulfilled.Note 3: SS-RSRP and Io levels have been derived from other parameters for information purposes. They are not settable parameters themselves.Note 4: SS-RSRP minimum requirements are specified assuming independent interference and noise at each receiver antenna port.Note 5: Information about types of UE beam is given in B.2.1.3, and does not limit UE implementation or test system implementation |

##### A.8.4.2.7.2 Test Requirements

the UE shall send one Event B1 triggered measurement report, with a measurement reporting delay less than D1 ms and D2 ms from the beginning of time period T2 for a UE incapable of per-FR gap and for a UE capable of per-FR gap, respectively. The UE shall not send event triggered measurement reports, as long as the reporting criteria are not fulfilled. The rate of correct events observed during repeated tests shall be at least 90%.

The UE is required to report SSB time index.

NOTE: The actual overall delays measured in the test may be up to 2xTTIDCCH higher than the measurement reporting delays above because of TTI insertion uncertainty of the measurement report in DCCH.

Table A.8.4.2.7.2-1: Test requirements for NR inter-RAT event triggered reporting for FR2 with SSB time index detection in non-DRX

|  |  |
| --- | --- |
| Test case | Measurement reporting delay (ms) |
| D1 ms | D2 ms |
| UE power class 3 | 4160 | 2080 |

#### A.8.4.2.8 NR Inter-RAT event triggered reporting tests for FR2 with SSB time index detection when DRX is used

##### A.8.4.2.8.1 Test Purpose and Environment

The purpose of this test is to verify that the UE makes correct reporting of an event. This test will partly verify the NR inter-RAT cell search requirements in clause 8.1.2.4.21 of TS 36.133 [15] for E-UTRAN FDD-NR measurements and clause 8.1.2.4.22 of TS 36.133 [15] for E-UTRAN TDD-NR measurements.

In this test, there are two cells: E-UTRA cell 1 as PCell on E-UTRA RF channel 1 and NR cell 2 as neighbour cell in FR2 on NR RF channel 1. The test parameters are given in Tables A.8.4.2.8.1-1, A.8.4.2.8.1-2 and A.8.4.2.8.1-3.

The cell specific test parameters for E-UTRA cell1 as PCell are defined in clause A.3.7.2.2.

Measurement gap pattern configuration defined in Table A.8.4.2.8.1-2 is provided for a UE that does not support per-FR gap, and no gap pattern (Gap Pattern Id and Measurement gap offset) is configured for a UE capable of per-FR gap.

In the measurement control information, it is indicated to the UE that event-triggered reporting with Event B1 (Inter RAT neighbour becomes better than threshold) [16] is used. In the measurement configuration the UE shall be indicated to report the SSB index of the identified NR cell. The test consists of two successive time periods, with time duration of T1, and T2 respectively. During time duration T1, the UE shall not have any timing information of NR cell 2.

Table A.8.4.2.8.1-1: NR inter-RAT event triggered reporting tests with SSB index reading for FR2 in DRX

|  |  |
| --- | --- |
| **Configuration** | **Description** |
| 1 | LTE FDD, NR 120 kHz SSB SCS, 100 MHz bandwidth, TDD duplex mode |
| 2 | LTE TDD, NR 120 kHz SSB SCS, 100 MHz bandwidth, TDD duplex mode |
| Note 1: The UE is only required to be tested in one of the supported test configurations. |

Table A.8.4.2.8.1-2: General test parameters for NR inter-RAT event triggered reporting for FR2 with SSB time index detection in DRX

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Parameter | Unit | Test configuration | Value | Comment |
| Test 1 | Test 2 |
| E-UTRA RF Channel Number |  | 1, 2 | 1 | One E-UTRA carrier frequency is used. |
| NR RF Channel Number |  | 1, 2 | 1 | One FR2 NR carrier frequency is used. |
| Active cell |  | 1, 2 | E-UTRA cell 1 (PCell) | E-UTRA cell 1 is on E-UTRA RF channel number 1 as defined in clause A.3.7.2.2. |
| Neighbour cell |  | 1, 2 | NR cell 2 | NR cell 2 is on NR RF channel number 1. |
| Gap Pattern Id |  | 1, 2 | 0 | As specified in clause Table 8.1.2.1-1 of TS 36.133 [15]. |
| Measurement gap offset |  | 1, 2 | 39 | As specified in TS 36.331 [16]. |
| b1-ThresholdNR | dBm | 1, 2 | Note 1 | SS-RSRP threshold for SS-RSRP measurement on cell 2 for event B1 [16] |
| Hysteresis | dB | 1, 2 | 0 |  |
| CP length |  | 1, 2 | Normal |  |
| TimeToTrigger | s | 1, 2 | 0 |  |
| Filter coefficient |  | 1, 2 | 0 | L3 filtering is not used |
| DRX |  |  | DRX.9 | DRX.12 | As specified in clause A.3.3 |
| Time offset between serving and neighbour cells |  | 1 | 3ms | Asynchronous cells.The timing of Cell 2 is 3ms later than the timing of Cell 1. |
|  | 2 | 3μs | Synchronous cells. |
| T1 | s | 1, 2 | 5 |  |
| T2 | s | 1, 2 | 7 | 70 |  |
| Note 1: The value of b1-ThresholdNR is defined in Table A.8.4.2.8.1-3 |

Table A.8.4.2.8.1-3: NR neighbour cell specific test parameters for NR inter-RAT event triggered reporting for FR2 with SSB time index detection

|  |  |  |  |
| --- | --- | --- | --- |
| **Parameter** | **Unit** | **Test configuration** | **Cell 2** |
| **T1** | **T2** |
| AoA setup defined in A.3.15.1 |  | 1, 2 | Setup 1 |
| Assumption for UE beamsNote 5 |  | 1, 2 | Rough |
| NR RF Channel Number |  | 1, 2 | 1 |
| Duplex mode |  | 1, 2 | TDD |
| TDD configuration |  | 1, 2 | TDDConf.3.1 |
| BWchannel | MHz | 1, 2 | 100: NRB,c = 66 |
| OCNG patterns defined in A.3.2.1.1  |  | 1, 2 | OP.1 |
| SMTC configuration defined in A.3.11.1 and A.3.11.2 |  | 1 | SMTC.2 |
| 2 | SMTC.1 |
| PDSCH/PDCCH subcarrier spacing | kHz | 1, 2 | 120 |
| b1-ThresholdNR | UE power class 3 | dBm/SCS | 1, 2 | -106 |
| EPRE ratio of PSS to SSS |  | 1, 2 | 0 |
| EPRE ratio of PBCH DMRS to SSS |  |
| EPRE ratio of PBCH to PBCH DMRS |  |
| EPRE ratio of PDCCH DMRS to SSS |  |
| EPRE ratio of PDCCH to PDCCH DMRS |  |
| EPRE ratio of PDSCH DMRS to SSS  |  |
| EPRE ratio of PDSCH to PDSCH  |  |
| EPRE ratio of OCNG DMRS to SSS (Note 1) |  |
| EPRE ratio of OCNG to OCNG DMRS (Note 1) |  |
| Note2 | dBm/15kHz | 1, 2 | -104.7 |
| Note2 | dBm/SCS | 1, 2 | -95.7 |
| SS-RSRP Note 3 | dBm/SCS | 1, 2 | -Infinity | -87.7 |
|  | dB | 1, 2 | -Infinity | 8 |
|  | dB | 1, 2 | -Infinity | 8 |
| IoNote3 | dBm/95.04MHz | 1, 2 | -66.7 | -58.0 |
| Propagation Condition  |  | 1, 2 | AWGN |
| Note 1: OCNG shall be used such that the cell is fully allocated and a constant total transmitted power spectral density is achieved for all OFDM symbols.Note 2: Interference from other cells and noise sources not specified in the test is assumed to be constant over subcarriers and time and shall be modelled as AWGN of appropriate power for to be fulfilled.Note 3: SS-RSRP and Io levels have been derived from other parameters for information purposes. They are not settable parameters themselves.Note 4: SS-RSRP minimum requirements are specified assuming independent interference and noise at each receiver antenna port.Note 5: Information about types of UE beam is given in B.2.1.3, and does not limit UE implementation or test system implementation |

##### A.8.4.2.8.2 Test Requirements

In test 1, the UE shall send one Event B1 triggered measurement report, with a measurement reporting delay less than D1 ms and D3 ms from the beginning of time period T2 for a UE incapable of per-FR gap and for a UE capable of per-FR gap, respectively. The UE shall not send event triggered measurement reports, as long as the reporting criteria are not fulfilled. The rate of correct events observed during repeated tests shall be at least 90%.

In test 2, the UE shall send one Event B1 triggered measurement report, with a measurement reporting delay less than D2 ms from the beginning of time period T2 for a UE incapable of per-FR gap and for a UE capable of per-FR gap, respectively. The UE shall not send event triggered measurement reports, as long as the reporting criteria are not fulfilled. The rate of correct events observed during repeated tests shall be at least 90%.

In tests 1 and 2, the UE is required to report SSB time index.

Table A.8.4.2.8.2-1: Test requirements for NR inter-RAT event triggered reporting for FR2 with SSB time index detection in DRX

|  |  |
| --- | --- |
| Test case | Measurement reporting delay (ms) |
| D1 ms | D2 ms | D3 ms | D4 ms |
| UE power class 3 | 6240 | 66560 | 6240 | 66560 |

NOTE: The actual overall delays measured in the test may be up to 2xTTIDCCH higher than the measurement reporting delays above because of TTI insertion uncertainty of the measurement report in DCCH.

<End of Change 1>