**3GPP TSG-RAN4 Meeting # 111 *R4-2409654***

**Fukuoka City, Fukuoka , Japan, 20th – 24th May, 2024**

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  | **38.133** | **CR** | **4581** | **rev** |  | **Current version:** | **17.13.0** |  |
|  |
| *For* ***[HE](http://www.3gpp.org/3G_Specs/CRs.htm%22%20%5Cl%20%22_blank)******[LP](http://www.3gpp.org/3G_Specs/CRs.htm%22%20%5Cl%20%22_blank)*** *on using this form: comprehensive instructions can be found at <http://www.3gpp.org/Change-Requests>.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | [NR\_NTN\_solutions-Core] CR for the TCI state indication of R17 NTN |
|  |  |
| ***Source to WG:*** | ZTE Corporation, Sanechips |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NR\_NTN\_solutions-Core |  | ***Date:*** | 2024-04-29 |
|  |  |  |  |  |
| ***Category:*** | F |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19) Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | In 110 meeting, one CR R4-2403412 approved to revise the MAC CE based TCI state switch delay and MAC CE based TCI state list update delay. Based on the revision, the description is more accurate and clear. Since the two procedures with same requirements are also applied to NTN but in seperate chapters, so it is necessary to do the same revision in NTN specific chapters. |
|  |  |
| ***Summary of change:*** | Repeat the same revisions approved for normal UE in NTN specific chapters |
|  |  |
| ***Consequences if not approved:*** | Not accurate enough |
|  |  |
| ***Clauses affected:*** | 8.10C.2, 8.10C.6 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** | **X** |  |  Test specifications | TS 38.533 |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

# <Start of Change #1>

## 8.10C Active TCI state switching delay for satellite access

### 8.10C.2 MAC-CE based TCI state switch delay

Upon receiving PDSCH carrying MAC-CE for indication of UE-specific PDCCH TCI state as defined in clause 6.1.3.15 of TS 38.321 [7] in slot n, UE shall be able to receive PDCCH with target TCI state of the serving cell on which TCI state switch occurs at the first slot that is after slot n+ THARQ + $3N\_{slot}^{subframe,µ}$+ TOk\*(Tfirst-SSB + TSSB-proc) / *NR slot length*. The UE shall be able to receive PDCCH with the old TCI state until slot n+ THARQ + $3N\_{slot}^{subframe,µ}$ .Where THARQ is the timing between DL data transmission and acknowledgement as specified in TS 38.213 [3];

- Tfirst-SSB is time to first SSB transmission after MAC CE command is decoded by the UE; The SSB shall be the QCL-TypeA or QCL-TypeC to target TCI state

- TSSB-proc = 2 ms;

- TOk = 1 if target TCI state is not in the active TCI state list for PDSCH, 0 otherwise.

# <End of Change #1>

# <End of Change #2>

### 8.10C.6 Active TCI state list update delay

Upon receiving PDSCH carrying MAC-CE for activation/deactivation of UE-specific PDSCH TCI state as defined in clause 6.1.3.14 of TS 38.321 [7] at slot n, UE shall be able to receive PDCCH to schedule PDSCH with the new target TCI state at the first slot that is after n+ THARQ +$3N\_{slot}^{subframe,µ}$ +TOk\*(Tfirst-SSB + TSSB-proc) / *NR slot length*. Where THARQ, Tfirst-SSB, TSSB-proc and TOk are defined in clause 8.10C.2.

# <End of Change #2>