**3GPP TSG- Meeting #111**

**, –**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  |  | **CR** |  | **rev** | **1** | **Current version:** |  |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** |  | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** |  | | | | | | | | | |
| ***Source to TSG:*** |  | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** |  | | | | |  | ***Date:*** | | |  |
|  |  | | | |  | |  | | |  |
| ***Category:*** |  |  | | | | | ***Release:*** | | |  |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | In a normative clause introduced by CR3650, what is intended to be a UE requirement has been phrased as “the UE is expected to”. However, the Forword section of TS 38.133 specifies that for requirements, the word “shall” is to be used.  The error shall be corrected in order to comply with the specification drafting rules (TR 21.801), particularly with the following objectives: to be consistent, clear and accurate, and to be comprehensible to qualified persons who have not participated in its preparation. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Clause 9.2D.5.3.2:  The requirement is phrased as that the UE “is expected to” perform an action. As “expected to” is not a requirement, it is changed to “shall”. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | The specification will remain inconsistent and unclear to those who have not participated in its preparation. The specification quality will degrade further over time as the errors will be copied when new requirements are added. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 9.2D.5.3.2 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | Corresponding changes are proposed across the normative part of TS 38.133 in related CRs: R4-2407783 (Cat F), R4-2407784 (Cat A), R4-2407785 (Cat F), R4-2407786 (Cat F), R4-2407787 (Cat F), R4-2407788 (Cat F) , R4-2407789 (Cat F). | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | | Rev.1: Changed “shall be able to” to “shall”. | | | | | | | | |

1st CORRECTION

9.2D.5.3.2 Scheduling availability of UE performing measurements with a different subcarrier spacing than PDSCH/PDCCH on FR1

For UE which do not support *simultaneousRxDataSSB-DiffNumerology* [14] the following restrictions apply due to SS-RSRP/RSRQ/SINR measurement

- If *deriveSSB\_IndexFromCell* is enabled the UE is not expected to transmit PUCCH/PUSCH/SRS or receive PDCCH/PDSCH/TRS/CSI-RS for CQI on SSB symbols to be measured, and on 1 data symbol before each consecutive SSB symbols to be measured and 1 data symbol after each consecutive SSB symbols to be measured within SMTC window duration. If the high layer signalling of *smtc2*is configured(in TS 38.331 [2]), the SMTC periodicityfollows *smtc2*; Otherwise the SMTC periodicity follows *smtc1.*

- If *deriveSSB\_IndexFromCell* is not enabled the UE is not expected to transmit PUCCH/PUSCH/SRS or receive PDCCH/PDSCH/TRS/CSI-RS for CQI on all symbols within SMTC window duration. If the high layer signalling of *smtc2*is configured in TS 38.331 [2], the SMTC periodicityfollows *smtc2*; Otherwise the SMTC periodicity follows *smtc1.*

If the following conditions are met:

- The UE has been notified about system information update through paging,

- The gap between the UE’s reception of PDCCH that UE monitors in the Type 2-PDCCH CSS set that notifies system information update, and the PDCCH that UE monitors in the Type0-PDCCH CSS set, is greater than 2 slots

The UE shall receive the PDCCH that the UE monitors in the Type0-PDCCH CSS set, and/or the corresponding PDSCH, on SSB symbols to be measured.

END OF CORRECTIONS