**3GPP TSG-RAN4 Meeting #** **111R4-2408561**

Fukuoka City, Fukuoka , Japan, 20th – 24th May, 2024

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  | **38.133** | **CR** | **Draft** | **rev** | **-** | **Current version:** | **18.5.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | DraftCR on TC3 fast beam sweeping for R18 FR2 multi-Rx |
|  |  |
| ***Source to WG:*** | Huawei, HiSilicon |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NR\_FR2\_multiRX\_DL-Perf |  | ***Date:*** | 2024-05-01 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* *Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | Following TC is to be introduced per WF R4-2406365* TC3: Fast beam sweeping for RLM OOS
 |
|  |  |
| ***Summary of change:*** | Introduce following TC:* TC3: Fast beam sweeping for RLM OOS
 |
|  |  |
| ***Consequences if not approved:*** | The requirements can not be verified. |
|  |  |
| ***Clauses affected:*** | A.5.5.1.X1 and A.7.5.1.X1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** | **X** |  |  Test specifications | TS 38.533  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

# <Start of Change #1>

#### A.5.5.1.X1 Radio Link Monitoring Out-of-sync Test for FR2 PSCell configured with SSB-based RLM RS in non-DRX mode for UE supporting fast beam sweeping in multi-Rx

##### A.5.5.1.X1.1 Test Purpose and Environment

The purpose of this test is to verify that the UE properly detects the out of sync for the purpose of monitoring downlink radio link quality of the PSCell. This test will partly verify the FR2 radio link monitoring requirements in clause 8.1.

In the test, UE is configured to perform RLM on SSB, with *detectionResource* included in *RadioLinkMonitoringRS* set to SSB#0 and SSB#1, and *purpose* set to ‘*rlf*’. Supported test configurations are shown in table A.5.5.1.X1.1-1. The test parameters are given in Tables A.5.5.1.X1.1-2, and A.5.5.1.X1.1-3. There are two cells, Cell 1 is the E-UTRAN PCell, and Cell 2 is the PSCell, in the test. The E-UTRAN PCell setting refers to Table A.3.7.2.1-2. The test consists of three successive time periods, with time duration of T1, T2 and T3 respectively. Figure A.5.5.1.X1.1-1 shows the variation of the downlink SNR in the active cell to emulate out-of-sync and in-sync states, and Figure A.5.5.1.X1.1-2 shows the Time multiplexed downlink transmissions from each Angle of Arrival. Prior to the start of the time duration T1, the UE shall be fully synchronized to Cell 1 and Cell 2 and configured with *groupBasedBeamReporting-r17*. The UE shall be configured for periodic CSI reporting with a reporting periodicity of 5 ms.

Table A.5.5.1.X1.1-1: Supported test configurations for FR2 PSCell

|  |  |
| --- | --- |
| Configuration | Description |
| 1 | FDD LTE PCell, NR 120 KHz SSB SCS, 100 MHz bandwidth, TDD duplex mode |
| 2 | TDD LTE PCell, NR 120 KHz SSB SCS, 100 MHz bandwidth, TDD duplex mode |
| Note: The UE is only required to pass in one of the supported test configurations in FR2 |

Table A.5.5.1.X1.1-2: General test parameters for FR2 out-of-sync testing in non-DRX mode

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Unit** | **Value** |
| **Test 1** |
| Active E-UTRA PCell  |  | Cell 1 |
| E-UTRA RF Channel Number |  | 1 |
| Active PSCell |  | Cell 2 |
| RF Channel Number |  | 2 |
| Duplex mode | Config 1, 2 |  | TDD |
| BWchannel | Config 1, 2 |  | 100: NRB,c = 66 |
| Data RBs allocated | Config 1, 2 |  | 24 |
| DL initial BWP configuration | Config 1, 2 |  | DLBWP.0.1 |
| DL dedicated BWP configuration | Config 1, 2 |  | DLBWP.1.1 |
| UL initial BWP configuration | Config 1, 2 |  | ULBWP.0.1 |
| UL dedicated BWP configuration | Config 1, 2 |  | ULBWP.1.1 |
| TDD Configuration | Config 1, 2 |  | TDDConf.3.1 |
| RMSI CORESET Reference Channel | Config 1, 2 |  | CR.3.1 TDD  |
| Dedicated CORESET Reference Channel | Config 1, 2 |  | CCR.3.4 TDD  |
| SSB Configuration | Config 1, 2 |  | SSB.1 FR2 |
| SMTC Configuration | Config 1, 2 |  | SMTC.1 |
| PDSCH/PDCCH subcarrier spacing | Config 1, 2 |  | 120 KHz |
| PRACH Configuration | Config 1, 2 |  | Table A.3.8.3.1 |
| SSB index assigned as RLM RS | Config 1, 2 |  | 0,1 |
| OCNG parameters |  | OP.5 |
| CP length |  | Normal |
| Out of sync transmission parameters  | DCI format |  | 1-0 |
| Number of Control OFDM symbols |  | 2 |
| Aggregation level  | CCE | 8 |
| Ratio of hypothetical PDCCH RE energy to average SSS RE energy | dB | 4 |
| Ratio of hypothetical PDCCH DMRS energy to average SSS RE energy | dB | 4 |
| DMRS precoder granularity |  | REG bundle size |
| REG bundle size |  | 6 |
| DRX |  | *OFF* |
| Gap pattern ID  |  | *NA* |
| Layer 3 filtering |  | *Enabled* |
| T310 timer | ms | *0* |
| T311 timer | ms | 1000 |
| N310 |  | 1 |
| N311 |  | 1 |
| CSI-RS for CSI reporting | Config 1, 2 |  | CSI-RS.3.1 TDD |
| reportConfigType |  | periodic |
| reportQuantity |  | cri-RI-PMI-CQI |
| CSI reporting periodicity | slot | 40 |
| CSI reporting offset | slot | 4 |
| TCI states for PDCCH/PDSCH |  | TCI.State.2 |
| CSI-RS for tracking | Config 1, 2 |  | TRS.2.1 TDD |
| T1 | s | 0.2 |
| T2 | s | 1.2\*N +0.08 Note 4 |
| T3 | s | 1.2\*N +0.08 Note 4 |
| D1 | s | 1.2\*N +0.04 Note 4 |
| Note 1: All configurations are assigned to the UE prior to the start of time period T1.Note 2: UE-specific PDCCH is not transmitted after T1 starts.Note 3: E-UTRAN is in non-DRX mode under test.Note 4: N is the value indicated by UE for [*UEcapablityFastbeamsweeping*] |

Table A.5.5.1.X1.1-3: OTA related cell specific test parameters for FR2 (Cell 2) for out-of-sync radio link monitoring tests in non-DRX mode

|  |  |  |
| --- | --- | --- |
| Parameter | Unit | Test 1 |
|  |  | T1 | T2 | T3 | T1 | T2 | T3 |
| AoA setup |  | Setup X2 defined in A.3.15 |
|  |  | AoA1 | AoA2 |
| Assumption for UE beamsNote 5 |  | Rough | Rough |
| EPRE ratio of PDCCH DMRS to SSS | dB | 4 |  |
| EPRE ratio of PDCCH to PDCCH DMRS | dB |  |  |
| EPRE ratio of PBCH DMRS to SSS | dB |  |  |
| EPRE ratio of PBCH to PBCH DMRS | dB |  |  |
| EPRE ratio of PSS to SSS | dB | 0 | Not sent |
| EPRE ratio of PDSCH DMRS to SSS  | dB |  |  |
| EPRE ratio of PDSCH to PDSCH DMRS | dB |  |  |
| EPRE ratio of OCNG DMRS to SSS | dB |  |  |
| EPRE ratio of OCNG to OCNG DMRS | dB |  |  |
| ssb-Index 0 SNR | Config 1, 2 | dB | 2Note 6 | -6Note 6 | -15 |  |
| ssb-Index 1 SNR | Config 1, 2 |  | Not sent | 2Note 6 | -15 | -15 |
|  | Config 1, 2 | dBm/15kHz | -92.1 | -92.1 |
| Time multiplexing of the downlink transmissions from each AoA |  | Defined in Figure A.5.5.1.X1.1-2 |
| Propagation condition |  | TDL-A 30ns 75Hz | TDL-A 30ns 75Hz |
| Note 1: OCNG shall be used such that a constant total transmitted power spectral density is achieved for all OFDM symbols.Note 2: The signal contains PDCCH for UEs other than the device under test as part of OCNG.Note 3: SNR levels correspond to the signal to noise ratio over the SSS REs.Note 4: The SNR values are specified for testing a UE which supports 2RX on at least one band. For testing of a UE which supports 4RX on all bands, the SNR during T3 is A.3.6.Note 5: Information about types of UE beam is given in B.2.1.3, and does not limit UE implementation or test system implementation Note 6: This value allows up to 1dB degradation from applied SNR to UE baseband |



Figure A.5.5.1.X1.1-1: SNR variation for out-of-sync testing



Figure A.5.5.1.X1.1-2: Time multiplexed downlink transmissions

##### A.5.5.1.X1.2 Test Requirements

The UE behavior in each test during time durations T1, T2 and T3 shall be as follows:

During the period from time point A to time point B the UE shall transmit uplink signal at least in all uplink slots configured for CSI transmission according to the configured periodic CSI reporting.

The UE shall stop transmitting uplink signal in Cell 2 no later than time point C (D1 second after the start of the time duration T3).

The rate of correct events observed during repeated tests shall be at least 90%.

# <End of Change #1>

# <Start of Change #2>

#### A.7.5.1.X1 Radio Link Monitoring Out-of-sync Test for FR2 PCell configured with SSB-based RLM RS in non-DRX mode for UE supporting fast beam sweeping in multi-Rx

##### A.7.5.1.X1.1 Test Purpose and Environment

The purpose of this test is to verify that the UE properly detects the out of sync and in sync for the purpose of monitoring downlink radio link quality of the PCell. This test will partly verify the FR2 radio link monitoring requirements in clause 8.1.

In the test, UE is configured to perform RLM on SSB, with *detectionResource* included in *RadioLinkMonitoringRS* set to SSB#0 and SSB#1, and *purpose* set to ‘*rlf*’. Supported test configurations are shown in table A.7.5.1.X1.1-1. The test parameters are given in Tables A.7.5.1.X1.1-2, and A.7.5.1.X1.1-3below. There is one cell (Cell 1), which is the active NR cell, in the test. The test consists of three successive time periods, with time duration of T1, T2 and T3 respectively. Figure A.7.5.1.X1.1-1 shows the variation of the downlink SNR in the active cell to emulate out-of-sync and in-sync states, and Figure A.7.5.1.X1.1-2 shows the Time multiplexed downlink transmissions from each Angle of Arrival. Prior to the start of the time duration T1, the UE shall be fully synchronized to Cell 1. The UE shall be configured for periodic CSI reporting with a reporting periodicity of 5 ms. In addition to RLM-RS radio link monitoring using SSB index 0 and SSB index 1.

Table A.7.5.1.X1.1-1: Supported test configurations for FR2 PCell

|  |  |
| --- | --- |
| Configuration | Description |
| 1 | TDD, SSB SCS 120 KHz, data SCS 120KHz, BW 100 MHz |

Table A.7.5.1.X1.1-2: General test parameters for FR2 out-of-sync testing in non-DRX mode

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Unit** | **Value** |
| **Test 1** |
| Active PCell |  | Cell 1 |
| RF Channel Number |  | 1 |
| Duplex mode | Config 1 |  | TDD |
| BWchannel | Config 1 |  | 100: NRB,c = 66 |
| Data RBs allocated | Config 1 |  | 24 |
| DL initial BWP configuration | Config 1 |  | DLBWP.0.1 |
| DL dedicated BWP configuration | Config 1 |  | DLBWP.1.1 |
| UL initial BWP configuration | Config 1 |  | ULBWP.0.1 |
| UL dedicated BWP configuration | Config 1 |  | ULBWP.1.1 |
| TDD Configuration | Config 1 |  | TDDConf.3.1 |
| RMSI CORESET Reference Channel | Config 1 |  | CR.3.1 TDD  |
| Dedicated CORESET Reference Channel | Config 1 |  | CCR.3.4 TDD  |
| SSB Configuration | Config 1 |  | SSB.1 FR2 |
| SMTC Configuration | Config 1 |  | SMTC.1 |
| PDSCH/PDCCH subcarrier spacing | Config 1 |  | 120 KHz |
| PRACH Configuration | Config 1 |  | Table A.3.8.3.1 |
| SSB index assigned as RLM RS | Config 1 |  | 0,1 |
| OCNG parameters |  | OP.5 |
| CP length |  | Normal |
| Out of sync transmission parameters  | DCI format |  | 1-0 |
| Number of Control OFDM symbols |  | 2 |
| Aggregation level  | CCE | 8 |
| Ratio of hypothetical PDCCH RE energy to average SSS RE energy | dB | 4 |
| Ratio of hypothetical PDCCH DMRS energy to average SSS RE energy | dB | 4 |
| DMRS precoder granularity |  | REG bundle size |
| REG bundle size |  | 6 |
| DRX |  | *OFF* |
| Gap pattern ID  |  | *NA* |
| Layer 3 filtering |  | *Enabled* |
| T310 timer | ms | *0* |
| T311 timer | ms | 1000 |
| N310 |  | 1 |
| N311 |  | 1 |
| CSI-RS for CSI reporting | Config 1 |  | CSI-RS.3.1 TDD |
| reportConfigType |  | periodic |
| reportQuantity |  | cri-RI-PMI-CQI |
| CSI reporting periodicity | slot | 40 |
| CSI reporting offset | slot | 4 |
| TCI states for PDCCH/PDSCH |  | TCI.State.2 |
| CSI-RS for tracking | Config 1 |  | TRS.2.1 TDD |
| T1 | s | 0.2 |
| T2 | s | 1.2\*N +0.08 Note 3 |
| T3 | s | 1.2\*N +0.08 Note 3 |
| D1 | s | 1.2\*N +0.04 Note 3 |
| Note 1: All configurations are assigned to the UE prior to the start of time period T1.Note 2: UE-specific PDCCH is not transmitted after T1 starts.Note 3: N is the value indicated by UE for [*UEcapablityFastbeamsweeping*] |

Table A.7.5.1.X1.1-3: OTA related cell specific test parameters for FR2 (Cell 1) for out-of-sync radio link monitoring tests in non-DRX mode

|  |  |  |
| --- | --- | --- |
| Parameter | Unit | Test 1 |
|  |  | T1 | T2 | T3 | T1 | T2 | T3 |
| AoA setup |  | Setup X2 defined in A.3.15 |
|  |  | AoA1 | AoA2 |
| Assumption for UE beams Note 5 |  | Rough | Rough |
| EPRE ratio of PDCCH DMRS to SSS | dB | 4 | Not sent |
| EPRE ratio of PDCCH to PDCCH DMRS | dB | 0 |  |
| EPRE ratio of PBCH DMRS to SSS | dB |  |  |
| EPRE ratio of PBCH to PBCH DMRS | dB |  |  |
| EPRE ratio of PSS to SSS | dB |  |  |
| EPRE ratio of PDSCH DMRS to SSS  | dB |  |  |
| EPRE ratio of PDSCH to PDSCH DMRS | dB |  |  |
| EPRE ratio of OCNG DMRS to SSS | dB |  |  |
| EPRE ratio of OCNG to OCNG DMRS | dB |  |  |
| ssb-Index 0 SNR | Config 1 | dB | 2Note 6 | -6Note 6 | -15 |  |
| ssb-Index 1 SNR | Config 1 |  | Not sent | 2Note 6 | -15 | -15 |
|  | Config 1 | dBm/15kHz | -92.1 | -92.1 |
| Time multiplexing of the downlink transmissions from each AoA |  | Defined in Figure A.7.5.1.X1.1-2 |
| Propagation condition |  | TDL-A 30ns 75Hz | TDL-A 30ns 75Hz |
| Note 1: OCNG shall be used such a constant total transmitted power spectral density is achieved for all OFDM symbols.Note 2: The signal contains PDCCH for UEs other than the device under test as part of OCNG.Note 3: SNR levels correspond to the signal to noise ratio over the SSS REs.Note 4: The SNR values are specified for testing a UE which supports 2RX on at least one band. For testing of a UE which supports 4RX on all bands, the SNR during T3 is A.3.6.Note 5: Information about types of UE beam is given in B.2.1.3 and does not limit UE implementation or test system implementation.Note 6: This value allows up to 1dB degradation from applied SNR to UE baseband |

Table A.7.5.1.X1.1-4: Measurement gap configuration for out-of-sync tests in non-DRX mode

|  |  |
| --- | --- |
| Field | Test 1 |
| Value |
| gapOffset | 0 |



Figure A.7.5.1.X1.1-1: SNR variation for out-of-sync testing



Figure A.7.5.1.X1.1-2: Time multiplexed downlink transmissions

##### A.7.5.1.X1.2 Test Requirements

The UE behavior in each test during time durations T1, T2 and T3 shall be as follows:

During the period from time point A to time point B the UE shall transmit uplink signal at least in all uplink slots configured for CSI transmission according to the configured periodic CSI reporting.

The UE shall stop transmitting uplink signal no later than time point C (D1 second after the start of the time duration T3).

The rate of correct events observed during repeated tests shall be at least 90%.

# <End of Change #2>