**3GPP TSG- Meeting #**

**, , -**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.3* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  |  | **CR** |  | **rev** | **1** | **Current version:** |  |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | DraftCR to 38.133 on core requirements for LPHAP | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** |  | | | | | | | | | |
| ***Source to TSG:*** |  | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** |  | | | | |  | ***Date:*** | | |  |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | |  |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)  Rel-20 (Release 20)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Correction of RSTD measurement core requirement in RRC\_IDLE and RRC\_INACTIVE modes. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | * FFS in 4.5.2.5 is removed. The core requirement in clause 4.5.2.5 is accordingly updated. * Unnecessary square brackets are removed from clause 5.6.2.5. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Core requirement for RSTD measurement in RRC\_IDLE mode is not correct. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 4.5.2.5 and 5.6.2.5. | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | This DraftCR is based on the Big CR endorsed (R4-2405983) in RAN4#110bis. The changes in the endorsed Big CR are kept intact and the additional changes are marked. | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

**START OF CHANGE**

#### 4.5.2.5 Measurements Period Requirements

After receiving both *NR-DL-TDOA-ProvideAssistanceData* message and *NR-DL-TDOA-RequestLocationInformation* message from the LMF via LPP [34]*,* the UE shall be able to measure multiple (up to the UE capability specified in Clause 4.5.2.3) DL RSTD measurements, defined in TS 38.215 [4], during the measurement period defined as:

Where:

- is the index of positioning frequency layer,

- is total number of positioning frequency layers, and

- is the periodicity of the PRS RSTD measurement in positioning frequency layer i

is the measurement period for PRS RSTD measurement in positioning frequency layer *i* as specified below:

,

Where:

- is the UE Rx beam sweeping factor:

- = 1 if positioning frequency layer *i* is in FR1, and if positioning frequency layer *i* is in FR2

- equals to the value as UE reported in *supportedLowerRxBeamSweepingFactor-FR2* if the capability is reported by the UE for the band containing positioning frequency layer i, and LMF indicates *lowerRxBeamSweepingFactor-FR2* in *NR-DL-TDOA-RequestLocationInformation* .

- equals to 8, otherwise.

- is a scaling factor for PRS-based NR positioning measurements in RRC\_IDLE. If the UE supports *parallelPRS-MeasRRC-Inactive-r17*, Kcarrier\_PRS = 1; otherwise,

- If Srxlev ≤ SnonIntraSearchP or Squal ≤ SnonIntraSearchQ, , where is defined in clause 4.2.2.4

- If Srxlev > SnonIntraSearchP and Squal > SnonIntraSearchQ, , where is defined in clause 4.2.2.7.

- is the Rx TEG specific scaling factor:

- =1 if the UE is not configured by the LMF to measure a PRS resource with multiple Rx TEGs via *measureSameDL-PRS-ResourceWithDifferentRxTEGs-r17* [34].

- is defined as follows if the UE is configured by the LMF with *measureSameDL-PRS-ResourceWithDifferentRxTEGs-r17* [34] to perform measurement on same DL PRS resource of a TRP using different Rx TEGs in *NR-DL-TDOA-RequestLocationInformation* [34]:

- , if the UE is not capable of receiving same DL PRS resource simultaneously from multiple Rx TEGs, where P is the number of UE Rx TEGs that the UE is requested by LMF to measure the same DL-PRS Resource of a TRP indicated by *measureSameDL-PRS-ResourceWithDifferentRxTEGs-r17* in [34], and in case ‘n0’ is indicated, P is the maximum number of Rx TEGs with which UE can support to measure the same PRS resource as reported in *NR-UE-TEG-Capability*.

- , if the UE is capable of receiving the same DL PRS resource simultaneously from multiple Rx TEGs, where is the number of UE Rx TEGs for measuring the same DL-PRS Resource simultaneously indicated by *measureSameDL-PRS-ResourceWithDifferentRxTEGsSimul-r17* in [34].

- is the maximum number of DL PRS resources in positioning frequency layer *i* configured in a slot.

- is the time duration of available PRS in positioning frequency layer *i* to be measured , and is calculated in the same way as PRS duration K defined in clause 5.1.6.5 of TS 38.214 [26]. For calculation of , only unmuted PRS resources that are not fully overlapped with other higher-priority DL signals/channels are considered.

- is the number of PRS RSTD samples, where

- = 1 if the UE supports *supportedDL-PRS-ProcessingSamples-RRC-Inactive-r17* [34], and the LMF requests the UE to perform positioning measurements with reduced number of samples, and meets the following conditions:

- PRS bandwidth is within the initial BWP and

- Magnitude of difference between the serving cell’s SS-RSRP and the neighbor cell’s PRS-RSRP is within 6 dB.

- = 2 if the UE supports *supportedDL-PRS-ProcessingSamples-RRC-Inactive-r17* [34], and the LMF requests the UE to perform positioning measurements with reduced number of samples, and does not meet the following conditions:

- PRS bandwidth is within the initial BWP and

- Magnitude of difference between the serving cell’s SS-RSRP and the neighbor cell’s PRS-RSRP is within 6 dB.

- = 4 otherwise.

- is the measurement duration for the last PRS RSTD sample in positioning frequency layer *i*, including the sampling time and processing time, = + ,

- is the periodicity of the PRS RSTD measurement in positioning frequency layer i defined as:

=

Where:

- corresponds to *durationOfPRS-ProcessingSymbolsInEveryTms-r17* in TS 37.355 [34],

- , the least common multiple between and , where is the DRX cycle of the UE, defined in TS 38.304, clause 7.1 [1].

- is the periodicity of DL PRS resource with muting on positioning frequency layer *i*.

If more than one PRS periodicities are configured in positioning frequency layer *i*, the least common multiple of PRS periodicities among all DL PRS resource sets in the positioning frequency layer is used to derive , where,

- , is the PRS periodicity with muting per PRS resource,

- is the periodicity of PRS resource sets given by the higher-layer parameter *DL-PRS-Periodicity*.

- is the scaling factor considering PRS resource muting. , where

- is the muting repetition factor given by the higher-layer parameter *DL-PRS-MutingBitRepetitionFactor*, and is the size of the bitmap .

- is the UE capability combination per band for RRC\_IDLE state where N is a duration of DL PRS symbols in ms corresponding to *durationOfPRS-ProcessingSymbols-r17* in TS 37.355 [34], T (ms) corresponds to *durationOfPRS-ProcessingSymbolsInEveryTms-r17* in TS 37.355 [34], for a given maximum bandwidth supported by UE corresponding to *supportedBandwidthPRS* in TS 37.355 [34],

- is UE capability for number of DL PRS resources that it can process in a slot in RRC\_IDLE state as indicated by *maxNumOfDL-PRS-ResProcessedPerSlot-RRC-Inactive-r17* specified in TS 37.355 [34].

If the following conditions are met, the time starts from the first DL PRS resource(s) instances inside a PTW after both the *NR-DL-TDOA-ProvideAssistanceData* message and *NR-DL-TDOA-RequestLocationInformation* message are delivered from LMF to the UE via LPP [34].

- UE is configured with CN eDRX > 10.24s, and

- periodic PRS measurement reporting is configured, and

- CN eDRX cycle is smaller or equal to the PRS measurement reporting periodicity configured via higher layer parameter *reportingInterval* in TS 37.355 [34], and

- there is one or more PRS resources occurring in PTW.

Otherwise, the timestarts from the first DL PRS resource(s) after both the *NR-DL-TDOA-ProvideAssistanceData* message and *NR-DL-TDOA-RequestLocationInformation* message are delivered from LMF to the UE via LPP [34].

Note: No per-positioning frequency layer requirement is applied in scenarios when multiple positioning frequency layers are configured.

If the UE DRX cycle changes during the RSTD measurement period, then the measurement period can be longer.

When PRS-RSRP is configured for DL-TDOA, RSTD and PRS-RSRP are performed over the same measurement period.

When PRS-RSRPP is configured for DL-TDOA, RSTD and PRS-RSRPP are performed over the same measurement period.

The measurement requirements do not apply to any PRS resource that always collides with other higher-priority DL signals/channels, as specified in clause 4.5.1.

Longer RSTD measurement period is expected when there are collisions between PRS resources and other higher-priority DL signals/channels.

If changes for any PFL during the measurement period, the measurement period could be longer.

The measurement requirements do not apply for a PRS resource, if the PRS resource is across two sampling duration of N within duration .

The measurement requirements do not apply for a PRS resource, if time span of the PRS resource instance (including at least the minimum number of repetitions specified in the accuracy requirements) is greater than UE reported capability N.

The requirements in clause 4.5.2 do not apply if the PRS configuration given by higher layer paramters *NR-DL-PRS-AssistanceData* exceeds any of the UE measurement capabilities given by *NR-DL-PRS-ResourcesCapability* in *NR-DL-TDOA-ProvideCapabilities*, and it is up to UE implementation which PRS resources are measured, subject to UE measurement capabilities*.*

If cell re-selection occurs while RSTD measurements are being performed, then the UE shall continue and complete the on-going RSTD measurements after the cell selection is completed. The RSTD measurement period can be longer.

If the RRC state transition occurs from RRC\_IDLE to RRC\_CONNECTED state during the RSTD measurement period then the UE shall continue the RSTD measurement in the RRC\_CONNECTED state. The RSTD measurement period can be longer.

The UE shall meet the RSTD measurement accuracy requirements in clause 10.1.23.2.

**END OF CHANGE**

**START OF CHANGE**

#### 5.6.2.5 Measurements Period Requirements

After receiving both *NR-DL-TDOA-ProvideAssistanceData* message and *NR-DL-TDOA-RequestLocationInformation* message from the LMF via LPP [34]*,* the UE shall be able to measure multiple (up to the UE capability specified in Clause 5.6.2.3) DL RSTD measurements, defined in TS 38.215 [4], during the measurement period defined as:

Where:

- is the index of positioning frequency layer,

- is total number of positioning frequency layers, and

- is the periodicity of the PRS RSTD measurement in positioning frequency layer i

is the measurement period for PRS RSTD measurement in positioning frequency layer *i* as specified below:

,

Where:

- is the UE Rx beam sweeping factor:

- = 1 if positioning frequency layer *i* is in FR1, and if positioning frequency layer *i* is in FR2

- equals to the value as UE reported in *supportedLowerRxBeamSweepingFactor-FR2* if the capability is reported by the UE for the band containing positioning frequency layer i, and LMF indicates *lowerRxBeamSweepingFactor-FR2* in *NR-DL-TDOA-RequestLocationInformation* .

- equals to 8, otherwise.

- is a scaling factor for PRS-based NR positioning measurements in RRC\_INACTIVE. If the UE supports *parallelPRS-MeasRRC-Inactive-r17*, Kcarrier\_PRS = 1; otherwise,

- If Srxlev ≤ SnonIntraSearchP or Squal ≤ SnonIntraSearchQ, , where is defined in clause 4.2.2.4

- If Srxlev > SnonIntraSearchP and Squal > SnonIntraSearchQ, , where is defined in clause 4.2.2.7.

- is the Rx TEG specific scaling factor:

- =1 if the UE is not configured by the LMF to measure a PRS resource with multiple Rx TEGs via *measureSameDL-PRS-ResourceWithDifferentRxTEGs-r17* [34].

- is defined as follows if the UE is configured by the LMF with *measureSameDL-PRS-ResourceWithDifferentRxTEGs-r17* [34] to perform measurement on same DL PRS resource of a TRP using different Rx TEGs in *NR-DL-TDOA-RequestLocationInformation* [34]:

- , if the UE is not capable of receiving same DL PRS resource simultaneously from multiple Rx TEGs, where P is the number of UE Rx TEGs that the UE is requested by LMF to measure the same DL-PRS Resource of a TRP indicated by *measureSameDL-PRS-ResourceWithDifferentRxTEGs-r17* in [34], and in case ‘n0’ is indicated, P is the maximum number of Rx TEGs with which UE can support to measure the same PRS resource as reported in *NR-UE-TEG-Capability*.

- , if the UE is capable of receiving the same DL PRS resource simultaneously from multiple Rx TEGs, where is the number of UE Rx TEGs for measuring the same DL-PRS Resource simultaneously indicated by *measureSameDL-PRS-ResourceWithDifferentRxTEGsSimul-r17* in [34].

- is the maximum number of DL PRS resources in positioning frequency layer *i* configured in a slot.

- is the time duration of available PRS in positioning frequency layer *i* to be measured , and is calculated in the same way as PRS duration K defined in clause 5.1.6.5 of TS 38.214 [26]. For calculation of , only unmuted PRS resources that are not fully overlapped with other higher-priority DL signals/channels are considered.

- is the number of PRS RSTD samples, where

- = 1 if the UE supports *supportedDL-PRS-ProcessingSamples-RRC-Inactive* [34], and the LMF requests the UE to perform positioning measurements with reduced number of samples, and meets the following conditions:

- PRS bandwidth is within the initial BWP and

- Magnitude of difference between the serving cell’s SS-RSRP and the neighbor cell’s PRS-RSRP is within 6 dB.

- = 2 if the UE supports *supportedDL-PRS-ProcessingSamples-RRC-Inactive* [34], and the LMF requests the UE to perform positioning measurements with reduced number of samples, and does not meet the following conditions:

- PRS bandwidth is within the initial BWP and

- Magnitude of difference between the serving cell’s SS-RSRP and the neighbor cell’s PRS-RSRP is within 6 dB.

- = 4 otherwise.

- is the measurement duration for the last PRS RSTD sample in positioning frequency layer *i*, including the sampling time and processing time, = + ,

- is the periodicity of the PRS RSTD measurement in positioning frequency layer i defined as:

=

Where:

- corresponds to *durationOfPRS-ProcessingSymbolsInEveryTms-r17* in TS 37.355 [34],

- , the least common multiple between and

- is defined as following:

- is DRX cycle length, defined in clause 7.1 TS 38.304, when no extended DRX (eDRX) cycle is configured

- is defined as T in clause 7.1 TS 38.304 when RAN eDRX <= 10.24s and CN eDRX <= 10.24s

- is the maximum of the T inside and outside of the CN PTW, where T inside and outside of the CN PTW are defined in clause 7.1 TS 38.304, when RAN eDRX <= 10.24s and CN eDRX > 10.24s

- is the maximum of the DRX cycles within the CN PTW and the RAN PTW when RAN eDRX > 10.24s

- is the periodicity of DL PRS resource with muting on positioning frequency layer *i*.

If more than one PRS periodicities are configured in positioning frequency layer *i*, the least common multiple of PRS periodicities among all DL PRS resource sets in the positioning frequency layer is used to derive , where,

- , is the PRS periodicity with muting per PRS resource,

- is the periodicity of PRS resource sets given by the higher-layer parameter *DL-PRS-Periodicity*.

- is the scaling factor considering PRS resource muting. , where

- is the muting repetition factor given by the higher-layer parameter *DL-PRS-MutingBitRepetitionFactor*, and is the size of the bitmap .

- is the UE capability combination per band for RRC\_INACTIVE state where N is a duration of DL PRS symbols in ms corresponding to *durationOfPRS-ProcessingSymbols-r17* in TS 37.355 [34], T (ms) corresponds to *durationOfPRS-ProcessingSymbolsInEveryTms-r17* in TS 37.355 [34], for a given maximum bandwidth supported by UE corresponding to *supportedBandwidthPRS* in TS 37.355 [34],

- is UE capability for number of DL PRS resources that it can process in a slot in RRC\_INACTIVE state as indicated by *maxNumOfDL-PRS-ResProcessedPerSlot-RRC-Inactive-r17* specified in TS 37.355 [34].

If the following conditions are met, the time starts from the first DL PRS resource(s) instances inside a PTW after both the *NR-DL-TDOA-ProvideAssistanceData* message and *NR-DL-TDOA-RequestLocationInformation* message are delivered from LMF to the UE via LPP [34].

- UE is configured with RAN eDRX > 10.24s, and

- periodic PRS measurement reporting is configured, and

- RAN eDRX cycle is smaller or equal to the PRS measurement reporting periodicity configured via higher layer parameter *reportingInterval* in TS 37.355 [34], and

- there is one or more PRS resources occurring in PTW.

Otherwise, the timestarts from the first DL PRS resource(s) after both the *NR-DL-TDOA-ProvideAssistanceData* message and *NR-DL-TDOA-RequestLocationInformation* message are delivered from LMF to the UE via LPP [34].

Note 1: No per-positioning frequency layer requirement is applied in scenarios when multiple positioning frequency layers are configured.

If the DRX cycle is reconfigured during the RSTD measurement period, then the measurement period can be longer.

When PRS-RSRP is configured for DL-TDOA, RSTD and PRS-RSRP are performed over the same measurement period.

When PRS-RSRPP is configured for DL-TDOA, RSTD and PRS-RSRPP are performed over the same measurement period.

The measurement requirements do not apply to any PRS resource that always collides with other higher-priority DL signals/channels, as specified in clause 5.6.1.

Longer RSTD measurement period is expected when there are collisions between PRS resources and other higher-priority DL signals/channels.

If changes for any PFL during the measurement period, the measurement period could be longer.

The measurement requirements do not apply for a PRS resource, if the PRS resource is across two sampling duration of N within duration .

The measurement requirements do not apply for a PRS resource, if time span of the PRS resource instance (including at least the minimum number of repetitions specified in the accuracy requirements) is greater than UE reported capability N.

The requirements in clause 5.6.2 do not apply if the PRS configuration given by higher layer paramters *NR-DL-PRS-AssistanceData* exceeds any of the UE measurement capabilities given by *NR-DL-PRS-ResourcesCapability* in *NR-DL-TDOA-ProvideCapabilities*, and it is up to UE implementation which PRS resources are measured, subject to UE measurement capabilities*.*

If cell re-selection occurs while RSTD measurements are being performed, then the UE shall continue and complete the on-going RSTD measurements after the cell selection is completed. The RSTD measurement period can be longer.

If the RRC state transition occurs from RRC\_INACTIVE to RRC\_CONNECTED state during the RSTD measurement period then the UE shall continue the RSTD measurement in the RRC\_CONNECTED state. The RSTD measurement period can be longer.

The UE shall meet the RSTD measurement accuracy requirements in clause 10.1.23.2.

**END OF CHANGE**