{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Cover","Parameters","PRACH FR2-1 1T2R"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cover","index":0,"n_rows":9,"n_cols":10,"rows_kept":9,"cut":false,"hidden":false,"merged":[]}
[]
[null,"3GPP TSG-RAN WG4 Meeting #111",null,null,null,null,null,null,null,"R4-2407109"]
[null,"Fukuoka City, JP, May 20-24, 2024"]
[]
[null,"Source: China Telecom"]
[null,"Title: Summary of simulation results for Rel-18 NR coverage enhancements BS demodulation requirements"]
[null,"Agenda: 7.17.2"]
[]
[null,"Reference: R4-2406137 WF on NR_cov_enh2_demod, China Telecom"]

{"sheet":"Parameters","index":1,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[[1,2,1,4],[7,2,7,4],[6,2,6,4]]}
[]
[null,null,"Parameters for deriving performance requirements"]
[null,null,"Ideal Span Threshold",2,"dB"]
[null,null,"Impairment Span Threshold",4,"dB"]
[]
[]
[null,"Notes","1. Call function DerivingPerfReq()"]
[null,null,"2. If the ruls does not apply, or fails, -100dB or less will be returned"]
[null,null,null,-100,"Not enough input"]
[null,null,null,-101,"Input should be pairs"]
[null,null,null,-102,"Too large span for impairment"]
[null,null,null,-103,"After removal iteration, not enough input"]

{"sheet":"PRACH FR2-1 1T2R","index":2,"n_rows":10,"n_cols":25,"rows_kept":10,"cut":false,"hidden":false,"merged":[[0,0,1,1],[2,1,9,1],[2,0,4,0],[5,0,6,0],[7,0,9,0],[0,21,0,22],[0,23,0,24],[0,9,0,10],[0,11,0,12],[0,13,0,14],[0,15,0,16],[0,17,0,18],[0,19,0,20],[3,2,4,2],[8,2,9,2],[3,3,4,3],[8,3,9,3],[0,7,0,8],[0,2,1,2],[0,3,1,3],[0,5,1,5],[0,6,1,6],[0,4,1,4]]}
[" PRACH FR2-1 1T2R",null,"Propagation condition","Frequency offset (Hz)","Repetition Interval","38.104 req","38.141 req","Nokia (R4-2407140)",null,"Ericsson (R4-2408346)",null,"Huawei (R4-2408957)",null,"ZTE (R4-2409082)",null,"Samsung (R4-2409475)",null,"Company 6",null,"Company 7",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["Format A2","120kHz","AWGN",0,"N/A","N/A","N/A",-18.8,-16.100000000000001,-17.78,null,-17.3,-14.8,-18.600000000000001,null,-16.7,null,null,null,null,null,{"$f":"MAX(H3,J3,L3,N3,P3,R3,T3)-MIN(H3,J3,L3,N3,P3,R3,T3)","v":2.1000000000000014},{"$f":"MAX(I3,K3,M3,O3,Q3,S3,U3)-MIN(I3,K3,M3,O3,Q3,S3,U3)","v":1.3000000000000007},{"$f":"AVERAGE(H3,J3,L3,N3,P3,R3,T3)","v":-17.835999999999999},{"$f":"AVERAGE(I3,K3,M3,O3,Q3,S3,U3)","v":-15.450000000000001}]
[null,null,"TDLA30-300 Low",4000,"Repetition within 1 slot",{"$f":"DerivingPerfReq(H4:U4)","v":-100},{"$f":"IF(F4>-100,F4+0.6,F4)","v":-100},null,null,null,null,-9.1999999999999993,-6.6999999999999993,null,null,null,null,null,null,null,null,{"$f":"MAX(H4,J4,L4,N4,P4,R4,T4)-MIN(H4,J4,L4,N4,P4,R4,T4)","v":0},0,{"$f":"AVERAGE(H4,J4,L4,N4,P4,R4,T4)","v":-9.1999999999999993},-6.6999999999999993]
[null,null,null,null,"10 slots",{"$f":"DerivingPerfReq(H5:U5)","v":-100},{"$f":"IF(F5>-100,F5+0.6,F5)","v":-100},-12.1,-9.4,-11.64,null,null,null,-11.2,null,null,null,null,null,null,null,{"$f":"MAX(H5,J5,L5,N5,P5,R5,T5)-MIN(H5,J5,L5,N5,P5,R5,T5)","v":0.90000000000000036},{"$f":"MAX(I5,K5,M5,O5,Q5,S5,U5)-MIN(I5,K5,M5,O5,Q5,S5,U5)","v":0},{"$f":"AVERAGE(H5,J5,L5,N5,P5,R5,T5)","v":-11.646666666666667},{"$f":"AVERAGE(I5,K5,M5,O5,Q5,S5,U5)","v":-9.4}]
["Format B4",null,"AWGN",0,"N/A","N/A","N/A",-23.5,-20.8,-22.23,null,-19.5,-17,-21.7,null,-20.9,null,null,null,null,null,{"$f":"MAX(H6,J6,L6,N6,P6,R6,T6)-MIN(H6,J6,L6,N6,P6,R6,T6)","v":4},3.8000000000000007,{"$f":"AVERAGE(H6,J6,L6,N6,P6,R6,T6)","v":-21.566000000000003},-18.899999999999999]
[null,null,"TDLA30-300 Low",4000,"10 slots",{"$f":"DerivingPerfReq(H7:U7)","v":-100},{"$f":"IF(F7>-100,F7+0.6,F7)","v":-100},-14.8,-12.1,-14.97,null,-11.2,-8.6999999999999993,-14,null,null,null,null,null,null,null,{"$f":"MAX(H7,J7,L7,N7,P7,R7,T7)-MIN(H7,J7,L7,N7,P7,R7,T7)","v":3.7700000000000014},3.4000000000000004,{"$f":"AVERAGE(H7,J7,L7,N7,P7,R7,T7)","v":-13.7425},-10.399999999999999]
["Format C2",null,"AWGN",0,"N/A",-100,{"$f":"IF(F8>-100,F8+0.3,F8)","v":-100},-18.8,-16.100000000000001,-17.75,null,-17.399999999999999,-14.899999999999999,-18.600000000000001,null,-16.61,null,null,null,null,null,{"$f":"MAX(H8,J8,L8,N8,P8,R8,T8)-MIN(H8,J8,L8,N8,P8,R8,T8)","v":2.1900000000000013},1.2000000000000028,{"$f":"AVERAGE(H8,J8,L8,N8,P8,R8,T8)","v":-17.832000000000001},-15.5]
[null,null,"TDLA30-300 Low",4000,"Repetition within 1 slot","N/A","N/A",null,null,null,null,-9.1999999999999993,-6.6999999999999993,null,null,null,null,null,null,null,null,{"$f":"MAX(H9,J9,L9,N9,P9,R9,T9)-MIN(H9,J9,L9,N9,P9,R9,T9)","v":0},{"$f":"MAX(I9,K9,M9,O9,Q9,S9,U9)-MIN(I9,K9,M9,O9,Q9,S9,U9)","v":0},{"$f":"AVERAGE(H9,J9,L9,N9,P9,R9,T9)","v":-9.1999999999999993},{"$f":"AVERAGE(I9,K9,M9,O9,Q9,S9,U9)","v":-6.6999999999999993}]
[null,null,null,null,"10 slots",{"$f":"DerivingPerfReq(H10:U10)","v":-100},{"$f":"IF(F10>-100,F10+0.6,F10)","v":-100},-12.3,-9.6,-11.86,null,-8.6,-6.1,-11.2,null,null,null,null,null,null,null,3.7000000000000011,3.5,-10.989999999999998,-7.85]