**3GPP TSG-RAN WG4 Meeting #111 *R4-2409913***

**Fukuoka City, Fukuoka, Japan, 20th – 24th May, 2024**

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** |  | **rev** |  | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Draft  |
|  |  |
| ***Source to WG:*** | , Cybercore |
| ***Source to TSG:*** |  |
|  |  |
| ***Work item code:*** | NR\_MIMO\_evo\_DL\_UL-Perf |  | ***Date:*** |  |
|  |  |  |  |  |
| ***Category:*** | ***B*** |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | Introduce new channel combination for PMI reporting requirements of Rel-18 Doppler codebook.  |
|  |  |
| ***Summary of change:*** | The summary of changes in this CR as below:* Add one row in Table B.2.2-1
 |
|  |  |
| ***Consequences if not approved:*** | * No channel combination for PMI reporting requirements of Rel-18 Doppler codebook.
 |
|  |  |
| ***Clauses affected:*** | B.2.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **x** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** | **x** |  |  Test specifications | TS 38.521-4  |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** | Revision of R4-2408500 |

**<Start of changes>**

## B.2.2 Combinations of channel model parameters

The propagation conditions used for the performance measurements in multi-path fading environment are indicated as a combination of a channel model name and a maximum Doppler frequency, i.e., TDLA<DS>-<Doppler>, TDLB<DS>-<Doppler>, TDLC<DS>-<Doppler>or TDLD<DS>-<Doppler> where '<DS>' indicates the desired delay spread and '<Doppler>' indicates the maximum Doppler frequency (Hz).

Table B.2.2-1 and Table B.2.2-2 show the propagation conditions that are used for the performance measurements in multi-path fading environment for low, medium and high Doppler frequencies for FR1 and FR2, respectively.

Table B.2.2-1: Channel model parameters for FR1

|  |  |  |
| --- | --- | --- |
| **Combination name** | **Model** | **Maximum Doppler frequency** |
| TDLA30-5 | TDLA30 | 5 Hz |
| TDLA30-10 | TDLA30 | 10 Hz |
| TDLA30-20 | TDLA30 | 20 Hz |
| TDLA30-180 | TDLA30 | 180 Hz |
| TDLA30-1400 | TDLA30 | 1400 Hz |
| TDLA30-2700 | TDLA30 | 2700 Hz |
| TDLB100-400 | TDLB100 | 400 Hz |
| TDLC300-100 | TDLC300 | 100 Hz |
| TDLC300-600 | TDLC300 | 600 Hz |
| TDLC300-1200 | TDLC300 | 1200 Hz |
| TDLD30-5 | TDLD30 | 5 Hz |

Table B.2.2-2: Channel model parameters for FR2

|  |  |  |
| --- | --- | --- |
| **Combination name** | **Model** | **Maximum Doppler frequency** |
| TDLA30-35 | TDLA30 | 35 Hz |
| TDLA30-75 | TDLA30 | 75 Hz |
| TDLA30-300 | TDLA30 | 300 Hz |
| TDLC60-300 | TDLC60 | 300 Hz |
| TDLD30-75 | TDLD30 | 75 Hz |

**<End of changes>**