**3GPP TSG-SA3 Meeting #116 *draft\_S3-242186-r1***

**Jeju, South Korea, 20 – 24 May 2024**  (revision of S3-yyxxxx)

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **33.501** | **CR** | **2010** | **rev** | **1** | **Current version:** | **18.5.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Clarification on the usage of N32-f message ID | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Huawei, HiSilicon, Nokia, Nokia Shanghai Bell | | | | | | | | | |
| ***Source to TSG:*** | S3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | Roaming5G | | | | |  | ***Date:*** | | | 2024-04-28 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-18 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | The reformattedData JSON element in the error message is defined to contain metadata with N32-f message ID and N32-f context ID, which are used to indicate that the message is the error message. However, the other usage of N32-f message ID remains unclear.  -r1 provides the reference for the explanation. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Clarify that N32-f message ID is used to indicate the message in which the error occurred.  -r1 - only reference needed. Updated accordingly. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | The usage of N32-f context ID is not clear. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 13.2.4.5.2a | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | | ***S3-242186*** | | | | | | | | |

\*\*\* BEGIN of 1st CHANGE \*\*\*

##### 13.2.4.5.2a Error messages originated by Roaming Hub

In case a roaming hub needs to originate an error message, then clause 13.2.4.5.2 shall also apply with the following addition: If an error message needs to be sent, the originating roaming hub shall insert a reformattedData JSON element including only the metadata IE as defined in TS 29.573 [73], Table 6.2.5.2.2 for the Request, and Table 6.2.5.2.3 for the response, and the patches shall be based on a reformattedData JSON element including only the metadata.

The reformattedData JSON element shall only contain metadata with N32-f message ID and N32-f context ID (as defined in clause 13.2.4.3.1.2).

\*\*\* END of 1st CHANGE \*\*\*