**3GPP TSG-SA5 Meeting #156 *S5-244944***

**Maastricht, Netherlands, 19 – 23 August 2024**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **28.558** | **CR** | **0016** | **rev** | **1** | **Current version:** | **19.0.0** |  |
|  |
| *For* [***HELP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Rel-19 CR TS 28.558 Add the missing measurement object class for UL PDCP SDU Loss Rate |
|  |  |
| ***Source to WG:*** | Nokia, Huawei |
| ***Source to TSG:*** | S5 |
|  |  |
| ***Work item code:*** |  |  | ***Date:*** | 2024-08-08 |
|  |  |  |  |  |
| ***Category:*** | **A** |  | ***Release:*** | Rel-19 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | The measured object classes for the measurement on UL PDCP SDU loss rate are GNBCUUPFunction and NRCellCU as per TS 28.552. The definition for UE specific measurement on the same topic is missing the object class NRCellCU. |
|  |  |
| ***Summary of change:*** | Add the NRCellCU measurement object class for UL PDCP SDU Loss rate |
|  |  |
| ***Consequences if not approved:*** | Incorrect specification |
|  |  |
| ***Clauses affected:*** | 6.3.1.3.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ... |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

***Start of first Change***

##### 6.3.1.3.1 UL PDCP SDU Loss Rate

a) This measurement provides the fraction of PDCP SDU packets which are not successfully received at gNB-CU-UP. It is a measure of the UL packet loss including any packet losses in the air interface, in the gNB-CU and on the F1-U interface. Only user-plane traffic (DTCH) and only PDCP SDUs that have entered PDCP (and given a PDCP sequence number) are considered. The measurement is optionally split into subcounters per QoS level (mapped 5QI or QCI in NR option 3), and subcounters per supported S-NSSAI. This measurement is also referred to as UL M7 in TS 37.320 [9].

b) SI

c) This measurement is obtained as: 1,000,000\* Number of missing UL PDCP sequence numbers, representing packets that are not delivered to higher layers, of a data radio bearer, divided by Total number of UL PDCP sequence numbers (also including missing sequence numbers) of a bearer, starting from the sequence number of the first packet delivered by UE PDCP to gNB-CU-UP until the sequence number of the last packet. If transmission of a packet might continue in another cell, it shall not be included in this count. Separate counters are optionally maintained for mapped 5QI (or QCI for NR option 3) and per supported S-NSSAI.

d) Each measurement is an integer value representing the loss rate multiplied by 1E6. The number of measurements is equal to one. If the optional QoS and S-NSSAI level measurements are performed, the measurements are equal to the number of mapped 5QIs and the number of supported S-NSSAIs.

e) The measurement name has the form DRB.PacketLossRateUlUe, and optionally
DRB.PacketLossRateUlUe.*QoS* where *QoS* identifies the target quality of service class, and DRB.PacketLossRateUlUe.*SNSSAI* where *SNSSAI* identifies the S-NSSAI.

f) GNBCUUPFunction (applicable to all split scenarios);

NRCellCU (only applicable to 2-split scenario).g) NA

h) One usage of this measurement is to support ML training and performance evaluation.

***End of Changes***