**3GPP TSG-CT WG3 Meeting #135 *C3-243352***

**Hyderabad, IN, 27 - 31 May, 2024**

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  | **29.122** | **CR** | **0849** | **rev** | **-** | **Current version:** | **18.5.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Data rate and congestion report |
|  |  |
| ***Source to WG:*** | Ericsson |
| ***Source to TSG:*** | CT3 |
|  |  |
| ***Work item code:*** | XRM |  | ***Date:*** | 2024-04-29 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | It is not detailed the description of the congestion and data rate report. |
|  |  |
| ***Summary of change:*** | As specified in TS 29.564:- The data rate report indicates an average data throughput- The congestion report indicates congestion information, expressed as an integer value in the range 0 to 10000, representing the percentage of congestion level in the downlink direction, up to two decimal points, for the QoS flow.Example: the value 9574 corresponds to a percentage of 95.74%. |
|  |  |
| ***Consequences if not approved:*** | Incomplete specification, with ambiguities about the received measurements |
|  |  |
| ***Clauses affected:*** | 5.14.2.1.8 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **x** |  Other core specifications  | TS/TR ... CR ... |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This CR does not have any impact in the OpenAPI specifications. |
|  |  |
| ***This CR's revision history:*** |  |

\* \* \* First Change \* \* \* \*

##### 5.14.2.1.8 Type: QosMonitoringReport

Table 5.14.2.1.8-1: Definition of type QosMonitoringReport

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | Cardinality | Description | Applicability |
| ulDelays | array(Uinteger) | 0..N | Uplink packet delay in units of milliseconds. (NOTE 1) |  |
| dlDelays | array(Uinteger) | 0..N | Downlink packet delay in units of milliseconds. (NOTE 1) |  |
| rtDelays | array(Uinteger) | 0..N | Round trip delay in units of milliseconds. (NOTE 1) |  |
| pdmf | boolean | 0..1 | Packet delay measurement failure indicator. When set to true, it indicates that a packet delay failure has occurred.Default value is false if omitted. (NOTE 2) | PacketDelayFailureReport, GMEC\_5G |
| ulDataRate | BitRate | 0..1 | Average data throughput in uplink direction (NOTE 3) | EnQoSMon, GMEC\_5G |
| dlDataRate | BitRate | 0..1 | Average data throughput in downlink direction.(NOTE 3) | EnQoSMon, GMEC\_5G |
| ulAggrDataRate | BitRate | 0..1 | Indicates the uplink aggregated Data Rate for the applicable list of UEs provided by AF. | ListUE\_5G |
| dlAggrDataRate | BitRate | 0..1 | Indicates the downlink aggregated Data Rate for the applicable list of UEs provided by AF. | ListUE\_5G |
| ulConInfo | Uinteger | 0..1 | Percentage of congestion information in uplink direction. | EnQoSMon, GMEC\_5G |
| dlConInfo | Uinteger | 0..1 | Percentage of congestion information in downlink direction. | EnQoSMon, GMEC\_5G |
| NOTE 1: In this release of the specification one element may be included in the array as difined in clause 4.4.9 in TS 29.522 [62].NOTE 2: When the "pdmf" attribute is set to true, "ulDelays", "dlDelays" and "rtDelays" and when the feature "EnQoSMon" is supported, "ulDataRate" and "dlDataRate" shall not be present.NOTE 3: When the "ulDataRate" and/or the "dlDataRate" attribute are included, the parameters related to packet delay and/or congestion information shall not be present. |

Editor’s Note: The presence conditions of the parameters of QosMonitoringReport are to be consolidated/detailed once all the possible reports are specified.

\* \* \* End Change \* \* \* \*