**3GPP TSG RAN WG1 #117 R1-2404090**

**Fukuoka, Japan, May 20th – 24th, 2024**

**Agenda item:** 8.1

**Source:** Moderator (Samsung)

**Title:** Summary for Rel-18 MIMO CSI maintenance

**Document for:** Discussion and Decision

## Introduction

This contribution includes the summary for maintenance issues on Rel-18 CSI enhancements for MIMO Evolution.

## Summary of companies’ proposals and views

### Issue 1: Type-II codebook refinement for CJT

(none)

Table 1 Additional inputs: issue 1

|  |  |
| --- | --- |
| **Company** | **Input** |
| Mod V0 | **none** |
|  |  |
|  |  |

### Issue 2: Type-II codebook refinement for high/medium UE velocities (with time/Doppler-domain compression)

**Proposal 1.A**: For the Rel-18 Type-II codebook refinement for high/medium-speed, adopt the following TP for TS 38.214

|  |
| --- |
| TS 38.214 |
| **Reason for change:** |
| In current specification, the value of w used for relaxing aperodic CSI reporting time for Rel-18 Type II codebook is not given. In addition, it is not clear how to obtain value of w. According to agreement on the UE feature achieved in RAN1#116-bis meeting, the value of w is equal to 14\*(KP–1)\*d or 14\*KP\*d symbols, where the value of K\_P∈{1,2,4} is indicated by UE capability, and d is is the periodicity of periodic or semi-persistent CSI-RS resource. The value of w is reported by UE capability indication. Such agreement should be caputured in current specification for clarification |
| **Summary of change:** |
| Clarify the value of w and how to obtain w in section 5.4.. |
| **Consequences if not approved:** |
| It is not unclear what is the value of w and how to obtain w.. |
| **Text proposal:** |
| 5.4 UE CSI computation time  -------------------------------------------Unchanged parts are omitted-------------------------------------------  ….  - or , according to UE reported capability, with of table 5.4-2, if *codebookType* is set to 'typeII-CJT-r18' or 'typeII-CJT-PortSelection-r18' and the corresponding *NZP-CSI-RS-ResourceSet* for channel measurement is configured with resources, or  - , with of table 5.4-2, if the CSI report is configured with , *codebookType* is set to ‘typeII-Doppler-r18’ or ‘typeII-Doppler-PortSelection-r18’ and the corresponding *NZP-CSI-RS-ResourceSet* for channel measurement is aperiodic with CSI-RS resources, or  - , with of table 5.4-2, where w=56.(*KP* –1) or 56.*KP* symbols, according to the reported UE capability, where the value of 𝐾𝑃 ∈{1,2,4} is indicated by UE capability, if the CSI report is configured with , *codebookType* is set to ‘typeII-Doppler-r18’ or ‘typeII-Doppler-PortSelection-r18’ and the corresponding *NZP-CSI-RS-ResourceSet* for channel measurement is periodic or semi-persistent with a single CSI-RS resource, or  - or , according to UE reported capability, with of table 5.4-2, if the CSI report is configured with , *codebookType* is set to ‘typeII-Doppler-r18’ and the corresponding *NZP-CSI-RS-ResourceSet* for channel measurement is aperiodic with CSI-RS resources, or  …  -------------------------------------------Unchanged parts are omitted------------------------------------------- |
| **Support/fine**: Xiaomi  **Not support**:  **FL assessment**: This TP seems correct (based on RAN1#116bis agreement in UE feature session) |

Table 2 Additional inputs: issue 2

|  |  |
| --- | --- |
| **Company** | **Input** |
| Mod V0 | **Please share your inputs on each of the above proposals** |
| Lenovo/ MotM | We are fine with this TP |
| Samsung | We are fine with the TP in principle. It seems that the value of d = 4 is only agreed in UE feature session (checked the agreed modification on FG 40-3-2-11 in R1-2403703), we would like to suggest a modification to reflect this.  where =14.(KP–1).d or 14.KP.d symbols is reported by UE capability indication and d=4 is the minimum periodicity of periodic or semi-persistent CSI-RS resource |
| Google | OK, we slightly prefer the following modification. Since the value of w has already been defined in UE capability, we only need to specify w is based on the UE capability. We can also mention the UE capability name if necessary.  where ~~=14.(K~~~~P~~~~–1).d or 14. K~~~~P~~~~.d symbols~~ is reported by UE capability ~~indication and d is the periodicity of periodic or semi-persistent CSI-RS resource~~ |
| Apple | We are fine with the proposal from Google, or we could replace d with 4, and align the Kp description with Section 5.2.1.6  where =56.(KP–1) or 56. KP symbols, according to UE reported capability, where the value of 𝐾𝑃∈{1,2,4} is indicated by UE capability. |
| ZTE | For readability, we are fine with either Samsung or Apple’s update. The original version is not sufficient due to the fact that the value of d is not defined in the corresponding paragraphs. |
| vivo | We are fine with the update from Samsung or Apple to make the spec. clarity. |
| Mod Final | Seems the TP is agreeable. Taking into all the wording suggestions (agree with clarity from Samsung, minimizing duplicate description across specs from Google, and conciseness from Apple):  Original Xiaomi’s wording:  where =14.(KP–1).d or 14. KP.d symbols is reported by UE capability indication and d is the periodicity of periodic or semi-persistent CSI-RS resource  Revised:  where =56.(KP –1) or 56.KP symbols, according to the reported UE capability, where the value of 𝐾𝑃∈{1,2,4} is indicated by UE capability. |

### Issue 3: TRS-based reporting of time-domain channel properties (TDCP)

(None)

Table 3 Additional inputs: issue 3

|  |  |
| --- | --- |
| **Company** | **Input** |
| Mod V0 | **None** |
|  |  |
|  |  |

# References

|  |  |  |  |
| --- | --- | --- | --- |
| 1 | R1-2404977 | Draft CR on Rel-18 Type II Doppler codebook based CSI enhancement | Xiaomi |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |