**3GPP TSG-RAN WG1 Meeting #117R1-240xxxx**

Fukuoka City, Fukuoka, Japan, May 20th – 24th, 2024

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  | **38.213** | **CR** | **xxxx** | **rev** | **-** | **Current version:** | **18.2.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Correction on priority for LTM CSI report |
|  |  |
| ***Source to WG:*** | Moderator (Fujitsu), , [Ericsson, Google, Huawei, HiSilicon, Nokia] |
| ***Source to TSG:*** | R1 |
|  |  |
| ***Work item code:*** | NR\_Mob\_enh2-Core |  | ***Date:*** | 23 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | 8 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | RAN1 has agreed that LTM CSI reports have higher priority than CSI reports. This has been captured in 38.214, with an explicit statement A CSI report configured with *LTM-CSI-ReportConfig* has a higher priority over all CSI report(s) configured with *CSI-ReportConfig* However, 38.213 states that …the UE selects  CSI report(s) for transmission together with HARQ-ACK information and SR, when any, in ascending priority value as described in [6, TS 38.214].Hence, 38.213 assumes that the priority value is a single numerical value, which is inconsistent with the current definition in 38.214. Therefore, it is necessary to the description to follow the priority rather than the priority value.  |
|  |  |
| ***Summary of change:*** | Clarify to follow descending priority when both *csi-ReportConfigToAddModList* and *ltm-CSI-ReportConfigToAddModList* are configured. |
|  |  |
| ***Consequences if not approved:*** | Unclear prioritization rules for LTM CSI reports |
|  |  |
| ***Clauses affected:*** | 9.2.5.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | **Isolated impact analysis:**This CR has no isolated impact on network and UE behavior.  |
|  |  |
| ***This CR's revision history:*** | This is the first version of this CR. |

#### 9.2.5.2 UE procedure for multiplexing HARQ-ACK/SR/CSI in a PUCCH

<Unchanged part is omitted>

If a UE has one or more CSI reports and zero or more HARQ-ACK/SR information bits to transmit in a PUCCH where the HARQ-ACK, if any, is in response to a PDSCH reception without a corresponding PDCCH

- if any of the CSI reports are overlapping and the UE is provided by *multi-CSI-PUCCH-ResourceList* with  PUCCH resources in a slot, for PUCCH format 2 and/or PUCCH format 3 and/or PUCCH format 4, as described in clause 9.2.1, where the resources are indexed according to an ascending order for the product of a number of corresponding REs, modulation order , and configured code rate ;

- if , the UE uses PUCCH format 2 resource , or the PUCCH format 3 resource , or the PUCCH format 4 resource 

- else if  and , , the UE transmits a PUCCH conveying HARQ-ACK information, SR and CSI report(s) in a respective PUCCH where the UE uses the PUCCH format 2 resource , or the PUCCH format 3 resource , or the PUCCH format 4 resource 

- else the UE uses the PUCCH format 2 resource , or the PUCCH format 3 resource , or the PUCCH format 4 resource  and the UE selects  CSI report(s) for transmission together with HARQ-ACK information and SR, when any, in descending priority as described in [6, TS 38.214] when both *csi-ReportConfigToAddModList* and *ltm-CSI-ReportConfigToAddModList* are configured, otherwise ascending priority value as described in [6, TS 38.214]

- else, the UE transmits the  bits in a PUCCH resource provided by *pucch-CSI-ResourceList* and determined as described in clause 9.2.5

<Unchanged part is omitted>