**3GPP TSG-RAN WG1 Meeting #1170xxxx**

Fukuoka City, Fukuoka, Japan, May 20th – 24th, 2024

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  | **38.213** | **CR** | **xxxx** | **rev** | **-** | **Current version:** | **18.2.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Correction on priority for LTM CSI report |
|  |  |
| ***Source to WG:*** | Moderator (Fujitsu), , [Ericsson, Google, Huawei, HiSilicon, Langbo, Lenovo, New H3C, Nokia, Samsung] |
| ***Source to TSG:*** | R1 |
|  |  |
| ***Work item code:*** | NR\_Mob\_enh2-Core |  | ***Date:*** | 23 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | 8 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | RAN1 has agreed that LTM CSI reports have higher priority than CSI reports. This has been captured in 38.214, with an explicit statement A CSI report configured with *LTM-CSI-ReportConfig* has a higher priority over all CSI report(s) configured with *CSI-ReportConfig* However, 38.213 states that …the UE selects  CSI report(s) for transmission together with HARQ-ACK information and SR, when any, in ascending priority value as described in [6, TS 38.214].The above text means that priority of LTM CSI report is lower than Legacy CSI report when priority value for LTM CSI report is greater than that of Legacy CSI report. But it is not true in fact. Therefore, it is necessary to update the description to follow the priority rather than the priority value.  |
|  |  |
| ***Summary of change:*** | Clarify to follow descending priority when both *csi-ReportConfigToAddModList* and *ltm-CSI-ReportConfigToAddModList* are configured. |
|  |  |
| ***Consequences if not approved:*** | Unclear prioritization rules for LTM CSI reports |
|  |  |
| ***Clauses affected:*** | 9.2.5.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | **Isolated impact analysis:**This CR has no isolated impact on network and UE behavior.  |
|  |  |
| ***This CR's revision history:*** | This is the first version of this CR. |

#### 9.2.5.2 UE procedure for multiplexing HARQ-ACK/SR/CSI in a PUCCH

<Unchanged part is omitted>

If a UE has one or more CSI reports and zero or more HARQ-ACK/SR information bits to transmit in a PUCCH where the HARQ-ACK, if any, is in response to a PDSCH reception without a corresponding PDCCH

- if any of the CSI reports are overlapping and the UE is provided by *multi-CSI-PUCCH-ResourceList* with  PUCCH resources in a slot, for PUCCH format 2 and/or PUCCH format 3 and/or PUCCH format 4, as described in clause 9.2.1, where the resources are indexed according to an ascending order for the product of a number of corresponding REs, modulation order , and configured code rate ;

- if , the UE uses PUCCH format 2 resource , or the PUCCH format 3 resource , or the PUCCH format 4 resource 

- else if  and , , the UE transmits a PUCCH conveying HARQ-ACK information, SR and CSI report(s) in a respective PUCCH where the UE uses the PUCCH format 2 resource , or the PUCCH format 3 resource , or the PUCCH format 4 resource 

- else the UE uses the PUCCH format 2 resource , or the PUCCH format 3 resource , or the PUCCH format 4 resource  and the UE selects  CSI report(s) for transmission together with HARQ-ACK information and SR, when any, in descending priority as described in [6, TS 38.214] when both *csi-ReportConfigToAddModList* and *ltm-CSI-ReportConfigToAddModList* are configured, otherwise ascending priority value as described in [6, TS 38.214]

- else, the UE transmits the  bits in a PUCCH resource provided by *pucch-CSI-ResourceList* and determined as described in clause 9.2.5

<Unchanged part is omitted>