**3GPP TSG-RAN WG4 Meeting # 112bis R4-2415941**

**Hefei, China, 14th-18th Oct, 2024**

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  | **38.106** | **CR** | **-** | **rev** | **-** | **Current version:** | **18.6.0** |  |
|  |
| *For* ***[HELP](http://www.3gpp.org/3G_Specs/CRs.htm%22%20%5Cl%20%22_blank)*** *on using this form: comprehensive instructions can be found at <http://www.3gpp.org/Change-Requests>.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **x** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | (NR\_bands\_n87\_n88-Core) Draft CR to TS38.106: Introduction of NR bands n87 and n88 |
|  |  |
| ***Source to WG:*** | ZTE Corporation, Sanechips |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NR\_bands\_n87\_n88-Core |  | ***Date:*** | 2024-08-30 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-19 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19) Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | Introduction of new NR bands n87 and n88. |
|  |  |
| ***Summary of change:*** | Required changes to support NR bands n87 and n88. |
|  |  |
| ***Consequences if not approved:*** | NR bands n87 and n88 are not supported. |
|  |  |
| ***Clauses affected:*** | 5.3.4, 6.5.3.2.1, 6.5.3.2.2, 6.5.4.2.2, 6.5.4.2.3 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **x** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **x** |  Test specifications | TS/TR ... CR ... |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

## << Start of change >>

### 5.3.4 TX–RX frequency separation

The default TX channel (carrier centre frequency) to RX channel (carrier centre frequency) separation for operating bands is specified in Table 5.3.4-1.

Table 5.3.4-1: NCR-MT TX-RX frequency separation

| NR Operating Band | TX – RX carrier centre frequencyseparation |
| --- | --- |
| n1 | 190 MHz |
| n2 | 80 MHz |
| n3 | 95 MHz |
| n5 | 45 MHz |
| n7 | 120 MHz |
| n8 | 45 MHz |
| n12 | 30 MHz |
| n13 | -31 MHz |
| n14 | -30 MHz |
| n18 | 45 MHz |
| n20 | -41 MHz |
| n24 | -101.5, -120.5 MHz |
| n25 | 80 MHz |
| n26 | 45 MHz |
| n28 | 55 MHz |
| n30 | 45 MHz |
| n65 | 190 MHz |
| n66 | 400 MHz |
| n70 | 300MHz |
| n71 | -46 MHz |
| n74 | 48 MHz |
| n85 | 30 MHz |
| n87 | 10MHz |
| n88 | 10MHz |
| n91 | 570 MHz – 595 MHz(NOTE 2) |
| n92 | 575 MHz – 680 MHz (*μ* = 0)580 MHz – 675 MHz (*μ* = 1)(NOTE 2) |
| n93 | 517 MHz – 547 MHz(NOTE 2) |
| n94 | 522 MHz – 632 MHz (*μ* = 0)527 MHz – 627 MHz (*μ* = 1)(NOTE 2) |
| n100 | 45 MHz |
| n105 | -51 MHz |
| NOTE 1: VoidNOTE 2: The range of TX-RX frequency separation given paired UL and DL channel bandwidths BWUL and BWDL is given by the respective lower and upper limit FDL\_low – FUL\_high + 0.5(BWDL + BWUL) and FDL\_high – FUL\_low – 0.5(BWDL + BWUL). The UL and DL channel bandwidth combinations specified in Clause 5.4 depend on the subcarrier spacing configuration *μ* [21]. |

## << Next change >>

##### 6.5.3.2.1 basic limits for Wide Area repeater type 1-C (Category A)

For repeater operating in Bands n5, n8, n12, n13, n14, n18, n26, n28, n29, n31, n71, n72, n85, n87, n88, basic limits are specified in table 6.5.3.2.1‑1.

Table 6.5.3.2.1-1: Wide Area operating band unwanted emission basic limits (NR bands below 1 GHz) for Category A

|  |  |  |  |
| --- | --- | --- | --- |
| Frequency offset of measurement filter ‑3dB point, Δf | Frequency offset of measurement filter centre frequency, f\_offset | *Basic limits* (Notes 1, 2) | *Measurement bandwidth* |
| 0 MHz ≤ Δf < 5 MHz | 0.05 MHz ≤ f\_offset < 5.05 MHz |  | 100 kHz  |
| 5 MHz ≤ Δf <min(10 MHz, Δfmax) | 5.05 MHz ≤ f\_offset <min(10.05 MHz, f\_offsetmax) | -14 dBm | 100 kHz  |
| 10 MHz ≤ Δf ≤ Δfmax | 10.05 MHz ≤ f\_offset < f\_offsetmax  | -13 dBm (Note 3) | 100 kHz  |
| NOTE 1: For a *repeater* supporting *non-contiguous spectrum* operation within any *operating band*, the emission basic limits within *gaps between passbands* is calculated as a cumulative sum of contributions from adjacent *sub-blocks* on each side of the *gap between passbands*. Exception is f ≥ 10MHz from both adjacent *sub-blocks* on each side of the *gap between passbands*, where the emission limits within *gaps between passbands* shall be ‑13 dBm/1 MHz.NOTE 2: For a *multi-band connector* with *inter-passband gap* < 2\*ΔfOBUE the emission basic limits within the *inter-passband gaps* is calculated as a cumulative sum of contributions from adjacent *sub-blocks* or *passband* on each side of the *inter-passband gap*, where the contribution from the far-end *sub-block* or *passband* shall be scaled according to the *measurement bandwidth* of the near-end *sub-block* or *passband*.NOTE 3: The basic limit is not applicable when Δfmax < 10 MHz. |

For repeater operating in Bands n1, n2, n3, n7, n24, n25, n30, n34, n38, n39, n40, n41, n48, n50, n54, n65, n66, n70, n74, n75, n77, n78, n79, n90, n92, n94, n109, basic limits are specified in table 6.5.3.2.1-2.

Table 6.5.3.2.1-2: Wide Area *operating band* unwanted emission basic limits (NR bands above 1 GHz) for Category A

|  |  |  |  |
| --- | --- | --- | --- |
| Frequency offset of measurement filter ‑3dB point, Δf | Frequency offset of measurement filter centre frequency, f\_offset | *Basic limit* (Notes 1, 2 | *Measurement bandwidth* |
| 0 MHz ≤ Δf < 5 MHz | 0.05 MHz ≤ f\_offset < 5.05 MHz |  | 100 kHz  |
| 5 MHz ≤ Δf <min(10 MHz, Δfmax) | 5.05 MHz ≤ f\_offset <min(10.05 MHz, f\_offsetmax) | -14 dBm | 100 kHz  |
| 10 MHz ≤ Δf ≤ Δfmax | 10.5 MHz ≤ f\_offset < f\_offsetmax  | -13 dBm (Note 3) | 1MHz  |
| NOTE 1: For a *repeater* supporting *non-contiguous spectrum* operation within any *operating band*, the emission basic limits within *gaps between passbands* is calculated as a cumulative sum of contributions from adjacent *sub-blocks* on each side of the *gap between passbands*, where the contribution from the far-end *sub-block* shall be scaled according to the *measurement bandwidth* of the near-end *sub-block*. Exception is f ≥ 10MHz from both adjacent *sub-blocks* on each side of the *gap between passbands*, where the emission basic limits within *gaps between passbands* shall be ‑13 dBm/1 MHz.NOTE 2: For a *multi-band connector* with *inter-passband gap* < 2\*ΔfOBUE the emission basic limits within the *inter-passband gaps* is calculated as a cumulative sum of contributions from adjacent *sub-blocks* or *passband* on each side of the *inter-passband gap*, where the contribution from the far-end *sub-block* or *passband* shall be scaled according to the *measurement bandwidth* of the near-end *sub-block* or *passband*.NOTE 3: The basic limit is not applicable when Δfmax < 10 MHz. |

##### 6.5.3.2.2 Basic limit for Wide Area *repeater type 1-C* (Category B)

For Category B Operating band unwanted emissions, there are two options for the *basic limits* that may be applied regionally. Either the *basic limits* in clause 6.5.3.2.2.1 or clause 6.5.3.2.2.2 shall be applied.

6.5.3.2.2.1 Category B basic limits (Option 1)

For *repeater type 1-C* operating in Bands n5, n8, n12, n20, n26, n28, n29, n31, n67, n71, n72, n85, n87, n88, the basic limits are specified in table 6.5.3.2.2.1-1:

Table 6.5.3.2.2.1-1: Wide Area operating band unwanted emission *basic limits* (NR bands below 1 GHz) for Category B

|  |  |  |  |
| --- | --- | --- | --- |
| Frequency offset of measurement filter ‑3dB point, Δf | Frequency offset of measurement filter centre frequency, f\_offset | *Basic limit* (Notes 1, 2) | *Measurement bandwidth* |
| 0 MHz ≤ Δf < 5 MHz | 0.05 MHz ≤ f\_offset < 5.05 MHz |  | 100 kHz  |
| 5 MHz ≤ Δf <min(10 MHz, Δfmax) | 5.05 MHz ≤ f\_offset <min(10.05 MHz, f\_offsetmax) | -14 dBm | 100 kHz  |
| 10 MHz ≤ Δf ≤ Δfmax | 10.05 MHz ≤ f\_offset < f\_offsetmax  | -16 dBm (Note 3) | 100 kHz  |
| NOTE 1: For a *repeater* supporting *non-contiguous spectrum* operation within any *operating band*, the emission basic limits within *gaps between passbands* is calculated as a cumulative sum of contributions from adjacent *sub-blocks* on each side of the *gap between passbands*. Exception is f ≥ 10MHz from both adjacent *sub-blocks* on each side of the *gap between passbands*, where the emission basic limits within *gaps between passbands* shall be ‑15 dBm/1 MHz.NOTE 2: For a *multi-band connector* with *inter-passband gap* < 2\*ΔfOBUE the emission basic limits within the *inter-passband gaps* is calculated as a cumulative sum of contributions from adjacent *sub-blocks* or *passband* on each side of the *inter-passband gap*.NOTE 3: The *basic limit* is not applicable when Δfmax < 10 MHz. |

For repeater operating in Bands n1, n2, n3, n7, n25, n34, n38, n39, n40, n41, n48, n50, n65, n66, n70, n75, n77, n78, n79, n90, n92, n94, n109 basic limits are specified in table 6.5.3.2.2.1-2.

Table 6.5.3.2.2.1-2: Wide Area *repeater type 1-C* operating band unwanted emission basic limits for Category B

|  |  |  |  |
| --- | --- | --- | --- |
| Frequency offset of measurement filter ‑3dB point, Δf | Frequency offset of measurement filter centre frequency, f\_offset | *Basic limits* (Notes 1, 2) | *Measurement bandwidth* |
| 0 MHz ≤ Δf < 5 MHz | 0.05 MHz ≤ f\_offset < 5.05 MHz |  | 100 kHz  |
| 5 MHz ≤ Δf <min(10 MHz, Δfmax) | 5.05 MHz ≤ f\_offset <min(10.05 MHz, f\_offsetmax) | -14 dBm | 100 kHz  |
| 10 MHz ≤ Δf ≤ Δfmax | 10.5 MHz ≤ f\_offset < f\_offsetmax  | -15 dBm (Note 3) | 1MHz  |
| NOTE 1: For a *repeater* supporting *non-contiguous spectrum* operation within any *operating band*, the emission basic limits within *gaps between passbands* is calculated as a cumulative sum of contributions from adjacent *sub-blocks* on each side of the *gap between passbands*, where the contribution from the far-end *sub-block* shall be scaled according to the *measurement bandwidth* of the near-end *sub-block*. Exception is f ≥ 10MHz from both adjacent *sub-blocks* on each side of the *gap between passbands*, where the emission basic limits within *gaps between passbands* shall be ‑15 dBm/1 MHz.NOTE 2: For a *multi-band connector* with *inter-passband gap* < 2\*ΔfOBUE the emission basic limits within the *inter-passband gaps* is calculated as a cumulative sum of contributions from adjacent *sub-blocks* or *passband* on each side of the *inter-passband gap*, where the contribution from the far-end *sub-block* or *passband* shall be scaled according to the *measurement bandwidth* of the near-end *sub-block* or *passband*.NOTE 3: The basic limit is not applicable when Δfmax < 10 MHz. |

For *repeater type 1-C* operating in Band n104, the *basic* limits are specified in tables 6.5.3.2.2.1-2a:

Table 6.5.3.2.2.1-2a: Wide Area operating band unwanted emission basic limits for band n104 for Category B

|  |  |  |  |
| --- | --- | --- | --- |
| Frequency offset of measurement filter ‑3dB point, Δf | Frequency offset of measurement filter centre frequency, f\_offset | Basic limits | Measurement bandwidth |
| 0 MHz ≤ Δf < 20 MHz | 0.05 MHz ≤ f\_offset < 20.05 MHz | $$−7dBm−\frac{7}{20}\left(\frac{f\_{offset}}{MHz}−0.05\right)$$ | 100 kHz  |
| 20 MHz ≤ Δf <min(40 MHz, Δfmax) | 20.05 MHz ≤ f\_offset <min(40.05 MHz, f\_offsetmax) | -14 dBm | 100 kHz  |
| 40 MHz ≤ Δf ≤ Δfmax | 40.5 MHz ≤ f\_offset < f\_offsetmax  | -15 dBm (Note 3) | 1MHz  |
| NOTE 1: For a *repeater* supporting *non-contiguous spectrum* operation within any *operating band*, the emission basic limits within *gaps between passbands* is calculated as a cumulative sum of contributions from adjacent *sub-blocks* on each side of the *gap between passband*, where the contribution from the far-end *sub-block* shall be scaled according to the *measurement bandwidth* of the near-end *sub-block*. Exception is f ≥ 40MHz from both adjacent *sub-blocks* on each side of the *gap between passband*, where the emission basic limits within *gaps between passbands* shall be ‑15 dBm/1 MHz.NOTE 2: For a *multi-band connector* with *inter-passband gap* < 2\*ΔfOBUE the emission basic limits within the *inter-passband gaps* is calculated as a cumulative sum of contributions from adjacent *sub-blocks* or *passband* on each side of the *inter-passband gap*, where the contribution from the far-end *sub-block* or *passband* shall be scaled according to the *measurement bandwidth* of the near-end *sub-block* or *passband*.NOTE 3: The *basic limit* is not applicable when Δfmax < 40 MHz. |

## << Next change >>

##### 6.5.4.2.2 Additional spurious emissions *basic limits*

These *basic limits* may be applied for the protection of system operating in other frequency ranges. The limits may apply as an optional protection of such systems that are deployed in the same geographical area as the repeater-Node, or they may be set by local or regional regulation as a mandatory requirement for an NR *operating band*. It is in some cases not stated in the present document whether a requirement is mandatory or under what exact circumstances that a limit applies, since this is set by local or regional regulation. An overview of regional requirements in the present document is given in clause 4.5.

Some requirements may apply for the protection of specific equipment (UE, MS and/or BS) or equipment operating in specific systems (GSM, CDMA, UTRA, E-UTRA, NR, etc.) as listed below.

The spurious emission *basic limits* are provided in table 6.5.4.2.2-1 where requirements for co-existence with the system listed in the first column apply for *repeater type 1-C*. For a *multi-band connector*, the exclusions and conditions in the Note column of table 6.5.4.2.2-1 apply for each supported *operating band*.

Table 6.5.4.2.2-1: *Repeater type 1-C* spurious emissions basic limits for co-existence with systems operating in other frequency bands

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| System type to co-exist with | Frequency range for co-existence requirement | *basic limits* | *Measurement bandwidth* | Note |
| GSM900 | 921 – 960 MHz | -57 dBm | 100 kHz | This basic limit does not apply to repeater operating in band n8 |
|  | 876 – 915 MHz | -61 dBm | 100 kHz | For the frequency range 880-915 MHz, this basic limit does not apply to repeater operating in band n8, since it is already covered by the basic limit in clause 6.5.5.2.2. |
| DCS1800 | 1805 – 1880 MHz | -47 dBm | 100 kHz | This basic limit does not apply to repeater operating in band n3.  |
|  | 1710 – 1785 MHz | -61 dBm | 100 kHz | This basic limit does not apply to repeater operating in band n3, since it is already covered by the basic limit in clause 6.5.5.2.2. |
| PCS1900 | 1930 – 1990 MHz | -47 dBm | 100 kHz | This basic limit does not apply to repeater operating in band n2, n25 or band n70.  |
|  | 1850 – 1910 MHz | -61 dBm | 100 kHz | This basic limit does not apply to repeater operating in band n2 or n25 since it is already covered by the basic limit in clause 6.6.5.2.2.  |
| GSM850 or  | 869 – 894 MHz | -57 dBm | 100 kHz | This basic limit does not apply to repeater operating in band n5 or n26.  |
| CDMA850 | 824 – 849 MHz | -61 dBm | 100 kHz | This basic limit does not apply to repeater operating in band n5 or n26, since it is already covered by the basic limit in clause 6.6.5.2.2. |
| UTRA FDD  | 2110 – 2170 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n1 or n65 |
| Band I or E-UTRA Band 1 or NR Band n1 | 1920 – 1980 MHz | -49 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n1 or n65, since it is already covered by the basic limit in clause 6.6.5.2.2. |
| UTRA FDD  | 1930 – 1990 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n2 or n70.  |
| Band II or E-UTRA Band 2 or NR Band n2 | 1850 – 1910 MHz | -49 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n2, since it is already covered by the basic limit in clause 6.6.5.2.2. |
| UTRA FDD  | 1805 – 1880 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n3. |
| Band III orE-UTRA Band 3 or NR Band n3 | 1710 – 1785 MHz | -49 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n3, since it is already covered by the basic limit in clause 6.6.5.2.2.  |
| UTRA FDD Band IV orE-UTRA Band 4 | 2110 – 2155 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n66 |
|  | 1710 – 1755 MHz | -49 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n66, since it is already covered by the basic limit in clause 6.6.5.2.2. |
| UTRA FDD Band V orE-UTRA Band 5 or NR Band n5 | 869 – 894 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n5 or n26.  |
|  | 824 – 849 MHz | -49 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n5 or n26, since it is already covered by the basic limit in clause 6.6.5.2.2. |
| UTRA FDD  | 860 – 890 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n18. |
| Band VI, XIX or | 815 – 830 MHz | -49 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n18, since it is already covered by the basic limit in clause 6.6.5.2.2. |
| E-UTRA Band 6, 18, 19 or NR Band n18 | 830 – 845 MHz | -49 dBm | 1 MHz |  |
| UTRA FDD Band VII orE-UTRA Band 7 or NR Band n7 | 2620 – 2690 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n7. |
|  | 2500 – 2570 MHz | -49 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n7, since it is already covered by the basic limit in clause 6.6.5.2.2. |
| UTRA FDD Band VIII orE-UTRA Band 8 or NR Band n8 | 925 – 960 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n8. |
|  | 880 – 915 MHz | -49 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n8, since it is already covered by the basic limit in clause 6.6.5.2.2. |
| UTRA FDD Band IX orE-UTRA Band 9 | 1844.9 – 1879.9 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n3. |
|  | 1749.9 – 1784.9 MHz | -49 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n3, since it is already covered by the basic limit in clause 6.6.5.2.2. |
| UTRA FDD Band X orE-UTRA Band 10 | 2110 – 2170 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n66 |
|  | 1710 – 1770 MHz | -49 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n66, since it is already covered by the basic limit in clause 6.6.5.2.2. |
| UTRA FDD Band XI or XXI orE-UTRA Band 11 or 21 | 1475.9 – 1510.9 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n50, n74, n75, n92, n94 or n109. |
|  | 1427.9 – 1447.9 MHz | -49 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n50, n51, n74, n75, n76, n91, n92, n93, n94 or n109. |
|  | 1447.9 – 1462.9 MHz | -49 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n50, n74, n75, n92, n94 or n109. |
| UTRA FDD Band XII orE-UTRA Band 12 or NR Band n12 | 729 – 746 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n12 or n85. |
|  | 699 – 716 MHz | -49 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n12 or n85, since it is already covered by the basic limit in clause 6.6.5.2.2.For NR repeater operating in n29, it applies 1 MHz below the Band n29 downlink operating band (Note 5). |
| UTRA FDD Band XIII orE-UTRA Band 13 | 746 – 756 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n13. |
|  | 777 – 787 MHz | -49 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n13, since it is already covered by the basic limit in clause 6.6.5.2.2. |
| UTRA FDD Band XIV orE-UTRA Band 14 or NR band n14 | 758 – 768 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n14. |
|  | 788 – 798 MHz | -49 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n14, since it is already covered by the basic limit in clause 6.6.5.2.2. |
|  E-UTRA Band 17 | 734 – 746 MHz | -52 dBm | 1 MHz |  |
|  | 704 – 716 MHz | -49 dBm | 1 MHz | For NR repeater operating in n29, it applies 1 MHz below the Band n29 downlink operating band (Note 5). |
| UTRA FDD Band XX or E-UTRA Band 20 or NR Band n20 | 791 – 821 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n20 or n28. |
|  | 832 – 862 MHz | -49 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n20, since it is already covered by the basic limit in clause 6.6.5.2.2. |
| UTRA FDD Band XXII or E-UTRA Band 22 | 3510 – 3590 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n48, n77 or n78. |
|  | 3410 – 3490 MHz | -49 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n77 or n78. |
| E-UTRA Band 24 | 1525 – 1559 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n24. |
|  | 1626.5 – 1660.5 MHz | -49 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n24, since it is already covered by the basic limit in clause 6.6.5.2.2. |
| UTRA FDD Band XXV orE-UTRA Band 25 or NR band n25 | 1930 – 1995 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n2, n25 or n70. |
|  | 1850 – 1915 MHz | -49 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n25 since it is already covered by the basic limit in clause 6.6.5.2.2. For repeater operating in Band n2, it applies for 1910 MHz to 1915 MHz, while the rest is covered in clause 6.6.5.2.2. |
| UTRA FDD Band XXVI orE-UTRA Band 26 or NR Band n26 | 859 – 894 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n5 or n26.  |
|  | 814 – 849 MHz | -49 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n26 since it is already covered by the basic limit in clause 6.6.5.2.2. For repeater operating in Band n5, it applies for 814 MHz to 824 MHz, while the rest is covered in clause 6.6.5.2.2. |
| E-UTRA Band 27 | 852 – 869 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in Band n5. |
|  | 807 – 824 MHz | -49 dBm | 1 MHz | This basic limit also applies to repeater operating in Band n28, starting 4 MHz above the Band n28 downlink operating band (Note 5). |
| E-UTRA Band 28 or NR Band n28 | 758 – 803 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n20, n67 or n28. |
|  | 703 – 748 MHz | -49 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n28, since it is already covered by the basic limit in clause 6.6.5.2.2.For repeater operating in band n67, it applies for 703 MHz to 736 MHz. |
| E-UTRA Band 29 or NR Band n29 | 717 – 728 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in Band n29 or n85 |
| E-UTRA Band 30 or NR Band n30 | 2350 – 2360 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n30 |
|  | 2305 – 2315 MHz | -49 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n30, since it is already covered by the basic limit in clause 6.6.5.2.2. |
| E-UTRA Band 31 or NR Band n31 | 462.5 – 467.5 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n31 or n72. |
|  | 452.5 – 457.5 MHz | -49 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n31, since it is already covered by the basic limit in clause 6.6.5.2.2. This basic limit does not apply to repeater operating in band n72. |
| UTRA FDD band XXXII or E-UTRA band 32 | 1452 – 1496 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n50, n74, n75, n92, n94 or n109. |
| UTRA TDD Band a) or E-UTRA Band 33 | 1900 – 1920 MHz | -52 dBm | 1 MHz |  |
| UTRA TDD Band a) or E-UTRA Band 34 or NR band n34 | 2010 – 2025 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in Band n34. |
| UTRA TDD Band b) or E-UTRA Band 35 | 1850 – 1910 MHz | -52 dBm | 1 MHz |  |
| UTRA TDD Band b) or E-UTRA Band 36 | 1930 – 1990 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in Band n2 or n25. |
| UTRA TDD Band c) or E-UTRA Band 37 | 1910 – 1930 MHz | -52 dBm | 1 MHz |  |
| UTRA TDD Band d) or E-UTRA Band 38 or NR Band n38 | 2570 – 2620 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in Band n38.  |
| UTRA TDD Band f) or E-UTRA Band 39 or NR band n39 | 1880 – 1920MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in Band n39. |
| UTRA TDD Band e) or E-UTRA Band 40 or NR Band n40 | 2300 – 2400MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in Band n30 or n40. |
| E-UTRA Band 41 or NR Band n41, n90 | 2496 – 2690 MHz | -52 dBm | 1 MHz | This is not applicable to repeater operating in Band n41, n53 or [n90]. |
| E-UTRA Band 42 | 3400 – 3600 MHz | -52 dBm | 1 MHz | This is not applicable to repeater operating in Band n48, n77 or n78. |
| E-UTRA Band 43 | 3600 – 3800 MHz | -52 dBm | 1 MHz | This is not applicable to repeater operating in Band n48, n77 or n78. |
| E-UTRA Band 44 | 703 – 803 MHz | -52 dBm | 1 MHz | This is not applicable to repeater operating in Band n28. |
| E-UTRA Band 45 | 1447 – 1467 MHz | -52 dBm | 1 MHz |  |
| E-UTRA Band 46 | 5150 – 5925 MHz | -52 dBm | 1 MHz |  |
| E-UTRA Band 47 | 5855 – 5925 MHz | -52 dBm | 1 MHz |  |
| E-UTRA Band 48 or NR Band n48 | 3550 – 3700 MHz | -52 dBm | 1 MHz | This is not applicable to repeater operating in Band n48, n77 or n78. |
| E-UTRA Band 50 or NR band n50  | 1432 – 1517 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in Band n50, n51, n74, n75, n76, n91, n92, n93, n94 or n109. |
| E-UTRA Band 51 or NR Band n51 | 1427 – 1432 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in Band n50, n51, n75, n76, n91, n92, n93, n94 or n109. |
| E-UTRA Band 53 or NR Band n53 | 2483.5 - 2495 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in Band n41, n53 or n90. |
| E-UTRA Band 54 or NR Band n54 | 1670 – 1675 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in Band n54 |
| E-UTRA Band 65 or NR Band n65 | 2110 – 2200 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n1 or n65.  |
|  | 1920 – 2010 MHz | -49 dBm | 1 MHz | For repeater operating in Band n1, it applies for 1980 MHz to 2010 MHz, while the rest is covered in clause 6.6.5.2.2. This basic limit does not apply to repeater operating in band n65, since it is already covered by the basic limit in clause 6.6.5.2.2. |
| E-UTRA Band 66 or NR Band n66 | 2110 – 2200 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n66. |
|  | 1710 – 1780 MHz | -49 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n66, since it is already covered by the basic limit in clause 6.6.5.2.2. |
| E-UTRA Band 67 | 738 – 758 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in Band n28 or n67. |
| E-UTRA Band 68 | 753 -783 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n28. |
|  | 698-728 MHz | -49 dBm | 1 MHz | For repeater operating in Band n28, this basic limit applies between 698 MHz and 703 MHz, while the rest is covered in clause 6.6.5.2.2. |
| E-UTRA Band 69 | 2570 – 2620 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in Band n38. |
| E-UTRA Band 70 or NR Band n70 | 1995 – 2020 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n2, n25 or n70 |
|  | 1695 – 1710 MHz | -49 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n70, since it is already covered by the basic limit in clause 6.6.5.2.2. |
| E-UTRA Band 71 or NR Band n71 | 617 – 652 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n71 or n105 |
|  | 663 – 698 MHz | -49 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n71 or n105, since it is already covered by the basic limit in clause 6.6.5.2.2. |
| E-UTRA Band 72 or NR Band n72 | 461 – 466 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n31 or n72. |
|  | 451 – 456 MHz | -49 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n72, since it is already covered by the basic limit in clause 6.6.5.2.2. This basic limit does not apply to BS operating in band n31. |
| E-UTRA Band 74 or NR Band n74 | 1475 – 1518 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n50, n74, n75, n92, n94 or n109. |
|  | 1427 – 1470 MHz | -49 dBm | 1MHz | This basic limit does not apply to repeater operating in band n50, n51, n74, n75, n76, n91, n92, n93, n94 or n109. |
| E-UTRA Band 75 or NR Band n75 | 1432 – 1517 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in Band n50, n51, n74, n75, n76, n91, n92, n93, n94 or n109. |
| E-UTRA Band 76 or NR Band n76 | 1427 – 1432 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in Band n50, n51, n75, n76, n91, n92, n93, n94 or n109. |
| NR Band n77 | 3.3 – 4.2 GHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in Band n48, n77 or n78 |
| NR Band n78 | 3.3 – 3.8 GHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in Band n48, n77 or n78 |
| NR Band n79 | 4.4 – 5.0 GHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in Band n79 |
| NR Band n80 | 1710 – 1785 MHz | -49 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n3, since it is already covered by the basic limit in clause 6.6.5.2.2. |
| NR Band n81 | 880 – 915 MHz | -49 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n8, since it is already covered by the basic limit in clause 6.6.5.2.2. |
| NR Band n82 | 832 – 862 MHz | -49 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n20, since it is already covered by the basic limit in clause 6.6.5.2.2. |
| NR Band n83 | 703 – 748 MHz | -49 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n28, since it is already covered by the basic limit in clause 6.6.5.2.2.For repeater operating in Band n67, it applies for 703 MHz to 736 MHz. |
| NR Band n84 | 1920 – 1980 MHz | -49 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n1, since it is already covered by the basic limit in clause 6.6.5.2.2. |
| E-UTRA Band 85 and NR Band n85 | 728 – 746 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n12 or n85.For NR repeater operating in n29, it applies 1 MHz below the Band n29 downlink operating band (Note 5). |
|  | 698 – 716 MHz | -49 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n12 or n85, since it is already covered by the basic limit in clause 6.6.5.2.2. |
| NR Band n86 | 1710 – 1780 MHz | -49 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n66, since it is already covered by the basic limit in clause 6.6.5.2.2. |
| E-UTRA Band 87 and NR Band n87 | 420 - 425 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n87 or n88. |
| 410 - 415 MHz | -49 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n87, since it is already covered by the basic limit in clause 6.6.5.2.2. |
| E-UTRA Band 88 and NR Band n88 | 422 - 427 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n87 or n88. |
| 412 - 417 MHz | -49 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n88, since it is already covered by the basic limit in clause 6.6.5.2.2. This basic limit does not apply to repeater operating in band n87. |
| NR Band n89 | 824 – 849 MHz | -49 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n5, since it is already covered by the basic limit in clause 6.6.5.2.2. |
| NR Band n91 | 1427 – 1432 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in Band n50, n51, n75, n76 or n109. |
|  | 832 – 862 MHz | -49 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n20, since it is already covered by the basic limit in clause 6.6.5.5.1.2. |
| NR Band n92 | 1432 – 1517 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in Band n50, n51, n74, n75, n76 or n109. |
|  | 832 – 862 MHz | -49 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n20, since it is already covered by the basic limit in clause 6.6.5.5.1.2. |
| NR Band n93 | 1427 – 1432 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in Band n50, n51, n75, n76 or n109. |
|  | 880 – 915 MHz | -49 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n8, since it is already covered by the basic limit in clause 6.6.5.5.1.2. |
| NR Band n94 | 1432 – 1517 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in Band n50, n51, n74, n75, n76 or n109. |
|  | 880 – 915 MHz | -49 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n8, since it is already covered by the basic limit in clause 6.6.5.5.1.2. |
| NR Band n95 | 2010 – 2025 MHz | -52 dBm | 1 MHz |  |
| NR Band n96 | 5925 – 7125 MHz | -52 dBm | 1 MHz |  |
| NR Band n97 | 2300 – 2400MHz | -52 dBm | 1 MHz |  |
| NR Band n98 | 1880 – 1920MHz | -52 dBm | 1 MHz |  |
| NR Band n99 | 1626.5 – 1660.5 MHz | -49 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n24, since it is already covered by the basic limit in clause 6.5.5.2.2. |
| NR band n101 | 1900 – 1910 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in Band n101. |
| NR Band n102 | 5925 – 6425 MHz | -52 dBm | 1 MHz |  |
| E-UTRA Band 103 | 757 – 758 MHz | -52 dBm | 1 MHz |  |
|  | 787 – 788 MHz | -49 dBm | 1 MHz |  |
| NR Band n104 | 6425 – 7125 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in Band n104 |
| NR band n105 | 612 – 652 MHz | -52 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n71 or n105 |
|  | 663 – 703 MHz | -49 dBm | 1 MHz | This basic limit does not apply to repeater operating in band n105, since it is already covered by the basic limit in clause 6.6.5.2.2. |
| E-UTRA Band 106 | 935 - 940 MHz | -52 dBm | 1 MHz |  |
|  | 896 – 901 MHz | -49 dBm | 1 MHz |  |
| NR band n109 | 1432 – 1517 MHz | -52 dBm | 1 MHz | This basic limit does not apply to BS operating in Band n50, n51, n74, n75, n76, n91, n92, n93, n94 or n109 |
|  | 703 – 733 MHz | -49 dBm | 1 MHz | This basic limit does not apply to BS operating in band n109, since it is already covered by the basic limit in clause 6.6.6.5.2.4. |

NOTE 1: As defined in the scope for spurious emissions in this clause, except for the cases where the noted basic limits apply to a repeater operating in Band n28, the co-existence requirements in table 6.5.4.2.3 -1 do not apply for the ΔfOBUE frequency range immediately outside the downlink *operating band* (see table 5.2-1). Emission limits for this excluded frequency range may be covered by local or regional requirements.

NOTE 2: Table 6.5.5.2.3 -1 assumes that two *operating bands*, where the frequency ranges in table 5.2-1 would be overlapping, are not deployed in the same geographical area. For such a case of operation with overlapping frequency arrangements in the same geographical area, special co-existence requirements may apply that are not covered by the 3GPP specifications.

NOTE 3: For unsynchronized operation, special co-existence requirements may apply that are not covered by the 3GPP specifications.

NOTE 4: For NR Band n28 repeater, specific solutions may be required to fulfil the spurious emissions limits for repeater for co-existence with E-UTRA Band 27 UL *operating band*.

NOTE 5: For NR Band n29 repeater, specific solutions may be required to fulfil the spurious emissions limits for NR repeater for co-existence with UTRA Band XII, E-UTRA Band 12 or NR Band n12 UL operating band, E-UTRA Band 17 UL operating band or E-UTRA Band 85 UL or NR Band n85 UL operating band.

The following requirement may be applied for the protection of PHS. This requirement is also applicable at specified frequencies falling between ΔfOBUE below the lowest repeater transmitter frequency of the downlink *operating band* and ΔfOBUE above the highest repeater transmitter frequency of the downlink *operating band*. ΔfOBUE is defined in clause 6.5.1.

The spurious emission *basic limit* for this requirement are:

Table 6.5.4.2.3-2: Repeater spurious emissions basic limit for repeater for co-existence with PHS for DL

|  |  |  |  |
| --- | --- | --- | --- |
| Frequency range | *basic limit* | *Measurement Bandwidth* | Note |
| 1884.5 – 1915.7 MHz | -41 dBm | 300 kHz | Applicable when co-existence with PHS system operating in 1884.5 – 1915.7 MHz  |

In certain regions, the following requirement may apply to NR repeater operating in Band n50 and n75 within the 1432 – 1452 MHz, and in Band n51 and Band n76. The *basic limit are* specified in Table 6.5.4.2.3-4. This requirement is also applicable at the frequency range from ΔfOBUE below the lowest frequency of the repeater downlink *operating band* up to ΔfOBUE above the highest frequency of the repeater downlink *operating band*.

Table 6.5.4.2.3-4: Additional operating band unwanted emission basic limit for NR repeater operating in Band n50 and n75 within 1432 – 1452 MHz, and in Band n51 and n76

|  |  |  |
| --- | --- | --- |
| Filter centre frequency, Ffilter | *basic limit* | *Measurement Bandwidth* |
| Ffilter = 1413.5 MHz | -42 dBm | 27 MHz |

In certain regions, the following requirement may apply to repeater operating in NR Band n50 and n75 within 1492-1517 MHz and in Band n74 within 1492-1518 MHz. The maximum level of emissions, measured on centre frequencies Ffilter with filter bandwidth according to Table 6.5.4.2.3-5, shall be defined according to the *basic limits* PEM,n50/n75,a nor PEM,n50/n75,b declared by the manufacturer.

Table 6.5.4.2.3-5: *Operating band* n50, n74 and n75 declared emission above 1518 MHz

|  |  |  |
| --- | --- | --- |
| Filter centre frequency, Ffilter | Declared *basic limits* (dBm) | *Measurement bandwidth* |
| 1518.5 MHz ≤ Ffilter ≤ 1519.5 MHz | PEM, n50/n75,a | 1 MHz |
| 1520.5 MHz ≤ Ffilter ≤ 1558.5 MHz | PEM,n50/n75,b | 1 MHz |

In certain regions, the following requirement shall be applied to repeater operating in Band n13 and n14 to ensure that appropriate interference protection is provided to 700 MHz public safety operations. This requirement is also applicable at the frequency range from 10 MHz below the lowest frequency of the repeater downlink operating band up to 10 MHz above the highest frequency of the repeater downlink operating band.

The power of any spurious emission shall not exceed:

Table 6.5.4.2.3-6: Repeater spurious emissions basic limits for protection of 700 MHz public safety operations

|  |  |  |  |
| --- | --- | --- | --- |
| Operating Band | Frequency range | *Basic limit* | *Measurement Bandwidth* |
| n13 | 763 - 775 MHz | -46 dBm | 6.25 kHz |
| n13 | 793 - 805 MHz | -46 dBm | 6.25 kHz |
| n14 | 769 - 775 MHz | -46 dBm | 6.25 kHz |
| n14 | 799 - 805 MHz | -46 dBm | 6.25 kHz |

In certain regions, the following requirement may apply to NR repeater operating in Band n30. This requirement is also applicable at the frequency range from 10 MHz below the lowest frequency of the repeater downlink operating band up to 10 MHz above the highest frequency of the repeater downlink operating band.

The power of any spurious emission shall not exceed:

Table 6.5.4.2.3-7: Additional NR repeater spurious emissions basic limits for Band n30

|  |  |  |  |
| --- | --- | --- | --- |
| Frequency range | *basic limits* | *Measurement Bandwidth* | Note |
| 2200 – 2345 MHz | -45 dBm | 1 MHz |  |
| 2362.5 – 2365 MHz | -25 dBm | 1 MHz |  |
| 2365 – 2367.5 MHz | -40 dBm | 1 MHz |  |
| 2367.5 – 2370 MHz | -42 dBm | 1 MHz |  |
| 2370 – 2395 MHz | -45 dBm | 1 MHz |  |

The following requirement may apply to repeater operating in Band n48 in certain regions. The power of any spurious emission shall not exceed:

Table 6.5.4.2.3-8: Additional repeater spurious emissions basic limits for Band n48

|  |  |  |  |
| --- | --- | --- | --- |
| Frequency range | *Basic limits* | *Measurement Bandwidth* (NOTE) | Note |
| 3530 MHz – 3720 MHz | -25 dBm | 1 MHz | Applicable 10 MHz from the assigned *passband edge*  |
| 3100 MHz – 3530 MHz3720 MHz – 4200 MHz | -40 dBm | 1 MHz |  |

NOTE: The resolution bandwidth of the measuring equipment should be equal to the measurement bandwidth. However, to improve measurement accuracy, sensitivity and efficiency, the resolution bandwidth may be smaller than the measurement bandwidth. When the resolution bandwidth is smaller than the measurement bandwidth, the result should be integrated over the measurement bandwidth in order to obtain the equivalent noise bandwidth of the measurement bandwidth.

NOTE: The regional requirement, included in [12], is defined in terms of EIRP, which is dependent on both the repeater emissions at the *antenna connector* and the deployment (including antenna gain and feeder loss). The requirement defined above provides the characteristics of the base station needed to verify compliance with the regional requirement. The assessment of the EIRP level is described in Annex F.

The following requirement shall be applied to repeater operating in Band n26 to ensure that appropriate interference protection is provided to 800 MHz public safety operations. This requirement is also applicable at the frequency range from 10 MHz below the lowest frequency of the repeater downlink operating band up to 10 MHz above the highest frequency of the repeater downlink operating band.

The power of any spurious emission shall not exceed:

Table 6.5.4.2.3-9: Repeater spurious emissions basic limits for protection of 800 MHz public safety operations

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Operating Band | Frequency range | *Basic limit* | Measurement Bandwidth | Note |
| n26 | 851 - 859 MHz | -13 dBm | 100 kHz | Applicable for offsets > 37.5kHz from the *passband* edge |

The following requirement may apply to Repeater for Band n41 and n90 operation in Japan. This requirement is also applicable at the frequency range from ΔfOBUE below the lowest frequency of the Repeater downlink operating band up to ΔfOBUE above the highest frequency of the Repeater downlink operating band.

The power of any spurious emission shall not exceed:

Table 6.5.4.2.3-10: Additional repeater spurious emissions basic limit for Band n41 and n90

|  |  |  |
| --- | --- | --- |
| Frequency range | *Basic limit* | *Measurement Bandwidth* |
| 2505 MHz – 2535 MHz | -42 dBm | 1 MHz |
| NOTE: This requirement applies for carriers allocated within 2545-2645 MHz. |

The following requirement may apply to repeater operating in 3.45-3.55 GHz in Band n77 in certain regions. Basic limits are specified in table 6.5.4.2.3-11.

Table 6.5.4.2.3-11: Additional repeater spurious emissions basic limits for Band n77

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Channel bandwidth [MHz] | Frequency range [MHz] | Filter centre frequency, Ffilter [MHz] | *Basic limit* [dBm] | *Measurement bandwidth* [MHz] |
| All | 3430 – 34403560 – 3570 | 3430.5 ≤ Ffilter < 3439.53560.5 ≤ Ffilter < 3569.5 | -25 | 1 |
| All | ≤ 3430> 3570 | Ffilter < 3429.53570.5 ≤ Ffilter | -40 | 1 |

NOTE: The resolution bandwidth of the measuring equipment should be equal to the measurement bandwidth. However, to improve measurement accuracy, sensitivity and efficiency, the resolution bandwidth may be smaller than the measurement bandwidth. When the resolution bandwidth is smaller than the measurement bandwidth, the result should be integrated over the measurement bandwidth in order to obtain the equivalent noise bandwidth of the measurement bandwidth.

The following requirement may also apply to repeater operating in Band n54 in certain regions. The level of emissions in the 1541 – 1650 MHz band, measured in measurement bandwidth according to Table 6.5.4.2.3-12 shall not exceed the maximum emission levels PEM,n54,a, PEM,n54,b, PEM,n54,c, PEM,n54,d, PEM,n54,e and PEM,n54,f declared by the manufacturer.

Table 6.5.4.2.3-12: Declared Band n54 emissions basic limits for protection of the 1541-1650 MHz band

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Operating Band | Frequency range | Declared emission level (dBW) (Measurement bandwidth = 1 MHz) | Declared emission level (dBW) of discrete emissions of less than 700 Hz bandwidth(Measurement bandwidth = 1 kHz) | Declared emission level (dBW) of discrete emissions of less than 2 kHz bandwidth(Measurement bandwidth = 1 kHz) |
| n54 | 1541 - 1559 MHz  | PEM,n54,a |  | PEM,n54,f |
|  | 1559 - 1610 MHz | PEM,n54,b | PEM,n54,d |  |
|  | 1610 - 1650 MHz | PEM,n54,c | PEM,n54,e |  |

Note: The regional requirements specified in attachment to the FCC reference document, 0007135419 are defined in terms of EIRP (effective isotropic radiated power), which is dependent on both the repeater emissions at the antenna connector and the deployment (including antenna gain and feeder loss). The EIRP level is calculated using: PEIRP = PE + Gant where PE denotes the repeater unwanted emission level at the antenna connector, Gant equals the repeater antenna gain minus feeder loss. The requirement defined above provides the characteristics of the base station needed to verify compliance with the regional requirement.

##### 6.5.4.2.3 Co-location with base stations and repeater Nodes

These requirements may be applied for the protection of other BS, IAB-DU, IAB-MT and repeater receivers when GSM900, DCS1800, PCS1900, GSM850, CDMA850, UTRA FDD, UTRA TDD, E-UTRA, NR BS, IAB-DU, IAB-MT, or repeater are co-located.

The requirements assume a 30 dB coupling loss between transmitter and receiver and are based on co-location with same class.

The *basic limits* are in table 6.5.4.2.3-1. Requirements for co-location with a system listed in the first column apply, depending on the declared class. For a *multi-band connector*, the exclusions and conditions in the Note column of table 6.5.4.2.3-1 shall apply for each supported *operating band*.

Table 6.5.4.2.3-1: Spurious emissions minimum requirements for co-location with BS, IAB-Node or repeater-Node

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Type of co-located BS | Frequency range for | *Basic limits* | Measurement | Note |
|  | co-location requirement | WA repeater | MR repeater | LA repeater | bandwidth |  |
|  GSM900 | 876 – 915 MHz | -98 dBm | -91 dBm | -70 dBm | 100 kHz |  |
|  DCS1800 | 1710 – 1785 MHz | -98 dBm | -91 dBm | -80 dBm | 100 kHz |  |
|  PCS1900 | 1850 – 1910 MHz | -98 dBm | -91 dBm | -80 dBm | 100 kHz |  |
|  GSM850 or CDMA850 | 824 – 849 MHz | -98 dBm | -91 dBm | -70 dBm | 100 kHz |  |
| UTRA FDD Band I or E-UTRA Band 1 or NR Band n1 | 1920 – 1980 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band II or E-UTRA Band 2 or NR Band n2 | 1850 – 1910 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band III or E-UTRA Band 3 or NR Band n3 | 1710 – 1785 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band IV or E-UTRA Band 4 | 1710 – 1755 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band V or E-UTRA Band 5 or NR Band n5 | 824 – 849 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band VI, XIX or E-UTRA Band 6, 19 | 830 – 845 MHz  | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band VII or E-UTRA Band 7 or NR Band n7 | 2500 – 2570 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band VIII or E-UTRA Band 8 or NR Band n8 | 880 – 915 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band IX or E-UTRA Band 9 | 1749.9 – 1784.9 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band X or E-UTRA Band 10 | 1710 – 1770 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band XI or E-UTRA Band 11 | 1427.9 –1447.9 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to repeater operating in Band n50, n75, n91, n92, n93 or n94 |
| UTRA FDD Band XII orE-UTRA Band 12 or NR Band n12 | 699 – 716 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band XIII orE-UTRA Band 13 or NR Band n13 | 777 – 787 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band XIV orE-UTRA Band 14 or NR Band n14 | 788 – 798 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 17 | 704 – 716 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 18 or NR Band n18 | 815 – 830 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band XX or E-UTRA Band 20 or NR Band n20 | 832 – 862 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band XXI or E-UTRA Band 21 | 1447.9 – 1462.9 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to repeater operating in Band n50, n75, n92 or n94 |
| UTRA FDD Band XXII or E-UTRA Band 22 | 3410 – 3490 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to repeater operating in Band n48, n77 or n78 |
| E-UTRA Band 24 or NR Band n24 | 1626.5 – 1660.5 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band XXV orE-UTRA Band 25 or NR Band n25 | 1850 – 1915 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA FDD Band XXVI orE-UTRA Band 26 or NR Band n26 | 814 – 849 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 27 | 807 – 824 MHz  | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 28 or NR Band n28 | 703 – 748 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 30 or NR Band n30 | 2305 – 2315 MHz  | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 31 or NR Band n31 | 452.5 – 457.5 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA TDD Band a) or E-UTRA Band 33 | 1900 – 1920 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA TDD Band a) or E-UTRA Band 34 or NR band n34 | 2010 – 2025 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to repeater operating in Band n34 |
| UTRA TDD Band b) or E-UTRA Band 35 | 1850 – 1910 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA TDD Band b) or E-UTRA Band 36 | 1930 – 1990 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to repeater operating in Band n2 or band n25 |
| UTRA TDD Band c) or E-UTRA Band 37 | 1910 – 1930 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| UTRA TDD Band d) or E-UTRA Band 38 or NR Band n38 | 2570 – 2620 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to repeater operating in Band n38.  |
| UTRA TDD Band f) or E-UTRA Band 39 or NR band n39 | 1880 – 1920MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to repeater operating in Band n39 |
| UTRA TDD Band e) or E-UTRA Band 40 or NR Band n40 | 2300 – 2400MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to repeater operating in Band n30 or n40. |
| E-UTRA Band 41 or NR Band n41, n90 | 2496 – 2690 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to repeater operating in Band n41, n53 or [n90] |
| E-UTRA Band 42 | 3400 – 3600 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to repeater operating in Band n48, n77 or n78 |
| E-UTRA Band 43 | 3600 – 3800 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to repeater operating in Band n48, n77 or n78 |
| E-UTRA Band 44 | 703 – 803 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to repeater operating in Band n28 |
| E-UTRA Band 45 | 1447 – 1467 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 46 or NR Band n46 | 5150 – 5925 MHz | N/A | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 48 or NR Band n48 | 3550 – 3700 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to repeater operating in Band n48, n77 or n78 |
| E-UTRA Band 50 or NR Band n50  | 1432 – 1517 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to repeater operating in Band n51, n74, n75, n91, n92, n93 or n94 |
| E-UTRA Band 51 or NR Band n51 | 1427 – 1432 MHz | N/A | N/A | -88 dBm | 100 kHz | This is not applicable to repeater operating in Band n50, n74, n75, n76, n91, n92, n93 or n94 |
| E-UTRA Band 53 or NR Band n53 | 2483.5 – 2495 MHz | N/A | -91 dBm | -88 dBm | 100 kHz | This is not applicable to repeater operating in Band n41, n53 or n90 |
| E-UTRA Band 54 or NR Band n54 | 1670 – 1675 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to repeater operating in Band n54 |
| E-UTRA Band 65 or NR Band n65 | 1920 – 2010 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 66 or NR Band n66 | 1710 – 1780 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 68 | 698 – 728 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 70 or NR Band n70 | 1695 – 1710 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 71 or NR Band n71 | 663 – 698 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 72 or NR Band n72 | 451 – 456 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 74 or NR Band n74  | 1427 – 1470 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to repeater operating in Band n50, n51, n91, n92, n93 or n94 |
| NR Band n77 | 3.3 – 4.2 GHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to repeater operating in Band n48, n77 or n78 |
| NR Band n78 | 3.3 – 3.8 GHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz | This is not applicable to repeater operating in Band n48, n77 or n78 |
| NR Band n79 | 4.4 – 5.0 GHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n80 | 1710 – 1785 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n81 | 880 – 915 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n82 | 832 – 862 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n83 | 703 – 748 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n84 | 1920 – 1980 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 85 or NR Band n85 | 698 – 716 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n86 | 1710 – 1780 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 87 or NR Band n87 | 410 – 415 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 88 or NR Band n88 | 412 – 417 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n89 | 824 – 849 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n91 | 832 – 862 MHz | N/A | N/A | -88 dBm | 100 kHz |  |
| NR Band n92 | 832 – 862 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n93 | 880 – 915 MHz | N/A | N/A | -88 dBm | 100 kHz |  |
| NR Band n94 | 880 – 915 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n95 | 2010 – 2025 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n96 | 5925 – 7125 MHz | N/A | -90 dBm | -87 dBm | 100 kHz |  |
| NR Band n97 | 2300 – 2400MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n98 | 1880 – 1920MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n99 | 1626.5 – 1660.5 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n101 | 1900 – 1910 MHz | -96 dBm | NA | NA | 100 kHz |  |
| NR Band n102 | 5925 – 6425 MHz | N/A | -90 dBm | -87 dBm | 100 kHz |  |
| E-UTRA Band 103 | 787 – 788 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n104 | 6425 – 7125 MHz | -95 dBm | -90 dBm | -87 dBm | 100 kHz | This requirement does not apply to repeater operating in Band n104. |
| NR Band n105 | 663 – 703 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| E-UTRA Band 106 | 896 – 901 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |
| NR Band n109 | 703 – 733 MHz | -96 dBm | -91 dBm | -88 dBm | 100 kHz |  |

NOTE 1: As defined in the scope for spurious emissions in this clause, the co-location requirements in table 6.5.4.2.4-1 do not apply for the frequency range extending ΔfOBUE immediately outside the transmit frequency range. The current state-of-the-art technology does not allow a single generic solution for co-location with other system on adjacent frequencies for 30dB antenna to antenna minimum coupling loss. However, there are certain site-engineering solutions that can be used. These techniques are addressed in TR 25.942 [3].

NOTE 2: Table 6.5.4.2.3-1 assumes that two *operating bands*, where the corresponding transmit and receive frequency ranges in table 5.2-1 would be overlapping, are not deployed in the same geographical area. For such a case of operation with overlapping frequency arrangements in the same geographical area, special co-location requirements may apply that are not covered by the 3GPP specifications.

## << End of change >>