**3GPP TSG-SA5 Meeting #157 *S5-246235***

Hyderabad, India, 14 - 18 October 2024

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** |  | **rev** |  | **Current version:** |  |  |
|  |
| *For* [*HE**LP*](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Rel-19 CR 28.537 Clarification of external management data |
|  |  |
| ***Source to WG:*** | Nokia |
| ***Source to TSG:*** | SA5 |
|  |  |
| ***Work item code:*** | TEI19 |  | ***Date:*** | 2024-10-02 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-19 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19) Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | In clause 6.4.1 external management data is described as follows:*Management data which is specified by 3GPP (clause 6.1.1) can be enriched by additional data not specified by 3GPP. This so-called external management data can be produced by data sources of different nature (e.g. sensors) with different formats.*The current definition is misleading, since it excludes the existing vendor-specific measurements that are related to regular IOC and are reported as part of the PM MnS.In the ASN.1 definition (Annex G of TS 28.550) as well of in the GPB definition (Annex I of TS 28.550) of PM streaming, there is an attribute "vendorSpecificMeasResults" or " vendor\_specific\_meas\_results" in the DataContent message to allow to report vendor specific measurements.Furthermore, in XML trace report file format definition (TS 32.423), there are parameters introduced to indicate whether the reported measurements or messages are vendor specific or not. Additionally, in the Streaming Trace Format definition (TS 32.423), it is specified that the trace record header includes a field "vendorExtension" allowing to report vendor specific measurements and messages. |
|  |  |
| ***Summary of change:*** |  Clarify meaning of "external management data" |
|  |  |
| ***Consequences if not approved:*** | Vendor-specific measurements that are related to regular IOC and are reported as part of the PM MnS are considered as external management data. |
|  |  |
| ***Clauses affected:*** | 2, 6.4.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

|  |
| --- |
| **Begin of modifications** |

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 28.532: "Management and orchestration; Generic management services".

[3] 3GPP TS 28.533: " Management and orchestration; Architecture framework".

[4] 3GPP TS 28.552: "Management and orchestration; 5G performance measurements".

[5] 3GPP TS 28.554: "Management and orchestration; 5G end to end Key Performance Indicators (KPI)".

[6] 3GPP TS 32.422: "Telecommunication management; Subscriber and equipment trace; Trace control and configuration management".

[7] 3GPP TS 32.404: "Telecommunication management; Performance Management (PM); Performance measurements; Definitions and template".

|  |
| --- |
| **Next modification** |

## 6.4 Managing external management data

### 6.4.1 Description

Management data which is specified by 3GPP (clause 6.1.1) can be enriched by additional data not specified by 3GPP. This so-called external management data can be produced by data sources of different nature (e.g. sensors) with different formats.

Note that management data that is not defined by 3GPP but specified based on 3GPP defined management data definition templates and frameworks (such as the measurement definition template in TS 32.404 [7]) is not considered as external management data.

External management data can be used for example as additional input for network optimization and prediction.

The management system should be able to manage this kind of data. That means data consumers should be able to request external management data to be produced and reported. The management system should provide support for storing it.

The definition of external data sources and the data formats they use is out of scope of this specification.

The target is to define generic management mechanisms that can cope with any kind of external data sources and data formats.

|  |
| --- |
| **End of modifications** |