**3GPP TSG-RAN WG2 Meeting #127 R2-2407735**

**Maastricht, Netherlands, Aug 19 – 23, 2024**

**Agenda item:** 7.14.2

**Source:** ZTE Corporation

**Title:** Draft Report of [AT127][504][QoE] Release of QoE configurations (ZTE)

**Document for:**  Discussion and decision

# Introduction

This is to discuss the following offline discussion:

* [AT127][504][QoE] Release of QoE configurations (ZTE)

      Scope: Discuss whether/what changes are needed for release of QoE configurations as per R2-2406998 and/or R2-2407090

      Intended outcome: Report in R2-2407735 with the agreeable TPs

      Deadline: Report available for CB session on Thursday

# Discussion

## 2.1 Scenario 1: Mobility from NR to EUTRA

It is noted in [1] that UE could improperly maintained idle/inactive QoE configuration for below cases, and UE behavior in such scenario is unclear:

* Case 1 mentioned in [1]: UE reselects to EUTRA after during RRC connection reestablishment and establish connections to EUTRA
* Case 2 raised by Huawei online: UE is in NR RRC IDLE state and then the UE moves to LTE cell for connection establishment.

**Q1: Do you agree that UE shall release its stored NR QoE configuration for case 1 and case 2? If not, what’s the intended UE behavior in such cases?**

|  |  |
| --- | --- |
| Company | comments |
|  |  |
|  |  |
|  |  |
|  |  |

If agrees on Q1, then the following question would be how to address this behavior in specifications. Below gives some preliminary analysis from rapporteur on the possible options to capture the UE behavior.

* Option 1: Capture in subclause xxx in **LTE RRC specs** that UE release stored NR QoE configuration/reports, if any upon successful RRC connection establishment in EUTRA, and inform upper layers to release the corresponding QoE configuration
* Option 2: Capture in subclause 5.3.7.3 in NR RRC specs that if UE reselects EUTRA cell during cell reselection UE release all stored QoE configuration/reports, if any, and inform upper layers to release the corresponding QoE configuration
* Option x: Please provide other solutions if any.

|  |  |  |
| --- | --- | --- |
| Solutions | Advantages | Disadvantages |
| Solution 1 | Cover all cases. Avoid loss of QoE configuration. It is possible that UE fails to establish RRC connection in LTE, UE might returns to NR, and the maintained LTE configuration can still be used. | Asking LTE AS/APP layer to release NR configurations, CT1/SA4 might be impacted |
| Solution 2 | Only impact NR specs, no impact on CT1/SA4. | NR idle/inactive configuration/reports will be lost when UE fails to establish RRC connection in LTE, and returns back to NR. |

**Q2: Please provide your preference on proposed solutions, and comments if any.**

|  |  |  |
| --- | --- | --- |
| Company | Supported options | comments |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

TPs for each solutions are provided in below for review and discussion

* **TP1 for option 1:**

**5.3.3.4 Reception of the *RRCConnectionSetup* by the UE**

NOTE 1: Prior to this, lower layer signalling is used to allocate a C-RNTI. For further details see TS 36.321 [6];

The UE shall:

[...]

1> If the UE has any stored NR application layer measurement configuration:

2> release all NR application layer measurement configurations;

2> inform upper layers to clear all stored NR application layer measurement configurations;

2> discard the stored NR application layer measurement reports if any;

2> consider itself not to be configured to send NR application layer measurement reports;

* **TP2 for option 1:**

5.3.7.3 Actions following cell selection while T311 is running

Upon selecting a suitable NR cell, the UE shall:

[....]

Upon selecting an inter-RAT cell, the UE shall:

1> perform the actions upon going to RRC\_IDLE as specified in 5.3.11, with release cause 'RRC connection failure';

1> if the UE is configured with any application layer measurement configuration:

2> inform upper layers about the release of all application layer measurement configurations;

2> release all application layer measurement configurations including their fields in UE variables *VarAppLayerIdleConfig* and *VarAppLayerPLMN-ListConfig*;

2> discard any application layer measurement reports which were not yet fully submitted to lower layers for transmission;

2> consider itself not to be configured to send application layer measurement reports;

**Q3: Please provide comments on the TPs for the solutions supported, if any. If you suggest different solutions, please provide the corresponding TPs in below table.**

|  |  |  |
| --- | --- | --- |
| Company | Supported solutions | Comments to the corresponding TPs |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Q4a .If agree on option 1, do you agree that LS is needed to inform SA4/CT1? If yes, do you agree the LS in the annex 2 of R2-2406998?**

|  |  |  |
| --- | --- | --- |
| Company | Agree/Disagree | Comments  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## Scenario 2: Mobility from EUTRA to NR

|  |
| --- |
| **Agreements RAN2#124*** For HO from LTE/5GC to NR, UE should release all LTE QoE configurations and apply NR QoE configuration if received. How UE releases old QoE configurations can be handled in CR phase.
 |

Corrections provided in [2] [R2-2407090](file:///D%3A%5C%5C3GPP%5C%5CExtracts%5C%5CR2-2407090%20-%20Correction%20CR%20for%20LTE%20QoE%20measurements.docx%22%20%5Co%20%22D%3A3GPPExtractsR2-2407090%20-%20Correction%20CR%20for%20LTE%20QoE%20measurements.docx) intends to address above agreements.

---------------------------------------------- corrections from [R2-2407090](file:///D%3A%5C%5C3GPP%5C%5CExtracts%5C%5CR2-2407090%20-%20Correction%20CR%20for%20LTE%20QoE%20measurements.docx%22%20%5Co%20%22D%3A3GPPExtractsR2-2407090%20-%20Correction%20CR%20for%20LTE%20QoE%20measurements.docx)-------------------------------------------------------

1> else if the UE was connected to 5GC prior to the reception of the *MobilityFromEUTRACommand* and the *targetRAT-Type* in the received *MobilityFromEUTRACommand* is set to *nr*:

2> reset MAC;

2> stop all timers that are running except T325, T330;

2> release *ran-NotificationAreaInfo*, if stored;

2> release the AS security context including the KRRCenc key, the KRRCint, the KUPint key and the KUPenc key, if stored;

2> release all radio resources, including release of the RLC entity, the MAC configuration and the associated PDCP entity and SDAP entity for all established RBs;

NOTE 1: PDCP and SDAP configured by the source configurations RAT prior to the handover that are reconfigured and re-used by target RAT when delta signalling (i.e., during inter-RAT intra-system handover when *fullConfig* is not present) is used, are not released as part of this procedure.

2> if a *serviceType* is stored in the current UE configuration:

3> release the stored *serviceType*:

3> inform upper layers to clear the stored application layer measurement configuration;

3> discard received application layer measurement report information from upper layers;

3> consider itself not to be configured to send application layer measurement report;

---------------------------------------------- corrections from [R2-2407090](file:///D%3A%5C%5C3GPP%5C%5CExtracts%5C%5CR2-2407090%20-%20Correction%20CR%20for%20LTE%20QoE%20measurements.docx%22%20%5Co%20%22D%3A3GPPExtractsR2-2407090%20-%20Correction%20CR%20for%20LTE%20QoE%20measurements.docx)-------------------------------------------------------

During online discussion, companies commented that this requirement has already fulfilled with existing specs. Shown below is current mobility from EUTRA description in 36.331:

---------------------------------------------------------- From TS 36.331 ----------------------------------------------------------

### 5.3.12 UE actions upon leaving RRC\_CONNECTED or RRC\_INACTIVE

Upon leaving RRC\_CONNECTED or RRC\_INACTIVE, the UE shall:

[....]

1> release the stored *serviceType*, if any;

1> inform upper layers to clear the stored application layer measurement configuration;

1> discard received application layer measurement report information from upper layers, if any;

1> consider itself not to be configured to send application layer measurement report;

[...]

#### 5.4.3.4 Successful completion of the mobility from E-UTRA

Upon successfully completing the handover, the cell change order or enhanced 1xRTT CS fallback, the UE shall:

1> if the *targetRAT-Type* in the received *MobilityFromEUTRACommand* is set to *eutra* (intra-E-UTRA inter-system HO):

2> indicate to the upper layers associated to the source system the release of the RRC connection together with the release cause 'other';

2> the procedure ends;

1> else if the UE was connected to 5GC prior to the reception of the *MobilityFromEUTRACommand* and the *targetRAT-Type* in the received *MobilityFromEUTRACommand* is set to *nr*:

2> reset MAC;

2> stop all timers that are running except T325, T330;

2> release *ran-NotificationAreaInfo*, if stored;

2> release the AS security context including the KRRCenc key, the KRRCint, the KUPint key and the KUPenc key, if stored;

2> release all radio resources, including release of the RLC entity, the MAC configuration and the associated PDCP entity and SDAP entity for all established RBs;

NOTE 1: PDCP and SDAP configured by the source configurations RAT prior to the handover that are reconfigured and re-used by target RAT when delta signalling (i.e., during inter-RAT intra-system handover when *fullConfig* is not present) is used, are not released as part of this procedure.

1> else:

2> perform the actions upon leaving RRC\_CONNECTED as specified in 5.3.12, with release cause 'other';

NOTE 2: If the UE performs enhanced 1xRTT CS fallback along with concurrent mobility to CDMA2000 HRPD and the connection to either CDMA2000 1xRTT or CDMA2000 HRPD succeeds, then the mobility from E-UTRA is considered successful.

--------------------------------------------------------- From TS 36.331 -----------------------------------------------------------

According to above highlighted description in yellow, UE will perform leaving RRC\_CONNECTED for inter-system mobility from EUTRA to NR, while for intra-system mobility from EUTRA to NR there is no such requirement. And when performing leaving RRC\_CONNECTED UE will release stored LTE QoE configuration.

It can be concluded that when UE leaves from LTE-EPC to NR, current LTE specs already allows UE to release LTE QoE configuration, no specs update is needed. While for LTE-5GC to NR there is no such requirement specified. It is rapporteur’s understanding that the corrections proposed in [2] intends to address the missing scenarios from LTE-5GC to NR, which seems needed.

**Q5 .Do companies agree with above analysis that the corrections in [R2-2407090](file:///D%3A%5C%5C3GPP%5C%5CExtracts%5C%5CR2-2407090%20-%20Correction%20CR%20for%20LTE%20QoE%20measurements.docx%22%20%5Co%20%22D%3A3GPPExtractsR2-2407090%20-%20Correction%20CR%20for%20LTE%20QoE%20measurements.docx) is needed.**

|  |  |  |
| --- | --- | --- |
| Company | Agree/Disagree | Comments  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# Summary

Based on the input from companies, we have the following proposals:

TBD

# Reference

[1] [R2-2406998](file:///D%3A%5C%5C3GPP%5C%5CExtracts%5C%5CR2-2406998%20Consideration%20on%20QoE%20configuration%20release%20during%20inter-RAT%20mobility.docx%22%20%5Co%20%22D%3A3GPPExtractsR2-2406998%20Consideration%20on%20QoE%20configuration%20release%20during%20inter-RAT%20mobility.docx) Consideration on QoE configuration release during inter-RAT mobility ZTE Corporation, Sanechips discussion Rel-18 NR\_QoE\_enh-Core

[2] [R2-2407090](file:///D%3A%5C%5C3GPP%5C%5CExtracts%5C%5CR2-2407090%20-%20Correction%20CR%20for%20LTE%20QoE%20measurements.docx%22%20%5Co%20%22D%3A3GPPExtractsR2-2407090%20-%20Correction%20CR%20for%20LTE%20QoE%20measurements.docx) Release of QoE measurements at successful handover from LTE Ericsson, Nokia, Nokia Shanghai Bell CR Rel-18 36.331 18.2.0 5048 - F NR\_QoE\_enh-Core