**3GPP TSG- Meeting # *r02***

**, , -**

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** | **1126** | **rev** |  | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | General inference procedure for vertical federated learning  |
|  |  |
| ***Source to WG:*** | OPPO, ETRI, China Telecom, Tencent, ICS |
| ***Source to TSG:*** | SA2 |
|  |  |
| ***Work item code:*** |  |  | ***Date:*** |  |
|  |  |  |  |  |
| ***Category:*** |  |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19) Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | Based on the conclusion captured in the TR 23.700-84 clause 8.2 P#2.4, this CR aims for specify the general inference procedure for vertical federated learning. The NWDAF contain AnLF is the consumer to request the VFL inference result to the VFL server. And the NWDAF contain AnLF based on the VFL inference result generate the analytics output and send the analytics output to the analytics consumer. |
|  |  |
| ***Summary of change:*** | New clause 6.2X is added. The sub-clause 6.2X.1 and 6.2X.2 are added to specify the general inference procedure for vertical federated learning. |
|  |  |
| ***Consequences if not approved:*** | Can not perform VFL inference if do not specify the VFL inference procedure. |
|  |  |
| ***Clauses affected:*** | 6.2X (new), 6.2X.1 (new). 6.2X.2 (new) |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

\* \* \* \* First change (all new)\* \* \* \*

## 6.2X Vertical Federated Learning

### 6.2X.1 General

This clause specifies how NWDAF(s) and AF(s) can leverage Vertical Federated Learning technique to perform VFL inference.

### 6.2X.2 Procedures

6.2X.2.X General inference procedure for vertical federated learning between NWDAF(s) and AF(s)

Figure 6.2X.2.X-1: General inference procedure for vertical federated learning between NWDAF(s) and AF(s)

Editor’s Note: whether one general procedure or two separate procedures for NWDAF/AF as server will be discussed and decided in future meeting when the procedures are stable.

Editor's note: In case any of the Consumer, Server and clients are untrusted AF(s), how the NEF assists the VFL inference process, and whether the existing or new NEF service should be invoked are FFS.

0. Analytics consumer NF sends an Analytics request/subscribe (Analytics ID, Target of Analytics Reporting= UE IDs, Analytics Filter Information (e.g. Application ID, S-NSSAI, DNN, Application Server Address(es), Area of Interest, Analytics Reporting Information=Analytics target period)) to NWDAF containing AnLF by invoking a Nnwdaf\_AnalyticsInfo\_Request or a Nnwdaf\_AnalyticsSubscription\_Subscribe.

1. If the NWDAF is the VFL server, the consumer (i.e NWDAF containing AnLF) sends a subscription request to VFL server NWDAF using Nnwdaf\_AnalyticsSubscription\_Subscribe including Analytics ID, Target of Analytics Reporting = UE IDs, Analytics Filter Information (e.g. Application ID, S-NSSAI, DNN, Application Server Address(es), Area of Interest, Analytics Reporting Information=Analytics target period).

2. Based on the information received in the step 1, VFL server decides to iniate the VFL inference procedure with the VFL clients to generate more accurate analytics result. Before tha, the VFL server determines the VFL clients which participated in the VFL training process, based on the VFL model correlation ID and information provided by ADRF. The VFL server may not select all VFL clients, e.g. depending on their contribution to the training result.

If the VFL server is the NWDAF and the VFL client is the NWDAF, VFL server sends a Nnwdaf\_AnalyticsSubscription\_Subscribe to the VFL client NWDAF including the information received in the step 1 and the VFL model correlation ID to indicate the VFL client which previously well-trained VFL local model associated with this ID will be used.

If the VFL server is the NWDAF and the VFL client is the trusted AF, VFL server NWDAF sends a Naf\_EventExposure\_Subscribe to the VFL client AF including the information received in the step 1 and the VFL model correlation ID to indicate the VFL client which previously well-trained VFL local model associated with this ID will be used.

If the VFL server is the NWDAF and the VFL client is the untrusted AF, VFL server NWDAF sends a request to the VFL client AF using Nnef\_AnalyticsExposure\_Subscribe and Naf\_EventExposure\_Subscribe including the information received in the step 1 and the VFL model correlation ID to indicate the VFL client which previously well-trained VFL local model associated with this ID will be used.

3. Each VFL Client collects its local data by using the current mechanism if the VFL Client has not local data available already.

4. Based on the VFL correlation ID, each VFL Client determines the VFL local model to generate the intermediate local inference results.

5. Each VFL Client sends the intermediate local inference results and the VFL model correlation ID to the VFL server using the notify service operation corresponsing to the subscribe service operation used in the step 2. Optionally, one VFL client may send the local intermediate inference results to the other VFL client and let other VFL client send the aggregates local intermediate inference results to the VFL server.

Editor's note: Whether VFL client may also provide local intermediate inference results to other VFL client is FFS.

 The intermediate local inference results, which are sent from the VFL Client to the VFL Server during the VFL inference process, are the information for the VFL Server to aggregates and generates the VFL inference results.

6. The VFL Server aggregates all the intermediate local inference results to generate the global VFL inference results The VFL server takes into account when generating the global VFL inference result factors such as weight of the feature supported by each VFL client, local accuracy metric,

7. If the NWDAF is the VFL server, the VFL server sends Nnwdaf\_AnalyticsSubscription\_Notify to the consumer (i.e NWDAF containing AnLF) including the VFL inference results.

8. The NWDAF containing AnLF provides the analytics output to the analytics consumer NF based on the VFL inference results by means of either Nnwdaf\_AnalyticsInfo\_Request response or Nnwdaf\_AnalyticsSubscription\_Notify, depending on the service used in step 0.

\* \* \* \* End of changes \* \* \* \*