**3GPP SA WG2 Meeting #164 *S2-240xxxx***

**Maastricht, NL, 19-23 August 2024 *(was S2-240xxxx)***

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.3* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  |  | **CR** |  | **rev** |  | **Current version:** |  |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps | **x** | ME | **x** | Radio Access Network | **x** | Core Network | **x** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Adding support of Mobile Wireless Access Backhaul in 5GS | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Qualcomm Incorporated, Sony?, Huawei?, Ericsson?, Nokia, LG Electronics, ZTE? | | | | | | | | | |
| ***Source to TSG:*** | SA2 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | VMR\_Ph2 | | | | |  | ***Date:*** | | | 2024-08-19 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | B |  | | | | | ***Release:*** | | | Rel-19 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)  Rel-20 (Release 20)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | The approved VMR\_Ph2 work item (SP-240632) is set to specify the architecture enhancements, functionalities and procedures to support MWAB based on conclusions of TR 23.700-06 (clause 8).  This contribution added the general description of the MWAB feature and corresponding architecture enhancements in TS 23.501. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Add general description of the system architecture for MWAB support in new clause 5.x. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | No support of VMR\_Ph2 feature in Rel-19. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | (new) 5.x | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  |  | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  |  | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  |  | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

*FIRST CHANGE*

5.x Support for Mobile gNB with Wireless Access Backhauling (MWAB)

### 5.x.1 General

#### 5.x.1.1 Principles and functional entities

Mobile gNB with Wireless Access Backhauling (MWAB) allows a mobile device to provide an NR access link to UEs in proximity and connects wirelessly to the 5GC through an IP connectivity provided by a backhaul PDU session(s), as illustrated in figure 5.x.1.1-1. The MWAB consists of a gNB component (MWAB-gNB) and a UE component (MWAB-UE). The MWAB-gNB is based on the gNB functionality specified in TS 38.300 [27] and TS 38.401 [42]. The UE(s) served by the MWAB-gNB may or may not move together with the MWAB, e.g. the MWAB may be mounted on a moving vehicle and the UEs may located inside or outside the vehicle .

Both scenarios when MWAB-UE is non-roaming and MWAB-UE is roaming are supported. UEs served by MWAB may be non-roaming or roaming in the PLMN/SNPN advertised by the MWAB in system information which is also referred to as Broadcasted PLMN/SNPN.



Figure 5.x.1.1-1: Non-Roaming MWAB architecture for 5GS

NOTE 1: In this release, the CU/DU split of the MWAB-gNB is not supported.

NOTE 2: The interface between MWAB-UE and MWAB-gNB is not in scope of this specification.

MWAB operation supports both PLMN and SNPN cases. The specific architectures for supporting PLMN are provided in clause 5.x.1.2, and the architectures for supporting SNPN are provided in clause 5.x.1.3.

MWAB-UE has a single NR Uu hop to the backhaul (BH) NG-RAN, using either TN or NTN access technology. NR access is used for the radio link between a MWAB-gNB and the served UEs. The NR Uu access link between the MWAB-gNB and the served UE(s) does not use NTN access technology. 5G MOCN is supported by the MWAB-gNB.

The MWAB-UE can be authorized by the BH 5GC to operate as MWAB, and establishes the necessary BH PDU Session(s). The detailed procedures for the authorization of MWAB is described in clause 5.x.3.

The IP based BH PDU Session(s) of the MWAB-UE in the BH PLMN/SNPN are used for the MWAB-gNB's connection to the OAM server of the PLMN/SNPN serving the UE(s), and the N2, N3, and Xn interfaces. The BH PLMN/SNPN and the Broadcasted PLMN/SNPN can be same or different. Same or different PDU Sessions of the MWAB-UE can be used for carrying the above traffic.

NOTE 3: The use of multiple PDU Sessions for N2, N3, Xn, OAM access, follows the existing URSP logic as defined in TS 23.503 [45].

The MWAB is assumed to be configured with the address(es) of the OAM server of the Broadcasted PLMN/SNPN and obtains the corresponding configurations for the MWAB-gNB from thisOAM server. The details of the MWAB configuration/provisioning process are described in clause 5.x.2.

Service continuity for the UE(s) served by the MWAB-gNB is supported, when the MWAB moves and whether the UE(s) move or do not move together with the MWAB. The detailed procedures for the support of mobility are described in clause 5.x.5.

The MWAB-gNB shall be able to serve UE(s) without any MWAB-specific enhancements.. For certain operations, the MWAB may be configured to provide access to only certain UEs. Existing access control mechanisms, e.g. CAG control, can be used to manage the UE(s)'s access to the MWAB-gNB. The details of the access control of the UEs served by MWAB are described in clause 5.x.6.

The LCS framework as defined in TS 23.273 [87] is used for providing the location service to the UE(s) served by MWAB. Details on supporting the LCS over MWAB are described in clause 5.x.7.

Regulatory services (e.g. emergency services, priority services) can be supported by the MWAB, and the details are provided in clause 5.x.8.

#### 5.x.1.2 Architectures to support MWAB in PLMN case

Figure 5.x.1.2-1 presents an example architecture for the MWAB operation when no roaming was involved for the MWAB-UE. In this case, there may be two PLMNs involved, i.e. the BH PLMN that serves the MWAB-UE, and the Broadcasted PLMN that serves the UE connected to the MWAB. . In some cases, the BH PLMN and Broadcasted PLMN can be the same PLMN.

The MWAB-gNB logically belongs to Broadcasted PLMN and announces the PLMN IDs of Broadcasted PLMN. The MWAB-gNB establishes N2 and N3 connection with the UE AMF and UE UPF in Broadcasted PLMN via the PDU Session of the MWAB-UE established with BH PLMN.

The BH UPF in the BH PLMN serves the MWAB-UE and provides the connection via a N6 interface towards Broadcasted PLMN core network, to carry the N2 and N3 traffic from MWAB-gNB. The BH UPF also supports the access to the OAM server of the Broadcasted PLMN by the MWAB-gNB.

NOTE: Depending on deployment requirement, a security gateway may be required between the BH UPF and the Broadcasted PLMN network. In that case, the MWAB-gNB needs to connect to the security gateway based on pre-configured security credentials. The traffic between MWAB-gNB and the Broadcasted PLMN goes inside the security tunnel established via the security gateway.

UE connected to the MWAB-gNB can access the 5GS services offered by Broadcasted PLMN. No MWAB-specific enhancement to the UE is required. The UE connected to the MWAB-gNB is not aware of BH PLMN, and thus does not need any roaming agreement between its HPLMN and the BH PLMN.



Figure 5.x.1.2-1: Architecture for MWAB operation support - MWAB-UE not roaming

Figure 5.x.1.2-2 presents an example architecture for the MWAB operation when MWAB-UE is roaming with a Local Breakout PDU Session for its operation. In this case, there may be three PLMNs involved, i.e. the BH PLMN that serves the MWAB-UE, and the Broadcasted PLMN that serves the UE connected to the MWAB, and the HPLMN of the MWAB-UE. The use of the Local Breakout PDU Session by the MWAB-UE can be configured by its HPLMN, e.g. with some VPLMN specific URSP rules. In some cases, the BH PLMN and Broadcasted PLMN can be the same PLMN. The BH PLMN is also named Backhaul PLMN (BH PLMN).

The BH PLMN can access the MWAB-UE's HPLMN UDM for the subscription information. The rest of the operation is similar to that shown in figure 5.x.1.2-1.Broadcasted PLMN

the

Figure 5.x.1.2-2: Architecture for MWAB operation support - MWAB-UE roaming with Local Breakout

Figure 5.x.1.2-3 presents an example architecture for the MWAB operation when MWAB-UE is roaming with a Home Routed PDU Session for its operation. In this case, PDU session of the MWAB-UE is routed by the BH PLMN to the HPLMN of the MWAB. The rest of the operation is similar to that shown in figure 5.x.1.2-2. In some cases, the BH PLMN and Broadcasted PLMN can be the same PLMN. Broadcasted PLMNBH PLMNBH PLMN

****

**Figure 5.x.1.2-3: Architecture for MWAB operation support – MWAB-UE roaming with Home Routed**

In Figure 5.x.1.2-1, Figure 5.x.1.2-2 and Figure 5.x.1.2-3, if the UE served by the MWAB is roaming, there can be another PLMN (not shown in the figures), i.e. the HPLMN of the UE served by the MWAB, involved. The interaction of the HPLMN of the UE and Broadcasted PLMN follows that described in clause 4.2.4 for the roaming case. The UE served by the MWAB-gNB is not aware of BH PLMN, and thus does not need any roaming agreement between its HPLMN and the BH PLMN.

#### 5.x.1.3 Architectures to support MWAB in SNPN case

The MWAB operation also supports SNPN, and the corresponding architectures are presented in figure 5.x.1.3-1 and 5.x.1.3-2. The MWAB operation also supports mixed PLMN and SNPN operation, i.e. in the architecture presented in 5.x.1.3-1 and 5.x.1.3-2, the BH SNPN can be replaced by a BH PLMN.

Figure 5.x.1.3-1 presents an example architecture for the MWAB operation when the Broadcasted SNPN of the is the same as the subscribed SNPN of the MWAB-UE. In this case, there may be two SNPNs involved, a BH SNPN that serves the MWAB-UE, and the Broadcasted SNPN that serves the UE connected to the MWAB-gNB. The MWAB-gNB logically belongs to the Broadcasted SNPN and establishes N2 and N3 connection with the UE AMF and UE UPF via the PDU Session of the MWAB-UE established with the BH SNPN. MWAB-gNB announces SNPN ID of the Broadcasted SNPN.

****

**Figure 5.x.1.3-1: Architecture for MWAB operation support for SNPN – with MWAB-UE served by BH SNPN which is the subscribed SNPN**

Figure 5.x.1.3-2 presents an example architecture for the MWAB operation when the serving SNPN of the MWAB-UE is different from the subscribed SNPN of MWAB-UE. In this case, there may be two SNPNs involved, i.e. the BH SNPN that serves the MWAB-UE, and the Broadcasted SNPN that serves the UE connected to the MWAB-gNB. The MWAB-gNB logically belongs to Broadcasted SNPN and establishes N2 and N3 connection with the UE AMF and UE UPF via the PDU Session of the MWAB-UE established with BH SNPN. MWAB-gNB announces SNPN ID of the Broadcasted SNPN.

****

**Figure 5.x.1.3-2: Architecture for MWAB operation support for SNPN – with MWAB-UE served by a BH SNPN other than the subscribed SNPN**

#### 5.x.1.4 Support of QoS for MWAB operations

If QoS optimization of the N3 connection is required, the MWAB-gNB may be configured with the traffic mapping to DSCP values used in the Broadcasted PLMN/SNPN for TNL in N3 connections (as defined in TS38.414 [x]), and the mapping of DSCP values in the Broadcasted PLMN/SNPN to a 5QI in the BH PLMN

he DSCP values are used in the QoS Flow binding of the BH PDU Session used for N3 connection(s) using the designated 5QI, based on existing procedures.

#### 5.x.1.5 Support of network slicing for MWAB operations

Network slicing optimization of the N3 is possible only if more than one N3 BH PDU session can be established for a MWAB by using each a different S-NSSAI in the BH PLMN/SNPN. If so, the MWAB-gNB can be configured (e.g. by OAM) with the mapping of the S-NSSAIs used in the PLMN/SNPN serving the UE via the MWAB-gNB to the S-NSSAIs used for the N3 BH PDU sessions. The related N3 connections are then associated with the specific N3 BH PDU sessions by using this mapping information. When a UE context at MWAB is received and it includes an Allowed/ Partially Allowed NSSAI which includes a S-NSSAI that maps to a N3 BH S-NSSAI that has no N3 BH PDU session established yet, the MWAB UE is requested to establish the related N3 BH PDU session (which may also trigger registration with the related N3 BH S-NSSAI as per normal UE behaviour). Likewise, when no S-NSSAI mapping to a N3 BH PDU session S-NSSAI exists in any MWAB-gNB UE context, the MWAB-UE may be instructed by the MWAB gNB to release this N3 BH PDU session (the deregistration of this N3 BH PDU session S-NSSAI is then based on normal policies when a S-NSSAI is now associated with any PDU session at a UE).

*End of CHANGEs*