**3GPP SA WG2 Meeting #164** **S2-240xxxx**

**Maastricht, NL August 19-23, 2024**

**Source:** **Rapporteurs**

**Title:** **Show of hands question**

**Document for:** **Approval**

**Agenda Item:** **19.3**

**Work Item / Release:** **FS\_XRM Ph2 / Rel-19**

*Abstract of the contribution: This paper lists the SoH questions for FS\_XRM\_Ph2*

# Show of hands question

**KI#2:**

1. Should both Media over QUIC (MoQ) and Proxy-UDP-in HTTP/3 + QUIC-Aware Proxying be supported?
2. Should Media over QUIC (MoQ) and Proxy-UDP-in HTTP/3 + QUIC-Aware Proxying and UDP-Option based RoQ (RTP Over QUIC) be supported?

**KI#1:**

1. AL-FEC: Can content ratio information be provided to RAN (e.g. as assistance information) for intelligent discard when it is congested?
2. Can all the parameters PSDB, PSER, PSIHI be provided to the NG-RAN in order to activate PDU Set QoS?
3. Can a new indicator be sent from SMF to the RAN in order to activate PDU Set Information marking (when PDU Set QoS is not activated)?

**KI#5:**

1. Can data boosting be supported by providing “expedited transfer indication” in N6 metadata?
2. Can Time to next burst be provided to NG-RAN for optimize power savings support?