**3GPP SA WG2 Meeting #164** **S2-240xxxx**

**Maastricht, NL August 19-23, 2024**

**Source:** **Rapporteurs**

**Title:** **Show of hands question**

**Document for:** **Approval**

**Agenda Item:** **19.3**

**Work Item / Release:** **FS\_XRM Ph2 / Rel-19**

*Abstract of the contribution: This paper lists the SoH questions for FS\_XRM\_Ph2*

# Show of hands question

**KI#2:**

1. Should both Media over QUIC (MoQ) and Proxy-UDP-in HTTP/3 + QUIC-Aware Proxying be supported?

**Informal SoH on MonQ4**

**Yes: 11**

**1 objection (google)**

1. Should Media over QUIC (MoQ) and Proxy-UDP-in HTTP/3 + QUIC-Aware Proxying and UDP-Option based RoQ (RTP Over QUIC) be supported?

**Informal SoH on MonQ4**

**Yes: 4**

**3 objections (InterDigital, Nokia, Lenovo)**

**KI#1:**

1. AL-FEC:
	1. Can content ratio information be provided to RAN via CP (e.g. as assistance information) for intelligent discard when it is congested?

**Informal SoH on MonQ4**

Yes: 13

3 objections (Ericsson, MediaTek, Samsung)

* 1. Can related information be provided to RAN via UP (e.g. as assistance information) for intelligent discard when it is congested?

**Informal SoH on MonQ4**

Yes: 3

5 objections (Nokia, E///, MediaTek, Huawei, Tencent)

1. In case no PDU Set QoS parameters are provided by the AF but PDU Set Information marking is supported, can SMF use new indicator to indicate support for PDU Set information marking is supported?
2. In case no PDU Set QoS parameters are provided by the AF but PDU Set Information marking is supported, can SMF use presence of PSIHI (with false value) to indicate support for PDU Set information marking is supported?

**KI#5:**

1. Can data boosting be supported by providing “expedited transfer indication” in N6 metadata?
2. Can Time to next burst be provided to NG-RAN for optimize power savings support?