**3GPP TSG-CT WG1 Meeting #129-eC1-212131**

**Electronic meeting, 19-23 April 2021**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **23.122** | **CR** | **0685** | **rev** | **-** | **Current version:** | **17.2.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Clarify the UE behaviour when the the last running Tsor-cm timer expires | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | ZTE | | | | | | | | | |
| ***Source to TSG:*** | C1 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | eCPSOR\_CON | | | | |  | ***Date:*** | | | 2021-04-02 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) ... Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | 1. During CT1 #127bis emeeting, it is agreed to avoid deregistration when the last running Tsor-cm timer stops due to going to idle mode has been agreed. However, the case that the UE enters idle mode or 5GMM-CONNECTED mode with RRC inactive indication can not lead to Tsor-cm timer expiriation. Thus the case of expiration should be clarified.  2. It is agreed that the timer Tsor-cm stops when the associated PDU session is released or the associated service is stopped. Thus the last running Tsor-cm timer may stop when all of the associated PDU sessions are released or all of the associated service are stopped. Thus when the UE performs the de-registration procedure, there may be no PDU session. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | - Clarify the case of de-regeistration due to the last running Tsor-cm timer expiration.  - Consider the case when the UE performs the de-registration procedure, there may be no PDU session. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | The UE behavior is unclear when the last running Tsor-cm timer expires before the UE entering idle mode. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | C.4.2 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

\*\*\*\*\* First change \*\*\*\*\*

## C.4.2 Applying SOR-CMCI in the UE

During SOR procedure and while applying SOR-CMCI, the UE shall determine the time to release the PDU session(s) as follows:

- If the UE has a configured "user controlled list of services exempted from release due to SOR" and a matching criterion is found for a service included in the "user controlled list of services exempted from release due to SOR", the UE shall set the Tsor-cm timer associated to the service to infinity;

- If one or more SOR-CMCI rules are included in SOR-CMCI, where for each criterion:

a) DNN of the PDU session:

the UE shall check whether it has a PDU session with a DNN matching to the DNN included in SOR-CMCI, and if any, the UE shall set the associated timer Tsor-cm to the value included in the SOR-CMCI;

b) S-NSSAI of the PDU session:

the UE shall check whether it has a PDU session with a S-NSSAI matching the S-NSSAI included in SOR-CMCI, and if any, the UE shall set the associated timer Tsor-cm to the value included in the SOR-CMCI;

c) IMS registration related signalling:

the UE shall check whether IMS registration related signalling is ongoing as specified in 3GPP TS 24.501 [64], and if it is ongoing, the UE shall set the associated timer Tsor-cm to the value included in the SOR-CMCI;

d) MMTEL voice call:

the UE shall check whether MMTEL voice call is ongoing as specified in 3GPP TS 24.501 [64], and if it is ongoing, the UE shall set the associated timer Tsor-cm to the value included in the SOR-CMCI;

e) MMTEL video call:

the UE shall check whether MMTEL video call is ongoing as specified in 3GPP TS 24.501 [64], and if it is ongoing, the UE shall set the associated timer Tsor-cm to the value included in the SOR-CMCI;

f) MO SMS over NAS or MO SMSoIP:

the UE shall check whether MO SMS over NAS or MO SMSoIP services is ongoing as specified in TS 24.501 [64], and if it is ongoing, the UE shall set the associated timer Tsor-cm to the value included in the SOR-CMCI; or

g) match all:

the UE shall set the associated timer Tsor-cm to the value included in the SOR-CMCI;

- otherwise, the UE shall consider the timer value for Tsor-cm equal to zero.

The UE shall start all applicable Tsor-cm timers.

While one or more Tsor-cm timers are running, the UE shall check the newly established PDU session or service for a matching criterion in the SOR-CMCI:

- If the UE has a configured "user controlled list of services exempted from release due to SOR" and a matching criterion is found for a service included in the "user controlled list of services exempted from release due to SOR", the UE shall set the Tsor-cm timer associated to the service to infinity;

- If a matching criterion is found and the applicable Tsor-cm timer indicated the value "infinity" then the UE shall set the Tsor-cm timer associated to the PDU session to infinity; or

- For all other cases, if a matching criterion is found then the UE shall set the Tsor-cm timer associated to the newly established PDU session, or service, with the exception that if the value of the Tsor-cm timer exceeds the highest value among the current values of all running Tsor-cm timers, then the value of the Tsor-cm timer for the new PDU session or service shall be set to the highest value among the current values of all running Tsor-cm timers.

NOTE 1: For newly established PDU session or service as described above, the timer is set irrespective of whether other ongoing PDU sessions or services that match the same criteria exist and for which corresponding Tsor-cm timers are running.

NOTE 2: NAS 5GMM layer will receive an explicit indication from the upper layers that a service is started or stopped. When a service is started, it is handled as a new service in the procedures described in this subclause.

NOTE 3: While one or more Tsor-cm timers are running, the UE can trigger any 5GSM procedure or start new services.

While one or more Tsor-cm timers are running, upon receiving a new SOR-CMCI as described in annex C.3, the UE shall check if there is a matching criterion found for any ongoing PDU session or service in the new SOR-CMCI:

- if the UE has a configured "user controlled list of services exempted from release due to SOR" and a matching criterion is found for a service included in the "user controlled list of services exempted from release due to SOR", the UE shall set the Tsor-cm timer associated to the service to infinity;

- if a matching criterion is found and the value of Tsor-cm timer in the new SOR-CMCI indicates the value "infinity", then the Tsor-cm timer value for the associated PDU session or service shall be set to infinity;

- if a matching criterion is found and the value of Tsor-cm timer in the new SOR-CMCI is other than infinity and is smaller than the current value of the running Tsor-cm timer for the associated PDU session or service, then the Tsor-cm timer value for the associated PDU session or service shall be replaced with the value in the new SOR-CMCI without stopping and restarting the timer; or

- for all other cases, the running Tsor-cm timers for the associated PDU sessions or services are kept unchanged.

The timer Tsor-cm shall be stopped when the associated PDU session is released or the associated service is stopped.

If the UE enters idle mode or 5GMM-CONNECTED mode with RRC inactive indication (see 3GPP TS 24.501 [64]), while one or more Tsor-cm timers are running, then the UE stops the timer(s). In this case, if:

a) the UE has a list of available and allowable PLMNs in the area and based on this list or any other implementation specific means, the UE determines that there is a higher priority PLMN than the selected VPLMN; or

b) the UE does not have a list of available and allowable PLMNs in the area and is unable to determine whether there is a higher priority PLMN than the selected VPLMN using any other implementation specific means;

then the UE attempts to obtain service on a higher priority PLMN as specified in subclause 4.4.3.3 by acting as if timer T that controls periodic attempts has expired.

When the last running Tsor-cm timer is stopped due to release of the associated PDU sessions or stop of associated servicesor the last running Tsor-cm timer expires, if:

i) the UE has a list of available and allowable PLMNs in the area and based on this list or any other implementation specific means, the UE determines that there is a higher priority PLMN than the selected VPLMN; or

ii) the UE does not have a list of available and allowable PLMNs in the area and is unable to determine whether there is a higher priority PLMN than the selected VPLMN using any other implementation specific means;

then the UE shall perform the deregistration procedure (see clause 4.2.2.3 of 3GPP TS 23.502 [63]) that releases all the established PDU sessions, if any, and the UE enters idle mode and attempts to obtain service on a higher priority PLMN as specified in subclause 4.4.3.3 by acting as if timer T that controls periodic attempts has expired.

NOTE 4: The list of available and allowable PLMNs in the area is implementation specific.

The UE which has an emergency PDU session, receives a request from the upper layers to establish an emergency PDU session or perform emergency services fallback, registers for emergency services, or is configured for high priority access in the selected PLMN is not required to enter idle mode the last running Tsor-cm timer stops or expires. The UE shall attempt to perform the PLMN selection after the emergency PDU session or the high priority service is released, if any Tsor-cm timer was running and the last running Tsor-cm timer stopped or expired when the emergency PDU session or the high priority service was established and after the UE enters idle mode or 5GMM-CONNECTED mode with RRC inactive indication (see 3GPP TS 24.501 [64]).

\*\*\*\*\* End of change \*\*\*\*\*