**3GPP TSG-CT WG1 Meeting #134-eC1-221118-r1**

**E-Meeting, 17th – 25th February 2022**

**Source: Huawei, HiSilicon**

**Title: UE** **reachability status monitoring**

**Spec: 3GPP TS 24.538**

**Agenda item: 17.2.30**

**Document for: Approval**

**1. Introduction**

This pCR proposes to remove the clause of UE reachability status monitoring.

**2. Reason for Change**

Based on the discussion during CT1#134e, the UE monitoring only needs MSGin5G Server to interact with network (SCEF/NEF), no additional procedure between MSGin5G Client and MSGin5G Server is needed, it’s not in the scope of CT1.

**3. Conclusions**

<Conclusion part (optional)>

**4. Proposal**

It is proposed to agree the following changes to 3GPP TS 24.538 v0.3.0

\* \* \* First Change \* \* \* \*

## 6.7 Void

\* \* \* End of Changes \* \* \* \*