**3GPP TSG-CT WG1 Meeting #135-eC1-222843**

**E-Meeting, 6th – 12th April 2022**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **24.554** | **CR** | **0047** | **rev** | **-** | **Current version:** | **17.0.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** |  | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** |  | | | | | | | | | |
| ***Source to TSG:*** | C1 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** |  | | | | |  | ***Date:*** | | |  |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | |  |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | According to TS 33.503, during the procedure of PDU session secondary authentication of 5G ProSe layer-3 remote UE, upon successful security establishment, the 5G ProSe layer-3 UE-to-network relay sends a DCA (Direct Communication Accept) message that may include an indication that a PDU Session with secondary authentication is pending. Based on the indication in the DCA message, the 5G ProSe Remote UE may refrain from sending any data traffic over the PC5 link until successful completion of subsequent PDU Session secondary authentication.  Hence, the corresponding indication IE needs to be defined in this specification. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Define the new IE Pending indication information element which indicates that PDU session authentication and authorization procedure for the 5G ProSe layer-3 remote UE via 5G ProSe layer-3 UE-to-network relay is pending. This IE may be included in the PROSE DIRECT LINK ESTABLISHMENT ACCEPT message. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | An indication that a PDU Session with secondary authentication is pending is not supported in PROSE DIRECT LINK ESTABLISHMENT ACCEPT message. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 7.2.2.3, 7.2.2.4, 10.3.2.1, 11.3.xx (new) | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

**\*\*\*\*\*\*\***

\* \* \* First Change \* \* \* \*

#### 7.2.2.3 5G ProSe direct link establishment procedure accepted by the target UE

Upon receipt of a PROSE DIRECT LINK ESTABLISHMENT REQUEST message, if the target UE accepts this request, the target UE shall uniquely assign a PC5 link identifier, create a 5G ProSe direct link context.

If the PROSE DIRECT LINK ESTABLISHMENT REQUEST message is not used for 5G ProSe direct communication between the remote UE and the UE-to-network relay UE, the target UE assigns a layer-2 ID for this 5G ProSe direct link. The newly assigned layer-2 ID replaces the target layer-2 ID as received on the PROSE DIRECT LINK ESTABLISHMENT REQUEST message. Then the target UE shall store this assigned layer-2 ID and the source layer-2 ID used in the transport of this message provided by the lower layers in the 5G ProSe direct link context.

The target UE may initiate 5G ProSe direct link authentication procedure as specified in clause 7.2.12 and shall initiate 5G ProSe direct link security mode control procedure as specified in clause 7.2.10.

NOTE 1: It is possible for the target UE to reuse the target UE's layer-2 ID used in the transport of the PROSE DIRECT LINK ESTABLISHMENT REQUEST message provided by the lower layers in case that the target UE's layer-2 ID has been used in previous 5G ProSe direct link with the same peer.

If:

a) the target user info IE is included in the PROSE DIRECT LINK ESTABLISHMENT REQUEST message and this IE includes the target UE's application layer ID; or

b) the target user info IE is not included in the PROSE DIRECT LINK ESTABLISHMENT REQUEST message and the target UE is interested in the ProSe application(s) identified by the ProSe identifier IE in the PROSE DIRECT LINK ESTABLISHMENT REQUEST message;

then the target UE shall either:

a) identify an existing KNRP based on the KNRP ID included in the PROSE DIRECT LINK ESTABLISHMENT REQUEST message; or

b) if KNRP ID is not included in the PROSE DIRECT LINK ESTABLISHMENT REQUEST message, the target UE does not have an existing KNRP for the KNRP ID included in PROSE DIRECT LINK ESTABLISHMENT REQUEST message or the target UE wishes to derive a new KNRP, derive a new KNRP. This may require performing one or more 5G ProSe direct link authentication procedures as specified in clause 7.2.12.

NOTE 2: How many times the 5G ProSe direct link authentication procedure needs to be performed to derive a new KNRP depends on the authentication method used.

After an existing KNRP was identified or a new KNRP was derived, the target UE shall initiate a 5G ProSe direct link security mode control procedure as specified in clause 7.2.10.

Upon successful completion of the 5G ProSe direct link security mode control procedure, in order to determine whether the PROSE DIRECT LINK ESTABLISHMENT REQUEST message can be accepted or not, in case of IP communication, the target UE checks whether there is at least one common IP address configuration option supported by both the initiating UE and the target UE.

Before sending the PROSE DIRECT LINK ESTABLISHMENT ACCEPT message to the remote UE, the target UE acting as a 5G ProSe layer-3 UE-to-network relay UE shall inform the lower layer to initiate the UE requested PDU session establishment procedure as specified in 3GPP TS 24.501 [11] if:

1) the PDU session for relaying the service associated with the RSC has not been established yet; or

2) the PDU session for relaying the service associated with the RSC has been established but the PDU session type is Unstructured.

If the target UE accepts the 5G ProSe direct link establishment procedure, the target UE shall create a PROSE DIRECT LINK ESTABLISHMENT ACCEPT message. The target UE:

a) shall include the source user info set to the target UE's application layer ID received from upper layers;

b) shall include PQFI(s), the corresponding PC5 QoS parameters and optionally the ProSe identifier(s) that the target UE accepts, if the target UE is not acting as a 5G ProSe layer-2 UE-to-network relay UE;

c) may include the PC5 QoS rule(s) if the target UE is not acting as a 5G ProSe layer-2 UE-to-network relay UE;

d) shall include an IP address configuration IE set to one of the following values if IP communication is used and the target UE is not acting as a 5G ProSe layer-2 UE-to-network relay UE:

1) "DHCPv4 server" if only IPv4 address allocation mechanism is supported by the target UE, i.e., acting as a DHCPv4 server; or

2) "IPv6 router" if only IPv6 address allocation mechanism is supported by the target UE, i.e., acting as an IPv6 router; or

3) "DHCPv4 server & IPv6 Router" if both IPv4 and IPv6 address allocation mechanism are supported by the target UE; or

4) "address allocation not supported" if neither IPv4 nor IPv6 address allocation mechanism is supported by the target UE and the target UE is not acting as a 5G ProSe layer-3 UE-to-network relay UE;

NOTE: The UE doesn't include an IP address configuration IE nor a link local IPv6 address IE, if Ethernet or Unstructured data unit type is used for communication.

e) shall include a link local IPv6 address IE formed locally based on IETF RFC 4862 [16] if IP address configuration IE is set to "address allocation not supported", the received PROSE DIRECT LINK SECURITY MODE COMPLETE message included a link local IPv6 address IE and the target UE is neither acting as a 5G ProSe layer-2 UE-to-network relay UE nor acting as a 5G ProSe layer-3 relay UE;

f) shall include the configuration of UE PC5 unicast user plane security protection based on the agreed user plane security policy, as specified in 3GPP TS 33.503 [34]; and

x) may include the Pending indication IE set to "PDU session authentication and authorization procedure for the 5G ProSe layer-3 remote UE is pending" if the remote UE id and EAP message is received in a PDU session authentication command message as specified in 3GPP TS 24.501 [11] and the target UE is acting as a 5G ProSe layer-3 UE-to-network relay UE.

After the PROSE DIRECT LINK ESTABLISHMENT ACCEPT message is generated, the target UE shall pass this message to the lower layers for transmission along with the initiating UE's layer-2 ID for unicast communication and the target UE's layer-2 ID for unicast communication, and shall start timer T5090 if at least one of ProSe identifiers for the 5G ProSe direct links satisfies the privacy requirements as specified in clause 5.2.

After sending the PROSE DIRECT LINK ESTABLISHMENT ACCEPT message, the target UE shall provide the following information along with the layer-2 IDs to the lower layer, which enables the lower layer to handle the coming PC5 signalling or traffic data:

a) the PC5 link identifier self-assigned for this 5G ProSe direct link;

b) PQFI(s) and its corresponding PC5 QoS parameters, if available; and

c) an indication of activation of the PC5 unicast user plane security protection for the 5G ProSe direct link, if applicable.

If the target UE accepts the 5G ProSe direct link establishment request and the 5G ProSe direct link is established not for 5G ProSe direct communication between the 5G ProSe remote UE and the 5G ProSe UE-to-network relay UE, then the target UE may perform the PC5 QoS flow establishment over 5G ProSe direct link as specified in clause 7.2.7. If the 5G ProSe direct link is established for 5G ProSe direct communication between the 5G ProSe layer-3 remote UE and the 5G ProSe layer-3 UE-to-network relay UE, then the target UE may perform the PC5 QoS flow establishment over 5G ProSe direct link as specified in clause 8.2.6.

\* \* \* Next Change \* \* \* \*

#### 7.2.2.4 5G ProSe direct link establishment procedure completion by the initiating UE

If the Target user info IE is included in the PROSE DIRECT LINK ESTABLISHMENT REQUEST message, upon receipt of the PROSE DIRECT LINK ESTABLISHMENT ACCEPT message, the initiating UE shall stop timer T5080. If the Target user info IE is not included in the PROSE DIRECT LINK ESTABLISHMENT REQUEST message the initiating UE may keep the timer T5080 running and continue to handle multiple response messages (i.e., the PROSE DIRECT LINK ESTABLISHMENT ACCEPT message) from multiple target UEs.

For each of the PROSE DIRECT LINK ESTABLISHMENT ACCEPT message received, the initiating UE shall uniquely assign a PC5 link identifier and create a 5G ProSe direct link context for each of the 5G ProSe direct link(s). Then the initiating UE shall store the source layer-2 ID and the destination layer-2 ID used in the transport of this message provided by the lower layers in the 5G ProSe direct link context(s) to complete the establishment of the 5G ProSe direct link with the target UE(s). From this time onward the initiating UE shall use the established link(s) for ProSe direct communication over PC5 and additional PC5 signalling messages to the target UE(s).

After receiving the PROSE DIRECT LINK ESTABLISHMENT ACCEPT message, the initiating UE shall delete the old security context it has for the target UE and shall provide the following information along with the layer-2 IDs to the lower layer, which enables the lower layer to handle the coming PC5 signalling or traffic data:

a) the PC5 link identifier self-assigned for this 5G ProSe direct link;

b) PQFI(s) and its corresponding PC5 QoS parameters, if available; and

c) an indication of activation of the PC5 unicast user plane security protection for the 5G ProSe direct link, if applicable.

If the Pending indication IE set to "PDU session authentication and authorization procedure for the 5G ProSe layer-3 remote UE is pending" is received in the PROSE DIRECT LINK ESTABLISHMENT ACCEPT message and the initiating UE is acting as a 5G ProSe layer-3 remote UE, the initiating UE may refrain from sending any PC5 user plane data until receipt of EAP-success message from the network via the target UE acting as a 5G ProSe layer-3 UE-to-network relay UE.

The initiating UE shall start timer T5090 if at least one of ProSe identifiers for the 5G ProSe direct links satisfies the privacy requirements as specified in clause 5.2.

In addition, the initiating UE may perform the PC5 QoS flow establishment over 5G ProSe direct link as specified in clause 7.2.7.

Upon expiry of the timer T5080, if the PROSE DIRECT LINK ESTABLISHMENT REQUEST message did not include the Target user info IE, and the initiating UE received at least one PROSE DIRECT LINK ESTABLISHMENT ACCEPT message, it is up to the UE implementation to consider the 5G ProSe direct link establishment procedure as complete or to restart the timer T5080.

\* \* \* Next Change \* \* \* \*

#### 10.3.2.1 Message definition

This message is sent by a UE to another peer UE to accept the received PROSE DIRECT LINK ESTABLISHMENT REQUEST message. See table 10.3.2.1.1.

Message type: PROSE DIRECT LINK ESTABLISHMENT ACCEPT

Significance: dual

Direction: UE to peer UE

Table 10.3.2.1.1: PROSE DIRECT LINK ESTABLISHMENT ACCEPT message content

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| IEI | Information Element | Type/Reference | Presence | Format | Length |
|  | PROSE DIRECT LINK ESTABLISHMENT ACCEPT message identity | ProSe PC5 signalling message type  11.3.1 | M | V | 1 |
|  | Sequence number | Sequence number  11.3.2 | M | V | 1 |
|  | Source user info | Application layer ID  11.3.4 | M | LV | 2-256 |
|  | Configuration of UE PC5 unicast user plane security protection | Configuration of UE PC5 unicast user plane security protection  11.3.23 | M | V | 1 |
| 79 | QoS flow descriptions | PC5 QoS flow descriptions  11.3.5 | O | TLV-E | 6-65538 |
| 7C | QoS rules | PC5 QoS rules  11.3.x | O | TLV-E | 7-65538 |
| 62 | IP address configuration | IP address configuration  11.3.6 | O | TV | 2 |
| 61 | Target link local IPv6 address | Link local IPv6 address  11.3.7 | O | TV | 17 |
| xx | Pending indication | Pending indication  11.3.x | O | TV | 1 |

\* \* \* Next Change \* \* \* \*

### 11.3.xx Pending indication

The purpose of the Pending indication information element is to indicate that PDU session authentication and authorization procedure for the 5G ProSe layer-3 remote UE via 5G ProSe layer-3 UE-to-network relay is pending.

The Pending indication information element is coded as shown in figure 9.11.3.xx.1 and table 9.11.3.xx.1.

The Pending indication is a type 1 information element.

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 8 | 7 | 6 | 5 | 4 | 3 | 2 | 1 |  |
| Pending indication IEI | | | | 0  Spare | 0  Spare | 0 | PI | octet 1 |

Figure 11.3.xx.1: Pending indication

Table 11.3.xx.1: Pending indication information element

|  |
| --- |
| Pending indication (PI) (octet 1, bit 1)  Bit  **1**  0 PDU session authentication and authorization procedure for the 5G ProSe layer-3 remote UE is not pending.  1 PDU session authentication and authorization procedure for the 5G ProSe layer-3 remote UE is pending.  Bits 2 to 4 of octet 1 are spare and shall be coded as zero. |
|  |

\* \* \* End of Changes \* \* \* \*