**3GPP TSG-CT WG1 Meeting #138-eC1-225535**

**E-Meeting, 10th – 14th October 2022**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **24.193** | **CR** | **0098** | **rev** | **-** | **Current version:** | **17.6.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  |  |
|  |  |
| ***Source to WG:*** | Huawei, HiSilicon, Ericsson |
| ***Source to TSG:*** | CT1 |
|  |  |
| ***Work item code:*** | ATSSS\_Ph2 |  | ***Date:*** | 2022-09-27 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | The specification contains an editor’s note on optional backoff timer for PMFP UAD under clause 6.2.1.13.1, quote:CT1 sent an LS to SA2 (in C1-223974), quote:The reply LS from SA2 (in S2-2207696) does not provide answer about the optional wait timer . However, since Rel-17 has become frozen it is proposed to remove the editor’s note on optional backoff timer for PMFP UAD. |
|  |  |
| ***Summary of change:*** | The editor’s note on optional backoff timer for PMFP UAD is removed. |
|  |  |
| ***Consequences if not approved:*** | Editor’s note remains in the Rel-17 version of the specification when it can be resolved by removing it. |
|  |  |
| ***Clauses affected:*** | 6.2.1.13.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **x** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

\* \* \* First Change \* \* \* \*

##### 6.2.1.13.1 Message definition

The PMFP UAD PROVISIONING COMPLETE message is sent by the UPF to the UE as response to PMFP UAD PROVISIONING message.

See table 6.2.1.13.1-1.

Message type: PMFP UAD PROVISIONING COMPLETE

Significance: dual

Direction: network to UE

Table 6.2.1.13.1-1: PMFP UAD PROVISIONING COMPLETE message content

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| IEI | Information Element | Type/Reference | Presence | Format | Length |
|  | PMFP UAD provisioning complete message identity | Message type6.2.2.1 | M | V | 1 |
|  | EPTI | Extended procedure transaction identity6.2.2.2 | M | V | 2 |

Editor's note [WI: ATSSS-Ph2, CR#96]: Whether an indication of whether the UPF aligns the DL traffic distribution based on the UE request is provided in the message is FFS.

\* \* \* End of Changes \* \* \* \*